IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView_V2.0]"
File name: "Project Number"
Time stamp: "2016-12-30T10:38:00"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.07 : 28 Aug 2013"
Originating system: "20150714_1515(x64) - Exporter 16.5.0.0 - Alternate UI 16.5.0.0"
Application: "Autodesk Revit 2016 (ENU)" version "2016" identifier "Revit" by Organization "Autodesk Revit 2016 (ENU)"

People and organizations
  Person "ryan@openingdesign.com" of Organization (no name given)
  Owner history of Person "ryan@openingdesign.com" of Organization (no name given) | application "Autodesk Revit 2016 (ENU)" version "2016" identifier "Revit" by Organization "Autodesk Revit 2016 (ENU)" | change NOCHANGE | created 1483112830 (2016-12-30T15:47:10Z)

Units
  LENGTHUNIT: FOOT (conversion based)
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"

Spatial structure
IFCPROJECT "Project Number" | long name "Project Name" | phase "Project Status"
  IFCSITE "Default" | latitude 42° 21′ 30.344238″ | longitude -71° 3′ 35.194702″ | elevation above sea level 0.
    IFCBUILDING | postal address: "Enter address here", "<Default>"
      IFCBUILDINGSTOREY "Level 1" | long name "Level 1" | elevation 0.
        contains 53 elements
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Rigid insulation 002:Rigid insulation 002:155913" | object type "Rigid insulation 002:155913 : Rigid insulation 002:Rigid insulation 002:155913" | names: "Rigid insulation 002:Rigid insulation 002:155913:Rigid insulation 002:155913 : Rigid insulation 002:Rigid insulation 002:155913:154955" | material: "EXISTING RIGID INSULATION AT ROOF (PATCH AND REPAIR AS NECESSARY)" | property sets: Pset_BuildingElementProxyCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Wood block 002:Wood block 002:155927" | object type "Wood block 002:155927 : Wood block 002:Wood block 002:155927" | names: "Wood block 002:Wood block 002:155927:Wood block 002:155927 : Wood block 002:Wood block 002:155927:154973" | material: "PRESSURE TREATED WOOD BLOCKING - SIZE AS NECESSARY" | property sets: Pset_BuildingElementProxyCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Sealant 002:Sealant 002:155941" | object type "Sealant 002:155941 : Sealant 002:Sealant 002:155941" | names: "Sealant 002:Sealant 002:155941:Sealant 002:155941 : Sealant 002:Sealant 002:155941:154987" | material: "SEALANT & BACKER ROD, IF NECESSARY" | property sets: Pset_BuildingElementProxyCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Aluminium profile 002:Aluminium profile 002:155954" | object type "Aluminium profile 002:155954 : Aluminium profile 002:Aluminium profile 002:155954" | names: "Aluminium profile 002:Aluminium profile 002:155954:Aluminium profile 002:155954 : Aluminium profile 002:Aluminium profile 002:155954:155000" | material: "IfcSurfaceStyle #179" | property sets: Pset_BuildingElementProxyCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Concrete wall 002:Concrete wall 002:155970" | object type "Concrete wall 002:155970 : Concrete wall 002:Concrete wall 002:155970" | names: "Concrete wall 002:Concrete wall 002:155970:Concrete wall 002:155970 : Concrete wall 002:Concrete wall 002:155970:155016" | material: "_EXISTING CAST-IN-PLACE CONCRETE" | property sets: Pset_BuildingElementProxyCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "WRB Membrane 002:WRB Membrane 002:155984" | object type "WRB Membrane 002:155984 : WRB Membrane 002:WRB Membrane 002:155984" | names: "WRB Membrane 002:WRB Membrane 002:155984:WRB Membrane 002:155984 : WRB Membrane 002:WRB Membrane 002:155984:155030" | material: "IMPERMEABLE WRB MEMBRANE" | property sets: Pset_BuildingElementProxyCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Cement bond coat 002:Cement bond coat 002:155998" | object type "Cement bond coat 002:155998 : Cement bond coat 002:Cement bond coat 002:155998" | names: "Cement bond coat 002:Cement bond coat 002:155998:Cement bond coat 002:155998 : Cement bond coat 002:Cement bond coat 002:155998:155044" | material: "IMPERMEABLE WRB MEMBRANE" | property sets: Pset_BuildingElementProxyCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "TPO Membrane 002:TPO Membrane 002:156012" | object type "TPO Membrane 002:156012 : TPO Membrane 002:TPO Membrane 002:156012" | names: "TPO Membrane 002:TPO Membrane 002:156012:TPO Membrane 002:156012 : TPO Membrane 002:TPO Membrane 002:156012:155058" | material: "PRESSURE TREATED WOOD BLOCKING - SIZE AS NECESSARY" | property sets: Pset_BuildingElementProxyCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Scratch coat 002:Scratch coat 002:156030" | object type "Scratch coat 002:156030 : Scratch coat 002:Scratch coat 002:156030" | names: "Scratch coat 002:Scratch coat 002:156030:Scratch coat 002:156030 : Scratch coat 002:Scratch coat 002:156030:155078" | material: "SEALANT & BACKER ROD, IF NECESSARY" | property sets: Pset_BuildingElementProxyCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Porcelain tiles 002:Porcelain tiles 002:156044" | object type "Porcelain tiles 002:156044 : Porcelain tiles 002:Porcelain tiles 002:156044" | names: "Porcelain tiles 002:Porcelain tiles 002:156044:Porcelain tiles 002:156044 : Porcelain tiles 002:Porcelain tiles 002:156044:155092" | material: "(CT-01) PORCELAIN WALL TILE" | property sets: Pset_BuildingElementProxyCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Counter flashing 002:Counter flashing 002:156072" | object type "Counter flashing 002:156072 : Counter flashing 002:Counter flashing 002:156072" | names: "Counter flashing 002:Counter flashing 002:156072:Counter flashing 002:156072 : Counter flashing 002:Counter flashing 002:156072:155120" | material: "SHEET METAL COPING" | property sets: Pset_BuildingElementProxyCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Front flashing 002:Front flashing 002:156098" | object type "Front flashing 002:156098 : Front flashing 002:Front flashing 002:156098" | names: "Front flashing 002:Front flashing 002:156098:Front flashing 002:156098 : Front flashing 002:Front flashing 002:156098:155127" | material: "SHEET METAL COPING" | property sets: Pset_BuildingElementProxyCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Top sealant 002:Top sealant 002:156116" | object type "Top sealant 002:156116 : Top sealant 002:Top sealant 002:156116" | names: "Top sealant 002:Top sealant 002:156116:Top sealant 002:156116 : Top sealant 002:Top sealant 002:156116:155145" | material: "SET IN BED OF SEALANT" | property sets: Pset_BuildingElementProxyCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Metal lath 002:Metal lath 002:156155" | object type "Metal lath 002:156155 : Metal lath 002:Metal lath 002:156155" | names: "Metal lath 002:Metal lath 002:156155:Metal lath 002:156155 : Metal lath 002:Metal lath 002:156155:155166" | material: "SEALANT & BACKER ROD, IF NECESSARY" | property sets: Pset_BuildingElementProxyCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Mortar bed 002:Mortar bed 002:156169" | object type "Mortar bed 002:156169 : Mortar bed 002:Mortar bed 002:156169" | names: "Mortar bed 002:Mortar bed 002:156169:Mortar bed 002:156169 : Mortar bed 002:Mortar bed 002:156169:155180" | material: "MORTAR BED" | property sets: Pset_BuildingElementProxyCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Mortar bed 1:Mortar bed 002:158850" | object type "Mortar bed 002:158850 : Mortar bed 1:Mortar bed 002:158850" | names: "Mortar bed 1:Mortar bed 002:158850:Mortar bed 002:158850 : Mortar bed 1:Mortar bed 002:158850:155194" | material: "1/4" PRESSURE TREATED PLYWOOD (PROTECTION BOARD OVER EXISTING CONCRETE)" | property sets: Pset_BuildingElementProxyCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Concrete wall001" | object type "Concrete wall001" | names: "Concrete wall001:Concrete wall001:155208" | material: "PRESSURE TREATED WOOD BLOCKING - SIZE AS NECESSARY" | property sets: Pset_BuildingElementProxyCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Metal stud 015" | object type "Metal stud 015" | names: "Metal stud 015:Metal stud 015:155222" | material: "METAL STUDS" | property sets: Pset_BuildingElementProxyCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Insulation horizontal001" | object type "Insulation horizontal001" | names: "Insulation horizontal001:Insulation horizontal001:155240" | material: "Rigid insulation" | property sets: Pset_BuildingElementProxyCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Insulation vertical001" | object type "Insulation vertical001" | names: "Insulation vertical001:Insulation vertical001:155279" | material: "Rigid insulation" | property sets: Pset_BuildingElementProxyCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Inner gypsum board001" | object type "Inner gypsum board001" | names: "Inner gypsum board001:Inner gypsum board001:155293" | material: "PRESSURE TREATED WOOD BLOCKING - SIZE AS NECESSARY" | property sets: Pset_BuildingElementProxyCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Inner ceiling001" | object type "Inner ceiling001" | names: "Inner ceiling001:Inner ceiling001:155307" | material: "PRESSURE TREATED WOOD BLOCKING - SIZE AS NECESSARY" | property sets: Pset_BuildingElementProxyCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Metal support for window frame001" | object type "Metal support for window frame001" | names: "Metal support for window frame001:Metal support for window frame001:155321" | material: "IfcSurfaceStyle #179" | property sets: Pset_BuildingElementProxyCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Outer ceiling001" | object type "Outer ceiling001" | names: "Outer ceiling001:Outer ceiling001:155335" | material: "PRESSURE TREATED WOOD BLOCKING - SIZE AS NECESSARY" | property sets: Pset_BuildingElementProxyCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Outer window frame001" | object type "Outer window frame001" | names: "Outer window frame001:Outer window frame001:155349" | material: "Window frame" | property sets: Pset_BuildingElementProxyCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Inner window frame001" | object type "Inner window frame001" | names: "Inner window frame001:Inner window frame001:155357" | material: "Window frame" | property sets: Pset_BuildingElementProxyCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Stud 004" | object type "Stud 004" | names: "Stud 004:Stud 004:155364" | material: "LIGHT GAUGE METAL STUDS AND/OR FURRING" | property sets: Pset_BuildingElementProxyCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Stud 003" | object type "Stud 003" | names: "Stud 003:Stud 003:155382" | material: "LIGHT GAUGE METAL STUDS AND/OR FURRING" | property sets: Pset_BuildingElementProxyCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Metal stud 014" | object type "Metal stud 014" | names: "Metal stud 014:Metal stud 014:155400" | material: "METAL STUDS" | property sets: Pset_BuildingElementProxyCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Metal stud 016" | object type "Metal stud 016" | names: "Metal stud 016:Metal stud 016:155418" | material: "METAL STUDS" | property sets: Pset_BuildingElementProxyCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Metal stud 011" | object type "Metal stud 011" | names: "Metal stud 011:Metal stud 011:155436" | material: "METAL STUDS" | property sets: Pset_BuildingElementProxyCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Metal stud 010" | object type "Metal stud 010" | names: "Metal stud 010:Metal stud 010:155454" | material: "METAL STUDS" | property sets: Pset_BuildingElementProxyCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Metal stud 009" | object type "Metal stud 009" | names: "Metal stud 009:Metal stud 009:155472" | material: "METAL STUDS" | property sets: Pset_BuildingElementProxyCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Metal stud 013" | object type "Metal stud 013" | names: "Metal stud 013:Metal stud 013:155490" | material: "METAL STUDS" | property sets: Pset_BuildingElementProxyCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Metal stud 012" | object type "Metal stud 012" | names: "Metal stud 012:Metal stud 012:155508" | material: "METAL STUDS" | property sets: Pset_BuildingElementProxyCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Window glass001" | object type "Window glass001" | names: "Window glass001:Window glass001:155526" | material: "Clear glass" | property sets: Pset_BuildingElementProxyCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Window frame lock001" | object type "Window frame lock001" | names: "Window frame lock001:Window frame lock001:155541" | material: "Window frame" | property sets: Pset_BuildingElementProxyCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Rysysta panel 006" | object type "Rysysta panel 006" | names: "Rysysta panel 006:Rysysta panel 006:155555" | material: "Rysysta" | property sets: Pset_BuildingElementProxyCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Rysysta panel 005" | object type "Rysysta panel 005" | names: "Rysysta panel 005:Rysysta panel 005:155578" | material: "Rysysta" | property sets: Pset_BuildingElementProxyCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Rysysta panel 007" | object type "Rysysta panel 007" | names: "Rysysta panel 007:Rysysta panel 007:155600" | material: "Rysysta" | property sets: Pset_BuildingElementProxyCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Rysysta panel 008" | object type "Rysysta panel 008" | names: "Rysysta panel 008:Rysysta panel 008:155622" | material: "Rysysta" | property sets: Pset_BuildingElementProxyCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Rysysta fixation device 010" | object type "Rysysta fixation device 010" | names: "Rysysta fixation device 010:Rysysta fixation device 010:155629" | material: "IfcSurfaceStyle #179" | property sets: Pset_BuildingElementProxyCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Rysysta fixation device 007" | object type "Rysysta fixation device 007" | names: "Rysysta fixation device 007:Rysysta fixation device 007:155651" | material: "IfcSurfaceStyle #179" | property sets: Pset_BuildingElementProxyCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Rysysta fixation device 008" | object type "Rysysta fixation device 008" | names: "Rysysta fixation device 008:Rysysta fixation device 008:155673" | material: "IfcSurfaceStyle #179" | property sets: Pset_BuildingElementProxyCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Rysysta fixation device 011" | object type "Rysysta fixation device 011" | names: "Rysysta fixation device 011:Rysysta fixation device 011:155695" | material: "IfcSurfaceStyle #179" | property sets: Pset_BuildingElementProxyCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Rysysta fixation device 009" | object type "Rysysta fixation device 009" | names: "Rysysta fixation device 009:Rysysta fixation device 009:155717" | material: "IfcSurfaceStyle #179" | property sets: Pset_BuildingElementProxyCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Rysysta fixation device 012" | object type "Rysysta fixation device 012" | names: "Rysysta fixation device 012:Rysysta fixation device 012:155739" | material: "IfcSurfaceStyle #179" | property sets: Pset_BuildingElementProxyCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "WRB Membrane 004" | object type "WRB Membrane 004" | names: "WRB Membrane 004:WRB Membrane 004:155761" | material: "IMPERMEABLE WRB MEMBRANE" | property sets: Pset_BuildingElementProxyCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "L-shaped aluminium profile 003" | object type "L-shaped aluminium profile 003" | names: "L-shaped aluminium profile 003:L-shaped aluminium profile 003:155775" | material: "IMPERMEABLE WRB MEMBRANE" | property sets: Pset_BuildingElementProxyCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Flashing 003" | object type "Flashing 003" | names: "Flashing 003:Flashing 003:155791" | material: "IMPERMEABLE WRB MEMBRANE" | property sets: Pset_BuildingElementProxyCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Counter-flashing 003" | object type "Counter-flashing 003" | names: "Counter-flashing 003:Counter-flashing 003:155798" | material: "IMPERMEABLE WRB MEMBRANE" | property sets: Pset_BuildingElementProxyCommon
          2 x IFCANNOTATION

Types
  IFCBUILDINGELEMENTPROXYTYPE "Rigid insulation 002:Rigid insulation 002:155913" | 1 occurrence | material: "EXISTING RIGID INSULATION AT ROOF (PATCH AND REPAIR AS NECESSARY)"
  IFCBUILDINGELEMENTPROXYTYPE "Wood block 002:Wood block 002:155927" | 1 occurrence | material: "PRESSURE TREATED WOOD BLOCKING - SIZE AS NECESSARY"
  IFCBUILDINGELEMENTPROXYTYPE "Sealant 002:Sealant 002:155941" | 1 occurrence | material: "SEALANT & BACKER ROD, IF NECESSARY"
  IFCBUILDINGELEMENTPROXYTYPE "Aluminium profile 002:Aluminium profile 002:155954" | 1 occurrence | material: "IfcSurfaceStyle #179"
  IFCBUILDINGELEMENTPROXYTYPE "Concrete wall 002:Concrete wall 002:155970" | 1 occurrence | material: "_EXISTING CAST-IN-PLACE CONCRETE"
  IFCBUILDINGELEMENTPROXYTYPE "WRB Membrane 002:WRB Membrane 002:155984" | 1 occurrence | material: "IMPERMEABLE WRB MEMBRANE"
  IFCBUILDINGELEMENTPROXYTYPE "Cement bond coat 002:Cement bond coat 002:155998" | 1 occurrence | material: "IMPERMEABLE WRB MEMBRANE"
  IFCBUILDINGELEMENTPROXYTYPE "TPO Membrane 002:TPO Membrane 002:156012" | 1 occurrence | material: "PRESSURE TREATED WOOD BLOCKING - SIZE AS NECESSARY"
  IFCBUILDINGELEMENTPROXYTYPE "Scratch coat 002:Scratch coat 002:156030" | 1 occurrence | material: "SEALANT & BACKER ROD, IF NECESSARY"
  IFCBUILDINGELEMENTPROXYTYPE "Porcelain tiles 002:Porcelain tiles 002:156044" | 1 occurrence | material: "(CT-01) PORCELAIN WALL TILE"
  IFCBUILDINGELEMENTPROXYTYPE "Counter flashing 002:Counter flashing 002:156072" | 1 occurrence | material: "SHEET METAL COPING"
  IFCBUILDINGELEMENTPROXYTYPE "Front flashing 002:Front flashing 002:156098" | 1 occurrence | material: "SHEET METAL COPING"
  IFCBUILDINGELEMENTPROXYTYPE "Top sealant 002:Top sealant 002:156116" | 1 occurrence | material: "SET IN BED OF SEALANT"
  IFCBUILDINGELEMENTPROXYTYPE "Metal lath 002:Metal lath 002:156155" | 1 occurrence | material: "SEALANT & BACKER ROD, IF NECESSARY"
  IFCBUILDINGELEMENTPROXYTYPE "Mortar bed 002:Mortar bed 002:156169" | 1 occurrence | material: "MORTAR BED"
  IFCBUILDINGELEMENTPROXYTYPE "Mortar bed 1:Mortar bed 002:158850" | 1 occurrence | material: "1/4" PRESSURE TREATED PLYWOOD (PROTECTION BOARD OVER EXISTING CONCRETE)"
  IFCBUILDINGELEMENTPROXYTYPE "Concrete wall001" | 1 occurrence | material: "PRESSURE TREATED WOOD BLOCKING - SIZE AS NECESSARY"
  IFCBUILDINGELEMENTPROXYTYPE "Metal stud 015" | 1 occurrence | material: "METAL STUDS"
  IFCBUILDINGELEMENTPROXYTYPE "Insulation horizontal001" | 1 occurrence | material: "Rigid insulation"
  IFCBUILDINGELEMENTPROXYTYPE "Insulation vertical001" | 1 occurrence | material: "Rigid insulation"
  IFCBUILDINGELEMENTPROXYTYPE "Inner gypsum board001" | 1 occurrence | material: "PRESSURE TREATED WOOD BLOCKING - SIZE AS NECESSARY"
  IFCBUILDINGELEMENTPROXYTYPE "Inner ceiling001" | 1 occurrence | material: "PRESSURE TREATED WOOD BLOCKING - SIZE AS NECESSARY"
  IFCBUILDINGELEMENTPROXYTYPE "Metal support for window frame001" | 1 occurrence | material: "IfcSurfaceStyle #179"
  IFCBUILDINGELEMENTPROXYTYPE "Outer ceiling001" | 1 occurrence | material: "PRESSURE TREATED WOOD BLOCKING - SIZE AS NECESSARY"
  IFCBUILDINGELEMENTPROXYTYPE "Outer window frame001" | 1 occurrence | material: "Window frame"
  IFCBUILDINGELEMENTPROXYTYPE "Inner window frame001" | 1 occurrence | material: "Window frame"
  IFCBUILDINGELEMENTPROXYTYPE "Stud 004" | 1 occurrence | material: "LIGHT GAUGE METAL STUDS AND/OR FURRING"
  IFCBUILDINGELEMENTPROXYTYPE "Stud 003" | 1 occurrence | material: "LIGHT GAUGE METAL STUDS AND/OR FURRING"
  IFCBUILDINGELEMENTPROXYTYPE "Metal stud 014" | 1 occurrence | material: "METAL STUDS"
  IFCBUILDINGELEMENTPROXYTYPE "Metal stud 016" | 1 occurrence | material: "METAL STUDS"
  IFCBUILDINGELEMENTPROXYTYPE "Metal stud 011" | 1 occurrence | material: "METAL STUDS"
  IFCBUILDINGELEMENTPROXYTYPE "Metal stud 010" | 1 occurrence | material: "METAL STUDS"
  IFCBUILDINGELEMENTPROXYTYPE "Metal stud 009" | 1 occurrence | material: "METAL STUDS"
  IFCBUILDINGELEMENTPROXYTYPE "Metal stud 013" | 1 occurrence | material: "METAL STUDS"
  IFCBUILDINGELEMENTPROXYTYPE "Metal stud 012" | 1 occurrence | material: "METAL STUDS"
  IFCBUILDINGELEMENTPROXYTYPE "Window glass001" | 1 occurrence | material: "Clear glass"
  IFCBUILDINGELEMENTPROXYTYPE "Window frame lock001" | 1 occurrence | material: "Window frame"
  IFCBUILDINGELEMENTPROXYTYPE "Rysysta panel 006" | 1 occurrence | material: "Rysysta"
  IFCBUILDINGELEMENTPROXYTYPE "Rysysta panel 005" | 1 occurrence | material: "Rysysta"
  IFCBUILDINGELEMENTPROXYTYPE "Rysysta panel 007" | 1 occurrence | material: "Rysysta"
  IFCBUILDINGELEMENTPROXYTYPE "Rysysta panel 008" | 1 occurrence | material: "Rysysta"
  IFCBUILDINGELEMENTPROXYTYPE "Rysysta fixation device 010" | 1 occurrence | material: "IfcSurfaceStyle #179"
  IFCBUILDINGELEMENTPROXYTYPE "Rysysta fixation device 007" | 1 occurrence | material: "IfcSurfaceStyle #179"
  IFCBUILDINGELEMENTPROXYTYPE "Rysysta fixation device 008" | 1 occurrence | material: "IfcSurfaceStyle #179"
  IFCBUILDINGELEMENTPROXYTYPE "Rysysta fixation device 011" | 1 occurrence | material: "IfcSurfaceStyle #179"
  IFCBUILDINGELEMENTPROXYTYPE "Rysysta fixation device 009" | 1 occurrence | material: "IfcSurfaceStyle #179"
  IFCBUILDINGELEMENTPROXYTYPE "Rysysta fixation device 012" | 1 occurrence | material: "IfcSurfaceStyle #179"
  IFCBUILDINGELEMENTPROXYTYPE "WRB Membrane 004" | 1 occurrence | material: "IMPERMEABLE WRB MEMBRANE"
  IFCBUILDINGELEMENTPROXYTYPE "L-shaped aluminium profile 003" | 1 occurrence | material: "IMPERMEABLE WRB MEMBRANE"
  IFCBUILDINGELEMENTPROXYTYPE "Flashing 003" | 1 occurrence | material: "IMPERMEABLE WRB MEMBRANE"
  IFCBUILDINGELEMENTPROXYTYPE "Counter-flashing 003" | 1 occurrence | material: "IMPERMEABLE WRB MEMBRANE"

Property sets
  Pset_BuildingElementProxyCommon | properties | on 2 objects (2 IFCBUILDINGELEMENTPROXY)
    Reference = "Mortar bed 002" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Reference = "Rigid insulation 002" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Reference = "Wood block 002" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Reference = "Sealant 002" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Reference = "Aluminium profile 002" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Reference = "Concrete wall 002" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Reference = "WRB Membrane 002" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Reference = "Cement bond coat 002" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon: 42 more contents on 42 objects not shown
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    NumberOfStoreys = 1 (IFCINTEGER)
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)