IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView_V2.0]"
File name: "Project Number"
Time stamp: "2017-01-02T15:07:15"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.07 : 28 Aug 2013"
Originating system: "20150714_1515(x64) - Exporter 16.5.0.0 - Alternate UI 16.5.0.0"
Application: "Autodesk Revit 2016 (ENU)" version "2016" identifier "Revit" by Organization "Autodesk Revit 2016 (ENU)"

People and organizations
  Person "ryan@openingdesign.com" of Organization (no name given)
  Owner history of Person "ryan@openingdesign.com" of Organization (no name given) | application "Autodesk Revit 2016 (ENU)" version "2016" identifier "Revit" by Organization "Autodesk Revit 2016 (ENU)" | change NOCHANGE | created 1483112830 (2016-12-30T15:47:10Z)

Units
  LENGTHUNIT: FOOT (conversion based)
  AREAUNIT: SQUARE FOOT (conversion based)
  VOLUMEUNIT: CUBIC FOOT (conversion based)
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"

Spatial structure
IFCPROJECT "Project Number" | long name "Project Name" | phase "Project Status"
  IFCSITE "Default" | latitude 42° 21′ 30.344238″ | longitude -71° 3′ 35.194702″ | elevation above sea level 0.
    IFCBUILDING | postal address: "Enter address here", "<Default>"
      IFCBUILDINGSTOREY "Level 1" | long name "Level 1" | elevation 0.
        contains 83 elements
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Rigid insulation 002:Rigid insulation 002:155913" | object type "Rigid insulation 002:155913 : Rigid insulation 002:Rigid insulation 002:155913" | names: "Rigid insulation 002:Rigid insulation 002:155913:Rigid insulation 002:155913 : Rigid insulation 002:Rigid insulation 002:155913:160341" | material: "EXISTING RIGID INSULATION AT ROOF (REPAIR/REPLACE AS NECESSARY) - (SLOPE TOWARD ROOF DRAINS)" | property sets: Pset_BuildingElementProxyCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Wood block 002:Wood block 002:155927" | object type "Wood block 002:155927 : Wood block 002:Wood block 002:155927" | names: "Wood block 002:Wood block 002:155927:Wood block 002:155927 : Wood block 002:Wood block 002:155927:160355" | material: "PRESSURE TREATED WOOD BLOCKING - SIZE AS NECESSARY" | property sets: Pset_BuildingElementProxyCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Aluminium profile 002:Aluminium profile 002:155954" | object type "Aluminium profile 002:155954 : Aluminium profile 002:Aluminium profile 002:155954" | names: "Aluminium profile 002:Aluminium profile 002:155954:Aluminium profile 002:155954 : Aluminium profile 002:Aluminium profile 002:155954:160382" | material: "3X5X1/4" ALUMINUM ANGLE" | property sets: Pset_BuildingElementProxyCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Concrete wall 002:Concrete wall 002:155970" | object type "Concrete wall 002:155970 : Concrete wall 002:Concrete wall 002:155970" | names: "Concrete wall 002:Concrete wall 002:155970:Concrete wall 002:155970 : Concrete wall 002:Concrete wall 002:155970:160398" | material: "_EXISTING CAST-IN-PLACE CONCRETE" | property sets: Pset_BuildingElementProxyCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "TPO Membrane 002:TPO Membrane 002:156012" | object type "TPO Membrane 002:156012 : TPO Membrane 002:TPO Membrane 002:156012" | names: "TPO Membrane 002:TPO Membrane 002:156012:TPO Membrane 002:156012 : TPO Membrane 002:TPO Membrane 002:156012:160440" | material: "TPO MEMBRANE ROOF MEMBRANE" | property sets: Pset_BuildingElementProxyCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Mortar bed 1:Mortar bed 002:158850" | object type "Mortar bed 002:158850 : Mortar bed 1:Mortar bed 002:158850" | names: "Mortar bed 1:Mortar bed 002:158850:Mortar bed 002:158850 : Mortar bed 1:Mortar bed 002:158850:160576" | material: "1/4" PRESSURE TREATED PLYWOOD (PROTECTION BOARD OVER EXISTING CONCRETE)" | property sets: Pset_BuildingElementProxyCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Concrete wall001" | object type "Concrete wall001" | names: "Concrete wall001:Concrete wall001:160590" | material: "PRESSURE TREATED WOOD BLOCKING - SIZE AS NECESSARY" | property sets: Pset_BuildingElementProxyCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Metal stud 015" | object type "Metal stud 015" | names: "Metal stud 015:Metal stud 015:160604" | material: "METAL STUDS" | property sets: Pset_BuildingElementProxyCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Insulation horizontal001" | object type "Insulation horizontal001" | names: "Insulation horizontal001:Insulation horizontal001:160622" | material: "Rigid insulation" | property sets: Pset_BuildingElementProxyCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Insulation vertical001" | object type "Insulation vertical001" | names: "Insulation vertical001:Insulation vertical001:160636" | material: "Rigid insulation" | property sets: Pset_BuildingElementProxyCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Inner gypsum board001" | object type "Inner gypsum board001" | names: "Inner gypsum board001:Inner gypsum board001:160650" | material: "PRESSURE TREATED WOOD BLOCKING - SIZE AS NECESSARY" | property sets: Pset_BuildingElementProxyCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Inner ceiling001" | object type "Inner ceiling001" | names: "Inner ceiling001:Inner ceiling001:160664" | material: "PRESSURE TREATED WOOD BLOCKING - SIZE AS NECESSARY" | property sets: Pset_BuildingElementProxyCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Metal support for window frame001" | object type "Metal support for window frame001" | names: "Metal support for window frame001:Metal support for window frame001:160678" | material: "IfcSurfaceStyle #179" | property sets: Pset_BuildingElementProxyCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Stud 004" | object type "Stud 004" | names: "Stud 004:Stud 004:160692" | material: "LIGHT GAUGE METAL STUDS AND/OR FURRING" | property sets: Pset_BuildingElementProxyCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Stud 003" | object type "Stud 003" | names: "Stud 003:Stud 003:160710" | material: "LIGHT GAUGE METAL STUDS AND/OR FURRING" | property sets: Pset_BuildingElementProxyCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Metal stud 014" | object type "Metal stud 014" | names: "Metal stud 014:Metal stud 014:160728" | material: "METAL STUDS" | property sets: Pset_BuildingElementProxyCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Metal stud 016" | object type "Metal stud 016" | names: "Metal stud 016:Metal stud 016:160746" | material: "METAL STUDS" | property sets: Pset_BuildingElementProxyCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Metal stud 011" | object type "Metal stud 011" | names: "Metal stud 011:Metal stud 011:160764" | material: "METAL STUDS" | property sets: Pset_BuildingElementProxyCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Metal stud 010" | object type "Metal stud 010" | names: "Metal stud 010:Metal stud 010:160782" | material: "METAL STUDS" | property sets: Pset_BuildingElementProxyCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Metal stud 009" | object type "Metal stud 009" | names: "Metal stud 009:Metal stud 009:160800" | material: "METAL STUDS" | property sets: Pset_BuildingElementProxyCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Metal stud 013" | object type "Metal stud 013" | names: "Metal stud 013:Metal stud 013:160818" | material: "METAL STUDS" | property sets: Pset_BuildingElementProxyCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Metal stud 012" | object type "Metal stud 012" | names: "Metal stud 012:Metal stud 012:160836" | material: "METAL STUDS" | property sets: Pset_BuildingElementProxyCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "WRB Membrane 004" | object type "WRB Membrane 004" | names: "WRB Membrane 004:WRB Membrane 004:160854" | material: "IMPERMEABLE WRB MEMBRANE (ANSI 118.10 OR BETTER) - COMPATIBLE W/ MORTAR BED" | property sets: Pset_BuildingElementProxyCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Flashing 003" | object type "Flashing 003" | names: "Flashing 003:Flashing 003:160868" | material: "IMPERMEABLE WRB MEMBRANE (ANSI 118.10 OR BETTER) - COMPATIBLE W/ MORTAR BED" | property sets: Pset_BuildingElementProxyCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Counter-flashing 003" | object type "Counter-flashing 003" | names: "Counter-flashing 003:Counter-flashing 003:160886" | material: "METAL COPING TO MATCH ADJACENT TILE COLOR (SLOPE BACK TOWARD ROOF)" | property sets: Pset_BuildingElementProxyCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Window frame 017" | object type "Window frame 017" | names: "Window frame 017:Window frame 017:160908" | material: "Window frame" | property sets: Pset_BuildingElementProxyCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Window frame 020" | object type "Window frame 020" | names: "Window frame 020:Window frame 020:160922" | material: "Window frame" | property sets: Pset_BuildingElementProxyCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Window frame 014" | object type "Window frame 014" | names: "Window frame 014:Window frame 014:160979" | material: "Window frame" | property sets: Pset_BuildingElementProxyCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Rysysta panel 021" | object type "Rysysta panel 021" | names: "Rysysta panel 021:Rysysta panel 021:161000" | material: "Rysysta" | property sets: Pset_BuildingElementProxyCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Rysysta panel 018" | object type "Rysysta panel 018" | names: "Rysysta panel 018:Rysysta panel 018:161044" | material: "Rysysta" | property sets: Pset_BuildingElementProxyCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Window frame 013" | object type "Window frame 013" | names: "Window frame 013:Window frame 013:161088" | material: "Window frame" | property sets: Pset_BuildingElementProxyCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Rysysta panel 015" | object type "Rysysta panel 015" | names: "Rysysta panel 015:Rysysta panel 015:161102" | material: "Rysysta" | property sets: Pset_BuildingElementProxyCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Glass panel 004" | object type "Glass panel 004" | names: "Glass panel 004:Glass panel 004:161160" | material: "Clear glass" | property sets: Pset_BuildingElementProxyCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Rysysta panel 019" | object type "Rysysta panel 019" | names: "Rysysta panel 019:Rysysta panel 019:161174" | material: "Rysysta" | property sets: Pset_BuildingElementProxyCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Rysysta panel 020" | object type "Rysysta panel 020" | names: "Rysysta panel 020:Rysysta panel 020:161218" | material: "Rysysta" | property sets: Pset_BuildingElementProxyCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Rysysta panel 024" | object type "Rysysta panel 024" | names: "Rysysta panel 024:Rysysta panel 024:161225" | material: "Rysysta" | property sets: Pset_BuildingElementProxyCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Rysysta panel 017" | object type "Rysysta panel 017" | names: "Rysysta panel 017:Rysysta panel 017:161269" | material: "Rysysta" | property sets: Pset_BuildingElementProxyCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Rysysta panel 014" | object type "Rysysta panel 014" | names: "Rysysta panel 014:Rysysta panel 014:161313" | material: "Rysysta" | property sets: Pset_BuildingElementProxyCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Rysysta panel 016" | object type "Rysysta panel 016" | names: "Rysysta panel 016:Rysysta panel 016:161357" | material: "Rysysta" | property sets: Pset_BuildingElementProxyCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Rysysta panel 023" | object type "Rysysta panel 023" | names: "Rysysta panel 023:Rysysta panel 023:161401" | material: "Rysysta" | property sets: Pset_BuildingElementProxyCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Rysysta panel 022" | object type "Rysysta panel 022" | names: "Rysysta panel 022:Rysysta panel 022:161445" | material: "Rysysta" | property sets: Pset_BuildingElementProxyCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Rysysta starter strip 006" | object type "Rysysta starter strip 006" | names: "Rysysta starter strip 006:Rysysta starter strip 006:161452" | material: "IfcSurfaceStyle #179" | property sets: Pset_BuildingElementProxyCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Rysysta panel 013" | object type "Rysysta panel 013" | names: "Rysysta panel 013:Rysysta panel 013:161470" | material: "Rysysta" | property sets: Pset_BuildingElementProxyCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Rysysta starter strip 004" | object type "Rysysta starter strip 004" | names: "Rysysta starter strip 004:Rysysta starter strip 004:161514" | material: "IfcSurfaceStyle #179" | property sets: Pset_BuildingElementProxyCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Rysysta starter strip 005" | object type "Rysysta starter strip 005" | names: "Rysysta starter strip 005:Rysysta starter strip 005:161532" | material: "IfcSurfaceStyle #179" | property sets: Pset_BuildingElementProxyCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Window frame 015" | object type "Window frame 015" | names: "Window frame 015:Window frame 015:161550" | material: "Window frame" | property sets: Pset_BuildingElementProxyCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Window frame 018" | object type "Window frame 018" | names: "Window frame 018:Window frame 018:161564" | material: "Window frame" | property sets: Pset_BuildingElementProxyCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Window frame 016" | object type "Window frame 016" | names: "Window frame 016:Window frame 016:161600" | material: "Window frame" | property sets: Pset_BuildingElementProxyCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Glass panel 003" | object type "Glass panel 003" | names: "Glass panel 003:Glass panel 003:161634" | material: "Clear glass" | property sets: Pset_BuildingElementProxyCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Window frame 018" | object type "Window frame 018" | names: "Window frame 1:Window frame 018:168435" | material: "Window frame" | property sets: Pset_BuildingElementProxyCommon
          9 x IFCANNOTATION
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Cement bond coat 002:Cement bond coat 002:155998" | object type "Cement bond coat 002:1 : Cement bond coat 002:Cement bond coat 002:155998" | names: "Cement bond coat 002:Cement bond coat 002:1:Cement bond coat 002:1 : Cement bond coat 002:Cement bond coat 002:155998:172036" | material: "IMPERMEABLE WRB MEMBRANE (ANSI 118.10 OR BETTER) - COMPATIBLE W/ MORTAR BED" | property sets: Pset_BuildingElementProxyCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Cement bond coat 002:Cement bond coat 002:155998" | object type "Cement bond coat 002:2 : Cement bond coat 002:Cement bond coat 002:155998" | names: "Cement bond coat 002:Cement bond coat 002:2:Cement bond coat 002:2 : Cement bond coat 002:Cement bond coat 002:155998:173575" | material: "CEMENTITIOUS BOND COAT (ANSI A118.4 OR BETTER) - (DISCONTINUOUS AT TILE MOVEMENT JOINTS)" | property sets: Pset_BuildingElementProxyCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Cement bond coat 002:Cement bond coat 002:155998" | object type "Cement bond coat 002:3 : Cement bond coat 002:Cement bond coat 002:155998" | names: "Cement bond coat 002:Cement bond coat 002:3:Cement bond coat 002:3 : Cement bond coat 002:Cement bond coat 002:155998:173874" | material: "(CT-01) PORCELAIN WALL TILE (W/ CEMENTITIOUS GROUT ANSI A118.6 OR BETTER) - (FLEXIBLE SEALANT MOVEMENT JOINTS EVERY 10FT)" | property sets: Pset_BuildingElementProxyCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Cement bond coat 002:Cement bond coat 002:155998" | object type "Cement bond coat 002:4 : Cement bond coat 002:Cement bond coat 002:155998" | names: "Cement bond coat 002:Cement bond coat 002:4:Cement bond coat 002:4 : Cement bond coat 002:Cement bond coat 002:155998:174008" | material: "3/4" TO 1 1/2" THICK LATEX-PORTLAND CEMENT MORTAR BED (ANSI 118.4 OR BETTER) - (DISCONTINUOUS AT TILE MOVEMENT JOINT)" | property sets: Pset_BuildingElementProxyCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Cement bond coat 002:Cement bond coat 002:155998" | object type "Cement bond coat 002:5 : Cement bond coat 002:Cement bond coat 002:155998" | names: "Cement bond coat 002:Cement bond coat 002:5:Cement bond coat 002:5 : Cement bond coat 002:Cement bond coat 002:155998:174380" | material: "SCRATCH COAT (MATCH MORTAR BED SPECS)" | property sets: Pset_BuildingElementProxyCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Cement bond coat 002:Cement bond coat 002:155998" | object type "Cement bond coat 002:6 : Cement bond coat 002:Cement bond coat 002:155998" | names: "Cement bond coat 002:Cement bond coat 002:6:Cement bond coat 002:6 : Cement bond coat 002:Cement bond coat 002:155998:174489" | material: "METAL LATH - (DISCONTINUOUS AT TILE MOVEMENT JOINTS)" | property sets: Pset_BuildingElementProxyCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Cement bond coat 002:Cement bond coat 002:155998" | object type "Cement bond coat 002:7 : Cement bond coat 002:Cement bond coat 002:155998" | names: "Cement bond coat 002:Cement bond coat 002:7:Cement bond coat 002:7 : Cement bond coat 002:Cement bond coat 002:155998:175099" | material: "METAL COPING TO MATCH ADJACENT TILE COLOR (SLOPE BACK TOWARD ROOF)" | property sets: Pset_BuildingElementProxyCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Cement bond coat 002:Cement bond coat 002:155998" | object type "Cement bond coat 002:8 : Cement bond coat 002:Cement bond coat 002:155998" | names: "Cement bond coat 002:Cement bond coat 002:8:Cement bond coat 002:8 : Cement bond coat 002:Cement bond coat 002:155998:177174" | material: "METAL COPING TO MATCH ADJACENT TILE COLOR (SLOPE BACK TOWARD ROOF)" | property sets: Pset_BuildingElementProxyCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Aluminium profile 002:Aluminium profile 002:155954" | object type "Aluminium profile 002:1 : Aluminium profile 002:Aluminium profile 002:155954" | names: "Aluminium profile 002:Aluminium profile 002:1:Aluminium profile 002:1 : Aluminium profile 002:Aluminium profile 002:155954:178474" | material: "SET IN BED OF SEALANT" | property sets: Pset_BuildingElementProxyCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Aluminium profile 002:Aluminium profile 002:155954" | object type "Aluminium profile 002:2 : Aluminium profile 002:Aluminium profile 002:155954" | names: "Aluminium profile 002:Aluminium profile 002:2:Aluminium profile 002:2 : Aluminium profile 002:Aluminium profile 002:155954:178867" | material: "3X5X1/4" ALUMINUM ANGLE" | property sets: Pset_BuildingElementProxyCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Wood block 002:Wood block 002:155927" | object type "Wood block 002:2 : Wood block 002:Wood block 002:155927" | names: "Wood block 002:Wood block 002:2:Wood block 002:2 : Wood block 002:Wood block 002:155927:179311" | material: "PRESSURE TREATED WOOD BLOCKING - SIZE AS NECESSARY" | property sets: Pset_BuildingElementProxyCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Wood block 002:Wood block 002:155927" | object type "Wood block 002:3 : Wood block 002:Wood block 002:155927" | names: "Wood block 002:Wood block 002:3:Wood block 002:3 : Wood block 002:Wood block 002:155927:179338" | material: "PRESSURE TREATED WOOD BLOCKING - SIZE AS NECESSARY" | property sets: Pset_BuildingElementProxyCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 1" | object type "Generic Models 1" | names: "Generic Models 1:Generic Models 1:179624" | property sets: Pset_BuildingElementProxyCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 1" | object type "Generic Models 1" | names: "Generic Models 2:Generic Models 1:179683" | property sets: Pset_BuildingElementProxyCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 1" | object type "Generic Models 1" | names: "Generic Models 3:Generic Models 1:179805" | property sets: Pset_BuildingElementProxyCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 1" | object type "Generic Models 1" | names: "Generic Models 4:Generic Models 1:179816" | property sets: Pset_BuildingElementProxyCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 1" | object type "Generic Models 1" | names: "Generic Models 5:Generic Models 1:179831" | property sets: Pset_BuildingElementProxyCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 1" | object type "Generic Models 1" | names: "Generic Models 6:Generic Models 1:179842" | property sets: Pset_BuildingElementProxyCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 7" | object type "Generic Models 7" | names: "Generic Models 7:Generic Models 7:181127" | material: "EXISTING METAL DECK (REPAIR/REPLACE AS NECESSARY)" | property sets: Pset_BuildingElementProxyCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Cement bond coat 002:Cement bond coat 002:155998" | object type "Cement bond coat 002:9 : Cement bond coat 002:Cement bond coat 002:155998" | names: "Cement bond coat 002:Cement bond coat 002:9:Cement bond coat 002:9 : Cement bond coat 002:Cement bond coat 002:155998:181295" | material: "EXISTING COVER BOARD (REPAIR/REPLACE AS NECESSARY)" | property sets: Pset_BuildingElementProxyCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "TPO Membrane 002:TPO Membrane 002:156012" | object type "TPO Membrane 002:1 : TPO Membrane 002:TPO Membrane 002:156012" | names: "TPO Membrane 002:TPO Membrane 002:1:TPO Membrane 002:1 : TPO Membrane 002:TPO Membrane 002:156012:181723" | material: "TPO MEMBRANE ROOF MEMBRANE" | property sets: Pset_BuildingElementProxyCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "TPO Membrane 002:TPO Membrane 002:156012" | object type "TPO Membrane 002:2 : TPO Membrane 002:TPO Membrane 002:156012" | names: "TPO Membrane 002:TPO Membrane 002:2:TPO Membrane 002:2 : TPO Membrane 002:TPO Membrane 002:156012:182744" | material: "METAL BAR ANCHOR FASTENED AS REQUIRED BY MANF." | property sets: Pset_BuildingElementProxyCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 1" | object type "Generic Models 1" | names: "Generic Models 8:Generic Models 1:182871" | property sets: Pset_BuildingElementProxyCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 1" | object type "Generic Models 1" | names: "Generic Models 9:Generic Models 1:182882" | property sets: Pset_BuildingElementProxyCommon

Types
  IFCBUILDINGELEMENTPROXYTYPE "Rigid insulation 002:Rigid insulation 002:155913" | 1 occurrence | material: "EXISTING RIGID INSULATION AT ROOF (REPAIR/REPLACE AS NECESSARY) - (SLOPE TOWARD ROOF DRAINS)"
  IFCBUILDINGELEMENTPROXYTYPE "Wood block 002:Wood block 002:155927" | 1 occurrence | material: "PRESSURE TREATED WOOD BLOCKING - SIZE AS NECESSARY"
  IFCBUILDINGELEMENTPROXYTYPE "Aluminium profile 002:Aluminium profile 002:155954" | 1 occurrence | material: "3X5X1/4" ALUMINUM ANGLE"
  IFCBUILDINGELEMENTPROXYTYPE "Concrete wall 002:Concrete wall 002:155970" | 1 occurrence | material: "_EXISTING CAST-IN-PLACE CONCRETE"
  IFCBUILDINGELEMENTPROXYTYPE "TPO Membrane 002:TPO Membrane 002:156012" | 1 occurrence | material: "TPO MEMBRANE ROOF MEMBRANE"
  IFCBUILDINGELEMENTPROXYTYPE "Mortar bed 1:Mortar bed 002:158850" | 1 occurrence | material: "1/4" PRESSURE TREATED PLYWOOD (PROTECTION BOARD OVER EXISTING CONCRETE)"
  IFCBUILDINGELEMENTPROXYTYPE "Concrete wall001" | 1 occurrence | material: "PRESSURE TREATED WOOD BLOCKING - SIZE AS NECESSARY"
  IFCBUILDINGELEMENTPROXYTYPE "Metal stud 015" | 1 occurrence | material: "METAL STUDS"
  IFCBUILDINGELEMENTPROXYTYPE "Insulation horizontal001" | 1 occurrence | material: "Rigid insulation"
  IFCBUILDINGELEMENTPROXYTYPE "Insulation vertical001" | 1 occurrence | material: "Rigid insulation"
  IFCBUILDINGELEMENTPROXYTYPE "Inner gypsum board001" | 1 occurrence | material: "PRESSURE TREATED WOOD BLOCKING - SIZE AS NECESSARY"
  IFCBUILDINGELEMENTPROXYTYPE "Inner ceiling001" | 1 occurrence | material: "PRESSURE TREATED WOOD BLOCKING - SIZE AS NECESSARY"
  IFCBUILDINGELEMENTPROXYTYPE "Metal support for window frame001" | 1 occurrence | material: "IfcSurfaceStyle #179"
  IFCBUILDINGELEMENTPROXYTYPE "Stud 004" | 1 occurrence | material: "LIGHT GAUGE METAL STUDS AND/OR FURRING"
  IFCBUILDINGELEMENTPROXYTYPE "Stud 003" | 1 occurrence | material: "LIGHT GAUGE METAL STUDS AND/OR FURRING"
  IFCBUILDINGELEMENTPROXYTYPE "Metal stud 014" | 1 occurrence | material: "METAL STUDS"
  IFCBUILDINGELEMENTPROXYTYPE "Metal stud 016" | 1 occurrence | material: "METAL STUDS"
  IFCBUILDINGELEMENTPROXYTYPE "Metal stud 011" | 1 occurrence | material: "METAL STUDS"
  IFCBUILDINGELEMENTPROXYTYPE "Metal stud 010" | 1 occurrence | material: "METAL STUDS"
  IFCBUILDINGELEMENTPROXYTYPE "Metal stud 009" | 1 occurrence | material: "METAL STUDS"
  IFCBUILDINGELEMENTPROXYTYPE "Metal stud 013" | 1 occurrence | material: "METAL STUDS"
  IFCBUILDINGELEMENTPROXYTYPE "Metal stud 012" | 1 occurrence | material: "METAL STUDS"
  IFCBUILDINGELEMENTPROXYTYPE "WRB Membrane 004" | 1 occurrence | material: "IMPERMEABLE WRB MEMBRANE (ANSI 118.10 OR BETTER) - COMPATIBLE W/ MORTAR BED"
  IFCBUILDINGELEMENTPROXYTYPE "Flashing 003" | 1 occurrence | material: "IMPERMEABLE WRB MEMBRANE (ANSI 118.10 OR BETTER) - COMPATIBLE W/ MORTAR BED"
  IFCBUILDINGELEMENTPROXYTYPE "Counter-flashing 003" | 1 occurrence | material: "METAL COPING TO MATCH ADJACENT TILE COLOR (SLOPE BACK TOWARD ROOF)"
  IFCBUILDINGELEMENTPROXYTYPE "Window frame 017" | 1 occurrence | material: "Window frame"
  IFCBUILDINGELEMENTPROXYTYPE "Window frame 020" | 1 occurrence | material: "Window frame"
  IFCBUILDINGELEMENTPROXYTYPE "Window frame 014" | 1 occurrence | material: "Window frame"
  IFCBUILDINGELEMENTPROXYTYPE "Rysysta panel 021" | 1 occurrence | material: "Rysysta"
  IFCBUILDINGELEMENTPROXYTYPE "Rysysta panel 018" | 1 occurrence | material: "Rysysta"
  IFCBUILDINGELEMENTPROXYTYPE "Window frame 013" | 1 occurrence | material: "Window frame"
  IFCBUILDINGELEMENTPROXYTYPE "Rysysta panel 015" | 1 occurrence | material: "Rysysta"
  IFCBUILDINGELEMENTPROXYTYPE "Glass panel 004" | 1 occurrence | material: "Clear glass"
  IFCBUILDINGELEMENTPROXYTYPE "Rysysta panel 019" | 1 occurrence | material: "Rysysta"
  IFCBUILDINGELEMENTPROXYTYPE "Rysysta panel 020" | 1 occurrence | material: "Rysysta"
  IFCBUILDINGELEMENTPROXYTYPE "Rysysta panel 024" | 1 occurrence | material: "Rysysta"
  IFCBUILDINGELEMENTPROXYTYPE "Rysysta panel 017" | 1 occurrence | material: "Rysysta"
  IFCBUILDINGELEMENTPROXYTYPE "Rysysta panel 014" | 1 occurrence | material: "Rysysta"
  IFCBUILDINGELEMENTPROXYTYPE "Rysysta panel 016" | 1 occurrence | material: "Rysysta"
  IFCBUILDINGELEMENTPROXYTYPE "Rysysta panel 023" | 1 occurrence | material: "Rysysta"
  IFCBUILDINGELEMENTPROXYTYPE "Rysysta panel 022" | 1 occurrence | material: "Rysysta"
  IFCBUILDINGELEMENTPROXYTYPE "Rysysta starter strip 006" | 1 occurrence | material: "IfcSurfaceStyle #179"
  IFCBUILDINGELEMENTPROXYTYPE "Rysysta panel 013" | 1 occurrence | material: "Rysysta"
  IFCBUILDINGELEMENTPROXYTYPE "Rysysta starter strip 004" | 1 occurrence | material: "IfcSurfaceStyle #179"
  IFCBUILDINGELEMENTPROXYTYPE "Rysysta starter strip 005" | 1 occurrence | material: "IfcSurfaceStyle #179"
  IFCBUILDINGELEMENTPROXYTYPE "Window frame 015" | 1 occurrence | material: "Window frame"
  IFCBUILDINGELEMENTPROXYTYPE "Window frame 018" | 1 occurrence | material: "Window frame"
  IFCBUILDINGELEMENTPROXYTYPE "Window frame 016" | 1 occurrence | material: "Window frame"
  IFCBUILDINGELEMENTPROXYTYPE "Glass panel 003" | 1 occurrence | material: "Clear glass"
  IFCBUILDINGELEMENTPROXYTYPE "Window frame 018" | 1 occurrence | material: "Window frame"
  IFCBUILDINGELEMENTPROXYTYPE "Cement bond coat 002:Cement bond coat 002:155998" | 1 occurrence | material: "IMPERMEABLE WRB MEMBRANE (ANSI 118.10 OR BETTER) - COMPATIBLE W/ MORTAR BED"
  IFCBUILDINGELEMENTPROXYTYPE "Cement bond coat 002:Cement bond coat 002:155998" | 1 occurrence | material: "CEMENTITIOUS BOND COAT (ANSI A118.4 OR BETTER) - (DISCONTINUOUS AT TILE MOVEMENT JOINTS)"
  IFCBUILDINGELEMENTPROXYTYPE "Cement bond coat 002:Cement bond coat 002:155998" | 1 occurrence | material: "(CT-01) PORCELAIN WALL TILE (W/ CEMENTITIOUS GROUT ANSI A118.6 OR BETTER) - (FLEXIBLE SEALANT MOVEMENT JOINTS EVERY 10FT)"
  IFCBUILDINGELEMENTPROXYTYPE "Cement bond coat 002:Cement bond coat 002:155998" | 1 occurrence | material: "3/4" TO 1 1/2" THICK LATEX-PORTLAND CEMENT MORTAR BED (ANSI 118.4 OR BETTER) - (DISCONTINUOUS AT TILE MOVEMENT JOINT)"
  IFCBUILDINGELEMENTPROXYTYPE "Cement bond coat 002:Cement bond coat 002:155998" | 1 occurrence | material: "SCRATCH COAT (MATCH MORTAR BED SPECS)"
  IFCBUILDINGELEMENTPROXYTYPE "Cement bond coat 002:Cement bond coat 002:155998" | 1 occurrence | material: "METAL LATH - (DISCONTINUOUS AT TILE MOVEMENT JOINTS)"
  IFCBUILDINGELEMENTPROXYTYPE "Cement bond coat 002:Cement bond coat 002:155998" | 1 occurrence | material: "METAL COPING TO MATCH ADJACENT TILE COLOR (SLOPE BACK TOWARD ROOF)"
  IFCBUILDINGELEMENTPROXYTYPE "Cement bond coat 002:Cement bond coat 002:155998" | 1 occurrence | material: "METAL COPING TO MATCH ADJACENT TILE COLOR (SLOPE BACK TOWARD ROOF)"
  IFCBUILDINGELEMENTPROXYTYPE "Aluminium profile 002:Aluminium profile 002:155954" | 1 occurrence | material: "SET IN BED OF SEALANT"
  IFCBUILDINGELEMENTPROXYTYPE "Aluminium profile 002:Aluminium profile 002:155954" | 1 occurrence | material: "3X5X1/4" ALUMINUM ANGLE"
  IFCBUILDINGELEMENTPROXYTYPE "Wood block 002:Wood block 002:155927" | 1 occurrence | material: "PRESSURE TREATED WOOD BLOCKING - SIZE AS NECESSARY"
  IFCBUILDINGELEMENTPROXYTYPE "Wood block 002:Wood block 002:155927" | 1 occurrence | material: "PRESSURE TREATED WOOD BLOCKING - SIZE AS NECESSARY"
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 1" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 1" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 1" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 1" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 1" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 1" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 7" | 1 occurrence | material: "EXISTING METAL DECK (REPAIR/REPLACE AS NECESSARY)"
  IFCBUILDINGELEMENTPROXYTYPE "Cement bond coat 002:Cement bond coat 002:155998" | 1 occurrence | material: "EXISTING COVER BOARD (REPAIR/REPLACE AS NECESSARY)"
  IFCBUILDINGELEMENTPROXYTYPE "TPO Membrane 002:TPO Membrane 002:156012" | 1 occurrence | material: "TPO MEMBRANE ROOF MEMBRANE"
  IFCBUILDINGELEMENTPROXYTYPE "TPO Membrane 002:TPO Membrane 002:156012" | 1 occurrence | material: "METAL BAR ANCHOR FASTENED AS REQUIRED BY MANF."
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 1" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 1" | 1 occurrence

Property sets
  Pset_BuildingElementProxyCommon | properties | on 9 objects (9 IFCBUILDINGELEMENTPROXY)
    Reference = "Cement bond coat 002" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 8 objects (8 IFCBUILDINGELEMENTPROXY)
    Reference = "Generic Models 1" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 3 objects (3 IFCBUILDINGELEMENTPROXY)
    Reference = "Wood block 002" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 3 objects (3 IFCBUILDINGELEMENTPROXY)
    Reference = "Aluminium profile 002" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 3 objects (3 IFCBUILDINGELEMENTPROXY)
    Reference = "TPO Membrane 002" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 2 objects (2 IFCBUILDINGELEMENTPROXY)
    Reference = "Window frame 018" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Reference = "Rigid insulation 002" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Reference = "Concrete wall 002" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon: 44 more contents on 44 objects not shown
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    NumberOfStoreys = 1 (IFCINTEGER)
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)