IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView_V2.0]"
File name: "Project Number"
Time stamp: "2016-12-28T20:52:08"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.07 : 28 Aug 2013"
Originating system: "20150714_1515(x64) - Exporter 16.5.0.0 - Alternate UI 16.5.0.0"
Application: "Autodesk Revit 2016 (ENU)" version "2016" identifier "Revit" by Organization "Autodesk Revit 2016 (ENU)"

People and organizations
  Person "ryan@openingdesign.com" of Organization (no name given)
  Owner history of Person "ryan@openingdesign.com" of Organization (no name given) | application "Autodesk Revit 2016 (ENU)" version "2016" identifier "Revit" by Organization "Autodesk Revit 2016 (ENU)" | change NOCHANGE | created 1482956207 (2016-12-28T20:16:47Z)

Units
  LENGTHUNIT: FOOT (conversion based)
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"

Spatial structure
IFCPROJECT "Project Number" | long name "Project Name" | phase "Project Status"
  IFCSITE "Default" | latitude 42° 21′ 30.344238″ | longitude -71° 3′ 35.194702″ | elevation above sea level 0.
    IFCBUILDING | postal address: "Enter address here", "<Default>"
      IFCBUILDINGSTOREY "Level 1" | long name "Level 1" | elevation 0.
        contains 17 elements
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Rigid insulation 002" | object type "Rigid insulation 002" | names: "Rigid insulation 002:Rigid insulation 002:155913" | material: "EXISTING RIGID INSULATION AT ROOF (PATCH AND REPAIR AS NECESSARY)" | property sets: Pset_BuildingElementProxyCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Wood block 002" | object type "Wood block 002" | names: "Wood block 002:Wood block 002:155927" | material: "PRESSURE TREATED WOOD BLOCKING - SIZE AS NECESSARY" | property sets: Pset_BuildingElementProxyCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Sealant 002" | object type "Sealant 002" | names: "Sealant 002:Sealant 002:155941" | material: "SEALANT & BACKER ROD, IF NECESSARY" | property sets: Pset_BuildingElementProxyCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Aluminium profile 002" | object type "Aluminium profile 002" | names: "Aluminium profile 002:Aluminium profile 002:155954" | material: "IfcSurfaceStyle #179" | property sets: Pset_BuildingElementProxyCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Concrete wall 002" | object type "Concrete wall 002" | names: "Concrete wall 002:Concrete wall 002:155970" | material: "_EXISTING CAST-IN-PLACE CONCRETE" | property sets: Pset_BuildingElementProxyCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "WRB Membrane 002" | object type "WRB Membrane 002" | names: "WRB Membrane 002:WRB Membrane 002:155984" | material: "IMPERMEABLE WRB MEMBRANE" | property sets: Pset_BuildingElementProxyCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Cement bond coat 002" | object type "Cement bond coat 002" | names: "Cement bond coat 002:Cement bond coat 002:155998" | material: "CEMENTITIOUS BOND COAT" | property sets: Pset_BuildingElementProxyCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "TPO Membrane 002" | object type "TPO Membrane 002" | names: "TPO Membrane 002:TPO Membrane 002:156012" | material: "TPO MEMBRANE ROOF MEMBRANE" | property sets: Pset_BuildingElementProxyCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Scratch coat 002" | object type "Scratch coat 002" | names: "Scratch coat 002:Scratch coat 002:156030" | material: "SCRATCH COAT" | property sets: Pset_BuildingElementProxyCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Porcelain tiles 002" | object type "Porcelain tiles 002" | names: "Porcelain tiles 002:Porcelain tiles 002:156044" | material: "(CT-01) PORCELAIN WALL TILE" | property sets: Pset_BuildingElementProxyCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Counter flashing 002" | object type "Counter flashing 002" | names: "Counter flashing 002:Counter flashing 002:156072" | material: "SHEET METAL COPING" | property sets: Pset_BuildingElementProxyCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Front flashing 002" | object type "Front flashing 002" | names: "Front flashing 002:Front flashing 002:156098" | material: "SHEET METAL COPING" | property sets: Pset_BuildingElementProxyCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Top sealant 002" | object type "Top sealant 002" | names: "Top sealant 002:Top sealant 002:156116" | material: "SET IN BED OF SEALANT" | property sets: Pset_BuildingElementProxyCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Steel deck 002" | object type "Steel deck 002" | names: "Steel deck 002:Steel deck 002:156148" | material: "IfcSurfaceStyle #1109" | property sets: Pset_BuildingElementProxyCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Metal lath 002" | object type "Metal lath 002" | names: "Metal lath 002:Metal lath 002:156155" | material: "METAL LATH OVER CLEAVAGE MEMBRANE" | property sets: Pset_BuildingElementProxyCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Mortar bed 002" | object type "Mortar bed 002" | names: "Mortar bed 002:Mortar bed 002:156169" | material: "MORTAR BED" | property sets: Pset_BuildingElementProxyCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Mortar bed 002" | object type "Mortar bed 002" | names: "Mortar bed 1:Mortar bed 002:158850" | material: "1/4" PRESSURE TREATED PLYWOOD (PROTECTION BOARD OVER EXISTING CONCRETE)" | property sets: Pset_BuildingElementProxyCommon

Types
  IFCBUILDINGELEMENTPROXYTYPE "Rigid insulation 002" | 1 occurrence | material: "EXISTING RIGID INSULATION AT ROOF (PATCH AND REPAIR AS NECESSARY)"
  IFCBUILDINGELEMENTPROXYTYPE "Wood block 002" | 1 occurrence | material: "PRESSURE TREATED WOOD BLOCKING - SIZE AS NECESSARY"
  IFCBUILDINGELEMENTPROXYTYPE "Sealant 002" | 1 occurrence | material: "SEALANT & BACKER ROD, IF NECESSARY"
  IFCBUILDINGELEMENTPROXYTYPE "Aluminium profile 002" | 1 occurrence | material: "IfcSurfaceStyle #179"
  IFCBUILDINGELEMENTPROXYTYPE "Concrete wall 002" | 1 occurrence | material: "_EXISTING CAST-IN-PLACE CONCRETE"
  IFCBUILDINGELEMENTPROXYTYPE "WRB Membrane 002" | 1 occurrence | material: "IMPERMEABLE WRB MEMBRANE"
  IFCBUILDINGELEMENTPROXYTYPE "Cement bond coat 002" | 1 occurrence | material: "CEMENTITIOUS BOND COAT"
  IFCBUILDINGELEMENTPROXYTYPE "TPO Membrane 002" | 1 occurrence | material: "TPO MEMBRANE ROOF MEMBRANE"
  IFCBUILDINGELEMENTPROXYTYPE "Scratch coat 002" | 1 occurrence | material: "SCRATCH COAT"
  IFCBUILDINGELEMENTPROXYTYPE "Porcelain tiles 002" | 1 occurrence | material: "(CT-01) PORCELAIN WALL TILE"
  IFCBUILDINGELEMENTPROXYTYPE "Counter flashing 002" | 1 occurrence | material: "SHEET METAL COPING"
  IFCBUILDINGELEMENTPROXYTYPE "Front flashing 002" | 1 occurrence | material: "SHEET METAL COPING"
  IFCBUILDINGELEMENTPROXYTYPE "Top sealant 002" | 1 occurrence | material: "SET IN BED OF SEALANT"
  IFCBUILDINGELEMENTPROXYTYPE "Steel deck 002" | 1 occurrence | material: "IfcSurfaceStyle #1109"
  IFCBUILDINGELEMENTPROXYTYPE "Metal lath 002" | 1 occurrence | material: "METAL LATH OVER CLEAVAGE MEMBRANE"
  IFCBUILDINGELEMENTPROXYTYPE "Mortar bed 002" | 1 occurrence | material: "MORTAR BED"
  IFCBUILDINGELEMENTPROXYTYPE "Mortar bed 002" | 1 occurrence | material: "1/4" PRESSURE TREATED PLYWOOD (PROTECTION BOARD OVER EXISTING CONCRETE)"

Property sets
  Pset_BuildingElementProxyCommon | properties | on 2 objects (2 IFCBUILDINGELEMENTPROXY)
    Reference = "Mortar bed 002" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Reference = "Rigid insulation 002" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Reference = "Wood block 002" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Reference = "Sealant 002" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Reference = "Aluminium profile 002" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Reference = "Concrete wall 002" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Reference = "WRB Membrane 002" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Reference = "Cement bond coat 002" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon: 8 more contents on 8 objects not shown
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    NumberOfStoreys = 1 (IFCINTEGER)