IFC building model
Schema: "IFC4"
Description: "ViewDefinition [ReferenceView_V1.1]"
File name: "0000.00"
Time stamp: "2020-05-05T15:58:46"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.07 : 28 Aug 2013"
Originating system: "20200206_0915(x64) - Exporter 20.2.11.3 - Interface utilisateur alternative 20.2.11.3"
Application: "Autodesk Revit 2020 (FRA)" version "2020" identifier "Revit" by Organization "Autodesk Revit 2020 (FRA)"

People and organizations
  Person "None" "None" of Organization "None" description "None"
  Owner history of Person "None" "None" of Organization "None" description "None" | application "Autodesk Revit 2020 (FRA)" version "2020" identifier "Revit" by Organization "Autodesk Revit 2020 (FRA)" | change NOCHANGE | created 1588684405 (2020-05-05T13:13:25Z)

Units
  LENGTHUNIT: METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"

Spatial structure
IFCPROJECT "0000.00" | long name "Nom du projet" | phase "Avant-Projet"
  IFCSITE "Default" | latitude 48° 51′ 23.999633″ | longitude 2° 21′ 3.553905″ | elevation above sea level 373.6
    IFCBUILDING "Revit Advanced Sample" | long name "Revit Advanced Sample"
      IFCBUILDINGSTOREY "S1" | long name "S1" | object type "Niveau:Niveaux fini" | elevation -3.
        contains 7 elements
          6 x IFCWALL | type IFCWALLTYPE "Mur de base:Ext - Béton - 45 cm" | object type "Mur de base:Ext - Béton - 45 cm" | names: "Mur de base:Ext - Béton - 45 cm:5675979", "Mur de base:Ext - Béton - 45 cm:5675980", "Mur de base:Ext - Béton - 45 cm:5675981" (+3 more) | material: layers "Mur de base:Ext - Béton - 45 cm" ("Stuc" 0.05, "Isolation extérieure" 0.2, "Béton, coulé sur place, gris" 0.2) | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCSLAB | type IFCSLABTYPE "Sol:EXT - Générique 30.0 cm" | object type "Sol:EXT - Générique 30.0 cm" | FLOOR | names: "Sol:EXT - Générique 30.0 cm:5676101" | material: layers "Sol:EXT - Générique 30.0 cm" ("Sol par défaut" 0.3) | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
        IFCSPACE "135" | long name "Espace" | SPACE
      IFCBUILDINGSTOREY "E0" | long name "E0" | object type "Niveau:Niveaux fini" | elevation 0.
        contains 11 elements
          6 x IFCWALL | type IFCWALLTYPE "Mur de base:Ext - Béton - 45 cm" | object type "Mur de base:Ext - Béton - 45 cm" | names: "Mur de base:Ext - Béton - 45 cm:5672713", "Mur de base:Ext - Béton - 45 cm:5672877", "Mur de base:Ext - Béton - 45 cm:5673046" (+3 more) | material: layers "Mur de base:Ext - Béton - 45 cm" ("Stuc" 0.05, "Isolation extérieure" 0.2, "Béton, coulé sur place, gris" 0.2) | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCDOOR | type IFCDOORTYPE "80 x 205" | object type "1 battant vide fini:80 x 205" | DOOR | names: "1 battant vide fini:80 x 205:5673107" | material: constituents "MaterialConstituentSet" ("Porte - poignée acier": "Porte - poignée acier", "Porte - bois de la feuille de porte": "Porte - bois de la feuille de porte") | property sets: Pset_DoorCommon, Pset_EnvironmentalImpactIndicators
          2 x IFCWINDOW | type IFCWINDOWTYPE "Type 4 - Fenêtre à 1 montant 255x235 cm sous balcon" | object type "Ouverture:Type 4 - Fenêtre à 1 montant 255x235 cm sous balcon" | WINDOW | names: "Ouverture:Type 4 - Fenêtre à 1 montant 255x235 cm sous balcon:5673117", "Ouverture:Type 4 - Fenêtre à 1 montant 255x235 cm sous balcon:5674348" | material: constituents "MaterialConstituentSet" ("Fenêtre - Vitrage": "Fenêtre - Vitrage", "Fenêtre - Cadre": "Fenêtre - Cadre") | property sets: Pset_EnvironmentalImpactIndicators, Pset_WindowCommon
          1 x IFCSLAB | type IFCSLABTYPE "Sol:EXT - Générique 30.0 cm" | object type "Sol:EXT - Générique 30.0 cm" | FLOOR | names: "Sol:EXT - Générique 30.0 cm:5673216" | material: layers "Sol:EXT - Générique 30.0 cm" ("Sol par défaut" 0.3) | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCWALL | type IFCWALLTYPE "Mur de base:Int - Brique 10.0" | object type "Mur de base:Int - Brique 10.0" | names: "Mur de base:Int - Brique 10.0:5674487" | material: layers "Mur de base:Int - Brique 10.0" ("Mur par défaut" 0.1) | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
        IFCSPACE "133" | long name "Espace" | SPACE
        IFCSPACE "134" | long name "Espace" | SPACE
        IFCSPACE "1" | SPACE
        IFCSPACE "2" | SPACE
        IFCSPACE "3" | SPACE
        IFCSPACE "4" | SPACE
      IFCBUILDINGSTOREY "E1" | long name "E1" | object type "Niveau:Niveaux fini" | elevation 3.80000000000133
        contains 3 elements
          1 x IFCROOF | type IFCROOFTYPE "Toit de base:Générique - 40 cm" | object type "Toit de base:Générique - 40 cm" | names: "Toit de base:Générique - 40 cm:5673258" | parts: 1 IFCSLAB | property sets: Pset_EnvironmentalImpactIndicators, Pset_RoofCommon
          2 x IFCWINDOW | type IFCWINDOWTYPE "600mm x 600mm" | object type "ENE_FenêtreDeToitRectangulaire:600mm x 600mm" | WINDOW | names: "ENE_FenêtreDeToitRectangulaire:600mm x 600mm:5673275", "ENE_FenêtreDeToitRectangulaire:600mm x 600mm:5674030" | material: "Métal - Aluminium" | property sets: Pset_EnvironmentalImpactIndicators, Pset_WindowCommon

Types
  IFCWALLTYPE "Mur de base:Ext - Béton - 45 cm" | 12 occurrences | material: layers "Mur de base:Ext - Béton - 45 cm" ("Stuc" 0.05, "Isolation extérieure" 0.2, "Béton, coulé sur place, gris" 0.2) | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCSLABTYPE "Sol:EXT - Générique 30.0 cm" | FLOOR | 1 occurrence | material: layers "Sol:EXT - Générique 30.0 cm" ("Sol par défaut" 0.3) | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
  IFCDOORTYPE "80 x 205" | DOOR | 1 occurrence | material: constituents "MaterialConstituentSet" ("Porte - poignée acier": "Porte - poignée acier", "Porte - bois de la feuille de porte": "Porte - bois de la feuille de porte") | property sets: 1 battant vide fini:80 x 205:5673107, Pset_DoorCommon, Pset_EnvironmentalImpactIndicators
  IFCWINDOWTYPE "Type 4 - Fenêtre à 1 montant 255x235 cm sous balcon" | WINDOW | 2 occurrences | material: constituents "MaterialConstituentSet" ("Fenêtre - Vitrage": "Fenêtre - Vitrage", "Fenêtre - Cadre": "Fenêtre - Cadre") | property sets: Ouverture:Type 4 - Fenêtre à 1 montant 255x235 cm sous balcon:5673117, Pset_EnvironmentalImpactIndicators, Pset_WindowCommon
  IFCSLABTYPE "Sol:EXT - Générique 30.0 cm" | FLOOR | 1 occurrence | material: layers "Sol:EXT - Générique 30.0 cm" ("Sol par défaut" 0.3) | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
  IFCWALLTYPE "Mur de base:Int - Brique 10.0" | 1 occurrence | material: layers "Mur de base:Int - Brique 10.0" ("Mur par défaut" 0.1) | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCROOFTYPE "Toit de base:Générique - 40 cm" | 1 occurrence | property sets: Pset_EnvironmentalImpactIndicators, Pset_RoofCommon
  IFCWINDOWTYPE "600mm x 600mm" | WINDOW | 2 occurrences | material: "Métal - Aluminium" | property sets: ENE_FenêtreDeToitRectangulaire:600mm x 600mm:5673275, Pset_EnvironmentalImpactIndicators, Pset_WindowCommon

Property sets
  Pset_SpaceCommon | properties | on 3 objects (3 IFCSPACE)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Surface" (IFCIDENTIFIER)
  Pset_SpaceCommon | properties | on 1 object (1 IFCSPACE)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Espace 133" (IFCIDENTIFIER)
  Pset_SpaceCommon | properties | on 1 object (1 IFCSPACE)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Espace 134" (IFCIDENTIFIER)
  Pset_SpaceCommon | properties | on 1 object (1 IFCSPACE)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Espace 135" (IFCIDENTIFIER)
  Pset_SpaceCommon | properties | on 1 object (1 IFCSPACE)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "4" (IFCIDENTIFIER)
  Pset_EnvironmentalImpactIndicators | properties | on 13 objects (12 IFCWALL, 1 IFCOPENINGELEMENT) | on 1 type object
    Reference = "Ext - Béton - 45 cm" (IFCIDENTIFIER)
  Pset_EnvironmentalImpactIndicators | properties | on 4 objects (2 IFCOPENINGELEMENT, 1 IFCROOF, 1 IFCSLAB) | on 1 type object
    Reference = "Générique - 40 cm" (IFCIDENTIFIER)
  Pset_EnvironmentalImpactIndicators | properties | on 2 objects (2 IFCSLAB) | on 2 type objects
    Reference = "EXT - Générique 30.0 cm" (IFCIDENTIFIER)
  Pset_EnvironmentalImpactIndicators | properties | on 2 objects (2 IFCWINDOW) | on 1 type object
    Reference = "Type 4 - Fenêtre à 1 montant 255x235 cm sous balcon" (IFCIDENTIFIER)
  Pset_EnvironmentalImpactIndicators | properties | on 2 objects (2 IFCWINDOW) | on 1 type object
    Reference = "600mm x 600mm" (IFCIDENTIFIER)
  Pset_EnvironmentalImpactIndicators | properties | on 1 object (1 IFCDOOR) | on 1 type object
    Reference = "80 x 205" (IFCIDENTIFIER)
  Pset_EnvironmentalImpactIndicators | properties | on 1 object (1 IFCWALL) | on 1 type object
    Reference = "Int - Brique 10.0" (IFCIDENTIFIER)
  Pset_ReinforcementBarPitchOfWall | properties | on 12 objects (12 IFCWALL) | on 1 type object
    Reference = "Ext - Béton - 45 cm" (IFCLABEL)
  Pset_ReinforcementBarPitchOfWall | properties | on 1 object (1 IFCWALL) | on 1 type object
    Reference = "Int - Brique 10.0" (IFCLABEL)
  Pset_WallCommon | properties | on 12 objects (12 IFCWALL)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "Ext - Béton - 45 cm" (IFCIDENTIFIER)
    ThermalTransmittance = 0.162786859608057 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_WallCommon | properties | on 1 object (1 IFCWALL)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "Int - Brique 10.0" (IFCIDENTIFIER)
  Pset_WallCommon | properties | on 1 type object
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Ext - Béton - 45 cm" (IFCIDENTIFIER)
    ThermalTransmittance = 0.162786859608057 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_WallCommon | properties | on 1 type object
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Int - Brique 10.0" (IFCIDENTIFIER)
  Pset_DoorCommon | properties | on 1 object (1 IFCDOOR) | on 1 type object
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "80 x 205" (IFCIDENTIFIER)
  Pset_WindowCommon | properties | on 2 objects (2 IFCWINDOW)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "Type 4 - Fenêtre à 1 montant 255x235 cm sous balcon" (IFCIDENTIFIER)
    ThermalTransmittance = 1.3 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_WindowCommon | properties | on 2 objects (2 IFCWINDOW)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "600mm x 600mm" (IFCIDENTIFIER)
    ThermalTransmittance = 3.6886 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_WindowCommon | properties | on 1 type object
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Type 4 - Fenêtre à 1 montant 255x235 cm sous balcon" (IFCIDENTIFIER)
    ThermalTransmittance = 1.3 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_WindowCommon | properties | on 1 type object
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "600mm x 600mm" (IFCIDENTIFIER)
    ThermalTransmittance = 3.6886 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_ReinforcementBarPitchOfSlab | properties | on 2 objects (2 IFCSLAB) | on 2 type objects
    Reference = "EXT - Générique 30.0 cm" (IFCLABEL)
  Pset_ReinforcementBarPitchOfSlab | properties | on 1 object (1 IFCSLAB)
    Reference = "Générique - 40 cm" (IFCLABEL)
  Pset_SlabCommon | properties | on 2 objects (2 IFCSLAB)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    PitchAngle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Reference = "EXT - Générique 30.0 cm" (IFCIDENTIFIER)
  Pset_SlabCommon | properties | on 1 object (1 IFCSLAB)
    IsExternal = TRUE (IFCBOOLEAN)
    PitchAngle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Reference = "Générique - 40 cm" (IFCIDENTIFIER)
  Pset_SlabCommon | properties | on 2 type objects
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "EXT - Générique 30.0 cm" (IFCIDENTIFIER)
  Pset_RoofCommon | properties | on 1 object (1 IFCROOF) | on 1 type object
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "Générique - 40 cm" (IFCIDENTIFIER)
  Pset_OpeningElementCommon | properties | on 2 objects (2 IFCOPENINGELEMENT)
    Reference = "Générique - 40 cm" (IFCIDENTIFIER)
  Pset_OpeningElementCommon | properties | on 1 object (1 IFCOPENINGELEMENT)
    Reference = "Ext - Béton - 45 cm" (IFCIDENTIFIER)
  Pset_ZoneCommon | properties | on 1 object (1 IFCZONE)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Par défaut" (IFCIDENTIFIER)
  Pset_BuildingStoreyCommon | properties | on 3 objects (3 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
    Reference = "Niveaux fini" (IFCIDENTIFIER)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    IsLandmarked = UNKNOWN (IFCLOGICAL)
    NumberOfStoreys = 3 (IFCINTEGER)
    Reference = "Informations sur le projet" (IFCIDENTIFIER)
  1 battant vide fini:80 x 205:5673107 | predefined | on 2 type objects
  Ouverture:Type 4 - Fenêtre à 1 montant 255x235 cm sous balcon:5673117 | predefined | on 1 type object
  ENE_FenêtreDeToitRectangulaire:600mm x 600mm:5673275 | predefined | on 1 type object

Other addresses and roles
  2 x postal address: "Entrer l'adresse ici", "Geneva", "Switzerland"