IFC building model
Schema: "IFC4"
Description: "ViewDefinition [ReferenceView_V1.0]"
File name: "项目编号"
Time stamp: "2019-05-22T11:08:01"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.07 : 28 Aug 2013"
Originating system: "20180328_1600(x64) - Exporter 19.0.1.1 - Alternate UI 19.0.1.1"
Application: "Autodesk Revit 2019 (ENU)" version "2019" identifier "Revit" by Organization "Autodesk Revit 2019 (ENU)"

People and organizations
  Person "Lingxi_LEI" of Organization (no name given)
  Owner history of Person "Lingxi_LEI" of Organization (no name given) | application "Autodesk Revit 2019 (ENU)" version "2019" identifier "Revit" by Organization "Autodesk Revit 2019 (ENU)" | change NOCHANGE | created 1541480755 (2018-11-06T05:05:55Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"

Spatial structure
IFCPROJECT "项目编号" | long name "项目名称" | phase "项目状态"
  IFCSITE "Default" | latitude 39° 54′ 57.601318″ | longitude 116° 25′ 58.795166″ | elevation above sea level 0.
    IFCBUILDING | postal address: "请在此处输入地址", "中国北京"
      IFCBUILDINGSTOREY "标高 1" | long name "标高 1" | elevation 0.
        contains 11 elements
          4 x IFCWALL | type IFCWALLTYPE "Basic Wall:常规 - 200mm" | object type "Basic Wall:常规 - 200mm:398" | names: "Basic Wall:常规 - 200mm:336251", "Basic Wall:常规 - 200mm:336252", "Basic Wall:常规 - 200mm:336253" (+1 more) | material: layers "Basic Wall:常规 - 200mm" ("默认墙" 200.) | property sets: Qto_WallBaseQuantities, Constraints, Dimensions, Other, Phasing, Structural
          1 x IFCSLAB | object type "Floor:常规 - 150mm" | FLOOR | names: "Floor:常规 - 150mm:336953" | material: layers "Floor:常规 - 150mm" ("默认楼板" 150.) | property sets: Pset_SlabCommon, Qto_SlabBaseQuantities, Constraints, Dimensions, Other, Phasing
          2 x IFCDOOR | type IFCDOORTYPE "750 x 2000mm" | object type "750 x 2000mm" | DOOR | SINGLE_SWING_RIGHT | names: "单扇 - 与墙齐:750 x 2000mm:337043", "单扇 - 与墙齐:750 x 2000mm:337083" | material: constituents "MaterialConstituentSet" ("门 - 框架": "门 - 框架", "门 - 嵌板": "门 - 嵌板") | property sets: Pset_DoorCommon, Qto_DoorBaseQuantities, Constraints, Dimensions, Identity Data, Other
          1 x IFCSTAIR | object type "Assembled Stair:190mm 最大踢面 250mm 梯段:252990" | names: "Assembled Stair:Stair:337334" | parts: 2 IFCMEMBER, 2 IFCRAILING, 1 IFCSTAIRFLIGHT | property sets: Pset_StairCommon, Constraints, Dimensions, Other, Phasing, Calculation Rules(Type)
          3 x IFCWINDOW | type IFCWINDOWTYPE "0915 x 1220mm" | object type "0915 x 1220mm" | WINDOW | names: "固定:0915 x 1220mm:338138", "固定:0915 x 1220mm:338176", "固定:0915 x 1220mm:338220" | material: constituents "MaterialConstituentSet" ("玻璃": "玻璃", "窗扇": "窗扇") | property sets: Pset_WindowCommon, Qto_WindowBaseQuantities, Constraints, Dimensions, Identity Data, Other
        IFCSPACE "1" | long name "房间" | SPACE
      IFCBUILDINGSTOREY "标高 2" | long name "标高 2" | elevation 4000.
        contains 5 elements
          1 x IFCSLAB | object type "Floor:常规 - 150mm" | FLOOR | names: "Floor:常规 - 150mm:336984" | material: layers "Floor:常规 - 150mm" ("默认楼板" 150.) | property sets: Pset_SlabCommon, Qto_SlabBaseQuantities, Constraints, Dimensions, Other, Phasing
          4 x IFCWINDOW | type IFCWINDOWTYPE "0915 x 1220mm" | object type "0915 x 1220mm" | WINDOW | names: "固定:0915 x 1220mm:337141", "固定:0915 x 1220mm:337206", "固定:0915 x 1220mm:337232" (+1 more) | material: constituents "MaterialConstituentSet" ("玻璃": "玻璃", "窗扇": "窗扇") | property sets: Pset_WindowCommon, Qto_WindowBaseQuantities, Constraints, Dimensions, Identity Data, Other
        IFCSPACE "2" | long name "房间" | SPACE

Types
  IFCWALLTYPE "Basic Wall:常规 - 200mm" | 4 occurrences | material: layers "Basic Wall:常规 - 200mm" ("默认墙" 200.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Other
  IFCDOORTYPE "750 x 2000mm" | DOOR | SINGLE_SWING_RIGHT | 2 occurrences | material: constituents "MaterialConstituentSet" ("门 - 框架": "门 - 框架", "门 - 嵌板": "门 - 嵌板") | property sets: 单扇 - 与墙齐:750 x 2000mm:337043, Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes
  IFCWINDOWTYPE "0915 x 1220mm" | WINDOW | 7 occurrences | material: constituents "MaterialConstituentSet" ("玻璃": "玻璃", "窗扇": "窗扇") | property sets: 固定:0915 x 1220mm:337141, Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes

Property sets
  Pset_SpaceCommon | properties | on 1 object (1 IFCSPACE)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "房间 1" (IFCIDENTIFIER)
  Pset_SpaceCommon | properties | on 1 object (1 IFCSPACE)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "房间 2" (IFCIDENTIFIER)
  Qto_SpaceBaseQuantities | quantities | on 2 objects (2 IFCSPACE)
    GrossFloorArea = 68.44 [SQUARE_METRE]
    GrossPerimeter = 35200. [MILLI METRE]
    GrossVolume = 166884.096 [CUBIC_METRE]
    Height = 2438.4 [MILLI METRE]
    NetFloorArea = 68.44 [SQUARE_METRE]
  Constraints | properties | on 4 objects (4 IFCWALL)
    Base Constraint = "Level: 标高 1" (IFCLABEL)
    Base Extension Distance = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Base Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Base is Attached = FALSE (IFCBOOLEAN)
    Location Line = "Wall Centerline" (IFCIDENTIFIER)
    Related to Mass = FALSE (IFCBOOLEAN)
    Room Bounding = TRUE (IFCBOOLEAN)
    Top Constraint = "Level: 标高 3" (IFCLABEL)
    Top Extension Distance = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Top Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Top is Attached = FALSE (IFCBOOLEAN)
    Unconnected Height = 8000.00000000018 (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 4 objects (4 IFCWINDOW)
    Level = "Level: 标高 2" (IFCLABEL)
    Sill Height = 915.000000000004 (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 3 objects (3 IFCWINDOW)
    Level = "Level: 标高 1" (IFCLABEL)
    Sill Height = 915.000000000005 (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 2 objects (2 IFCDOOR)
    Level = "Level: 标高 1" (IFCLABEL)
    Sill Height = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 2 objects (2 IFCMEMBER)
    Lower End Cut = "Vertical Cut" (IFCIDENTIFIER)
    Trim Support at Upper = "Do not trim" (IFCIDENTIFIER)
    Upper End Cut = "Vertical Cut" (IFCIDENTIFIER)
  Constraints | properties | on 2 objects (2 IFCRAILING)
    Base Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Offset from Path = 25.4 (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 object (1 IFCSPACE)
    Base Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Level = "标高 1" (IFCTEXT)
    Limit Offset = 2438.4 (IFCLENGTHMEASURE) [MILLI METRE]
    Upper Limit = "Level: 标高 1" (IFCLABEL)
  Constraints | properties | on 1 object (1 IFCSPACE)
    Base Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Level = "Level: 标高 2" (IFCLABEL)
    Limit Offset = 2438.4 (IFCLENGTHMEASURE) [MILLI METRE]
    Upper Limit = "Level: 标高 2" (IFCLABEL)
  Constraints: 6 more contents on 6 objects not shown
  Dimensions | properties | on 7 objects (7 IFCWINDOW)
    Area = 2.2765640000001 (IFCAREAMEASURE) [SQUARE_METRE]
    Volume = 0.0411684500000015 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 2 objects (2 IFCSPACE)
    Area = 68.44 (IFCAREAMEASURE) [SQUARE_METRE]
    Computation Height = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Perimeter = 35200. (IFCLENGTHMEASURE) [MILLI METRE]
    Unbounded Height = 2438.4 (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 2 objects (2 IFCDOOR)
    Area = 2.63425399999998 (IFCAREAMEASURE) [SQUARE_METRE]
    Volume = 0.0951275999999994 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 2 objects (2 IFCRAILING)
    Length = 6491.61092462373 (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 2 objects (2 IFCBUILDINGSTOREY)
    Computation Height = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 1 object (1 IFCWALL)
    Area = 94.8837000000022 (IFCAREAMEASURE) [SQUARE_METRE]
    Length = 12000. (IFCLENGTHMEASURE) [MILLI METRE]
    Volume = 18.9767400000004 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 1 object (1 IFCWALL)
    Area = 45.3837000000011 (IFCAREAMEASURE) [SQUARE_METRE]
    Length = 6000. (IFCLENGTHMEASURE) [MILLI METRE]
    Volume = 9.0767400000002 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 1 object (1 IFCWALL)
    Area = 91.1511000000022 (IFCAREAMEASURE) [SQUARE_METRE]
    Length = 12000. (IFCLENGTHMEASURE) [MILLI METRE]
    Volume = 18.2302200000004 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions: 7 more contents on 5 objects not shown
  Energy Analysis | properties | on 2 objects (2 IFCSPACE)
    Actual Lighting Load = 0. (IFCPOWERMEASURE) [WATT]
    Actual Lighting Load per area = 0. (IFCREAL)
    Actual Power Load = 0. (IFCPOWERMEASURE) [WATT]
    Actual Power Load per area = 0. (IFCREAL)
    Area per Person = 28.5714285714286 (IFCAREAMEASURE) [SQUARE_METRE]
    Base Lighting Load on = "By Space Type" (IFCIDENTIFIER)
    Base Power Load on = "By Space Type" (IFCIDENTIFIER)
    Heat Load Values = "By Space Type" (IFCIDENTIFIER)
    Latent Heat Gain per person = 630.91814901261 (IFCREAL)
    Lighting Load Units = "Power Density" (IFCIDENTIFIER)
    Number of People = 0. (IFCREAL)
    Plenum Lighting Contribution = 0.2 (IFCREAL)
    Power Load Units = "Power Density" (IFCIDENTIFIER)
    Sensible Heat Gain per person = 788.647686265762 (IFCREAL)
    Specified Lighting Load = 0. (IFCPOWERMEASURE) [WATT]
    Specified Lighting Load per area = 10.7639104167097 (IFCREAL)
    Specified Power Load = 0. (IFCPOWERMEASURE) [WATT]
    Specified Power Load per area = 13.9930835417226 (IFCREAL)
    Total Heat Gain per person = 1419.56583527837 (IFCREAL)
  Identity Data | properties | on 2 objects (1 IFCDOOR, 1 IFCWINDOW)
    Mark = "2" (IFCTEXT)
  Identity Data | properties | on 2 objects (1 IFCDOOR, 1 IFCWINDOW)
    Mark = "3" (IFCTEXT)
  Identity Data | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Author = "" (IFCTEXT)
    Building Name = "" (IFCTEXT)
    Organization Description = "" (IFCTEXT)
    Organization Name = "" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCSPACE)
    Name = "房间" (IFCTEXT)
    Number = "1" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCSPACE)
    Name = "房间" (IFCTEXT)
    Number = "2" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCWINDOW)
    Mark = "1" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCWINDOW)
    Mark = "4" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCWINDOW)
    Mark = "5" (IFCTEXT)
  Identity Data: 7 more contents on 4 objects not shown
  Other | properties | on 7 objects (7 IFCWINDOW)
    Category = "Windows" (IFCLABEL)
    Family = "固定: 0915 x 1220mm" (IFCLABEL)
    Family and Type = "固定: 0915 x 1220mm" (IFCLABEL)
    Head Height = 2135. (IFCLENGTHMEASURE) [MILLI METRE]
    Host Id = "Basic Wall: 常规 - 200mm" (IFCLABEL)
    Type = "固定: 0915 x 1220mm" (IFCLABEL)
    Type Id = "固定: 0915 x 1220mm" (IFCLABEL)
  Other | properties | on 4 objects (4 IFCWALL)
    Category = "Walls" (IFCLABEL)
    Family = "Basic Wall: 常规 - 200mm" (IFCLABEL)
    Family and Type = "Basic Wall: 常规 - 200mm" (IFCLABEL)
    Type = "Basic Wall: 常规 - 200mm" (IFCLABEL)
    Type Id = "Basic Wall: 常规 - 200mm" (IFCLABEL)
  Other | properties | on 2 objects (2 IFCSPACE)
    Category = "Rooms" (IFCLABEL)
    Phase Id = "新构造" (IFCLABEL)
  Other | properties | on 2 objects (2 IFCSLAB)
    Category = "Floors" (IFCLABEL)
    Family = "Floor: 常规 - 150mm" (IFCLABEL)
    Family and Type = "Floor: 常规 - 150mm" (IFCLABEL)
    Type = "Floor: 常规 - 150mm" (IFCLABEL)
    Type Id = "Floor: 常规 - 150mm" (IFCLABEL)
  Other | properties | on 2 objects (2 IFCDOOR)
    Category = "Doors" (IFCLABEL)
    Family = "单扇 - 与墙齐: 750 x 2000mm" (IFCLABEL)
    Family and Type = "单扇 - 与墙齐: 750 x 2000mm" (IFCLABEL)
    Head Height = 2000. (IFCLENGTHMEASURE) [MILLI METRE]
    Host Id = "Basic Wall: 常规 - 200mm" (IFCLABEL)
    Type = "单扇 - 与墙齐: 750 x 2000mm" (IFCLABEL)
    Type Id = "单扇 - 与墙齐: 750 x 2000mm" (IFCLABEL)
  Other | properties | on 2 objects (2 IFCMEMBER)
    Category = "Supports" (IFCLABEL)
    Family = "Stringer: 梯边梁 - 50mm 宽度" (IFCLABEL)
    Family and Type = "Stringer: 梯边梁 - 50mm 宽度" (IFCLABEL)
    Type = "Stringer: 梯边梁 - 50mm 宽度" (IFCLABEL)
    Type Id = "Stringer: 梯边梁 - 50mm 宽度" (IFCLABEL)
  Other | properties | on 2 objects (2 IFCRAILING)
    Category = "Railings" (IFCLABEL)
    Family = "Railing: 900mm 圆管" (IFCLABEL)
    Family and Type = "Railing: 900mm 圆管" (IFCLABEL)
    Type = "Railing: 900mm 圆管" (IFCLABEL)
    Type Id = "Railing: 900mm 圆管" (IFCLABEL)
  Other | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
    Client Name = "所有者" (IFCTEXT)
    Project Address = "请在此处输入地址" (IFCTEXT)
    Project Issue Date = "出图日期" (IFCTEXT)
    Project Name = "项目名称" (IFCTEXT)
    Project Number = "项目编号" (IFCTEXT)
    Project Status = "项目状态" (IFCTEXT)
  Other: 7 more contents on 4 objects not shown
  Phasing | properties | on 21 objects (7 IFCWINDOW, 4 IFCWALL, 2 IFCDOOR, 2 IFCMEMBER)
    Phase Created = "新构造" (IFCLABEL)
  Phasing | properties | on 2 objects (2 IFCSPACE)
    Phase = "新构造" (IFCLABEL)
  Qto_WallBaseQuantities | quantities | on 1 object (1 IFCWALL)
    GrossFootprintArea = 2.4 [SQUARE_METRE]
    GrossSideArea = 94.8837000000022 [SQUARE_METRE]
    GrossVolume = 18.9767400000004 [CUBIC_METRE]
    Height = 8000.00000000018 [MILLI METRE]
    Length = 12000. [MILLI METRE]
    Width = 200. [MILLI METRE]
  Qto_WallBaseQuantities | quantities | on 1 object (1 IFCWALL)
    GrossFootprintArea = 1.2 [SQUARE_METRE]
    GrossSideArea = 45.3837000000011 [SQUARE_METRE]
    GrossVolume = 9.0767400000002 [CUBIC_METRE]
    Height = 8000.00000000018 [MILLI METRE]
    Length = 6000. [MILLI METRE]
    Width = 200. [MILLI METRE]
  Qto_WallBaseQuantities | quantities | on 1 object (1 IFCWALL)
    GrossFootprintArea = 2.4 [SQUARE_METRE]
    GrossSideArea = 91.1511000000022 [SQUARE_METRE]
    GrossVolume = 18.2302200000004 [CUBIC_METRE]
    Height = 8000.00000000018 [MILLI METRE]
    Length = 12000. [MILLI METRE]
    Width = 200. [MILLI METRE]
  Qto_WallBaseQuantities | quantities | on 1 object (1 IFCWALL)
    GrossFootprintArea = 1.2 [SQUARE_METRE]
    GrossSideArea = 45.7674000000011 [SQUARE_METRE]
    GrossVolume = 9.1534800000002 [CUBIC_METRE]
    Height = 8000.00000000018 [MILLI METRE]
    Length = 6000. [MILLI METRE]
    Width = 200. [MILLI METRE]
  Structural | properties | on 4 objects (4 IFCWALL)
    Enable Analytical Model = FALSE (IFCBOOLEAN)
    Structural = FALSE (IFCBOOLEAN)
    Structural Usage = "Non-bearing" (IFCIDENTIFIER)
  Structural | properties | on 2 objects (2 IFCSLAB)
    Enable Analytical Model = FALSE (IFCBOOLEAN)
    Structural = FALSE (IFCBOOLEAN)
  Pset_WallCommon | properties | on 4 objects (4 IFCWALL)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "Basic Wall:常规 - 200mm" (IFCIDENTIFIER)
  Pset_SlabCommon | properties | on 1 object (1 IFCSLAB)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    PitchAngle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Reference = "Floor:常规 - 150mm" (IFCIDENTIFIER)
  Pset_SlabCommon | properties | on 1 object (1 IFCSLAB)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "Floor:常规 - 150mm" (IFCIDENTIFIER)
  Qto_SlabBaseQuantities | quantities | on 1 object (1 IFCSLAB)
    GrossArea = 75.64 [SQUARE_METRE]
    GrossVolume = 11346. [CUBIC_METRE]
    Perimeter = 36800. [MILLI METRE]
    Width = 150. [MILLI METRE]
  Qto_SlabBaseQuantities | quantities | on 1 object (1 IFCSLAB)
    GrossArea = 75.64 [SQUARE_METRE]
    Perimeter = 44487.9218803945 [MILLI METRE]
  BaseQuantities | quantities | on 1 object (1 IFCOPENINGELEMENT)
    Depth = 150. [MILLI METRE]
    Height = 2743.96094019726 [MILLI METRE]
    Width = 1099.99999999999 [MILLI METRE]
  Pset_DoorCommon | properties | on 2 objects (2 IFCDOOR)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "单扇 - 与墙齐:750 x 2000mm" (IFCIDENTIFIER)
    ThermalTransmittance = 3.7021 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Qto_DoorBaseQuantities | quantities | on 2 objects (2 IFCDOOR)
    Area = 2.63425399999998 [SQUARE_METRE]
    Height = 2000. [MILLI METRE]
    Width = 750. [MILLI METRE]
  Pset_WindowCommon | properties | on 7 objects (7 IFCWINDOW)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "固定:0915 x 1220mm" (IFCIDENTIFIER)
    ThermalTransmittance = 3.6886 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Qto_WindowBaseQuantities | quantities | on 7 objects (7 IFCWINDOW)
    Area = 2.2765640000001 [SQUARE_METRE]
    Height = 1220. [MILLI METRE]
    Width = 915. [MILLI METRE]
  Pset_StairCommon | properties | on 1 object (1 IFCSTAIR)
    IsExternal = FALSE (IFCBOOLEAN)
    NumberOfRiser = 22. (IFCCOUNTMEASURE)
    NumberOfTreads = 21. (IFCCOUNTMEASURE)
    Reference = "Assembled Stair:Stair" (IFCIDENTIFIER)
    RiserHeight = 181.818181818182 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    TreadLength = 250. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_StairFlightCommon | properties | on 1 object (1 IFCSTAIRFLIGHT)
    NosingLength = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    NumberOfRiser = 22. (IFCCOUNTMEASURE)
    NumberOfTreads = 21. (IFCCOUNTMEASURE)
    Reference = "Non-Monolithic Run:50mm 踏板 13mm 踢面" (IFCIDENTIFIER)
    RiserHeight = 181.818181818182 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    TreadLength = 250. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    TreadLengthAtOffset = 250. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    WaistThickness = 1000. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    WalkingLineOffset = 500. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_MemberCommon | properties | on 2 objects (2 IFCMEMBER)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "Assembled Stair:Stair" (IFCIDENTIFIER)
    Slope = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Span = 50. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Qto_MemberBaseQuantities | quantities | on 2 objects (2 IFCMEMBER)
    CrossSectionArea = 2.55552342241084 [SQUARE_METRE]
    GrossSurfaceArea = 682421.383710445 [SQUARE_METRE]
    GrossVolume = 127.776171120542 [CUBIC_METRE]
    Length = 50. [MILLI METRE]
    NetSurfaceArea = 33.2606762349704 [SQUARE_METRE]
    NetVolume = 0.567427342241083 [CUBIC_METRE]
    OuterSurfaceArea = 682416.272663601 [SQUARE_METRE]
  Construction | properties | on 1 object (1 IFCSTAIRFLIGHT)
    Begin with Riser = TRUE (IFCBOOLEAN)
    End with Riser = TRUE (IFCBOOLEAN)
    Extend Below Riser Base = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Construction | properties | on 1 type object
    Function = "Exterior" (IFCIDENTIFIER)
    Width = 200. (IFCLENGTHMEASURE) [MILLI METRE]
    Wrapping at Ends = "None" (IFCIDENTIFIER)
    Wrapping at Inserts = "Do not wrap" (IFCIDENTIFIER)
  Construction | properties | on 1 type object
    Function = "Interior" (IFCIDENTIFIER)
    Wall Closure = "By host" (IFCIDENTIFIER)
  Construction | properties | on 1 type object
    Wall Closure = "By host" (IFCIDENTIFIER)
  Pset_RailingCommon | properties | on 2 objects (2 IFCRAILING)
    Height = 900. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Railing:900mm 圆管" (IFCIDENTIFIER)
  Qto_RailingBaseQuantities | quantities | on 2 objects (2 IFCRAILING)
    Length = 6491.61092462373 [MILLI METRE]
  Qto_OpeningElementBaseQuantities | quantities | on 4 objects (4 IFCOPENINGELEMENT)
    Depth = 200. [MILLI METRE]
    Height = 914.999999999999 [MILLI METRE]
    Width = 1220. [MILLI METRE]
  Qto_OpeningElementBaseQuantities | quantities | on 3 objects (3 IFCOPENINGELEMENT)
    Depth = 200. [MILLI METRE]
    Height = 915. [MILLI METRE]
    Width = 1220. [MILLI METRE]
  Qto_OpeningElementBaseQuantities | quantities | on 2 objects (2 IFCOPENINGELEMENT)
    Depth = 200. [MILLI METRE]
    Height = 750. [MILLI METRE]
    Width = 2000. [MILLI METRE]
  Pset_BuildingStoreyCommon | properties | on 2 objects (2 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    NumberOfStoreys = 2 (IFCINTEGER)
    Reference = "Project Information" (IFCIDENTIFIER)
  Analytical Properties(Type) | properties | on 2 objects (2 IFCSLAB)
    Absorptance = 0.7 (IFCREAL)
    Roughness = 3 (IFCINTEGER)
  Construction(Type) | properties | on 2 objects (2 IFCSLAB)
    Default Thickness = 150. (IFCLENGTHMEASURE) [MILLI METRE]
    Function = "Interior" (IFCIDENTIFIER)
  Construction(Type) | properties | on 2 objects (2 IFCRAILING)
    Angled Joins = "Add Vertical/Horizontal Segments" (IFCIDENTIFIER)
    Baluster Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Landing Height Adjustment = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Rail Connections = "Trim" (IFCIDENTIFIER)
    Railing Height = 900. (IFCLENGTHMEASURE) [MILLI METRE]
    Tangent Joins = "Extend Rails to Meet" (IFCIDENTIFIER)
    Use Landing Height Adjustment = FALSE (IFCBOOLEAN)
  Construction(Type) | properties | on 1 object (1 IFCSTAIR)
    Function = "Interior" (IFCIDENTIFIER)
    Landing Type = "Non-Monolithic Landing: 非整体休息平台" (IFCLABEL)
    Run Type = "Non-Monolithic Run: 50mm 踏板 13mm 踢面" (IFCLABEL)
  Graphics(Type) | properties | on 2 objects (2 IFCSLAB)
    Coarse Scale Fill Color = 0 (IFCINTEGER)
  Graphics(Type) | properties | on 1 object (1 IFCSTAIR)
    Cut Mark Type = "Stair Cut Mark: 单锯齿线" (IFCLABEL)
  Graphics(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Color = 8421504 (IFCINTEGER)
    Line Pattern = "中心线" (IFCLABEL)
    Line Weight = "1" (IFCIDENTIFIER)
    Symbol = "标高标头_正负零: 标高标头_正负零" (IFCLABEL)
    Symbol at End 1 Default = FALSE (IFCBOOLEAN)
    Symbol at End 2 Default = TRUE (IFCBOOLEAN)
  Graphics(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Color = 8421504 (IFCINTEGER)
    Line Pattern = "中心线" (IFCLABEL)
    Line Weight = "1" (IFCIDENTIFIER)
    Symbol = "上标高标头: 上标高标头" (IFCLABEL)
    Symbol at End 1 Default = FALSE (IFCBOOLEAN)
    Symbol at End 2 Default = TRUE (IFCBOOLEAN)
  Identity Data(Type) | properties | on 2 objects (2 IFCSLAB)
    Assembly Code = "" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    Type Name = "常规 - 150mm" (IFCTEXT)
  Identity Data(Type) | properties | on 2 objects (2 IFCMEMBER)
    Assembly Code = "" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    Type Name = "梯边梁 - 50mm 宽度" (IFCTEXT)
  Identity Data(Type) | properties | on 2 objects (2 IFCRAILING)
    Assembly Code = "" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    Type Name = "900mm 圆管" (IFCTEXT)
  Identity Data(Type) | properties | on 1 object (1 IFCSTAIR)
    Assembly Code = "" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    Type Name = "190mm 最大踢面 250mm 梯段" (IFCTEXT)
  Identity Data(Type) | properties | on 1 object (1 IFCSTAIRFLIGHT)
    Assembly Code = "" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    Type Name = "50mm 踏板 13mm 踢面" (IFCTEXT)
  Identity Data(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Type Name = "正负零标高" (IFCTEXT)
  Identity Data(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Type Name = "上标头" (IFCTEXT)
  Other(Type) | properties | on 2 objects (2 IFCSLAB)
    Category = "Floors" (IFCLABEL)
    Family Name = "Floor" (IFCTEXT)
  Other(Type) | properties | on 2 objects (2 IFCMEMBER)
    Category = "Supports" (IFCLABEL)
    Family Name = "Stringer" (IFCTEXT)
  Other(Type) | properties | on 2 objects (2 IFCRAILING)
    Category = "Railings" (IFCLABEL)
    Family Name = "Railing" (IFCTEXT)
  Other(Type) | properties | on 2 objects (2 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family Name = "Level" (IFCTEXT)
  Other(Type) | properties | on 1 object (1 IFCSTAIR)
    Category = "Stairs" (IFCLABEL)
    Family Name = "Assembled Stair" (IFCTEXT)
  Other(Type) | properties | on 1 object (1 IFCSTAIRFLIGHT)
    Category = "Runs" (IFCLABEL)
    Family Name = "Non-Monolithic Run" (IFCTEXT)
  Calculation Rules(Type) | properties | on 1 object (1 IFCSTAIR)
    Maximum Riser Height = 190. (IFCLENGTHMEASURE) [MILLI METRE]
    Minimum Run Width = 1000. (IFCLENGTHMEASURE) [MILLI METRE]
    Minimum Tread Depth = 250. (IFCLENGTHMEASURE) [MILLI METRE]
  Supports(Type) | properties | on 1 object (1 IFCSTAIR)
    Left Lateral Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Left Support = "Stringer (Closed)" (IFCIDENTIFIER)
    Left Support Type = "Stringer: 梯边梁 - 50mm 宽度" (IFCLABEL)
    Middle Support = FALSE (IFCBOOLEAN)
    Middle Support Number = 0 (IFCINTEGER)
    Right Lateral Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Right Support = "Stringer (Closed)" (IFCIDENTIFIER)
    Right Support Type = "Stringer: 梯边梁 - 50mm 宽度" (IFCLABEL)
  Risers(Type) | properties | on 1 object (1 IFCSTAIRFLIGHT)
    Riser = TRUE (IFCBOOLEAN)
    Riser Thickness = 12.5 (IFCLENGTHMEASURE) [MILLI METRE]
    Riser To Tread Connection = "Extend Riser Behind Tread" (IFCIDENTIFIER)
    Slanted = FALSE (IFCBOOLEAN)
  Treads(Type) | properties | on 1 object (1 IFCSTAIRFLIGHT)
    Apply Nosing Profile = "Front Only" (IFCIDENTIFIER)
    Nosing Length = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Tread = TRUE (IFCBOOLEAN)
    Tread Thickness = 50. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions(Type) | properties | on 2 objects (2 IFCMEMBER)
    Flip Section Profile = FALSE (IFCBOOLEAN)
    Structural Depth On Landing = 300. (IFCLENGTHMEASURE) [MILLI METRE]
    Structural Depth On Run = 150. (IFCLENGTHMEASURE) [MILLI METRE]
    Total Depth = 400. (IFCLENGTHMEASURE) [MILLI METRE]
    Width = 50. (IFCLENGTHMEASURE) [MILLI METRE]
  Handrail 1(Type) | properties | on 2 objects (2 IFCRAILING)
    Position = "None" (IFCIDENTIFIER)
  Handrail 2(Type) | properties | on 2 objects (2 IFCRAILING)
    Position = "None" (IFCIDENTIFIER)
  Top Rail(Type) | properties | on 2 objects (2 IFCRAILING)
    Height = 900. (IFCLENGTHMEASURE) [MILLI METRE]
    Type = "Top Rail Type: 圆形 - 40mm" (IFCLABEL)
    Use Top Rail = TRUE (IFCBOOLEAN)
  Constraints(Type) | properties | on 2 objects (2 IFCBUILDINGSTOREY)
    Elevation Base = "Project Base Point" (IFCIDENTIFIER)
  Analytical Properties | properties | on 1 type object
    Absorptance = 0.7 (IFCREAL)
    Roughness = 3 (IFCINTEGER)
  Analytical Properties | properties | on 1 type object
    Analytic Construction = "金属" (IFCTEXT)
    Heat Transfer Coefficient (U) = 3.7021 (IFCREAL)
    Solar Heat Gain Coefficient = 0. (IFCREAL)
    Thermal Resistance (R) = 0.270116960643959 (IFCREAL)
    Visual Light Transmittance = 0. (IFCREAL)
  Analytical Properties | properties | on 1 type object
    Analytic Construction = "1/8 英寸 Pilkington 单层玻璃" (IFCTEXT)
    Heat Transfer Coefficient (U) = 3.6886 (IFCREAL)
    Solar Heat Gain Coefficient = 0.78 (IFCREAL)
    Thermal Resistance (R) = 0.271105568508377 (IFCREAL)
    Visual Light Transmittance = 0.9 (IFCREAL)
  Graphics | properties | on 1 type object
    Coarse Scale Fill Color = 0 (IFCINTEGER)
  单扇 - 与墙齐:750 x 2000mm:337043 | predefined | on 2 type objects
  Materials and Finishes | properties | on 1 type object
    框架材质 = "门 - 框架" (IFCLABEL)
    门材质 = "门 - 嵌板" (IFCLABEL)
  Materials and Finishes | properties | on 1 type object
    框架内部材质 = "窗扇" (IFCLABEL)
    框架外部材质 = "窗扇" (IFCLABEL)
    玻璃嵌板材质 = "玻璃" (IFCLABEL)
    窗扇 = "窗扇" (IFCLABEL)
  固定:0915 x 1220mm:337141 | predefined | on 1 type object