IFC building model
Schema: "IFC4"
Description: "ViewDefinition [DesignTransferView_V1.0]"
File name: "Project Number"
Time stamp: "2022-04-28T12:31:27"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.07 : 28 Aug 2013"
Originating system: "20200210_1400(x64) - Exporter 20.3.3.0 - Alternate UI 20.3.3.0"
Application: "Autodesk Revit 2020 (ENU)" version "2020" identifier "Revit" by Organization "Autodesk Revit 2020 (ENU)"

People and organizations
  Person "ryan@openingdesign.com" of Organization (no name given)
  Owner history of Person "ryan@openingdesign.com" of Organization (no name given) | application "Autodesk Revit 2020 (ENU)" version "2020" identifier "Revit" by Organization "Autodesk Revit 2020 (ENU)" | change NOCHANGE | created 1651106052 (2022-04-28T00:34:12Z)

Units
  LENGTHUNIT: FOOT (conversion based)
  AREAUNIT: SQUARE FOOT (conversion based)
  VOLUMEUNIT: CUBIC FOOT (conversion based)
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  MOMENTOFINERTIAUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"
  LINEARFORCEUNIT: derived
  PLANARFORCEUNIT: derived

Spatial structure
IFCPROJECT "Project Number" | long name "**NAME OF PROJECT**" | phase "Project Status"
  IFCSITE "Default" | latitude 42° 21′ 30.344238″ | longitude -71° 3′ 35.194702″ | elevation above sea level 100.
    IFCBUILDING | postal address: "**ADDRESS OF PROJECT**", "<Default>"
      IFCBUILDINGSTOREY "BASEMENT (RENAME, BUT DON'T DELETE THIS LEVEL)" | long name "BASEMENT (RENAME, BUT DON'T DELETE THIS LEVEL)" | object type "Level:Project Base Point" | elevation -8.
        contains 9 elements
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 680:Generic Models 1" | object type "Generic Models 680:Generic Models 1" | names: "Generic Models 680:Generic Models 1:3349499" | material: "CONCRETE GRADE BEAM W/ 4" CONCRETE SLAB" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 668:Generic Models 1" | object type "Generic Models 668:Generic Models 1" | names: "Generic Models 668:Generic Models 1:3376299" | material: "CONCRETE SLAB - 2% SLOPE AWAY FROM BUILDING" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 691:Generic Models 1" | object type "Generic Models 691:Generic Models 1" | names: "Generic Models 691:Generic Models 1:3376333" | material: "1/2" JOINT FILLER" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Dowel2:Dowel" | object type "Dowel2:Dowel" | names: "Dowel2:Dowel:3377841" | material: "#4 J's @ 24" O.C. - GROUTED IN PRECAST KEYS AND CORES" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 694:Generic Models 1" | object type "Generic Models 694:Generic Models 1" | names: "Generic Models 694:Generic Models 1:3378539" | material: "(2) #5's" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 695:Generic Models 1" | object type "Generic Models 695:Generic Models 1" | names: "Generic Models 695:Generic Models 1:3378568" | material: "(2) #5's" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 696:Generic Models 1" | object type "Generic Models 696:Generic Models 1" | names: "Generic Models 696:Generic Models 1:3378646" | material: "(2) #5's" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 697:Generic Models 1" | object type "Generic Models 697:Generic Models 1" | names: "Generic Models 697:Generic Models 1:3378657" | material: "(2) #5's" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 16:Walls 16" | object type "Walls 16:Walls 16" | names: "Walls 16:Walls 16:3379606" | material: "6 MIL POLYETHILENE VAPOR BARRIER" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
      IFCBUILDINGSTOREY "1ST FLOOR (RENAME, BUT DON'T DELETE THIS LEVEL)" | long name "1ST FLOOR (RENAME, BUT DON'T DELETE THIS LEVEL)" | object type "Level:Project Base Point" | elevation 0.
        contains 306 elements
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 630:Generic Models 1" | object type "Generic Models 630:Generic Models 1" | names: "Generic Models 630:Generic Models 1:3348881" | material: "WOOD TOP PLATE" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 637:Generic Models 1" | object type "Generic Models 637:Generic Models 1" | names: "Generic Models 637:Generic Models 1:3348961" | material: "DOUBLE 2X WOOD TOP PLATE" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 639:Generic Models 1" | object type "Generic Models 639:Generic Models 1" | names: "Generic Models 639:Generic Models 1:3348980" | material: "FIBER CEMENT LAPSIDING" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 645:Generic Models 1" | object type "Generic Models 645:Generic Models 1" | names: "Generic Models 645:Generic Models 1:3349044" | material: "2X WOOD STUD" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 650:Generic Models 1" | object type "Generic Models 650:Generic Models 1" | names: "Generic Models 650:Generic Models 1:3349107" | material: "WOOD TRUSS FLOOR ASSEMBLY - FILL CAVITY WITH BATT. INSULATION - (UL - L521 FLOOR ASSEMBLY)" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 653:Generic Models 1" | object type "Generic Models 653:Generic Models 1" | names: "Generic Models 653:Generic Models 1:3349148" | material: "5/8" GYP. BD" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 660:Generic Models 1" | object type "Generic Models 660:Generic Models 1" | names: "Generic Models 660:Generic Models 1:3349240" | material: "LVL RIM BOARD - SEE STRUCT. DWGS" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 669:Generic Models 1" | object type "Generic Models 669:Generic Models 1" | names: "Generic Models 669:Generic Models 1:3349361" | material: "DOUBLE 2X WOOD TOP PLATE" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 603:Generic Models 1" | object type "Generic Models 603:Generic Models 1" | names: "Generic Models 603:Generic Models 1:3355245" | material: "CLAD WOOD DOOR W/ INSULATED TEMPERED GLAZING" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 632:Generic Models 1" | object type "Generic Models 632:Generic Models 1" | names: "Generic Models 632:Generic Models 1:3355274" | material: "CLAD WOOD DOOR W/ INSULATED TEMPERED GLAZING" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 633:Generic Models 1" | object type "Generic Models 633:Generic Models 1" | names: "Generic Models 633:Generic Models 1:3358740" | material: "JAMB EXTENSION" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 634:Generic Models 1" | object type "Generic Models 634:Generic Models 1" | names: "Generic Models 634:Generic Models 1:3358753" | material: "JAMB EXTENSION" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          3 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "060523 - W_P_C - Fastenings - Generic:Screw - SDWS" | object type "060523 - W_P_C - Fastenings - Generic:Screw - SDWS" | names: "060523 - W_P_C - Fastenings - Generic:Screw - SDWS:3359177", "060523 - W_P_C - Fastenings - Generic:Screw - SDWS:3359226", "060523 - W_P_C - Fastenings - Generic:Screw - SDWS:3414576" | material: "STRONG-DRIVE SDWS TIMBER SCREW (EXTERIOR GRADE)" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          4 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "060523 - W_P_C - Fastenings - Generic:_METAL STUD - HEAD - GENERIC" | object type "060523 - W_P_C - Fastenings - Generic:_METAL STUD - HEAD - GENERIC" | names: "060523 - W_P_C - Fastenings - Generic:_METAL STUD - HEAD - GENERIC:3359401", "060523 - W_P_C - Fastenings - Generic:_METAL STUD - HEAD - GENERIC:3372860", "060523 - W_P_C - Fastenings - Generic:_METAL STUD - HEAD - GENERIC:3372916" (+1 more) | material: "AT HEAD FASTENER AT 24" O.C." | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 655:Generic Models 1" | object type "Generic Models 655:Generic Models 1" | names: "Generic Models 655:Generic Models 1:3361700" | material: "STARTER STRIP" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 656:Generic Models 1" | object type "Generic Models 656:Generic Models 1" | names: "Generic Models 656:Generic Models 1:3361895" | material: "DRAINAGE WRAP - ASTM 2273" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 674:Generic Models 1" | object type "Generic Models 674:Generic Models 1" | names: "Generic Models 674:Generic Models 1:3362580" | material: "METAL FLASHING" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 629:Generic Models 1" | object type "Generic Models 629:Generic Models 1" | names: "Generic Models 629:Generic Models 1:3365566" | material: "5/8" GYP. BD @ CEILING" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 13:Walls 12" | object type "Walls 13:Walls 12" | names: "Walls 13:Walls 12:3365967" | material: "LVL HEADER - SEE STRUCT. DWGS" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 683:Generic Models 1" | object type "Generic Models 683:Generic Models 1" | names: "Generic Models 683:Generic Models 1:3366838" | material: "1/2" CDX OR OSB PLYWOOD - SEE STRUCT DWGS" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 684:Generic Models 1" | object type "Generic Models 684:Generic Models 1" | names: "Generic Models 684:Generic Models 1:3369281" | material: "BATT INSULATION - FILL ENTIRE CAVITY" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          2 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "050523 - Metal fastenings - Joist Hanger - Generic:HUCQ1.81/9-SDS" | object type "050523 - Metal fastenings - Joist Hanger - Generic:HUCQ1.81/9-SDS" | names: "050523 - Metal fastenings - Joist Hanger - Generic:HUCQ1.81/9-SDS:3370663", "050523 - Metal fastenings - Joist Hanger - Generic:HUCQ1.81/9-SDS:3385371" | material: "SIMPSON HUC46 JOIST HANGER WITH CONCEALED FLANGES - HDG - UNPAINTED" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 652:Generic Models 1" | object type "Generic Models 652:Generic Models 1" | names: "Generic Models 652:Generic Models 1:3374336" | material: "WOOD TOP PLATE" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 689:Generic Models 1" | object type "Generic Models 689:Generic Models 1" | names: "Generic Models 689:Generic Models 1:3375827" | material: "#4 @ 16" OC EACH WAY - LOCATED AT MID-DEPTH" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 693:Generic Models 1" | object type "Generic Models 693:Generic Models 1" | names: "Generic Models 693:Generic Models 1:3377082" | material: "(2) #5's" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 690:Generic Models 1" | object type "Generic Models 690:Generic Models 1" | names: "Generic Models 690:Generic Models 1:3377121" | material: "(2) #5's" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 692:Generic Models 1" | object type "Generic Models 692:Generic Models 1" | names: "Generic Models 692:Generic Models 1:3377442" | material: "(2) #5's" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 698:Generic Models 1" | object type "Generic Models 698:Generic Models 1" | names: "Generic Models 698:Generic Models 1:3379663" | material: "RESILIENT CHANNEL - 25 GA. FURRING CHANNELS INSTALLED HORIZONTALLY SPACED 24 IN. OC" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          3 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "060523 - W_P_C - Fastenings - Generic:Screw - SDWS" | object type "060523 - W_P_C - Fastenings - Generic:Screw - SDWS" | names: "060523 - W_P_C - Fastenings - Generic:Screw - SDWS:3385094", "060523 - W_P_C - Fastenings - Generic:Screw - SDWS:3385095", "060523 - W_P_C - Fastenings - Generic:Screw - SDWS:3414135" | material: "STRONG-DRIVE SDWS TIMBER SCREW (EXTERIOR GRADE)" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 671:Generic Models 1" | object type "Generic Models 671:Generic Models 1" | names: "Generic Models 671:Generic Models 1:3391046" | material: "FIBER CEMENT LAPSIDING" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 673:Generic Models 1" | object type "Generic Models 673:Generic Models 1" | names: "Generic Models 673:Generic Models 1:3392722" | material: "WOOD TRUSS - SEE STRUCT DWGS" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 705:Generic Models 1" | object type "Generic Models 705:Generic Models 1" | names: "Generic Models 705:Generic Models 1:3392727" | material: "WOOD TRUSS - SEE STRUCT DWGS" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 688:Generic Models 1" | object type "Generic Models 688:Generic Models 1" | names: "Generic Models 688:Generic Models 1:3392814" | material: "2X BLOCKING" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 631:Generic Models 1" | object type "Generic Models 631:Generic Models 1" | names: "Generic Models 631:Generic Models 1:3416914" | material: "FIBER CEMENT LAPSIDING" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 657:Generic Models 1" | object type "Generic Models 657:Generic Models 1" | names: "Generic Models 657:Generic Models 1:3416939" | material: "FIBER CEMENT LAPSIDING" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 658:Generic Models 1" | object type "Generic Models 658:Generic Models 1" | names: "Generic Models 658:Generic Models 1:3416954" | material: "FIBER CEMENT LAPSIDING" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 663:Generic Models 1" | object type "Generic Models 663:Generic Models 1" | names: "Generic Models 663:Generic Models 1:3416984" | material: "FIBER CEMENT LAPSIDING" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 672:Generic Models 1" | object type "Generic Models 672:Generic Models 1" | names: "Generic Models 672:Generic Models 1:3417015" | material: "FIBER CEMENT LAPSIDING" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 678:Generic Models 1" | object type "Generic Models 678:Generic Models 1" | names: "Generic Models 678:Generic Models 1:3417040" | material: "FIBER CEMENT LAPSIDING" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          36 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "060523 - W_P_C - Fastenings - Generic:_METAL STUD - HEAD - GENERIC" | object type "060523 - W_P_C - Fastenings - Generic:_METAL STUD - HEAD - GENERIC" | names: "060523 - W_P_C - Fastenings - Generic:_METAL STUD - HEAD - GENERIC:3417216", "060523 - W_P_C - Fastenings - Generic:_METAL STUD - HEAD - GENERIC:3417255", "060523 - W_P_C - Fastenings - Generic:_METAL STUD - HEAD - GENERIC:3422568" (+33 more) | material: "AT HEAD FASTENER AT 24" O.C." | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "C CHANNEL 2:C CHANNEL 2" | object type "C CHANNEL 2:C CHANNEL 2" | names: "C CHANNEL 2:C CHANNEL 2:3419724" | material: "STEEL C CHANNEL - HDG - SEE STRUCT DWGS" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "RAILING 2:RAILING 2" | object type "RAILING 2:RAILING 2" | names: "RAILING 2:RAILING 2:3421799" | material: "(2) 2X4s - EXT STAIN - DARK" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "RAILING 14:RAILING 3" | object type "RAILING 14:RAILING 3" | names: "RAILING 14:RAILING 3:3422279" | material: "2" X 4" - 6GA GALV. MESH" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "RAILING 15:RAILING 3" | object type "RAILING 15:RAILING 3" | names: "RAILING 15:RAILING 3:3422300" | material: "2" X 4" - 6GA GALV. MESH" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "RAILING 16:RAILING 3" | object type "RAILING 16:RAILING 3" | names: "RAILING 16:RAILING 3:3422321" | material: "2" X 4" - 6GA GALV. MESH" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "RAILING 17:RAILING 3" | object type "RAILING 17:RAILING 3" | names: "RAILING 17:RAILING 3:3422345" | material: "2" X 4" - 6GA GALV. MESH" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "RAILING 18:RAILING 3" | object type "RAILING 18:RAILING 3" | names: "RAILING 18:RAILING 3:3422367" | material: "2" X 4" - 6GA GALV. MESH" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "RAILING 30:RAILING 20" | object type "RAILING 30:RAILING 20" | names: "RAILING 30:RAILING 20:3423266" | material: "2" X 4" - 6GA GALV. MESH" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "RAILING 31:RAILING 20" | object type "RAILING 31:RAILING 20" | names: "RAILING 31:RAILING 20:3423313" | material: "2" X 4" - 6GA GALV. MESH" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "RAILING 32:RAILING 20" | object type "RAILING 32:RAILING 20" | names: "RAILING 32:RAILING 20:3423363" | material: "2" X 4" - 6GA GALV. MESH" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "RAILING 33:RAILING 20" | object type "RAILING 33:RAILING 20" | names: "RAILING 33:RAILING 20:3423382" | material: "2" X 4" - 6GA GALV. MESH" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "RAILING 34:RAILING 20" | object type "RAILING 34:RAILING 20" | names: "RAILING 34:RAILING 20:3423401" | material: "2" X 4" - 6GA GALV. MESH" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "RAILING 29:RAILING 20" | object type "RAILING 29:RAILING 20" | names: "RAILING 29:RAILING 20:3424241" | material: "2" X 4" - 6GA GALV. MESH" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "RAILING 35:RAILING 20" | object type "RAILING 35:RAILING 20" | names: "RAILING 35:RAILING 20:3424259" | material: "2" X 4" - 6GA GALV. MESH" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          2 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "060523 - W_P_C - Fastenings - Generic:Screw - SDWS 3" | object type "060523 - W_P_C - Fastenings - Generic:Screw - SDWS 3" | names: "060523 - W_P_C - Fastenings - Generic:Screw - SDWS 3:3424901", "060523 - W_P_C - Fastenings - Generic:Screw - SDWS 3:3474092" | material: "TRIM HEAD SCREWS AT RAILING - EXTERIOR GRADE" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          2 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "060523 - W_P_C - Fastenings - Generic:Thru-Bolt - .8750 - 7/8 2" | object type "060523 - W_P_C - Fastenings - Generic:Thru-Bolt - .8750 - 7/8 2" | names: "060523 - W_P_C - Fastenings - Generic:Thru-Bolt - .8750 - 7/8 2:3426754", "060523 - W_P_C - Fastenings - Generic:Thru-Bolt - .8750 - 7/8 2:3449876" | material: "EXPOSED LAG BOLTS" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "RAILING 37:RAILING 20" | object type "RAILING 37:RAILING 20" | names: "RAILING 37:RAILING 20:3429977" | material: "3/4" DEEP ROUTED NOTCH" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "RAILING 19:RAILING 2" | object type "RAILING 19:RAILING 2" | names: "RAILING 19:RAILING 2:3443527" | material: "(2) 2X4s - EXT STAIN - DARK" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "RAILING 38:RAILING 2" | object type "RAILING 38:RAILING 2" | names: "RAILING 38:RAILING 2:3443871" | material: "(2) 2X4s - EXT STAIN - DARK" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "RAILING 39:RAILING 20" | object type "RAILING 39:RAILING 20" | names: "RAILING 39:RAILING 20:3444095" | material: "2" X 4" - 6GA GALV. MESH" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "RAILING 40:RAILING 20" | object type "RAILING 40:RAILING 20" | names: "RAILING 40:RAILING 20:3444114" | material: "2" X 4" - 6GA GALV. MESH" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "RAILING 41:RAILING 20" | object type "RAILING 41:RAILING 20" | names: "RAILING 41:RAILING 20:3444142" | material: "2" X 4" - 6GA GALV. MESH" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "RAILING 42:RAILING 20" | object type "RAILING 42:RAILING 20" | names: "RAILING 42:RAILING 20:3444159" | material: "2" X 4" - 6GA GALV. MESH" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "RAILING 43:RAILING 20" | object type "RAILING 43:RAILING 20" | names: "RAILING 43:RAILING 20:3444218" | material: "3/4" DEEP ROUTED NOTCH" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "RAILING 44:RAILING 20" | object type "RAILING 44:RAILING 20" | names: "RAILING 44:RAILING 20:3444239" | material: "3/4" DEEP ROUTED NOTCH" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "RAILING 45:RAILING 20" | object type "RAILING 45:RAILING 20" | names: "RAILING 45:RAILING 20:3444258" | material: "3/4" DEEP ROUTED NOTCH" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          2 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "060523 - W_P_C - Fastenings - Generic:Screw - SDWS 4" | object type "060523 - W_P_C - Fastenings - Generic:Screw - SDWS 4" | names: "060523 - W_P_C - Fastenings - Generic:Screw - SDWS 4:3445799", "060523 - W_P_C - Fastenings - Generic:Screw - SDWS 4:3474418" | material: "(X) TRIM HEAD SCREW (EXTERIOR GRADE) AT EACH JOIST" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          3 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "060523 - W_P_C - Fastenings - Generic:Screw - SDWS 3" | object type "060523 - W_P_C - Fastenings - Generic:Screw - SDWS 3" | names: "060523 - W_P_C - Fastenings - Generic:Screw - SDWS 3:3446159", "060523 - W_P_C - Fastenings - Generic:Screw - SDWS 3:3468478", "060523 - W_P_C - Fastenings - Generic:Screw - SDWS 3:3468784" | material: "TRIM HEAD SCREWS AT RAILING - EXTERIOR GRADE" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          3 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "060523 - W_P_C - Fastenings - Generic:Screw - SDWS 3" | object type "060523 - W_P_C - Fastenings - Generic:Screw - SDWS 3" | names: "060523 - W_P_C - Fastenings - Generic:Screw - SDWS 3:3446161", "060523 - W_P_C - Fastenings - Generic:Screw - SDWS 3:3468479", "060523 - W_P_C - Fastenings - Generic:Screw - SDWS 3:3468785" | material: "TRIM HEAD SCREWS AT RAILING - EXTERIOR GRADE" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "RAILING 49:RAILING 20" | object type "RAILING 49:RAILING 20" | names: "RAILING 49:RAILING 20:3446183" | material: "3/4" DEEP ROUTED NOTCH" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "RAILING 51:RAILING 20" | object type "RAILING 51:RAILING 20" | names: "RAILING 51:RAILING 20:3446196" | material: "3/4" DEEP ROUTED NOTCH" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "RAILING 52:RAILING 20" | object type "RAILING 52:RAILING 20" | names: "RAILING 52:RAILING 20:3446209" | material: "3/4" DEEP ROUTED NOTCH" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "RAILING 53:RAILING 20" | object type "RAILING 53:RAILING 20" | names: "RAILING 53:RAILING 20:3446222" | material: "3/4" DEEP ROUTED NOTCH" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "RAILING 55:RAILING 20" | object type "RAILING 55:RAILING 20" | names: "RAILING 55:RAILING 20:3446256" | material: "3/4" DEEP ROUTED NOTCH" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "RAILING 56:RAILING 20" | object type "RAILING 56:RAILING 20" | names: "RAILING 56:RAILING 20:3446269" | material: "3/4" DEEP ROUTED NOTCH" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "RAILING 57:RAILING 20" | object type "RAILING 57:RAILING 20" | names: "RAILING 57:RAILING 20:3446282" | material: "3/4" DEEP ROUTED NOTCH" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          4 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "060523 - W_P_C - Fastenings - Generic:Thru-Bolt - .8750 - 7/8 2" | object type "060523 - W_P_C - Fastenings - Generic:Thru-Bolt - .8750 - 7/8 2" | names: "060523 - W_P_C - Fastenings - Generic:Thru-Bolt - .8750 - 7/8 2:3446826", "060523 - W_P_C - Fastenings - Generic:Thru-Bolt - .8750 - 7/8 2:3446834", "060523 - W_P_C - Fastenings - Generic:Thru-Bolt - .8750 - 7/8 2:3446971" (+1 more) | material: "EXPOSED LAG BOLTS" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "060523 - W_P_C - Fastenings - Generic:Thru-Bolt - .8750 - 7/8 2" | object type "060523 - W_P_C - Fastenings - Generic:Thru-Bolt - .8750 - 7/8 2" | names: "060523 - W_P_C - Fastenings - Generic:Thru-Bolt - .8750 - 7/8 2:3448553" | material: "EXPOSED LAG BOLTS" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "060523 - W_P_C - Fastenings - Generic:Thru-Bolt - .8750 - 7/8 2" | object type "060523 - W_P_C - Fastenings - Generic:Thru-Bolt - .8750 - 7/8 2" | names: "060523 - W_P_C - Fastenings - Generic:Thru-Bolt - .8750 - 7/8 2:3453879" | material: "EXPOSED LAG BOLTS" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "060523 - W_P_C - Fastenings - Generic:Thru-Bolt - .8750 - 7/8 2" | object type "060523 - W_P_C - Fastenings - Generic:Thru-Bolt - .8750 - 7/8 2" | names: "060523 - W_P_C - Fastenings - Generic:Thru-Bolt - .8750 - 7/8 2:3453881" | material: "EXPOSED LAG BOLTS" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 679:Generic Models 1" | object type "Generic Models 679:Generic Models 1" | names: "Generic Models 679:Generic Models 1:3454853" | material: "WOOD TRUSS - SEE STRUCT DWGS" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 737:Generic Models 1" | object type "Generic Models 737:Generic Models 1" | names: "Generic Models 737:Generic Models 1:3456254" | material: "BLOCKING TYP - SEE STRUCTURAL" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "060523 - W_P_C - Fastenings - Generic:_3/4" x 4"" | object type "060523 - W_P_C - Fastenings - Generic:_3/4" x 4"" | names: "060523 - W_P_C - Fastenings - Generic:_3/4" x 4":3456552" | material: "EXPOSED LAG BOLTS" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          2 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "060523 - W_P_C - Fastenings - Generic:_3/4" x 4"" | object type "060523 - W_P_C - Fastenings - Generic:_3/4" x 4"" | names: "060523 - W_P_C - Fastenings - Generic:_3/4" x 4":3458145", "060523 - W_P_C - Fastenings - Generic:_3/4" x 4":3468077" | material: "EXPOSED LAG BOLTS" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 740:Generic Models 1" | object type "Generic Models 740:Generic Models 1" | names: "Generic Models 740:Generic Models 1:3460333" | material: "BLOCKING TYP - SEE STRUCTURAL" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "corrugated metal wall4:corrugated metal wall" | object type "corrugated metal wall4:corrugated metal wall" | names: "corrugated metal wall4:corrugated metal wall:3462272" | material: "7/8" CORRUGATED METAL - EXPOSED FASTENERS" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 33:Walls 13" | object type "Walls 33:Walls 13" | names: "Walls 33:Walls 13:3463178" | material: "(3) 2X6" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 34:Walls 13" | object type "Walls 34:Walls 13" | names: "Walls 34:Walls 13:3463192" | material: "(3) 2X6" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 35:Walls 13" | object type "Walls 35:Walls 13" | names: "Walls 35:Walls 13:3463206" | material: "(3) 2X6" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 36:Walls 13" | object type "Walls 36:Walls 13" | names: "Walls 36:Walls 13:3463220" | material: "(3) 2X6" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 37:Walls 13" | object type "Walls 37:Walls 13" | names: "Walls 37:Walls 13:3463234" | material: "(3) 2X6" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 38:Walls 13" | object type "Walls 38:Walls 13" | names: "Walls 38:Walls 13:3463248" | material: "(3) 2X6" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 39:Walls 13" | object type "Walls 39:Walls 13" | names: "Walls 39:Walls 13:3463262" | material: "(2) 2X6" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 40:Walls 13" | object type "Walls 40:Walls 13" | names: "Walls 40:Walls 13:3463276" | material: "(2) 2X6" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 41:Walls 13" | object type "Walls 41:Walls 13" | names: "Walls 41:Walls 13:3463290" | material: "(2) 2X6" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 42:Walls 13" | object type "Walls 42:Walls 13" | names: "Walls 42:Walls 13:3463304" | material: "(2) 2X6" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 665:Generic Models 1" | object type "Generic Models 665:Generic Models 1" | names: "Generic Models 665:Generic Models 1:3463455" | material: "BLOCKING TYP - SEE STRUCTURAL" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 741:Generic Models 1" | object type "Generic Models 741:Generic Models 1" | names: "Generic Models 741:Generic Models 1:3464049" | material: "BLOCKING TYP - SEE STRUCTURAL" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 742:Generic Models 1" | object type "Generic Models 742:Generic Models 1" | names: "Generic Models 742:Generic Models 1:3467023" | material: "BLOCKING TYP" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 45:Walls 13" | object type "Walls 45:Walls 13" | names: "Walls 45:Walls 13:3467139" | material: "DOUBLE 2X WOOD TOP PLATE" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 46:Walls 13" | object type "Walls 46:Walls 13" | names: "Walls 46:Walls 13:3467153" | material: "2X10 JOISTS" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 744:Generic Models 1" | object type "Generic Models 744:Generic Models 1" | names: "Generic Models 744:Generic Models 1:3467325" | material: "WOOD TRUSS - SEE STRUCT DWGS" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 745:Generic Models 1" | object type "Generic Models 745:Generic Models 1" | names: "Generic Models 745:Generic Models 1:3467338" | material: "WOOD TRUSS - SEE STRUCT DWGS" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 748:Generic Models 1" | object type "Generic Models 748:Generic Models 1" | names: "Generic Models 748:Generic Models 1:3467383" | material: "WOOD TRUSS - SEE STRUCT DWGS" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "RAILING 50:RAILING 20" | object type "RAILING 50:RAILING 20" | names: "RAILING 50:RAILING 20:3467824" | material: "2" X 4" - 6GA GALV. MESH" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "RAILING 58:RAILING 20" | object type "RAILING 58:RAILING 20" | names: "RAILING 58:RAILING 20:3467842" | material: "2" X 4" - 6GA GALV. MESH" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "RAILING 59:RAILING 20" | object type "RAILING 59:RAILING 20" | names: "RAILING 59:RAILING 20:3467860" | material: "2" X 4" - 6GA GALV. MESH" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 738:Generic Models 1" | object type "Generic Models 738:Generic Models 1" | names: "Generic Models 738:Generic Models 1:3467993" | material: "WOOD TRUSS - SEE STRUCT DWGS" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 750:Generic Models 1" | object type "Generic Models 750:Generic Models 1" | names: "Generic Models 750:Generic Models 1:3468031" | material: "BLOCKING TYP - SEE STRUCTURAL" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          3 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "060523 - W_P_C - Fastenings - Generic:Thru-Bolt - .8750 - 7/8 2" | object type "060523 - W_P_C - Fastenings - Generic:Thru-Bolt - .8750 - 7/8 2" | names: "060523 - W_P_C - Fastenings - Generic:Thru-Bolt - .8750 - 7/8 2:3469013", "060523 - W_P_C - Fastenings - Generic:Thru-Bolt - .8750 - 7/8 2:3469023", "060523 - W_P_C - Fastenings - Generic:Thru-Bolt - .8750 - 7/8 2:3469031" | material: "EXPOSED LAG BOLTS" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          2 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "060523 - W_P_C - Fastenings - Generic:Thru-Bolt - .8750 - 7/8 2" | object type "060523 - W_P_C - Fastenings - Generic:Thru-Bolt - .8750 - 7/8 2" | names: "060523 - W_P_C - Fastenings - Generic:Thru-Bolt - .8750 - 7/8 2:3469129", "060523 - W_P_C - Fastenings - Generic:Thru-Bolt - .8750 - 7/8 2:3469130" | material: "EXPOSED LAG BOLTS" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "060523 - W_P_C - Fastenings - Generic:Thru-Bolt - .8750 - 7/8 2" | object type "060523 - W_P_C - Fastenings - Generic:Thru-Bolt - .8750 - 7/8 2" | names: "060523 - W_P_C - Fastenings - Generic:Thru-Bolt - .8750 - 7/8 2:3469167" | material: "EXPOSED LAG BOLTS" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "060523 - W_P_C - Fastenings - Generic:Thru-Bolt - .8750 - 7/8 2" | object type "060523 - W_P_C - Fastenings - Generic:Thru-Bolt - .8750 - 7/8 2" | names: "060523 - W_P_C - Fastenings - Generic:Thru-Bolt - .8750 - 7/8 2:3469168" | material: "EXPOSED LAG BOLTS" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          3 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "060523 - W_P_C - Fastenings - Generic:Thru-Bolt - .8750 - 7/8 2" | object type "060523 - W_P_C - Fastenings - Generic:Thru-Bolt - .8750 - 7/8 2" | names: "060523 - W_P_C - Fastenings - Generic:Thru-Bolt - .8750 - 7/8 2:3473235", "060523 - W_P_C - Fastenings - Generic:Thru-Bolt - .8750 - 7/8 2:3474010", "060523 - W_P_C - Fastenings - Generic:Thru-Bolt - .8750 - 7/8 2:3474019" | material: "EXPOSED LAG BOLTS" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "060523 - W_P_C - Fastenings - Generic:Thru-Bolt - .8750 - 7/8 2" | object type "060523 - W_P_C - Fastenings - Generic:Thru-Bolt - .8750 - 7/8 2" | names: "060523 - W_P_C - Fastenings - Generic:Thru-Bolt - .8750 - 7/8 2:3473950" | material: "EXPOSED LAG BOLTS" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "060523 - W_P_C - Fastenings - Generic:Thru-Bolt - .8750 - 7/8 2" | object type "060523 - W_P_C - Fastenings - Generic:Thru-Bolt - .8750 - 7/8 2" | names: "060523 - W_P_C - Fastenings - Generic:Thru-Bolt - .8750 - 7/8 2:3473960" | material: "EXPOSED LAG BOLTS" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 746:Generic Models 1" | object type "Generic Models 746:Generic Models 1" | names: "Generic Models 746:Generic Models 1:3476264" | material: "WOOD TRUSS - SEE STRUCT DWGS" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 757:Generic Models 1" | object type "Generic Models 757:Generic Models 1" | names: "Generic Models 757:Generic Models 1:3476297" | material: "WOOD TRUSS - SEE STRUCT DWGS" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 760:Generic Models 1" | object type "Generic Models 760:Generic Models 1" | names: "Generic Models 760:Generic Models 1:3476325" | material: "BLOCKING TYP" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 765:Generic Models 1" | object type "Generic Models 765:Generic Models 1" | names: "Generic Models 765:Generic Models 1:3476667" | material: "WOOD TRUSS - SEE STRUCT DWGS" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 766:Generic Models 1" | object type "Generic Models 766:Generic Models 1" | names: "Generic Models 766:Generic Models 1:3476680" | material: "WOOD TRUSS - SEE STRUCT DWGS" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 771:Generic Models 1" | object type "Generic Models 771:Generic Models 1" | names: "Generic Models 771:Generic Models 1:3476742" | material: "WOOD TRUSS - SEE STRUCT DWGS" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 772:Generic Models 1" | object type "Generic Models 772:Generic Models 1" | names: "Generic Models 772:Generic Models 1:3476755" | material: "BLOCKING TYP - SEE STRUCTURAL" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "corrugated metal wall11:corrugated metal wall" | object type "corrugated metal wall11:corrugated metal wall" | names: "corrugated metal wall11:corrugated metal wall:3476834" | material: "1/2" CDX OR OSB PLYWOOD - SEE STRUCT DWGS" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "C CHANNEL1:C CHANNEL" | object type "C CHANNEL1:C CHANNEL" | names: "C CHANNEL1:C CHANNEL:3479589" | material: "1/4" COPED STEEL C CHANNEL - HDG - SEE STRUCT DWGS" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "3/8" BENT STEEL PLATE2:3/8" BENT STEEL PLATE" | object type "3/8" BENT STEEL PLATE2:3/8" BENT STEEL PLATE" | names: "3/8" BENT STEEL PLATE2:3/8" BENT STEEL PLATE:3479659" | material: "3/8" BENT STEEL PLATE - HDG" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCWALL | type IFCWALLTYPE "corrugated metal wall8:corrugated metal wall" | object type "corrugated metal wall8:corrugated metal wall" | names: "corrugated metal wall8:corrugated metal wall:3480466" | material: "5/8" GYP. BD" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 48:Walls 13" | object type "Walls 48:Walls 13" | names: "Walls 48:Walls 13:3481030" | material: "2X10 JOISTS" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 635:Generic Models 1" | object type "Generic Models 635:Generic Models 1" | names: "Generic Models 635:Generic Models 1:3482508" | material: "WOOD TRUSS - SEE STRUCT DWGS" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "060523 - W_P_C - Fastenings - Generic:_3/4" x 4"" | object type "060523 - W_P_C - Fastenings - Generic:_3/4" x 4"" | names: "060523 - W_P_C - Fastenings - Generic:_3/4" x 4":3490142" | material: "EXPOSED LAG BOLTS" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "WASHER193:WASHER" | object type "WASHER193:WASHER" | names: "WASHER193:WASHER:3493050" | material: "(2) GALV. WASHERS (FOR DRAINAGE)" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "WASHER194:WASHER" | object type "WASHER194:WASHER" | names: "WASHER194:WASHER:3494303" | material: "(2) GALV. WASHERS (FOR DRAINAGE)" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "WASHER197:WASHER" | object type "WASHER197:WASHER" | names: "WASHER197:WASHER:3494379" | material: "(2) GALV. WASHERS (FOR DRAINAGE)" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "WASHER199:WASHER" | object type "WASHER199:WASHER" | names: "WASHER199:WASHER:3494453" | material: "(2) GALV. WASHERS (FOR DRAINAGE)" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "WASHER201:WASHER" | object type "WASHER201:WASHER" | names: "WASHER201:WASHER:3494529" | material: "(2) GALV. WASHERS (FOR DRAINAGE)" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "WASHER226:WASHER" | object type "WASHER226:WASHER" | names: "WASHER226:WASHER:3502551" | material: "(2) GALV. WASHERS (FOR DRAINAGE)" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "WASHER229:WASHER" | object type "WASHER229:WASHER" | names: "WASHER229:WASHER:3502583" | material: "(2) GALV. WASHERS (FOR DRAINAGE)" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "WASHER198:WASHER" | object type "WASHER198:WASHER" | names: "WASHER198:WASHER:3502764" | material: "(2) GALV. WASHERS (FOR DRAINAGE)" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "WASHER202:WASHER" | object type "WASHER202:WASHER" | names: "WASHER202:WASHER:3502796" | material: "(2) GALV. WASHERS (FOR DRAINAGE)" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "WASHER204:WASHER" | object type "WASHER204:WASHER" | names: "WASHER204:WASHER:3502832" | material: "(2) GALV. WASHERS (FOR DRAINAGE)" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "WASHER205:WASHER" | object type "WASHER205:WASHER" | names: "WASHER205:WASHER:3503083" | material: "(2) GALV. WASHERS (FOR DRAINAGE)" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "WASHER238:WASHER" | object type "WASHER238:WASHER" | names: "WASHER238:WASHER:3503161" | material: "(2) GALV. WASHERS (FOR DRAINAGE)" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "WASHER200:WASHER" | object type "WASHER200:WASHER" | names: "WASHER200:WASHER:3503473" | material: "(2) GALV. WASHERS (FOR DRAINAGE)" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "WASHER225:WASHER" | object type "WASHER225:WASHER" | names: "WASHER225:WASHER:3503763" | material: "(2) GALV. WASHERS (FOR DRAINAGE)" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "WASHER240:WASHER" | object type "WASHER240:WASHER" | names: "WASHER240:WASHER:3503795" | material: "(2) GALV. WASHERS (FOR DRAINAGE)" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "WASHER241:WASHER" | object type "WASHER241:WASHER" | names: "WASHER241:WASHER:3503831" | material: "(2) GALV. WASHERS (FOR DRAINAGE)" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "WASHER242:WASHER" | object type "WASHER242:WASHER" | names: "WASHER242:WASHER:3503863" | material: "(2) GALV. WASHERS (FOR DRAINAGE)" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "WASHER243:WASHER" | object type "WASHER243:WASHER" | names: "WASHER243:WASHER:3503895" | material: "(2) GALV. WASHERS (FOR DRAINAGE)" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "WASHER244:WASHER" | object type "WASHER244:WASHER" | names: "WASHER244:WASHER:3503927" | material: "(2) GALV. WASHERS (FOR DRAINAGE)" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "WASHER309:WASHER" | object type "WASHER309:WASHER" | names: "WASHER309:WASHER:3504034" | material: "(2) GALV. WASHERS (FOR DRAINAGE)" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "WASHER315:WASHER" | object type "WASHER315:WASHER" | names: "WASHER315:WASHER:3504066" | material: "(2) GALV. WASHERS (FOR DRAINAGE)" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 721:Generic Models 1" | object type "Generic Models 721:Generic Models 1" | names: "Generic Models 721:Generic Models 1:3504639" | material: "BUILDING WRAP" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "060523 - W_P_C - Fastenings - Generic:_3/4" x 4"" | object type "060523 - W_P_C - Fastenings - Generic:_3/4" x 4"" | names: "060523 - W_P_C - Fastenings - Generic:_3/4" x 4":3504810" | material: "EXPOSED LAG BOLTS" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "060523 - W_P_C - Fastenings - Generic:_3/4" x 4"" | object type "060523 - W_P_C - Fastenings - Generic:_3/4" x 4"" | names: "060523 - W_P_C - Fastenings - Generic:_3/4" x 4":3504812" | material: "EXPOSED LAG BOLTS" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 720:Generic Models 1" | object type "Generic Models 720:Generic Models 1" | names: "Generic Models 720:Generic Models 1:3505827" | material: "BUILDING WRAP" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 747:Generic Models 1" | object type "Generic Models 747:Generic Models 1" | names: "Generic Models 747:Generic Models 1:3506185" | material: "METAL FLASHING - BLACK" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 752:Generic Models 1" | object type "Generic Models 752:Generic Models 1" | names: "Generic Models 752:Generic Models 1:3506795" | material: "BUILDING WRAP" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "WASHER321:WASHER" | object type "WASHER321:WASHER" | names: "WASHER321:WASHER:3509091" | material: "(2) GALV. WASHERS (FOR DRAINAGE)" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "WASHER195:WASHER" | object type "WASHER195:WASHER" | names: "WASHER195:WASHER:3509594" | material: "(2) GALV. WASHERS (FOR DRAINAGE)" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "WASHER196:WASHER" | object type "WASHER196:WASHER" | names: "WASHER196:WASHER:3510103" | material: "(2) GALV. WASHERS (FOR DRAINAGE)" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "WASHER322:WASHER" | object type "WASHER322:WASHER" | names: "WASHER322:WASHER:3510123" | material: "(2) GALV. WASHERS (FOR DRAINAGE)" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCWALL | type IFCWALLTYPE "Metal stud4:Metal stud" | object type "Metal stud4:Metal stud" | names: "Metal stud4:Metal stud:3513310" | material: "2" GALV. METAL STUDS" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Metal stud6:Metal stud" | object type "Metal stud6:Metal stud" | names: "Metal stud6:Metal stud:3513745" | material: "2" GALV. METAL STUDS" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCPIPEFITTING | type IFCPIPEFITTINGTYPE "Pipe:Pipe" | object type "Pipe:Pipe" | names: "Pipe:Pipe:3514139" | material: "MINI SPLIT LINE SETS" | property sets: Pset_EnvironmentalImpactIndicators, Pset_PipeFittingTypeCommon
          1 x IFCWALL | type IFCWALLTYPE "Metal stud5:Metal stud" | object type "Metal stud5:Metal stud" | names: "Metal stud5:Metal stud:3516097" | material: "GALV. METAL STUD - TOP TRACK" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          10 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "060523 - W_P_C - Fastenings - Generic:_METAL STUD - DRYWALL - GENERIC" | object type "060523 - W_P_C - Fastenings - Generic:_METAL STUD - DRYWALL - GENERIC" | names: "060523 - W_P_C - Fastenings - Generic:_METAL STUD - DRYWALL - GENERIC:3516765", "060523 - W_P_C - Fastenings - Generic:_METAL STUD - DRYWALL - GENERIC:3625518", "060523 - W_P_C - Fastenings - Generic:_METAL STUD - DRYWALL - GENERIC:3625769" (+7 more) | material: "ATTACH GYPSUM BOARD TO STUDS AND NOT TO TOP TRACK" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCWALL | type IFCWALLTYPE "PERFORATED GALV. STEEL PANEL1:PERFORATED GALV. STEEL PANEL" | object type "PERFORATED GALV. STEEL PANEL1:PERFORATED GALV. STEEL PANEL" | names: "PERFORATED GALV. STEEL PANEL1:PERFORATED GALV. STEEL PANEL:3517519" | material: "16 GA. PERFORATED GALV. STEEL PANEL" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Metal stud8:Metal stud" | object type "Metal stud8:Metal stud" | names: "Metal stud8:Metal stud:3517658" | material: "INTERMITTENT GALV BRACKETS" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          4 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "060523 - W_P_C - Fastenings - Generic:_METAL STUD - DRYWALL - GENERIC" | object type "060523 - W_P_C - Fastenings - Generic:_METAL STUD - DRYWALL - GENERIC" | names: "060523 - W_P_C - Fastenings - Generic:_METAL STUD - DRYWALL - GENERIC:3517965", "060523 - W_P_C - Fastenings - Generic:_METAL STUD - DRYWALL - GENERIC:3518052", "060523 - W_P_C - Fastenings - Generic:_METAL STUD - DRYWALL - GENERIC:3627695" (+1 more) | material: "ATTACH GYPSUM BOARD TO STUDS AND NOT TO TOP TRACK" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          33 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "060523 - W_P_C - Fastenings - Generic:_METAL STUD - DRYWALL - GENERIC" | object type "060523 - W_P_C - Fastenings - Generic:_METAL STUD - DRYWALL - GENERIC" | names: "060523 - W_P_C - Fastenings - Generic:_METAL STUD - DRYWALL - GENERIC:3518079", "060523 - W_P_C - Fastenings - Generic:_METAL STUD - DRYWALL - GENERIC:3614146", "060523 - W_P_C - Fastenings - Generic:_METAL STUD - DRYWALL - GENERIC:3624754" (+30 more) | material: "ATTACH GYPSUM BOARD TO STUDS AND NOT TO TOP TRACK" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCWALL | type IFCWALLTYPE "PERFORATED GALV. STEEL PANEL2:PERFORATED GALV. STEEL PANEL" | object type "PERFORATED GALV. STEEL PANEL2:PERFORATED GALV. STEEL PANEL" | names: "PERFORATED GALV. STEEL PANEL2:PERFORATED GALV. STEEL PANEL:3552678" | material: "16 GA. PERFORATED GALV. STEEL PANEL" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCPIPEFITTING | type IFCPIPEFITTINGTYPE "Pipe1:Pipe" | object type "Pipe1:Pipe" | names: "Pipe1:Pipe:3597799" | material: "GALV. PIPE" | property sets: Pset_EnvironmentalImpactIndicators, Pset_PipeFittingTypeCommon
          1 x IFCVALVE | type IFCVALVETYPE "U BRACKET1:U BRACKET" | object type "U BRACKET1:U BRACKET" | names: "U BRACKET1:U BRACKET:3624989" | material: "GALV. U BRACKET AT GALV. PIPE" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ValveTypeCommon
          1 x IFCPIPEFITTING | type IFCPIPEFITTINGTYPE "Pipe2:Pipe" | object type "Pipe2:Pipe" | names: "Pipe2:Pipe:3625505" | material: "MINI SPLIT LINE SETS" | property sets: Pset_EnvironmentalImpactIndicators, Pset_PipeFittingTypeCommon
          1 x IFCPIPEFITTING | type IFCPIPEFITTINGTYPE "Pipe3:Pipe" | object type "Pipe3:Pipe" | names: "Pipe3:Pipe:3625532" | material: "GALV. PIPE" | property sets: Pset_EnvironmentalImpactIndicators, Pset_PipeFittingTypeCommon
          1 x IFCVALVE | type IFCVALVETYPE "U BRACKET4:U BRACKET" | object type "U BRACKET4:U BRACKET" | names: "U BRACKET4:U BRACKET:3625563" | material: "GALV. U BRACKET AT GALV. PIPE" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ValveTypeCommon
          1 x IFCPIPEFITTING | type IFCPIPEFITTINGTYPE "Pipe4:Pipe" | object type "Pipe4:Pipe" | names: "Pipe4:Pipe:3625756" | material: "MINI SPLIT LINE SETS" | property sets: Pset_EnvironmentalImpactIndicators, Pset_PipeFittingTypeCommon
          1 x IFCPIPEFITTING | type IFCPIPEFITTINGTYPE "Pipe5:Pipe" | object type "Pipe5:Pipe" | names: "Pipe5:Pipe:3625783" | material: "GALV. PIPE" | property sets: Pset_EnvironmentalImpactIndicators, Pset_PipeFittingTypeCommon
          1 x IFCVALVE | type IFCVALVETYPE "U BRACKET6:U BRACKET" | object type "U BRACKET6:U BRACKET" | names: "U BRACKET6:U BRACKET:3625814" | material: "GALV. U BRACKET AT GALV. PIPE" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ValveTypeCommon
          1 x IFCPIPEFITTING | type IFCPIPEFITTINGTYPE "Pipe6:Pipe" | object type "Pipe6:Pipe" | names: "Pipe6:Pipe:3625848" | material: "MINI SPLIT LINE SETS" | property sets: Pset_EnvironmentalImpactIndicators, Pset_PipeFittingTypeCommon
          1 x IFCPIPEFITTING | type IFCPIPEFITTINGTYPE "Pipe7:Pipe" | object type "Pipe7:Pipe" | names: "Pipe7:Pipe:3625875" | material: "GALV. PIPE" | property sets: Pset_EnvironmentalImpactIndicators, Pset_PipeFittingTypeCommon
          1 x IFCVALVE | type IFCVALVETYPE "U BRACKET8:U BRACKET" | object type "U BRACKET8:U BRACKET" | names: "U BRACKET8:U BRACKET:3625906" | material: "GALV. U BRACKET AT GALV. PIPE" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ValveTypeCommon
          1 x IFCPIPEFITTING | type IFCPIPEFITTINGTYPE "Pipe8:Pipe" | object type "Pipe8:Pipe" | names: "Pipe8:Pipe:3625939" | material: "MINI SPLIT LINE SETS" | property sets: Pset_EnvironmentalImpactIndicators, Pset_PipeFittingTypeCommon
          1 x IFCPIPEFITTING | type IFCPIPEFITTINGTYPE "Pipe9:Pipe" | object type "Pipe9:Pipe" | names: "Pipe9:Pipe:3625966" | material: "GALV. PIPE" | property sets: Pset_EnvironmentalImpactIndicators, Pset_PipeFittingTypeCommon
          1 x IFCVALVE | type IFCVALVETYPE "U BRACKET10:U BRACKET" | object type "U BRACKET10:U BRACKET" | names: "U BRACKET10:U BRACKET:3625997" | material: "GALV. U BRACKET AT GALV. PIPE" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ValveTypeCommon
          1 x IFCPIPEFITTING | type IFCPIPEFITTINGTYPE "Pipe10:Pipe" | object type "Pipe10:Pipe" | names: "Pipe10:Pipe:3626030" | material: "MINI SPLIT LINE SETS" | property sets: Pset_EnvironmentalImpactIndicators, Pset_PipeFittingTypeCommon
          1 x IFCPIPEFITTING | type IFCPIPEFITTINGTYPE "Pipe11:Pipe" | object type "Pipe11:Pipe" | names: "Pipe11:Pipe:3626057" | material: "GALV. PIPE" | property sets: Pset_EnvironmentalImpactIndicators, Pset_PipeFittingTypeCommon
          1 x IFCVALVE | type IFCVALVETYPE "U BRACKET12:U BRACKET" | object type "U BRACKET12:U BRACKET" | names: "U BRACKET12:U BRACKET:3626088" | material: "GALV. U BRACKET AT GALV. PIPE" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ValveTypeCommon
          1 x IFCPIPEFITTING | type IFCPIPEFITTINGTYPE "Pipe12:Pipe" | object type "Pipe12:Pipe" | names: "Pipe12:Pipe:3626119" | material: "MINI SPLIT LINE SETS" | property sets: Pset_EnvironmentalImpactIndicators, Pset_PipeFittingTypeCommon
          1 x IFCPIPEFITTING | type IFCPIPEFITTINGTYPE "Pipe13:Pipe" | object type "Pipe13:Pipe" | names: "Pipe13:Pipe:3626146" | material: "GALV. PIPE" | property sets: Pset_EnvironmentalImpactIndicators, Pset_PipeFittingTypeCommon
          1 x IFCVALVE | type IFCVALVETYPE "U BRACKET14:U BRACKET" | object type "U BRACKET14:U BRACKET" | names: "U BRACKET14:U BRACKET:3626177" | material: "GALV. U BRACKET AT GALV. PIPE" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ValveTypeCommon
          1 x IFCPIPEFITTING | type IFCPIPEFITTINGTYPE "Pipe14:Pipe" | object type "Pipe14:Pipe" | names: "Pipe14:Pipe:3626208" | material: "MINI SPLIT LINE SETS" | property sets: Pset_EnvironmentalImpactIndicators, Pset_PipeFittingTypeCommon
          1 x IFCPIPEFITTING | type IFCPIPEFITTINGTYPE "Pipe15:Pipe" | object type "Pipe15:Pipe" | names: "Pipe15:Pipe:3626235" | material: "GALV. PIPE" | property sets: Pset_EnvironmentalImpactIndicators, Pset_PipeFittingTypeCommon
          1 x IFCVALVE | type IFCVALVETYPE "U BRACKET16:U BRACKET" | object type "U BRACKET16:U BRACKET" | names: "U BRACKET16:U BRACKET:3626266" | material: "GALV. U BRACKET AT GALV. PIPE" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ValveTypeCommon
          1 x IFCPIPEFITTING | type IFCPIPEFITTINGTYPE "Pipe16:Pipe" | object type "Pipe16:Pipe" | names: "Pipe16:Pipe:3626299" | material: "MINI SPLIT LINE SETS" | property sets: Pset_EnvironmentalImpactIndicators, Pset_PipeFittingTypeCommon
          1 x IFCPIPEFITTING | type IFCPIPEFITTINGTYPE "Pipe17:Pipe" | object type "Pipe17:Pipe" | names: "Pipe17:Pipe:3626326" | material: "GALV. PIPE" | property sets: Pset_EnvironmentalImpactIndicators, Pset_PipeFittingTypeCommon
          1 x IFCVALVE | type IFCVALVETYPE "U BRACKET18:U BRACKET" | object type "U BRACKET18:U BRACKET" | names: "U BRACKET18:U BRACKET:3626357" | material: "GALV. U BRACKET AT GALV. PIPE" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ValveTypeCommon
          1 x IFCPIPEFITTING | type IFCPIPEFITTINGTYPE "Pipe18:Pipe" | object type "Pipe18:Pipe" | names: "Pipe18:Pipe:3626392" | material: "MINI SPLIT LINE SETS" | property sets: Pset_EnvironmentalImpactIndicators, Pset_PipeFittingTypeCommon
          1 x IFCPIPEFITTING | type IFCPIPEFITTINGTYPE "Pipe19:Pipe" | object type "Pipe19:Pipe" | names: "Pipe19:Pipe:3626419" | material: "GALV. PIPE" | property sets: Pset_EnvironmentalImpactIndicators, Pset_PipeFittingTypeCommon
          1 x IFCVALVE | type IFCVALVETYPE "U BRACKET20:U BRACKET" | object type "U BRACKET20:U BRACKET" | names: "U BRACKET20:U BRACKET:3626450" | material: "GALV. U BRACKET AT GALV. PIPE" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ValveTypeCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "060523 - W_P_C - Fastenings - Generic:_METAL STUD - HEAD - GENERIC" | object type "060523 - W_P_C - Fastenings - Generic:_METAL STUD - HEAD - GENERIC" | names: "060523 - W_P_C - Fastenings - Generic:_METAL STUD - HEAD - GENERIC:3626834" | material: "AT HEAD FASTENER AT 24" O.C." | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "060523 - W_P_C - Fastenings - Generic:_METAL STUD - SILL - GENERIC" | object type "060523 - W_P_C - Fastenings - Generic:_METAL STUD - SILL - GENERIC" | names: "060523 - W_P_C - Fastenings - Generic:_METAL STUD - SILL - GENERIC:3626963" | material: "AT SILL - FASTENER AT 24" O.C." | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "060523 - W_P_C - Fastenings - Generic:_METAL STUD - DRYWALL - GENERIC" | object type "060523 - W_P_C - Fastenings - Generic:_METAL STUD - DRYWALL - GENERIC" | names: "060523 - W_P_C - Fastenings - Generic:_METAL STUD - DRYWALL - GENERIC:3627471" | material: "ATTACH GYPSUM BOARD TO STUDS AND NOT TO TOP TRACK" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
      IFCBUILDINGSTOREY "2ND FLOOR" | long name "2ND FLOOR" | object type "Level:Project Base Point" | elevation 10.0000000000002
        contains 162 elements
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 681:Generic Models 1" | object type "Generic Models 681:Generic Models 1" | names: "Generic Models 681:Generic Models 1:3353981" | material: "CLAD WOOD DOOR W/ INSULATED TEMPERED GLAZING" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 647:Generic Models 1" | object type "Generic Models 647:Generic Models 1" | names: "Generic Models 647:Generic Models 1:3355105" | material: "COMPOSITE DECKING W/ HIDDEN FASTENERS" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 14:Walls 13" | object type "Walls 14:Walls 13" | names: "Walls 14:Walls 13:3358847" | material: "2X10 LEDGER - STAIN BEFORE INSTALL" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 640:Generic Models 1" | object type "Generic Models 640:Generic Models 1" | names: "Generic Models 640:Generic Models 1:3359257" | material: "2X10 JOISTS" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 624:Generic Models 1" | object type "Generic Models 624:Generic Models 1" | names: "Generic Models 624:Generic Models 1:3360230" | material: "3/4 HARDWOOD FLOOR" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 642:Generic Models 1" | object type "Generic Models 642:Generic Models 1" | names: "Generic Models 642:Generic Models 1:3360243" | material: "3/4" GYP. CRETE" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 644:Generic Models 1" | object type "Generic Models 644:Generic Models 1" | names: "Generic Models 644:Generic Models 1:3361001" | material: "1/8" SOUND MAT" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 677:Generic Models 1" | object type "Generic Models 677:Generic Models 1" | names: "Generic Models 677:Generic Models 1:3363923" | material: "METAL FLASHING" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 651:Generic Models 1" | object type "Generic Models 651:Generic Models 1" | names: "Generic Models 651:Generic Models 1:3364310" | material: "FLEXIBLE FLASHING" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 670:Generic Models 1" | object type "Generic Models 670:Generic Models 1" | names: "Generic Models 670:Generic Models 1:3364448" | material: "METAL FLASHING" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "HIDDEN FASTENING:HIDDEN FASTENING" | object type "HIDDEN FASTENING:HIDDEN FASTENING" | names: "HIDDEN FASTENING:HIDDEN FASTENING:3371559" | material: "CONCEALED FASTENERS" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 641:Generic Models 1" | object type "Generic Models 641:Generic Models 1" | names: "Generic Models 641:Generic Models 1:3372566" | material: "COMPOSITE DECKING W/ HIDDEN FASTENERS" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "HIDDEN FASTENING1:HIDDEN FASTENING" | object type "HIDDEN FASTENING1:HIDDEN FASTENING" | names: "HIDDEN FASTENING1:HIDDEN FASTENING:3372878" | material: "CONCEALED FASTENERS" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 646:Generic Models 1" | object type "Generic Models 646:Generic Models 1" | names: "Generic Models 646:Generic Models 1:3372883" | material: "COMPOSITE DECKING W/ HIDDEN FASTENERS" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "HIDDEN FASTENING2:HIDDEN FASTENING" | object type "HIDDEN FASTENING2:HIDDEN FASTENING" | names: "HIDDEN FASTENING2:HIDDEN FASTENING:3372933" | material: "CONCEALED FASTENERS" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 648:Generic Models 1" | object type "Generic Models 648:Generic Models 1" | names: "Generic Models 648:Generic Models 1:3372938" | material: "COMPOSITE DECKING W/ HIDDEN FASTENERS" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "HIDDEN FASTENING3:HIDDEN FASTENING" | object type "HIDDEN FASTENING3:HIDDEN FASTENING" | names: "HIDDEN FASTENING3:HIDDEN FASTENING:3372985" | material: "CONCEALED FASTENERS" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 654:Generic Models 1" | object type "Generic Models 654:Generic Models 1" | names: "Generic Models 654:Generic Models 1:3372990" | material: "COMPOSITE DECKING W/ HIDDEN FASTENERS" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 659:Generic Models 1" | object type "Generic Models 659:Generic Models 1" | names: "Generic Models 659:Generic Models 1:3379910" | material: "3/4" CDX OR OSB PLYWOOD - SEE STRUCT DWGS" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 666:Generic Models 1" | object type "Generic Models 666:Generic Models 1" | names: "Generic Models 666:Generic Models 1:3384993" | material: "2X WOOD STUD" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 701:Generic Models 1" | object type "Generic Models 701:Generic Models 1" | names: "Generic Models 701:Generic Models 1:3385006" | material: "WOOD TRUSS FLOOR ASSEMBLY - FILL CAVITY WITH BATT. INSULATION - (UL - L521 FLOOR ASSEMBLY)" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 702:Generic Models 1" | object type "Generic Models 702:Generic Models 1" | names: "Generic Models 702:Generic Models 1:3385021" | material: "5/8" GYP. BD" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 17:Walls 13" | object type "Walls 17:Walls 13" | names: "Walls 17:Walls 13:3385092" | material: "2X10 LEDGER - STAIN BEFORE INSTALL" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 707:Generic Models 1" | object type "Generic Models 707:Generic Models 1" | names: "Generic Models 707:Generic Models 1:3385100" | material: "2X10 JOISTS" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 708:Generic Models 1" | object type "Generic Models 708:Generic Models 1" | names: "Generic Models 708:Generic Models 1:3385120" | material: "TPO ROOFING MEMBRANE" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 709:Generic Models 1" | object type "Generic Models 709:Generic Models 1" | names: "Generic Models 709:Generic Models 1:3385133" | material: "1" MIN. POLYISO INSULATION OVER AIR BARRIER (WRAP UP/OVER PARAPET)" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 717:Generic Models 1" | object type "Generic Models 717:Generic Models 1" | names: "Generic Models 717:Generic Models 1:3385247" | material: "FIBER CEMENT LAPSIDING" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 719:Generic Models 1" | object type "Generic Models 719:Generic Models 1" | names: "Generic Models 719:Generic Models 1:3385277" | material: "METAL FLASHING" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 722:Generic Models 1" | object type "Generic Models 722:Generic Models 1" | names: "Generic Models 722:Generic Models 1:3385331" | material: "5/8" GYP. BD @ CEILING" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 723:Generic Models 1" | object type "Generic Models 723:Generic Models 1" | names: "Generic Models 723:Generic Models 1:3385347" | material: "1/2" CDX OR OSB PLYWOOD - SEE STRUCT DWGS" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 724:Generic Models 1" | object type "Generic Models 724:Generic Models 1" | names: "Generic Models 724:Generic Models 1:3385360" | material: "BATT INSULATION - FILL ENTIRE CAVITY" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 729:Generic Models 1" | object type "Generic Models 729:Generic Models 1" | names: "Generic Models 729:Generic Models 1:3385538" | material: "RESILIENT CHANNEL - 25 GA. FURRING CHANNELS INSTALLED HORIZONTALLY SPACED 24 IN. OC" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 730:Generic Models 1" | object type "Generic Models 730:Generic Models 1" | names: "Generic Models 730:Generic Models 1:3385557" | material: "WOOD TRUSS - SEE STRUCT DWGS" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 731:Generic Models 1" | object type "Generic Models 731:Generic Models 1" | names: "Generic Models 731:Generic Models 1:3385562" | material: "WOOD TRUSS - SEE STRUCT DWGS" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 732:Generic Models 1" | object type "Generic Models 732:Generic Models 1" | names: "Generic Models 732:Generic Models 1:3385580" | material: "WOOD TRUSS - SEE STRUCT DWGS" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 733:Generic Models 1" | object type "Generic Models 733:Generic Models 1" | names: "Generic Models 733:Generic Models 1:3385586" | material: "3/4" CDX OR OSB PLYWOOD - SEE STRUCT DWGS" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 662:Generic Models 1" | object type "Generic Models 662:Generic Models 1" | names: "Generic Models 662:Generic Models 1:3385891" | material: "PLYTANIUM T1-11 SYP PLYWOOD PANEL SIDING - 4" GROOVES - EXTERIOR GRADE" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 703:Generic Models 1" | object type "Generic Models 703:Generic Models 1" | names: "Generic Models 703:Generic Models 1:3387855" | material: "TAPERED RIGID INSULATION - FOR DRAINAGE" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 704:Generic Models 1" | object type "Generic Models 704:Generic Models 1" | names: "Generic Models 704:Generic Models 1:3388068" | material: "TPO ROOFING MEMBRANE" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Vert" | object type "Vert 1:Vert 62091" | names: "Vert 1:Vert 62091:3390018" | material: "METAL DRIP FLASHING" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Vert" | object type "Vert 2:Vert 9" | names: "Vert 2:Vert 9:3390042" | material: "DRAINAGE WRAP - ASTM 2273" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 1:Generic Models 1:15607" | object type "Generic Models 1:Generic Models 1:15607 1:Generic Models 1:15607 1 : Generic Models 1:Generic Models 1:15607 3" | names: "Generic Models 1:Generic Models 1:15607 1:Generic Models 1:15607 1 : Generic Models 1:Generic Models 1:15607 3:3390061" | material: "7/8" CORRUGATED METAL - EXPOSED FASTENERS" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 711:Generic Models 1" | object type "Generic Models 711:Generic Models 1" | names: "Generic Models 711:Generic Models 1:3391486" | material: "DRAINAGE WRAP - ASTM 2273" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 706:Generic Models 1" | object type "Generic Models 706:Generic Models 1" | names: "Generic Models 706:Generic Models 1:3392745" | material: "WOOD TRUSS - SEE STRUCT DWGS" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 699:Generic Models 1" | object type "Generic Models 699:Generic Models 1" | names: "Generic Models 699:Generic Models 1:3394337" | material: "1/2" CDX OR OSB PLYWOOD - SEE STRUCT DWGS" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Vert" | object type "Vert 3:Vert 62091" | names: "Vert 3:Vert 62091:3401325" | material: "METAL DRIP FLASHING" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Vert" | object type "Vert 4:Vert 9" | names: "Vert 4:Vert 9:3401349" | material: "DRAINAGE WRAP - ASTM 2273" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 1:Generic Models 1:15607" | object type "Generic Models 1:Generic Models 1:15607 2:Generic Models 1:15607 2 : Generic Models 1:Generic Models 1:15607 3" | names: "Generic Models 1:Generic Models 1:15607 2:Generic Models 1:15607 2 : Generic Models 1:Generic Models 1:15607 3:3401368" | material: "7/8" CORRUGATED METAL - EXPOSED FASTENERS" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 700:Generic Models 1" | object type "Generic Models 700:Generic Models 1" | names: "Generic Models 700:Generic Models 1:3416742" | material: "FIBER CEMENT LAPSIDING" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 710:Generic Models 1" | object type "Generic Models 710:Generic Models 1" | names: "Generic Models 710:Generic Models 1:3416768" | material: "FIBER CEMENT LAPSIDING" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 712:Generic Models 1" | object type "Generic Models 712:Generic Models 1" | names: "Generic Models 712:Generic Models 1:3416783" | material: "FIBER CEMENT LAPSIDING" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 713:Generic Models 1" | object type "Generic Models 713:Generic Models 1" | names: "Generic Models 713:Generic Models 1:3416798" | material: "FIBER CEMENT LAPSIDING" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 714:Generic Models 1" | object type "Generic Models 714:Generic Models 1" | names: "Generic Models 714:Generic Models 1:3416813" | material: "FIBER CEMENT LAPSIDING" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 636:Generic Models 1" | object type "Generic Models 636:Generic Models 1" | names: "Generic Models 636:Generic Models 1:3417199" | material: "COMPOSITE DECKING W/ HIDDEN FASTENERS" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "HIDDEN FASTENING4:HIDDEN FASTENING" | object type "HIDDEN FASTENING4:HIDDEN FASTENING" | names: "HIDDEN FASTENING4:HIDDEN FASTENING:3417233" | material: "CONCEALED FASTENERS" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 638:Generic Models 1" | object type "Generic Models 638:Generic Models 1" | names: "Generic Models 638:Generic Models 1:3417238" | material: "COMPOSITE DECKING W/ HIDDEN FASTENERS" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "HIDDEN FASTENING5:HIDDEN FASTENING" | object type "HIDDEN FASTENING5:HIDDEN FASTENING" | names: "HIDDEN FASTENING5:HIDDEN FASTENING:3417272" | material: "CONCEALED FASTENERS" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 643:Generic Models 1" | object type "Generic Models 643:Generic Models 1" | names: "Generic Models 643:Generic Models 1:3417277" | material: "COMPOSITE DECKING W/ HIDDEN FASTENERS" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "RAILING:RAILING" | object type "RAILING:RAILING" | names: "RAILING:RAILING:3420944" | material: "CONT. TREATED 4X6 WITH ROUNDED EDGES AT TOP" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "RAILING 1:RAILING 3" | object type "RAILING 1:RAILING 3" | names: "RAILING 1:RAILING 3:3421993" | material: "2" X 4" - 6GA GALV. MESH" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "RAILING 3:RAILING 3" | object type "RAILING 3:RAILING 3" | names: "RAILING 3:RAILING 3:3422029" | material: "2" X 4" - 6GA GALV. MESH" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "RAILING 4:RAILING 3" | object type "RAILING 4:RAILING 3" | names: "RAILING 4:RAILING 3:3422057" | material: "2" X 4" - 6GA GALV. MESH" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "RAILING 5:RAILING 3" | object type "RAILING 5:RAILING 3" | names: "RAILING 5:RAILING 3:3422081" | material: "2" X 4" - 6GA GALV. MESH" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "RAILING 6:RAILING 3" | object type "RAILING 6:RAILING 3" | names: "RAILING 6:RAILING 3:3422102" | material: "2" X 4" - 6GA GALV. MESH" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "RAILING 7:RAILING 3" | object type "RAILING 7:RAILING 3" | names: "RAILING 7:RAILING 3:3422124" | material: "2" X 4" - 6GA GALV. MESH" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "RAILING 8:RAILING 3" | object type "RAILING 8:RAILING 3" | names: "RAILING 8:RAILING 3:3422150" | material: "2" X 4" - 6GA GALV. MESH" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "RAILING 9:RAILING 3" | object type "RAILING 9:RAILING 3" | names: "RAILING 9:RAILING 3:3422171" | material: "2" X 4" - 6GA GALV. MESH" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "RAILING 10:RAILING 3" | object type "RAILING 10:RAILING 3" | names: "RAILING 10:RAILING 3:3422193" | material: "2" X 4" - 6GA GALV. MESH" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "RAILING 11:RAILING 3" | object type "RAILING 11:RAILING 3" | names: "RAILING 11:RAILING 3:3422215" | material: "2" X 4" - 6GA GALV. MESH" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "RAILING 12:RAILING 3" | object type "RAILING 12:RAILING 3" | names: "RAILING 12:RAILING 3:3422238" | material: "2" X 4" - 6GA GALV. MESH" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 649:Generic Models 1" | object type "Generic Models 649:Generic Models 1" | names: "Generic Models 649:Generic Models 1:3422551" | material: "COMPOSITE DECKING W/ HIDDEN FASTENERS" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "HIDDEN FASTENING6:HIDDEN FASTENING" | object type "HIDDEN FASTENING6:HIDDEN FASTENING" | names: "HIDDEN FASTENING6:HIDDEN FASTENING:3422585" | material: "CONCEALED FASTENERS" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 661:Generic Models 1" | object type "Generic Models 661:Generic Models 1" | names: "Generic Models 661:Generic Models 1:3422597" | material: "COMPOSITE DECKING W/ HIDDEN FASTENERS" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "HIDDEN FASTENING7:HIDDEN FASTENING" | object type "HIDDEN FASTENING7:HIDDEN FASTENING" | names: "HIDDEN FASTENING7:HIDDEN FASTENING:3422631" | material: "CONCEALED FASTENERS" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "RAILING 20:RAILING 20" | object type "RAILING 20:RAILING 20" | names: "RAILING 20:RAILING 20:3422725" | material: "2" X 4" - 6GA GALV. MESH" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "RAILING 21:RAILING 20" | object type "RAILING 21:RAILING 20" | names: "RAILING 21:RAILING 20:3422920" | material: "2" X 4" - 6GA GALV. MESH" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "RAILING 22:RAILING 20" | object type "RAILING 22:RAILING 20" | names: "RAILING 22:RAILING 20:3422967" | material: "2" X 4" - 6GA GALV. MESH" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "RAILING 23:RAILING 20" | object type "RAILING 23:RAILING 20" | names: "RAILING 23:RAILING 20:3422987" | material: "2" X 4" - 6GA GALV. MESH" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "RAILING 24:RAILING 20" | object type "RAILING 24:RAILING 20" | names: "RAILING 24:RAILING 20:3423005" | material: "2" X 4" - 6GA GALV. MESH" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "RAILING 25:RAILING 20" | object type "RAILING 25:RAILING 20" | names: "RAILING 25:RAILING 20:3423023" | material: "2" X 4" - 6GA GALV. MESH" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "RAILING 26:RAILING 20" | object type "RAILING 26:RAILING 20" | names: "RAILING 26:RAILING 20:3423041" | material: "2" X 4" - 6GA GALV. MESH" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "RAILING 27:RAILING 20" | object type "RAILING 27:RAILING 20" | names: "RAILING 27:RAILING 20:3423059" | material: "2" X 4" - 6GA GALV. MESH" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "RAILING 28:RAILING 20" | object type "RAILING 28:RAILING 20" | names: "RAILING 28:RAILING 20:3423077" | material: "2" X 4" - 6GA GALV. MESH" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "RAILING 36:RAILING 20" | object type "RAILING 36:RAILING 20" | names: "RAILING 36:RAILING 20:3424672" | material: "2" X 4" - 6GA GALV. MESH" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCWALL | type IFCWALLTYPE "Walls 20:Walls 13" | object type "Walls 20:Walls 13" | names: "Walls 20:Walls 13:3424816" | material: "2X10 JOISTS" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 664:Generic Models 1" | object type "Generic Models 664:Generic Models 1" | names: "Generic Models 664:Generic Models 1:3432645" | material: "METAL FLASHING - BLACK" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 667:Generic Models 1" | object type "Generic Models 667:Generic Models 1" | names: "Generic Models 667:Generic Models 1:3449969" | material: "METAL FLASHING - BLACK" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 685:Generic Models 1" | object type "Generic Models 685:Generic Models 1" | names: "Generic Models 685:Generic Models 1:3454876" | material: "WOOD TRUSS - SEE STRUCT DWGS" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 686:Generic Models 1" | object type "Generic Models 686:Generic Models 1" | names: "Generic Models 686:Generic Models 1:3454984" | material: "COMPOSITE DECKING W/ HIDDEN FASTENERS" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 687:Generic Models 1" | object type "Generic Models 687:Generic Models 1" | names: "Generic Models 687:Generic Models 1:3455005" | material: "COMPOSITE DECKING W/ HIDDEN FASTENERS" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 715:Generic Models 1" | object type "Generic Models 715:Generic Models 1" | names: "Generic Models 715:Generic Models 1:3455034" | material: "COMPOSITE DECKING W/ HIDDEN FASTENERS" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 716:Generic Models 1" | object type "Generic Models 716:Generic Models 1" | names: "Generic Models 716:Generic Models 1:3455055" | material: "COMPOSITE DECKING W/ HIDDEN FASTENERS" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 718:Generic Models 1" | object type "Generic Models 718:Generic Models 1" | names: "Generic Models 718:Generic Models 1:3455090" | material: "COMPOSITE DECKING W/ HIDDEN FASTENERS" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 727:Generic Models 1" | object type "Generic Models 727:Generic Models 1" | names: "Generic Models 727:Generic Models 1:3455771" | material: "COMPOSITE DECKING W/ HIDDEN FASTENERS" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 728:Generic Models 1" | object type "Generic Models 728:Generic Models 1" | names: "Generic Models 728:Generic Models 1:3455798" | material: "COMPOSITE DECKING W/ HIDDEN FASTENERS" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 734:Generic Models 1" | object type "Generic Models 734:Generic Models 1" | names: "Generic Models 734:Generic Models 1:3455831" | material: "COMPOSITE DECKING W/ HIDDEN FASTENERS" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 735:Generic Models 1" | object type "Generic Models 735:Generic Models 1" | names: "Generic Models 735:Generic Models 1:3455860" | material: "COMPOSITE DECKING W/ HIDDEN FASTENERS" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 736:Generic Models 1" | object type "Generic Models 736:Generic Models 1" | names: "Generic Models 736:Generic Models 1:3455887" | material: "COMPOSITE DECKING W/ HIDDEN FASTENERS" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "HIDDEN FASTENING8:HIDDEN FASTENING" | object type "HIDDEN FASTENING8:HIDDEN FASTENING" | names: "HIDDEN FASTENING8:HIDDEN FASTENING:3455983" | material: "CONCEALED FASTENERS" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "HIDDEN FASTENING9:HIDDEN FASTENING" | object type "HIDDEN FASTENING9:HIDDEN FASTENING" | names: "HIDDEN FASTENING9:HIDDEN FASTENING:3456006" | material: "CONCEALED FASTENERS" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "HIDDEN FASTENING10:HIDDEN FASTENING" | object type "HIDDEN FASTENING10:HIDDEN FASTENING" | names: "HIDDEN FASTENING10:HIDDEN FASTENING:3456029" | material: "CONCEALED FASTENERS" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "HIDDEN FASTENING11:HIDDEN FASTENING" | object type "HIDDEN FASTENING11:HIDDEN FASTENING" | names: "HIDDEN FASTENING11:HIDDEN FASTENING:3456052" | material: "CONCEALED FASTENERS" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "HIDDEN FASTENING12:HIDDEN FASTENING" | object type "HIDDEN FASTENING12:HIDDEN FASTENING" | names: "HIDDEN FASTENING12:HIDDEN FASTENING:3456075" | material: "CONCEALED FASTENERS" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "HIDDEN FASTENING13:HIDDEN FASTENING" | object type "HIDDEN FASTENING13:HIDDEN FASTENING" | names: "HIDDEN FASTENING13:HIDDEN FASTENING:3456098" | material: "CONCEALED FASTENERS" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "HIDDEN FASTENING14:HIDDEN FASTENING" | object type "HIDDEN FASTENING14:HIDDEN FASTENING" | names: "HIDDEN FASTENING14:HIDDEN FASTENING:3456121" | material: "CONCEALED FASTENERS" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "HIDDEN FASTENING15:HIDDEN FASTENING" | object type "HIDDEN FASTENING15:HIDDEN FASTENING" | names: "HIDDEN FASTENING15:HIDDEN FASTENING:3456144" | material: "CONCEALED FASTENERS" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "HIDDEN FASTENING16:HIDDEN FASTENING" | object type "HIDDEN FASTENING16:HIDDEN FASTENING" | names: "HIDDEN FASTENING16:HIDDEN FASTENING:3456167" | material: "CONCEALED FASTENERS" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "HIDDEN FASTENING17:HIDDEN FASTENING" | object type "HIDDEN FASTENING17:HIDDEN FASTENING" | names: "HIDDEN FASTENING17:HIDDEN FASTENING:3456192" | material: "CONCEALED FASTENERS" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 739:Generic Models 1" | object type "Generic Models 739:Generic Models 1" | names: "Generic Models 739:Generic Models 1:3459980" | material: "2X10 JOISTS" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "corrugated metal wall2:corrugated metal wall" | object type "corrugated metal wall2:corrugated metal wall" | names: "corrugated metal wall2:corrugated metal wall:3461341" | material: "1/2" CDX OR OSB PLYWOOD - SEE STRUCT DWGS" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "RAILING 13:RAILING 20" | object type "RAILING 13:RAILING 20" | names: "RAILING 13:RAILING 20:3467788" | material: "2" X 4" - 6GA GALV. MESH" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "RAILING 48:RAILING 20" | object type "RAILING 48:RAILING 20" | names: "RAILING 48:RAILING 20:3467806" | material: "2" X 4" - 6GA GALV. MESH" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "RAILING 60:RAILING 3" | object type "RAILING 60:RAILING 3" | names: "RAILING 60:RAILING 3:3467906" | material: "2" X 4" - 6GA GALV. MESH" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "RAILING 61:RAILING 20" | object type "RAILING 61:RAILING 20" | names: "RAILING 61:RAILING 20:3468158" | material: "2" X 4" - 6GA GALV. MESH" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "RAILING 62:RAILING 3" | object type "RAILING 62:RAILING 3" | names: "RAILING 62:RAILING 3:3468188" | material: "2" X 4" - 6GA GALV. MESH" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "RAILING1:RAILING" | object type "RAILING1:RAILING" | names: "RAILING1:RAILING:3468288" | material: "CONT. TREATED 4X6 WITH ROUNDED EDGES AT TOP" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 751:Generic Models 1" | object type "Generic Models 751:Generic Models 1" | names: "Generic Models 751:Generic Models 1:3469494" | material: "WOOD TRUSS - SEE STRUCT DWGS" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 682:Generic Models 1" | object type "Generic Models 682:Generic Models 1" | names: "Generic Models 682:Generic Models 1:3476254" | material: "WOOD TRUSS - SEE STRUCT DWGS" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 759:Generic Models 1" | object type "Generic Models 759:Generic Models 1" | names: "Generic Models 759:Generic Models 1:3476320" | material: "WOOD TRUSS - SEE STRUCT DWGS" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "corrugated metal wall6:corrugated metal wall" | object type "corrugated metal wall6:corrugated metal wall" | names: "corrugated metal wall6:corrugated metal wall:3476362" | material: "7/8" CORRUGATED METAL - EXPOSED FASTENERS" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "corrugated metal wall9:corrugated metal wall" | object type "corrugated metal wall9:corrugated metal wall" | names: "corrugated metal wall9:corrugated metal wall:3476402" | material: "5/8" GYP. BD" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 773:Generic Models 1" | object type "Generic Models 773:Generic Models 1" | names: "Generic Models 773:Generic Models 1:3476774" | material: "WOOD TRUSS - SEE STRUCT DWGS" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 774:Generic Models 1" | object type "Generic Models 774:Generic Models 1" | names: "Generic Models 774:Generic Models 1:3476779" | material: "3/4 HARDWOOD FLOOR" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 775:Generic Models 1" | object type "Generic Models 775:Generic Models 1" | names: "Generic Models 775:Generic Models 1:3476792" | material: "3/4" GYP. CRETE" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 776:Generic Models 1" | object type "Generic Models 776:Generic Models 1" | names: "Generic Models 776:Generic Models 1:3476805" | material: "1/8" SOUND MAT" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 743:Generic Models 1" | object type "Generic Models 743:Generic Models 1" | names: "Generic Models 743:Generic Models 1:3478803" | material: "METAL FLASHING - BLACK" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 32:Walls 13" | object type "Walls 32:Walls 13" | names: "Walls 32:Walls 13:3480579" | material: "2X WOOD JOISTS" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 749:Generic Models 1" | object type "Generic Models 749:Generic Models 1" | names: "Generic Models 749:Generic Models 1:3481279" | material: "METAL FLASHING - BLACK" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 675:Generic Models 1" | object type "Generic Models 675:Generic Models 1" | names: "Generic Models 675:Generic Models 1:3487193" | material: "WOOD TRUSS - SEE STRUCT DWGS" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "building wrap:building wrap" | object type "building wrap:building wrap" | names: "building wrap:building wrap:3497566" | material: "BUILDING WRAP" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 676:Generic Models 1" | object type "Generic Models 676:Generic Models 1" | names: "Generic Models 676:Generic Models 1:3497701" | material: "BUILDING WRAP" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 726:Generic Models 1" | object type "Generic Models 726:Generic Models 1" | names: "Generic Models 726:Generic Models 1:3501597" | material: "METAL FLASHING - BLACK" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "WASHER232:WASHER" | object type "WASHER232:WASHER" | names: "WASHER232:WASHER:3502615" | material: "(2) GALV. WASHERS (FOR DRAINAGE)" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "WASHER234:WASHER" | object type "WASHER234:WASHER" | names: "WASHER234:WASHER:3502647" | material: "(2) GALV. WASHERS (FOR DRAINAGE)" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "WASHER235:WASHER" | object type "WASHER235:WASHER" | names: "WASHER235:WASHER:3502679" | material: "(2) GALV. WASHERS (FOR DRAINAGE)" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "WASHER236:WASHER" | object type "WASHER236:WASHER" | names: "WASHER236:WASHER:3502932" | material: "(2) GALV. WASHERS (FOR DRAINAGE)" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "WASHER237:WASHER" | object type "WASHER237:WASHER" | names: "WASHER237:WASHER:3502964" | material: "(2) GALV. WASHERS (FOR DRAINAGE)" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "WASHER203:WASHER" | object type "WASHER203:WASHER" | names: "WASHER203:WASHER:3503658" | material: "(2) GALV. WASHERS (FOR DRAINAGE)" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "WASHER206:WASHER" | object type "WASHER206:WASHER" | names: "WASHER206:WASHER:3503690" | material: "(2) GALV. WASHERS (FOR DRAINAGE)" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "WASHER297:WASHER" | object type "WASHER297:WASHER" | names: "WASHER297:WASHER:3503959" | material: "(2) GALV. WASHERS (FOR DRAINAGE)" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "WASHER303:WASHER" | object type "WASHER303:WASHER" | names: "WASHER303:WASHER:3503991" | material: "(2) GALV. WASHERS (FOR DRAINAGE)" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "WASHER316:WASHER" | object type "WASHER316:WASHER" | names: "WASHER316:WASHER:3504098" | material: "(2) GALV. WASHERS (FOR DRAINAGE)" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "WASHER319:WASHER" | object type "WASHER319:WASHER" | names: "WASHER319:WASHER:3504130" | material: "(2) GALV. WASHERS (FOR DRAINAGE)" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "WASHER320:WASHER" | object type "WASHER320:WASHER" | names: "WASHER320:WASHER:3504162" | material: "(2) GALV. WASHERS (FOR DRAINAGE)" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 725:Generic Models 1" | object type "Generic Models 725:Generic Models 1" | names: "Generic Models 725:Generic Models 1:3505315" | material: "BUILDING WRAP" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 753:Generic Models 1" | object type "Generic Models 753:Generic Models 1" | names: "Generic Models 753:Generic Models 1:3509678" | material: "METAL FLASHING - BLACK" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Metal stud1:Metal stud" | object type "Metal stud1:Metal stud" | names: "Metal stud1:Metal stud:3511056" | material: "GALV. METAL STUD - SILL TRACK" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Metal stud3:Metal stud" | object type "Metal stud3:Metal stud" | names: "Metal stud3:Metal stud:3513248" | material: "2" GALV. METAL STUDS" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Metal stud7:Metal stud" | object type "Metal stud7:Metal stud" | names: "Metal stud7:Metal stud:3514303" | material: "2" GALV. METAL STUDS" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCVALVE | type IFCVALVETYPE "U BRACKET2:U BRACKET" | object type "U BRACKET2:U BRACKET" | names: "U BRACKET2:U BRACKET:3516182" | material: "GALV. U BRACKET AT GALV. PIPE" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ValveTypeCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 754:Generic Models 1" | object type "Generic Models 754:Generic Models 1" | names: "Generic Models 754:Generic Models 1:3516224" | material: "2X JOIST UNDER METAL STUDS" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "PERFORATED GALV. STEEL PANEL4:PERFORATED GALV. STEEL PANEL" | object type "PERFORATED GALV. STEEL PANEL4:PERFORATED GALV. STEEL PANEL" | names: "PERFORATED GALV. STEEL PANEL4:PERFORATED GALV. STEEL PANEL:3563524" | material: "16 GA. PERFORATED GALV. STEEL PANEL" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "PERFORATED GALV. STEEL PANEL5:PERFORATED GALV. STEEL PANEL" | object type "PERFORATED GALV. STEEL PANEL5:PERFORATED GALV. STEEL PANEL" | names: "PERFORATED GALV. STEEL PANEL5:PERFORATED GALV. STEEL PANEL:3564714" | material: "16 GA. PERFORATED GALV. STEEL PANEL" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCVALVE | type IFCVALVETYPE "U BRACKET3:U BRACKET" | object type "U BRACKET3:U BRACKET" | names: "U BRACKET3:U BRACKET:3625517" | material: "GALV. U BRACKET AT GALV. PIPE" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ValveTypeCommon
          1 x IFCVALVE | type IFCVALVETYPE "U BRACKET5:U BRACKET" | object type "U BRACKET5:U BRACKET" | names: "U BRACKET5:U BRACKET:3625768" | material: "GALV. U BRACKET AT GALV. PIPE" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ValveTypeCommon
          1 x IFCVALVE | type IFCVALVETYPE "U BRACKET7:U BRACKET" | object type "U BRACKET7:U BRACKET" | names: "U BRACKET7:U BRACKET:3625860" | material: "GALV. U BRACKET AT GALV. PIPE" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ValveTypeCommon
          1 x IFCVALVE | type IFCVALVETYPE "U BRACKET9:U BRACKET" | object type "U BRACKET9:U BRACKET" | names: "U BRACKET9:U BRACKET:3625951" | material: "GALV. U BRACKET AT GALV. PIPE" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ValveTypeCommon
          1 x IFCVALVE | type IFCVALVETYPE "U BRACKET11:U BRACKET" | object type "U BRACKET11:U BRACKET" | names: "U BRACKET11:U BRACKET:3626042" | material: "GALV. U BRACKET AT GALV. PIPE" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ValveTypeCommon
          1 x IFCVALVE | type IFCVALVETYPE "U BRACKET13:U BRACKET" | object type "U BRACKET13:U BRACKET" | names: "U BRACKET13:U BRACKET:3626131" | material: "GALV. U BRACKET AT GALV. PIPE" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ValveTypeCommon
          1 x IFCVALVE | type IFCVALVETYPE "U BRACKET15:U BRACKET" | object type "U BRACKET15:U BRACKET" | names: "U BRACKET15:U BRACKET:3626220" | material: "GALV. U BRACKET AT GALV. PIPE" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ValveTypeCommon
          1 x IFCVALVE | type IFCVALVETYPE "U BRACKET17:U BRACKET" | object type "U BRACKET17:U BRACKET" | names: "U BRACKET17:U BRACKET:3626311" | material: "GALV. U BRACKET AT GALV. PIPE" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ValveTypeCommon
          1 x IFCVALVE | type IFCVALVETYPE "U BRACKET19:U BRACKET" | object type "U BRACKET19:U BRACKET" | names: "U BRACKET19:U BRACKET:3626404" | material: "GALV. U BRACKET AT GALV. PIPE" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ValveTypeCommon

Types
  IFCWALLTYPE "Generic Models 680:Generic Models 1" | 1 occurrence | material: "CONCRETE GRADE BEAM W/ 4" CONCRETE SLAB" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 668:Generic Models 1" | 1 occurrence | material: "CONCRETE SLAB - 2% SLOPE AWAY FROM BUILDING" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 691:Generic Models 1" | 1 occurrence | material: "1/2" JOINT FILLER" | property sets: Pset_WallCommon
  IFCWALLTYPE "Dowel2:Dowel" | 1 occurrence | material: "#4 J's @ 24" O.C. - GROUTED IN PRECAST KEYS AND CORES" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 694:Generic Models 1" | 1 occurrence | material: "(2) #5's" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 695:Generic Models 1" | 1 occurrence | material: "(2) #5's" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 696:Generic Models 1" | 1 occurrence | material: "(2) #5's" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 697:Generic Models 1" | 1 occurrence | material: "(2) #5's" | property sets: Pset_WallCommon
  IFCWALLTYPE "Walls 16:Walls 16" | 1 occurrence | material: "6 MIL POLYETHILENE VAPOR BARRIER" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 630:Generic Models 1" | 1 occurrence | material: "WOOD TOP PLATE" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 637:Generic Models 1" | 1 occurrence | material: "DOUBLE 2X WOOD TOP PLATE" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 639:Generic Models 1" | 1 occurrence | material: "FIBER CEMENT LAPSIDING" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 645:Generic Models 1" | 1 occurrence | material: "2X WOOD STUD" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 650:Generic Models 1" | 1 occurrence | material: "WOOD TRUSS FLOOR ASSEMBLY - FILL CAVITY WITH BATT. INSULATION - (UL - L521 FLOOR ASSEMBLY)" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 653:Generic Models 1" | 1 occurrence | material: "5/8" GYP. BD" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 660:Generic Models 1" | 1 occurrence | material: "LVL RIM BOARD - SEE STRUCT. DWGS" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 669:Generic Models 1" | 1 occurrence | material: "DOUBLE 2X WOOD TOP PLATE" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 603:Generic Models 1" | 1 occurrence | material: "CLAD WOOD DOOR W/ INSULATED TEMPERED GLAZING" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 632:Generic Models 1" | 1 occurrence | material: "CLAD WOOD DOOR W/ INSULATED TEMPERED GLAZING" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 633:Generic Models 1" | 1 occurrence | material: "JAMB EXTENSION" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 634:Generic Models 1" | 1 occurrence | material: "JAMB EXTENSION" | property sets: Pset_WallCommon
  IFCBUILDINGELEMENTPROXYTYPE "060523 - W_P_C - Fastenings - Generic:Screw - SDWS" | 3 occurrences | material: "STRONG-DRIVE SDWS TIMBER SCREW (EXTERIOR GRADE)" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "060523 - W_P_C - Fastenings - Generic:_METAL STUD - HEAD - GENERIC" | 4 occurrences | material: "AT HEAD FASTENER AT 24" O.C." | property sets: Pset_BuildingElementProxyCommon
  IFCWALLTYPE "Generic Models 655:Generic Models 1" | 1 occurrence | material: "STARTER STRIP" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 656:Generic Models 1" | 1 occurrence | material: "DRAINAGE WRAP - ASTM 2273" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 674:Generic Models 1" | 1 occurrence | material: "METAL FLASHING" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 629:Generic Models 1" | 1 occurrence | material: "5/8" GYP. BD @ CEILING" | property sets: Pset_WallCommon
  IFCWALLTYPE "Walls 13:Walls 12" | 1 occurrence | material: "LVL HEADER - SEE STRUCT. DWGS" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 683:Generic Models 1" | 1 occurrence | material: "1/2" CDX OR OSB PLYWOOD - SEE STRUCT DWGS" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 684:Generic Models 1" | 1 occurrence | material: "BATT INSULATION - FILL ENTIRE CAVITY" | property sets: Pset_WallCommon
  IFCBUILDINGELEMENTPROXYTYPE "050523 - Metal fastenings - Joist Hanger - Generic:HUCQ1.81/9-SDS" | 2 occurrences | material: "SIMPSON HUC46 JOIST HANGER WITH CONCEALED FLANGES - HDG - UNPAINTED" | property sets: Pset_BuildingElementProxyCommon
  IFCWALLTYPE "Generic Models 652:Generic Models 1" | 1 occurrence | material: "WOOD TOP PLATE" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 689:Generic Models 1" | 1 occurrence | material: "#4 @ 16" OC EACH WAY - LOCATED AT MID-DEPTH" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 693:Generic Models 1" | 1 occurrence | material: "(2) #5's" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 690:Generic Models 1" | 1 occurrence | material: "(2) #5's" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 692:Generic Models 1" | 1 occurrence | material: "(2) #5's" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 698:Generic Models 1" | 1 occurrence | material: "RESILIENT CHANNEL - 25 GA. FURRING CHANNELS INSTALLED HORIZONTALLY SPACED 24 IN. OC" | property sets: Pset_WallCommon
  IFCBUILDINGELEMENTPROXYTYPE "060523 - W_P_C - Fastenings - Generic:Screw - SDWS" | 3 occurrences | material: "STRONG-DRIVE SDWS TIMBER SCREW (EXTERIOR GRADE)" | property sets: Pset_BuildingElementProxyCommon
  IFCWALLTYPE "Generic Models 671:Generic Models 1" | 1 occurrence | material: "FIBER CEMENT LAPSIDING" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 673:Generic Models 1" | 1 occurrence | material: "WOOD TRUSS - SEE STRUCT DWGS" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 705:Generic Models 1" | 1 occurrence | material: "WOOD TRUSS - SEE STRUCT DWGS" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 688:Generic Models 1" | 1 occurrence | material: "2X BLOCKING" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 631:Generic Models 1" | 1 occurrence | material: "FIBER CEMENT LAPSIDING" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 657:Generic Models 1" | 1 occurrence | material: "FIBER CEMENT LAPSIDING" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 658:Generic Models 1" | 1 occurrence | material: "FIBER CEMENT LAPSIDING" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 663:Generic Models 1" | 1 occurrence | material: "FIBER CEMENT LAPSIDING" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 672:Generic Models 1" | 1 occurrence | material: "FIBER CEMENT LAPSIDING" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 678:Generic Models 1" | 1 occurrence | material: "FIBER CEMENT LAPSIDING" | property sets: Pset_WallCommon
  IFCBUILDINGELEMENTPROXYTYPE "060523 - W_P_C - Fastenings - Generic:_METAL STUD - HEAD - GENERIC" | 36 occurrences | material: "AT HEAD FASTENER AT 24" O.C." | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "C CHANNEL 2:C CHANNEL 2" | 1 occurrence | material: "STEEL C CHANNEL - HDG - SEE STRUCT DWGS" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "RAILING 2:RAILING 2" | 1 occurrence | material: "(2) 2X4s - EXT STAIN - DARK" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "RAILING 14:RAILING 3" | 1 occurrence | material: "2" X 4" - 6GA GALV. MESH" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "RAILING 15:RAILING 3" | 1 occurrence | material: "2" X 4" - 6GA GALV. MESH" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "RAILING 16:RAILING 3" | 1 occurrence | material: "2" X 4" - 6GA GALV. MESH" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "RAILING 17:RAILING 3" | 1 occurrence | material: "2" X 4" - 6GA GALV. MESH" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "RAILING 18:RAILING 3" | 1 occurrence | material: "2" X 4" - 6GA GALV. MESH" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "RAILING 30:RAILING 20" | 1 occurrence | material: "2" X 4" - 6GA GALV. MESH" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "RAILING 31:RAILING 20" | 1 occurrence | material: "2" X 4" - 6GA GALV. MESH" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "RAILING 32:RAILING 20" | 1 occurrence | material: "2" X 4" - 6GA GALV. MESH" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "RAILING 33:RAILING 20" | 1 occurrence | material: "2" X 4" - 6GA GALV. MESH" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "RAILING 34:RAILING 20" | 1 occurrence | material: "2" X 4" - 6GA GALV. MESH" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "RAILING 29:RAILING 20" | 1 occurrence | material: "2" X 4" - 6GA GALV. MESH" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "RAILING 35:RAILING 20" | 1 occurrence | material: "2" X 4" - 6GA GALV. MESH" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "060523 - W_P_C - Fastenings - Generic:Screw - SDWS 3" | 2 occurrences | material: "TRIM HEAD SCREWS AT RAILING - EXTERIOR GRADE" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "060523 - W_P_C - Fastenings - Generic:Thru-Bolt - .8750 - 7/8 2" | 2 occurrences | material: "EXPOSED LAG BOLTS" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "RAILING 37:RAILING 20" | 1 occurrence | material: "3/4" DEEP ROUTED NOTCH" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "RAILING 19:RAILING 2" | 1 occurrence | material: "(2) 2X4s - EXT STAIN - DARK" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "RAILING 38:RAILING 2" | 1 occurrence | material: "(2) 2X4s - EXT STAIN - DARK" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "RAILING 39:RAILING 20" | 1 occurrence | material: "2" X 4" - 6GA GALV. MESH" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "RAILING 40:RAILING 20" | 1 occurrence | material: "2" X 4" - 6GA GALV. MESH" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "RAILING 41:RAILING 20" | 1 occurrence | material: "2" X 4" - 6GA GALV. MESH" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "RAILING 42:RAILING 20" | 1 occurrence | material: "2" X 4" - 6GA GALV. MESH" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "RAILING 43:RAILING 20" | 1 occurrence | material: "3/4" DEEP ROUTED NOTCH" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "RAILING 44:RAILING 20" | 1 occurrence | material: "3/4" DEEP ROUTED NOTCH" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "RAILING 45:RAILING 20" | 1 occurrence | material: "3/4" DEEP ROUTED NOTCH" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "060523 - W_P_C - Fastenings - Generic:Screw - SDWS 4" | 2 occurrences | material: "(X) TRIM HEAD SCREW (EXTERIOR GRADE) AT EACH JOIST" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "060523 - W_P_C - Fastenings - Generic:Screw - SDWS 3" | 3 occurrences | material: "TRIM HEAD SCREWS AT RAILING - EXTERIOR GRADE" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "060523 - W_P_C - Fastenings - Generic:Screw - SDWS 3" | 3 occurrences | material: "TRIM HEAD SCREWS AT RAILING - EXTERIOR GRADE" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "RAILING 49:RAILING 20" | 1 occurrence | material: "3/4" DEEP ROUTED NOTCH" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "RAILING 51:RAILING 20" | 1 occurrence | material: "3/4" DEEP ROUTED NOTCH" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "RAILING 52:RAILING 20" | 1 occurrence | material: "3/4" DEEP ROUTED NOTCH" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "RAILING 53:RAILING 20" | 1 occurrence | material: "3/4" DEEP ROUTED NOTCH" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "RAILING 55:RAILING 20" | 1 occurrence | material: "3/4" DEEP ROUTED NOTCH" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "RAILING 56:RAILING 20" | 1 occurrence | material: "3/4" DEEP ROUTED NOTCH" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "RAILING 57:RAILING 20" | 1 occurrence | material: "3/4" DEEP ROUTED NOTCH" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "060523 - W_P_C - Fastenings - Generic:Thru-Bolt - .8750 - 7/8 2" | 4 occurrences | material: "EXPOSED LAG BOLTS" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "060523 - W_P_C - Fastenings - Generic:Thru-Bolt - .8750 - 7/8 2" | 1 occurrence | material: "EXPOSED LAG BOLTS" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "060523 - W_P_C - Fastenings - Generic:Thru-Bolt - .8750 - 7/8 2" | 1 occurrence | material: "EXPOSED LAG BOLTS" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "060523 - W_P_C - Fastenings - Generic:Thru-Bolt - .8750 - 7/8 2" | 1 occurrence | material: "EXPOSED LAG BOLTS" | property sets: Pset_BuildingElementProxyCommon
  IFCWALLTYPE "Generic Models 679:Generic Models 1" | 1 occurrence | material: "WOOD TRUSS - SEE STRUCT DWGS" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 737:Generic Models 1" | 1 occurrence | material: "BLOCKING TYP - SEE STRUCTURAL" | property sets: Pset_WallCommon
  IFCBUILDINGELEMENTPROXYTYPE "060523 - W_P_C - Fastenings - Generic:_3/4" x 4"" | 1 occurrence | material: "EXPOSED LAG BOLTS" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "060523 - W_P_C - Fastenings - Generic:_3/4" x 4"" | 2 occurrences | material: "EXPOSED LAG BOLTS" | property sets: Pset_BuildingElementProxyCommon
  IFCWALLTYPE "Generic Models 740:Generic Models 1" | 1 occurrence | material: "BLOCKING TYP - SEE STRUCTURAL" | property sets: Pset_WallCommon
  IFCWALLTYPE "corrugated metal wall4:corrugated metal wall" | 1 occurrence | material: "7/8" CORRUGATED METAL - EXPOSED FASTENERS" | property sets: Pset_WallCommon
  IFCWALLTYPE "Walls 33:Walls 13" | 1 occurrence | material: "(3) 2X6" | property sets: Pset_WallCommon
  IFCWALLTYPE "Walls 34:Walls 13" | 1 occurrence | material: "(3) 2X6" | property sets: Pset_WallCommon
  IFCWALLTYPE "Walls 35:Walls 13" | 1 occurrence | material: "(3) 2X6" | property sets: Pset_WallCommon
  IFCWALLTYPE "Walls 36:Walls 13" | 1 occurrence | material: "(3) 2X6" | property sets: Pset_WallCommon
  IFCWALLTYPE "Walls 37:Walls 13" | 1 occurrence | material: "(3) 2X6" | property sets: Pset_WallCommon
  IFCWALLTYPE "Walls 38:Walls 13" | 1 occurrence | material: "(3) 2X6" | property sets: Pset_WallCommon
  IFCWALLTYPE "Walls 39:Walls 13" | 1 occurrence | material: "(2) 2X6" | property sets: Pset_WallCommon
  IFCWALLTYPE "Walls 40:Walls 13" | 1 occurrence | material: "(2) 2X6" | property sets: Pset_WallCommon
  IFCWALLTYPE "Walls 41:Walls 13" | 1 occurrence | material: "(2) 2X6" | property sets: Pset_WallCommon
  IFCWALLTYPE "Walls 42:Walls 13" | 1 occurrence | material: "(2) 2X6" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 665:Generic Models 1" | 1 occurrence | material: "BLOCKING TYP - SEE STRUCTURAL" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 741:Generic Models 1" | 1 occurrence | material: "BLOCKING TYP - SEE STRUCTURAL" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 742:Generic Models 1" | 1 occurrence | material: "BLOCKING TYP" | property sets: Pset_WallCommon
  IFCWALLTYPE "Walls 45:Walls 13" | 1 occurrence | material: "DOUBLE 2X WOOD TOP PLATE" | property sets: Pset_WallCommon
  IFCWALLTYPE "Walls 46:Walls 13" | 1 occurrence | material: "2X10 JOISTS" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 744:Generic Models 1" | 1 occurrence | material: "WOOD TRUSS - SEE STRUCT DWGS" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 745:Generic Models 1" | 1 occurrence | material: "WOOD TRUSS - SEE STRUCT DWGS" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 748:Generic Models 1" | 1 occurrence | material: "WOOD TRUSS - SEE STRUCT DWGS" | property sets: Pset_WallCommon
  IFCBUILDINGELEMENTPROXYTYPE "RAILING 50:RAILING 20" | 1 occurrence | material: "2" X 4" - 6GA GALV. MESH" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "RAILING 58:RAILING 20" | 1 occurrence | material: "2" X 4" - 6GA GALV. MESH" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "RAILING 59:RAILING 20" | 1 occurrence | material: "2" X 4" - 6GA GALV. MESH" | property sets: Pset_BuildingElementProxyCommon
  IFCWALLTYPE "Generic Models 738:Generic Models 1" | 1 occurrence | material: "WOOD TRUSS - SEE STRUCT DWGS" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 750:Generic Models 1" | 1 occurrence | material: "BLOCKING TYP - SEE STRUCTURAL" | property sets: Pset_WallCommon
  IFCBUILDINGELEMENTPROXYTYPE "060523 - W_P_C - Fastenings - Generic:Thru-Bolt - .8750 - 7/8 2" | 3 occurrences | material: "EXPOSED LAG BOLTS" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "060523 - W_P_C - Fastenings - Generic:Thru-Bolt - .8750 - 7/8 2" | 2 occurrences | material: "EXPOSED LAG BOLTS" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "060523 - W_P_C - Fastenings - Generic:Thru-Bolt - .8750 - 7/8 2" | 1 occurrence | material: "EXPOSED LAG BOLTS" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "060523 - W_P_C - Fastenings - Generic:Thru-Bolt - .8750 - 7/8 2" | 1 occurrence | material: "EXPOSED LAG BOLTS" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "060523 - W_P_C - Fastenings - Generic:Thru-Bolt - .8750 - 7/8 2" | 3 occurrences | material: "EXPOSED LAG BOLTS" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "060523 - W_P_C - Fastenings - Generic:Thru-Bolt - .8750 - 7/8 2" | 1 occurrence | material: "EXPOSED LAG BOLTS" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "060523 - W_P_C - Fastenings - Generic:Thru-Bolt - .8750 - 7/8 2" | 1 occurrence | material: "EXPOSED LAG BOLTS" | property sets: Pset_BuildingElementProxyCommon
  IFCWALLTYPE "Generic Models 746:Generic Models 1" | 1 occurrence | material: "WOOD TRUSS - SEE STRUCT DWGS" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 757:Generic Models 1" | 1 occurrence | material: "WOOD TRUSS - SEE STRUCT DWGS" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 760:Generic Models 1" | 1 occurrence | material: "BLOCKING TYP" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 765:Generic Models 1" | 1 occurrence | material: "WOOD TRUSS - SEE STRUCT DWGS" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 766:Generic Models 1" | 1 occurrence | material: "WOOD TRUSS - SEE STRUCT DWGS" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 771:Generic Models 1" | 1 occurrence | material: "WOOD TRUSS - SEE STRUCT DWGS" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 772:Generic Models 1" | 1 occurrence | material: "BLOCKING TYP - SEE STRUCTURAL" | property sets: Pset_WallCommon
  IFCWALLTYPE "corrugated metal wall11:corrugated metal wall" | 1 occurrence | material: "1/2" CDX OR OSB PLYWOOD - SEE STRUCT DWGS" | property sets: Pset_WallCommon
  IFCBUILDINGELEMENTPROXYTYPE "C CHANNEL1:C CHANNEL" | 1 occurrence | material: "1/4" COPED STEEL C CHANNEL - HDG - SEE STRUCT DWGS" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "3/8" BENT STEEL PLATE2:3/8" BENT STEEL PLATE" | 1 occurrence | material: "3/8" BENT STEEL PLATE - HDG" | property sets: Pset_BuildingElementProxyCommon
  IFCWALLTYPE "corrugated metal wall8:corrugated metal wall" | 1 occurrence | material: "5/8" GYP. BD" | property sets: Pset_WallCommon
  IFCWALLTYPE "Walls 48:Walls 13" | 1 occurrence | material: "2X10 JOISTS" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 635:Generic Models 1" | 1 occurrence | material: "WOOD TRUSS - SEE STRUCT DWGS" | property sets: Pset_WallCommon
  IFCBUILDINGELEMENTPROXYTYPE "060523 - W_P_C - Fastenings - Generic:_3/4" x 4"" | 1 occurrence | material: "EXPOSED LAG BOLTS" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "WASHER193:WASHER" | 1 occurrence | material: "(2) GALV. WASHERS (FOR DRAINAGE)" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "WASHER194:WASHER" | 1 occurrence | material: "(2) GALV. WASHERS (FOR DRAINAGE)" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "WASHER197:WASHER" | 1 occurrence | material: "(2) GALV. WASHERS (FOR DRAINAGE)" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "WASHER199:WASHER" | 1 occurrence | material: "(2) GALV. WASHERS (FOR DRAINAGE)" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "WASHER201:WASHER" | 1 occurrence | material: "(2) GALV. WASHERS (FOR DRAINAGE)" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "WASHER226:WASHER" | 1 occurrence | material: "(2) GALV. WASHERS (FOR DRAINAGE)" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "WASHER229:WASHER" | 1 occurrence | material: "(2) GALV. WASHERS (FOR DRAINAGE)" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "WASHER198:WASHER" | 1 occurrence | material: "(2) GALV. WASHERS (FOR DRAINAGE)" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "WASHER202:WASHER" | 1 occurrence | material: "(2) GALV. WASHERS (FOR DRAINAGE)" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "WASHER204:WASHER" | 1 occurrence | material: "(2) GALV. WASHERS (FOR DRAINAGE)" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "WASHER205:WASHER" | 1 occurrence | material: "(2) GALV. WASHERS (FOR DRAINAGE)" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "WASHER238:WASHER" | 1 occurrence | material: "(2) GALV. WASHERS (FOR DRAINAGE)" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "WASHER200:WASHER" | 1 occurrence | material: "(2) GALV. WASHERS (FOR DRAINAGE)" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "WASHER225:WASHER" | 1 occurrence | material: "(2) GALV. WASHERS (FOR DRAINAGE)" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "WASHER240:WASHER" | 1 occurrence | material: "(2) GALV. WASHERS (FOR DRAINAGE)" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "WASHER241:WASHER" | 1 occurrence | material: "(2) GALV. WASHERS (FOR DRAINAGE)" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "WASHER242:WASHER" | 1 occurrence | material: "(2) GALV. WASHERS (FOR DRAINAGE)" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "WASHER243:WASHER" | 1 occurrence | material: "(2) GALV. WASHERS (FOR DRAINAGE)" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "WASHER244:WASHER" | 1 occurrence | material: "(2) GALV. WASHERS (FOR DRAINAGE)" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "WASHER309:WASHER" | 1 occurrence | material: "(2) GALV. WASHERS (FOR DRAINAGE)" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "WASHER315:WASHER" | 1 occurrence | material: "(2) GALV. WASHERS (FOR DRAINAGE)" | property sets: Pset_BuildingElementProxyCommon
  IFCWALLTYPE "Generic Models 721:Generic Models 1" | 1 occurrence | material: "BUILDING WRAP" | property sets: Pset_WallCommon
  IFCBUILDINGELEMENTPROXYTYPE "060523 - W_P_C - Fastenings - Generic:_3/4" x 4"" | 1 occurrence | material: "EXPOSED LAG BOLTS" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "060523 - W_P_C - Fastenings - Generic:_3/4" x 4"" | 1 occurrence | material: "EXPOSED LAG BOLTS" | property sets: Pset_BuildingElementProxyCommon
  IFCWALLTYPE "Generic Models 720:Generic Models 1" | 1 occurrence | material: "BUILDING WRAP" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 747:Generic Models 1" | 1 occurrence | material: "METAL FLASHING - BLACK" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 752:Generic Models 1" | 1 occurrence | material: "BUILDING WRAP" | property sets: Pset_WallCommon
  IFCBUILDINGELEMENTPROXYTYPE "WASHER321:WASHER" | 1 occurrence | material: "(2) GALV. WASHERS (FOR DRAINAGE)" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "WASHER195:WASHER" | 1 occurrence | material: "(2) GALV. WASHERS (FOR DRAINAGE)" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "WASHER196:WASHER" | 1 occurrence | material: "(2) GALV. WASHERS (FOR DRAINAGE)" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "WASHER322:WASHER" | 1 occurrence | material: "(2) GALV. WASHERS (FOR DRAINAGE)" | property sets: Pset_BuildingElementProxyCommon
  IFCWALLTYPE "Metal stud4:Metal stud" | 1 occurrence | material: "2" GALV. METAL STUDS" | property sets: Pset_WallCommon
  IFCWALLTYPE "Metal stud6:Metal stud" | 1 occurrence | material: "2" GALV. METAL STUDS" | property sets: Pset_WallCommon
  IFCPIPEFITTINGTYPE "Pipe:Pipe" | 1 occurrence | material: "MINI SPLIT LINE SETS"
  IFCWALLTYPE "Metal stud5:Metal stud" | 1 occurrence | material: "GALV. METAL STUD - TOP TRACK" | property sets: Pset_WallCommon
  IFCBUILDINGELEMENTPROXYTYPE "060523 - W_P_C - Fastenings - Generic:_METAL STUD - DRYWALL - GENERIC" | 10 occurrences | material: "ATTACH GYPSUM BOARD TO STUDS AND NOT TO TOP TRACK" | property sets: Pset_BuildingElementProxyCommon
  IFCWALLTYPE "PERFORATED GALV. STEEL PANEL1:PERFORATED GALV. STEEL PANEL" | 1 occurrence | material: "16 GA. PERFORATED GALV. STEEL PANEL" | property sets: Pset_WallCommon
  IFCWALLTYPE "Metal stud8:Metal stud" | 1 occurrence | material: "INTERMITTENT GALV BRACKETS" | property sets: Pset_WallCommon
  IFCBUILDINGELEMENTPROXYTYPE "060523 - W_P_C - Fastenings - Generic:_METAL STUD - DRYWALL - GENERIC" | 4 occurrences | material: "ATTACH GYPSUM BOARD TO STUDS AND NOT TO TOP TRACK" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "060523 - W_P_C - Fastenings - Generic:_METAL STUD - DRYWALL - GENERIC" | 33 occurrences | material: "ATTACH GYPSUM BOARD TO STUDS AND NOT TO TOP TRACK" | property sets: Pset_BuildingElementProxyCommon
  IFCWALLTYPE "PERFORATED GALV. STEEL PANEL2:PERFORATED GALV. STEEL PANEL" | 1 occurrence | material: "16 GA. PERFORATED GALV. STEEL PANEL" | property sets: Pset_WallCommon
  IFCPIPEFITTINGTYPE "Pipe1:Pipe" | 1 occurrence | material: "GALV. PIPE"
  IFCVALVETYPE "U BRACKET1:U BRACKET" | 1 occurrence | material: "GALV. U BRACKET AT GALV. PIPE"
  IFCPIPEFITTINGTYPE "Pipe2:Pipe" | 1 occurrence | material: "MINI SPLIT LINE SETS"
  IFCPIPEFITTINGTYPE "Pipe3:Pipe" | 1 occurrence | material: "GALV. PIPE"
  IFCVALVETYPE "U BRACKET4:U BRACKET" | 1 occurrence | material: "GALV. U BRACKET AT GALV. PIPE"
  IFCPIPEFITTINGTYPE "Pipe4:Pipe" | 1 occurrence | material: "MINI SPLIT LINE SETS"
  IFCPIPEFITTINGTYPE "Pipe5:Pipe" | 1 occurrence | material: "GALV. PIPE"
  IFCVALVETYPE "U BRACKET6:U BRACKET" | 1 occurrence | material: "GALV. U BRACKET AT GALV. PIPE"
  IFCPIPEFITTINGTYPE "Pipe6:Pipe" | 1 occurrence | material: "MINI SPLIT LINE SETS"
  IFCPIPEFITTINGTYPE "Pipe7:Pipe" | 1 occurrence | material: "GALV. PIPE"
  IFCVALVETYPE "U BRACKET8:U BRACKET" | 1 occurrence | material: "GALV. U BRACKET AT GALV. PIPE"
  IFCPIPEFITTINGTYPE "Pipe8:Pipe" | 1 occurrence | material: "MINI SPLIT LINE SETS"
  IFCPIPEFITTINGTYPE "Pipe9:Pipe" | 1 occurrence | material: "GALV. PIPE"
  IFCVALVETYPE "U BRACKET10:U BRACKET" | 1 occurrence | material: "GALV. U BRACKET AT GALV. PIPE"
  IFCPIPEFITTINGTYPE "Pipe10:Pipe" | 1 occurrence | material: "MINI SPLIT LINE SETS"
  IFCPIPEFITTINGTYPE "Pipe11:Pipe" | 1 occurrence | material: "GALV. PIPE"
  IFCVALVETYPE "U BRACKET12:U BRACKET" | 1 occurrence | material: "GALV. U BRACKET AT GALV. PIPE"
  IFCPIPEFITTINGTYPE "Pipe12:Pipe" | 1 occurrence | material: "MINI SPLIT LINE SETS"
  IFCPIPEFITTINGTYPE "Pipe13:Pipe" | 1 occurrence | material: "GALV. PIPE"
  IFCVALVETYPE "U BRACKET14:U BRACKET" | 1 occurrence | material: "GALV. U BRACKET AT GALV. PIPE"
  IFCPIPEFITTINGTYPE "Pipe14:Pipe" | 1 occurrence | material: "MINI SPLIT LINE SETS"
  IFCPIPEFITTINGTYPE "Pipe15:Pipe" | 1 occurrence | material: "GALV. PIPE"
  IFCVALVETYPE "U BRACKET16:U BRACKET" | 1 occurrence | material: "GALV. U BRACKET AT GALV. PIPE"
  IFCPIPEFITTINGTYPE "Pipe16:Pipe" | 1 occurrence | material: "MINI SPLIT LINE SETS"
  IFCPIPEFITTINGTYPE "Pipe17:Pipe" | 1 occurrence | material: "GALV. PIPE"
  IFCVALVETYPE "U BRACKET18:U BRACKET" | 1 occurrence | material: "GALV. U BRACKET AT GALV. PIPE"
  IFCPIPEFITTINGTYPE "Pipe18:Pipe" | 1 occurrence | material: "MINI SPLIT LINE SETS"
  IFCPIPEFITTINGTYPE "Pipe19:Pipe" | 1 occurrence | material: "GALV. PIPE"
  IFCVALVETYPE "U BRACKET20:U BRACKET" | 1 occurrence | material: "GALV. U BRACKET AT GALV. PIPE"
  IFCBUILDINGELEMENTPROXYTYPE "060523 - W_P_C - Fastenings - Generic:_METAL STUD - HEAD - GENERIC" | 1 occurrence | material: "AT HEAD FASTENER AT 24" O.C." | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "060523 - W_P_C - Fastenings - Generic:_METAL STUD - SILL - GENERIC" | 1 occurrence | material: "AT SILL - FASTENER AT 24" O.C." | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "060523 - W_P_C - Fastenings - Generic:_METAL STUD - DRYWALL - GENERIC" | 1 occurrence | material: "ATTACH GYPSUM BOARD TO STUDS AND NOT TO TOP TRACK" | property sets: Pset_BuildingElementProxyCommon
  IFCWALLTYPE "Generic Models 681:Generic Models 1" | 1 occurrence | material: "CLAD WOOD DOOR W/ INSULATED TEMPERED GLAZING" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 647:Generic Models 1" | 1 occurrence | material: "COMPOSITE DECKING W/ HIDDEN FASTENERS" | property sets: Pset_WallCommon
  IFCWALLTYPE "Walls 14:Walls 13" | 1 occurrence | material: "2X10 LEDGER - STAIN BEFORE INSTALL" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 640:Generic Models 1" | 1 occurrence | material: "2X10 JOISTS" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 624:Generic Models 1" | 1 occurrence | material: "3/4 HARDWOOD FLOOR" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 642:Generic Models 1" | 1 occurrence | material: "3/4" GYP. CRETE" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 644:Generic Models 1" | 1 occurrence | material: "1/8" SOUND MAT" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 677:Generic Models 1" | 1 occurrence | material: "METAL FLASHING" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 651:Generic Models 1" | 1 occurrence | material: "FLEXIBLE FLASHING" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 670:Generic Models 1" | 1 occurrence | material: "METAL FLASHING" | property sets: Pset_WallCommon
  IFCBUILDINGELEMENTPROXYTYPE "HIDDEN FASTENING:HIDDEN FASTENING" | 1 occurrence | material: "CONCEALED FASTENERS" | property sets: Pset_BuildingElementProxyCommon
  IFCWALLTYPE "Generic Models 641:Generic Models 1" | 1 occurrence | material: "COMPOSITE DECKING W/ HIDDEN FASTENERS" | property sets: Pset_WallCommon
  IFCBUILDINGELEMENTPROXYTYPE "HIDDEN FASTENING1:HIDDEN FASTENING" | 1 occurrence | material: "CONCEALED FASTENERS" | property sets: Pset_BuildingElementProxyCommon
  IFCWALLTYPE "Generic Models 646:Generic Models 1" | 1 occurrence | material: "COMPOSITE DECKING W/ HIDDEN FASTENERS" | property sets: Pset_WallCommon
  IFCBUILDINGELEMENTPROXYTYPE "HIDDEN FASTENING2:HIDDEN FASTENING" | 1 occurrence | material: "CONCEALED FASTENERS" | property sets: Pset_BuildingElementProxyCommon
  IFCWALLTYPE "Generic Models 648:Generic Models 1" | 1 occurrence | material: "COMPOSITE DECKING W/ HIDDEN FASTENERS" | property sets: Pset_WallCommon
  IFCBUILDINGELEMENTPROXYTYPE "HIDDEN FASTENING3:HIDDEN FASTENING" | 1 occurrence | material: "CONCEALED FASTENERS" | property sets: Pset_BuildingElementProxyCommon
  IFCWALLTYPE "Generic Models 654:Generic Models 1" | 1 occurrence | material: "COMPOSITE DECKING W/ HIDDEN FASTENERS" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 659:Generic Models 1" | 1 occurrence | material: "3/4" CDX OR OSB PLYWOOD - SEE STRUCT DWGS" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 666:Generic Models 1" | 1 occurrence | material: "2X WOOD STUD" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 701:Generic Models 1" | 1 occurrence | material: "WOOD TRUSS FLOOR ASSEMBLY - FILL CAVITY WITH BATT. INSULATION - (UL - L521 FLOOR ASSEMBLY)" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 702:Generic Models 1" | 1 occurrence | material: "5/8" GYP. BD" | property sets: Pset_WallCommon
  IFCWALLTYPE "Walls 17:Walls 13" | 1 occurrence | material: "2X10 LEDGER - STAIN BEFORE INSTALL" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 707:Generic Models 1" | 1 occurrence | material: "2X10 JOISTS" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 708:Generic Models 1" | 1 occurrence | material: "TPO ROOFING MEMBRANE" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 709:Generic Models 1" | 1 occurrence | material: "1" MIN. POLYISO INSULATION OVER AIR BARRIER (WRAP UP/OVER PARAPET)" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 717:Generic Models 1" | 1 occurrence | material: "FIBER CEMENT LAPSIDING" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 719:Generic Models 1" | 1 occurrence | material: "METAL FLASHING" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 722:Generic Models 1" | 1 occurrence | material: "5/8" GYP. BD @ CEILING" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 723:Generic Models 1" | 1 occurrence | material: "1/2" CDX OR OSB PLYWOOD - SEE STRUCT DWGS" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 724:Generic Models 1" | 1 occurrence | material: "BATT INSULATION - FILL ENTIRE CAVITY" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 729:Generic Models 1" | 1 occurrence | material: "RESILIENT CHANNEL - 25 GA. FURRING CHANNELS INSTALLED HORIZONTALLY SPACED 24 IN. OC" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 730:Generic Models 1" | 1 occurrence | material: "WOOD TRUSS - SEE STRUCT DWGS" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 731:Generic Models 1" | 1 occurrence | material: "WOOD TRUSS - SEE STRUCT DWGS" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 732:Generic Models 1" | 1 occurrence | material: "WOOD TRUSS - SEE STRUCT DWGS" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 733:Generic Models 1" | 1 occurrence | material: "3/4" CDX OR OSB PLYWOOD - SEE STRUCT DWGS" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 662:Generic Models 1" | 1 occurrence | material: "PLYTANIUM T1-11 SYP PLYWOOD PANEL SIDING - 4" GROOVES - EXTERIOR GRADE" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 703:Generic Models 1" | 1 occurrence | material: "TAPERED RIGID INSULATION - FOR DRAINAGE" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 704:Generic Models 1" | 1 occurrence | material: "TPO ROOFING MEMBRANE" | property sets: Pset_WallCommon
  IFCBUILDINGELEMENTPROXYTYPE "Vert" | 1 occurrence | material: "METAL DRIP FLASHING" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Vert" | 1 occurrence | material: "DRAINAGE WRAP - ASTM 2273" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 1:Generic Models 1:15607" | 1 occurrence | material: "7/8" CORRUGATED METAL - EXPOSED FASTENERS" | property sets: Pset_BuildingElementProxyCommon
  IFCWALLTYPE "Generic Models 711:Generic Models 1" | 1 occurrence | material: "DRAINAGE WRAP - ASTM 2273" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 706:Generic Models 1" | 1 occurrence | material: "WOOD TRUSS - SEE STRUCT DWGS" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 699:Generic Models 1" | 1 occurrence | material: "1/2" CDX OR OSB PLYWOOD - SEE STRUCT DWGS" | property sets: Pset_WallCommon
  IFCBUILDINGELEMENTPROXYTYPE "Vert" | 1 occurrence | material: "METAL DRIP FLASHING" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Vert" | 1 occurrence | material: "DRAINAGE WRAP - ASTM 2273" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 1:Generic Models 1:15607" | 1 occurrence | material: "7/8" CORRUGATED METAL - EXPOSED FASTENERS" | property sets: Pset_BuildingElementProxyCommon
  IFCWALLTYPE "Generic Models 700:Generic Models 1" | 1 occurrence | material: "FIBER CEMENT LAPSIDING" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 710:Generic Models 1" | 1 occurrence | material: "FIBER CEMENT LAPSIDING" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 712:Generic Models 1" | 1 occurrence | material: "FIBER CEMENT LAPSIDING" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 713:Generic Models 1" | 1 occurrence | material: "FIBER CEMENT LAPSIDING" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 714:Generic Models 1" | 1 occurrence | material: "FIBER CEMENT LAPSIDING" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 636:Generic Models 1" | 1 occurrence | material: "COMPOSITE DECKING W/ HIDDEN FASTENERS" | property sets: Pset_WallCommon
  IFCBUILDINGELEMENTPROXYTYPE "HIDDEN FASTENING4:HIDDEN FASTENING" | 1 occurrence | material: "CONCEALED FASTENERS" | property sets: Pset_BuildingElementProxyCommon
  IFCWALLTYPE "Generic Models 638:Generic Models 1" | 1 occurrence | material: "COMPOSITE DECKING W/ HIDDEN FASTENERS" | property sets: Pset_WallCommon
  IFCBUILDINGELEMENTPROXYTYPE "HIDDEN FASTENING5:HIDDEN FASTENING" | 1 occurrence | material: "CONCEALED FASTENERS" | property sets: Pset_BuildingElementProxyCommon
  IFCWALLTYPE "Generic Models 643:Generic Models 1" | 1 occurrence | material: "COMPOSITE DECKING W/ HIDDEN FASTENERS" | property sets: Pset_WallCommon
  IFCBUILDINGELEMENTPROXYTYPE "RAILING:RAILING" | 1 occurrence | material: "CONT. TREATED 4X6 WITH ROUNDED EDGES AT TOP" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "RAILING 1:RAILING 3" | 1 occurrence | material: "2" X 4" - 6GA GALV. MESH" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "RAILING 3:RAILING 3" | 1 occurrence | material: "2" X 4" - 6GA GALV. MESH" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "RAILING 4:RAILING 3" | 1 occurrence | material: "2" X 4" - 6GA GALV. MESH" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "RAILING 5:RAILING 3" | 1 occurrence | material: "2" X 4" - 6GA GALV. MESH" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "RAILING 6:RAILING 3" | 1 occurrence | material: "2" X 4" - 6GA GALV. MESH" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "RAILING 7:RAILING 3" | 1 occurrence | material: "2" X 4" - 6GA GALV. MESH" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "RAILING 8:RAILING 3" | 1 occurrence | material: "2" X 4" - 6GA GALV. MESH" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "RAILING 9:RAILING 3" | 1 occurrence | material: "2" X 4" - 6GA GALV. MESH" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "RAILING 10:RAILING 3" | 1 occurrence | material: "2" X 4" - 6GA GALV. MESH" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "RAILING 11:RAILING 3" | 1 occurrence | material: "2" X 4" - 6GA GALV. MESH" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "RAILING 12:RAILING 3" | 1 occurrence | material: "2" X 4" - 6GA GALV. MESH" | property sets: Pset_BuildingElementProxyCommon
  IFCWALLTYPE "Generic Models 649:Generic Models 1" | 1 occurrence | material: "COMPOSITE DECKING W/ HIDDEN FASTENERS" | property sets: Pset_WallCommon
  IFCBUILDINGELEMENTPROXYTYPE "HIDDEN FASTENING6:HIDDEN FASTENING" | 1 occurrence | material: "CONCEALED FASTENERS" | property sets: Pset_BuildingElementProxyCommon
  IFCWALLTYPE "Generic Models 661:Generic Models 1" | 1 occurrence | material: "COMPOSITE DECKING W/ HIDDEN FASTENERS" | property sets: Pset_WallCommon
  IFCBUILDINGELEMENTPROXYTYPE "HIDDEN FASTENING7:HIDDEN FASTENING" | 1 occurrence | material: "CONCEALED FASTENERS" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "RAILING 20:RAILING 20" | 1 occurrence | material: "2" X 4" - 6GA GALV. MESH" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "RAILING 21:RAILING 20" | 1 occurrence | material: "2" X 4" - 6GA GALV. MESH" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "RAILING 22:RAILING 20" | 1 occurrence | material: "2" X 4" - 6GA GALV. MESH" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "RAILING 23:RAILING 20" | 1 occurrence | material: "2" X 4" - 6GA GALV. MESH" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "RAILING 24:RAILING 20" | 1 occurrence | material: "2" X 4" - 6GA GALV. MESH" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "RAILING 25:RAILING 20" | 1 occurrence | material: "2" X 4" - 6GA GALV. MESH" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "RAILING 26:RAILING 20" | 1 occurrence | material: "2" X 4" - 6GA GALV. MESH" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "RAILING 27:RAILING 20" | 1 occurrence | material: "2" X 4" - 6GA GALV. MESH" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "RAILING 28:RAILING 20" | 1 occurrence | material: "2" X 4" - 6GA GALV. MESH" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "RAILING 36:RAILING 20" | 1 occurrence | material: "2" X 4" - 6GA GALV. MESH" | property sets: Pset_BuildingElementProxyCommon
  IFCWALLTYPE "Walls 20:Walls 13" | 1 occurrence | material: "2X10 JOISTS" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 664:Generic Models 1" | 1 occurrence | material: "METAL FLASHING - BLACK" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 667:Generic Models 1" | 1 occurrence | material: "METAL FLASHING - BLACK" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 685:Generic Models 1" | 1 occurrence | material: "WOOD TRUSS - SEE STRUCT DWGS" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 686:Generic Models 1" | 1 occurrence | material: "COMPOSITE DECKING W/ HIDDEN FASTENERS" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 687:Generic Models 1" | 1 occurrence | material: "COMPOSITE DECKING W/ HIDDEN FASTENERS" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 715:Generic Models 1" | 1 occurrence | material: "COMPOSITE DECKING W/ HIDDEN FASTENERS" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 716:Generic Models 1" | 1 occurrence | material: "COMPOSITE DECKING W/ HIDDEN FASTENERS" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 718:Generic Models 1" | 1 occurrence | material: "COMPOSITE DECKING W/ HIDDEN FASTENERS" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 727:Generic Models 1" | 1 occurrence | material: "COMPOSITE DECKING W/ HIDDEN FASTENERS" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 728:Generic Models 1" | 1 occurrence | material: "COMPOSITE DECKING W/ HIDDEN FASTENERS" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 734:Generic Models 1" | 1 occurrence | material: "COMPOSITE DECKING W/ HIDDEN FASTENERS" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 735:Generic Models 1" | 1 occurrence | material: "COMPOSITE DECKING W/ HIDDEN FASTENERS" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 736:Generic Models 1" | 1 occurrence | material: "COMPOSITE DECKING W/ HIDDEN FASTENERS" | property sets: Pset_WallCommon
  IFCBUILDINGELEMENTPROXYTYPE "HIDDEN FASTENING8:HIDDEN FASTENING" | 1 occurrence | material: "CONCEALED FASTENERS" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "HIDDEN FASTENING9:HIDDEN FASTENING" | 1 occurrence | material: "CONCEALED FASTENERS" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "HIDDEN FASTENING10:HIDDEN FASTENING" | 1 occurrence | material: "CONCEALED FASTENERS" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "HIDDEN FASTENING11:HIDDEN FASTENING" | 1 occurrence | material: "CONCEALED FASTENERS" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "HIDDEN FASTENING12:HIDDEN FASTENING" | 1 occurrence | material: "CONCEALED FASTENERS" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "HIDDEN FASTENING13:HIDDEN FASTENING" | 1 occurrence | material: "CONCEALED FASTENERS" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "HIDDEN FASTENING14:HIDDEN FASTENING" | 1 occurrence | material: "CONCEALED FASTENERS" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "HIDDEN FASTENING15:HIDDEN FASTENING" | 1 occurrence | material: "CONCEALED FASTENERS" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "HIDDEN FASTENING16:HIDDEN FASTENING" | 1 occurrence | material: "CONCEALED FASTENERS" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "HIDDEN FASTENING17:HIDDEN FASTENING" | 1 occurrence | material: "CONCEALED FASTENERS" | property sets: Pset_BuildingElementProxyCommon
  IFCWALLTYPE "Generic Models 739:Generic Models 1" | 1 occurrence | material: "2X10 JOISTS" | property sets: Pset_WallCommon
  IFCWALLTYPE "corrugated metal wall2:corrugated metal wall" | 1 occurrence | material: "1/2" CDX OR OSB PLYWOOD - SEE STRUCT DWGS" | property sets: Pset_WallCommon
  IFCBUILDINGELEMENTPROXYTYPE "RAILING 13:RAILING 20" | 1 occurrence | material: "2" X 4" - 6GA GALV. MESH" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "RAILING 48:RAILING 20" | 1 occurrence | material: "2" X 4" - 6GA GALV. MESH" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "RAILING 60:RAILING 3" | 1 occurrence | material: "2" X 4" - 6GA GALV. MESH" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "RAILING 61:RAILING 20" | 1 occurrence | material: "2" X 4" - 6GA GALV. MESH" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "RAILING 62:RAILING 3" | 1 occurrence | material: "2" X 4" - 6GA GALV. MESH" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "RAILING1:RAILING" | 1 occurrence | material: "CONT. TREATED 4X6 WITH ROUNDED EDGES AT TOP" | property sets: Pset_BuildingElementProxyCommon
  IFCWALLTYPE "Generic Models 751:Generic Models 1" | 1 occurrence | material: "WOOD TRUSS - SEE STRUCT DWGS" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 682:Generic Models 1" | 1 occurrence | material: "WOOD TRUSS - SEE STRUCT DWGS" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 759:Generic Models 1" | 1 occurrence | material: "WOOD TRUSS - SEE STRUCT DWGS" | property sets: Pset_WallCommon
  IFCWALLTYPE "corrugated metal wall6:corrugated metal wall" | 1 occurrence | material: "7/8" CORRUGATED METAL - EXPOSED FASTENERS" | property sets: Pset_WallCommon
  IFCWALLTYPE "corrugated metal wall9:corrugated metal wall" | 1 occurrence | material: "5/8" GYP. BD" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 773:Generic Models 1" | 1 occurrence | material: "WOOD TRUSS - SEE STRUCT DWGS" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 774:Generic Models 1" | 1 occurrence | material: "3/4 HARDWOOD FLOOR" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 775:Generic Models 1" | 1 occurrence | material: "3/4" GYP. CRETE" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 776:Generic Models 1" | 1 occurrence | material: "1/8" SOUND MAT" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 743:Generic Models 1" | 1 occurrence | material: "METAL FLASHING - BLACK" | property sets: Pset_WallCommon
  IFCWALLTYPE "Walls 32:Walls 13" | 1 occurrence | material: "2X WOOD JOISTS" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 749:Generic Models 1" | 1 occurrence | material: "METAL FLASHING - BLACK" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 675:Generic Models 1" | 1 occurrence | material: "WOOD TRUSS - SEE STRUCT DWGS" | property sets: Pset_WallCommon
  IFCWALLTYPE "building wrap:building wrap" | 1 occurrence | material: "BUILDING WRAP" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 676:Generic Models 1" | 1 occurrence | material: "BUILDING WRAP" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 726:Generic Models 1" | 1 occurrence | material: "METAL FLASHING - BLACK" | property sets: Pset_WallCommon
  IFCBUILDINGELEMENTPROXYTYPE "WASHER232:WASHER" | 1 occurrence | material: "(2) GALV. WASHERS (FOR DRAINAGE)" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "WASHER234:WASHER" | 1 occurrence | material: "(2) GALV. WASHERS (FOR DRAINAGE)" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "WASHER235:WASHER" | 1 occurrence | material: "(2) GALV. WASHERS (FOR DRAINAGE)" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "WASHER236:WASHER" | 1 occurrence | material: "(2) GALV. WASHERS (FOR DRAINAGE)" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "WASHER237:WASHER" | 1 occurrence | material: "(2) GALV. WASHERS (FOR DRAINAGE)" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "WASHER203:WASHER" | 1 occurrence | material: "(2) GALV. WASHERS (FOR DRAINAGE)" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "WASHER206:WASHER" | 1 occurrence | material: "(2) GALV. WASHERS (FOR DRAINAGE)" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "WASHER297:WASHER" | 1 occurrence | material: "(2) GALV. WASHERS (FOR DRAINAGE)" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "WASHER303:WASHER" | 1 occurrence | material: "(2) GALV. WASHERS (FOR DRAINAGE)" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "WASHER316:WASHER" | 1 occurrence | material: "(2) GALV. WASHERS (FOR DRAINAGE)" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "WASHER319:WASHER" | 1 occurrence | material: "(2) GALV. WASHERS (FOR DRAINAGE)" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "WASHER320:WASHER" | 1 occurrence | material: "(2) GALV. WASHERS (FOR DRAINAGE)" | property sets: Pset_BuildingElementProxyCommon
  IFCWALLTYPE "Generic Models 725:Generic Models 1" | 1 occurrence | material: "BUILDING WRAP" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 753:Generic Models 1" | 1 occurrence | material: "METAL FLASHING - BLACK" | property sets: Pset_WallCommon
  IFCWALLTYPE "Metal stud1:Metal stud" | 1 occurrence | material: "GALV. METAL STUD - SILL TRACK" | property sets: Pset_WallCommon
  IFCWALLTYPE "Metal stud3:Metal stud" | 1 occurrence | material: "2" GALV. METAL STUDS" | property sets: Pset_WallCommon
  IFCWALLTYPE "Metal stud7:Metal stud" | 1 occurrence | material: "2" GALV. METAL STUDS" | property sets: Pset_WallCommon
  IFCVALVETYPE "U BRACKET2:U BRACKET" | 1 occurrence | material: "GALV. U BRACKET AT GALV. PIPE"
  IFCWALLTYPE "Generic Models 754:Generic Models 1" | 1 occurrence | material: "2X JOIST UNDER METAL STUDS" | property sets: Pset_WallCommon
  IFCWALLTYPE "PERFORATED GALV. STEEL PANEL4:PERFORATED GALV. STEEL PANEL" | 1 occurrence | material: "16 GA. PERFORATED GALV. STEEL PANEL" | property sets: Pset_WallCommon
  IFCWALLTYPE "PERFORATED GALV. STEEL PANEL5:PERFORATED GALV. STEEL PANEL" | 1 occurrence | material: "16 GA. PERFORATED GALV. STEEL PANEL" | property sets: Pset_WallCommon
  IFCVALVETYPE "U BRACKET3:U BRACKET" | 1 occurrence | material: "GALV. U BRACKET AT GALV. PIPE"
  IFCVALVETYPE "U BRACKET5:U BRACKET" | 1 occurrence | material: "GALV. U BRACKET AT GALV. PIPE"
  IFCVALVETYPE "U BRACKET7:U BRACKET" | 1 occurrence | material: "GALV. U BRACKET AT GALV. PIPE"
  IFCVALVETYPE "U BRACKET9:U BRACKET" | 1 occurrence | material: "GALV. U BRACKET AT GALV. PIPE"
  IFCVALVETYPE "U BRACKET11:U BRACKET" | 1 occurrence | material: "GALV. U BRACKET AT GALV. PIPE"
  IFCVALVETYPE "U BRACKET13:U BRACKET" | 1 occurrence | material: "GALV. U BRACKET AT GALV. PIPE"
  IFCVALVETYPE "U BRACKET15:U BRACKET" | 1 occurrence | material: "GALV. U BRACKET AT GALV. PIPE"
  IFCVALVETYPE "U BRACKET17:U BRACKET" | 1 occurrence | material: "GALV. U BRACKET AT GALV. PIPE"
  IFCVALVETYPE "U BRACKET19:U BRACKET" | 1 occurrence | material: "GALV. U BRACKET AT GALV. PIPE"

Property sets
  Pset_SiteCommon | properties | on 1 object (1 IFCSITE)
    Reference = "Project Information" (IFCIDENTIFIER)
  Pset_EnvironmentalImpactIndicators | properties | on 139 objects (139 IFCWALL)
    Reference = "Generic Models 1" (IFCIDENTIFIER)
  Pset_EnvironmentalImpactIndicators | properties | on 48 objects (48 IFCBUILDINGELEMENTPROXY)
    Reference = "_METAL STUD - DRYWALL - GENERIC" (IFCIDENTIFIER)
  Pset_EnvironmentalImpactIndicators | properties | on 41 objects (41 IFCBUILDINGELEMENTPROXY)
    Reference = "_METAL STUD - HEAD - GENERIC" (IFCIDENTIFIER)
  Pset_EnvironmentalImpactIndicators | properties | on 38 objects (38 IFCBUILDINGELEMENTPROXY)
    Reference = "RAILING 20" (IFCIDENTIFIER)
  Pset_EnvironmentalImpactIndicators | properties | on 37 objects (37 IFCBUILDINGELEMENTPROXY)
    Reference = "WASHER" (IFCIDENTIFIER)
  Pset_EnvironmentalImpactIndicators | properties | on 21 objects (21 IFCBUILDINGELEMENTPROXY)
    Reference = "Thru-Bolt - .8750 - 7/8 2" (IFCIDENTIFIER)
  Pset_EnvironmentalImpactIndicators | properties | on 20 objects (20 IFCPIPEFITTING)
    Reference = "Pipe" (IFCIDENTIFIER)
  Pset_EnvironmentalImpactIndicators | properties | on 20 objects (20 IFCVALVE)
    Reference = "U BRACKET" (IFCIDENTIFIER)
  Pset_EnvironmentalImpactIndicators: 25 more contents on 113 objects not shown
  Pset_ReinforcementBarPitchOfWall | properties | on 139 objects (139 IFCWALL)
    Reference = "Generic Models 1" (IFCLABEL)
  Pset_ReinforcementBarPitchOfWall | properties | on 17 objects (17 IFCWALL)
    Reference = "Walls 13" (IFCLABEL)
  Pset_ReinforcementBarPitchOfWall | properties | on 7 objects (7 IFCWALL)
    Reference = "Metal stud" (IFCLABEL)
  Pset_ReinforcementBarPitchOfWall | properties | on 6 objects (6 IFCWALL)
    Reference = "corrugated metal wall" (IFCLABEL)
  Pset_ReinforcementBarPitchOfWall | properties | on 4 objects (4 IFCWALL)
    Reference = "PERFORATED GALV. STEEL PANEL" (IFCLABEL)
  Pset_ReinforcementBarPitchOfWall | properties | on 1 object (1 IFCWALL)
    Reference = "Walls 12" (IFCLABEL)
  Pset_ReinforcementBarPitchOfWall | properties | on 1 object (1 IFCWALL)
    Reference = "Dowel" (IFCLABEL)
  Pset_ReinforcementBarPitchOfWall | properties | on 1 object (1 IFCWALL)
    Reference = "Walls 16" (IFCLABEL)
  Pset_ReinforcementBarPitchOfWall: 1 more content on 1 objects not shown
  Pset_WallCommon | properties | on 139 objects (139 IFCWALL)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Generic Models 1" (IFCIDENTIFIER)
  Pset_WallCommon | properties | on 17 objects (17 IFCWALL)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Walls 13" (IFCIDENTIFIER)
  Pset_WallCommon | properties | on 7 objects (7 IFCWALL)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Metal stud" (IFCIDENTIFIER)
  Pset_WallCommon | properties | on 6 objects (6 IFCWALL)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "corrugated metal wall" (IFCIDENTIFIER)
  Pset_WallCommon | properties | on 4 objects (4 IFCWALL)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "PERFORATED GALV. STEEL PANEL" (IFCIDENTIFIER)
  Pset_WallCommon | properties | on 1 object (1 IFCWALL)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Walls 12" (IFCIDENTIFIER)
  Pset_WallCommon | properties | on 1 object (1 IFCWALL)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Dowel" (IFCIDENTIFIER)
  Pset_WallCommon | properties | on 1 object (1 IFCWALL)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Walls 16" (IFCIDENTIFIER)
  Pset_WallCommon: 2 more contents on 1 objects not shown
  Pset_BuildingElementProxyCommon | properties | on 48 objects (48 IFCBUILDINGELEMENTPROXY)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "_METAL STUD - DRYWALL - GENERIC" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 41 objects (41 IFCBUILDINGELEMENTPROXY)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "_METAL STUD - HEAD - GENERIC" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 38 objects (38 IFCBUILDINGELEMENTPROXY)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "RAILING 20" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 37 objects (37 IFCBUILDINGELEMENTPROXY)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "WASHER" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 21 objects (21 IFCBUILDINGELEMENTPROXY)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Thru-Bolt - .8750 - 7/8 2" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 18 objects (18 IFCBUILDINGELEMENTPROXY)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "HIDDEN FASTENING" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 18 objects (18 IFCBUILDINGELEMENTPROXY)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "RAILING 3" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 8 objects (8 IFCBUILDINGELEMENTPROXY)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Screw - SDWS 3" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon: 17 more contents on 32 objects not shown
  Pset_PipeFittingTypeCommon | properties | on 20 objects (20 IFCPIPEFITTING)
    Reference = "Pipe" (IFCIDENTIFIER)
  Pset_ValveTypeCommon | properties | on 20 objects (20 IFCVALVE)
    Reference = "U BRACKET" (IFCIDENTIFIER)
  Pset_BuildingStoreyCommon | properties | on 3 objects (3 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
    Reference = "Project Base Point" (IFCIDENTIFIER)
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDING)
    AboveGround = UNKNOWN (IFCLOGICAL)
    Reference = "Project Information" (IFCIDENTIFIER)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    IsLandmarked = UNKNOWN (IFCLOGICAL)
    NumberOfStoreys = 3 (IFCINTEGER)
    Reference = "Project Information" (IFCIDENTIFIER)
  Pset_BuildingSystemCommon | properties | on 1 object (1 IFCBUILDING)
    Reference = "Project Information" (IFCIDENTIFIER)