IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView_V2.0]"
File name: "Details from 2154 Collady Point.ifc"
Time stamp: "2022-03-01T10:25:56-06:00"
Preprocessor: "IfcOpenShell v0.7.0-4c40fc16"
Originating system: "BlenderBIM 0.0.220218"
Application: "Autodesk Revit 2020 (ENU)" version "2020" identifier "Revit" by Organization "Autodesk Revit 2020 (ENU)"
Application: "BlenderBIM Add-on" version "0.0.220218" identifier "BlenderBIM" by Organization "IfcOpenShell" id "IfcOpenShell" description "IfcOpenShell is an open source software library that helps users and software developers to work with IFC data." (roles: "CONTRIBUTOR"; telecom address "WEBPAGE": web page "https://ifcopenshell.org")

People and organizations
  Person "ryan@openingdesign.com" of Organization (no name given)
  Owner history of Person "ryan@openingdesign.com" of Organization (no name given) | application "Autodesk Revit 2020 (ENU)" version "2020" identifier "Revit" by Organization "Autodesk Revit 2020 (ENU)" | change NOCHANGE | created 1646055635 (2022-02-28T13:40:35Z)
  Owner history of Person "ryan@openingdesign.com" of Organization (no name given) | application "Autodesk Revit 2020 (ENU)" version "2020" identifier "Revit" by Organization "Autodesk Revit 2020 (ENU)" | change MODIFIED | created 1646055635 (2022-02-28T13:40:35Z) | last modified 1646149844 (2022-03-01T15:50:44Z) by Person "ryan@openingdesign.com" of Organization (no name given) with "BlenderBIM Add-on" version "0.0.220218" identifier "BlenderBIM" by Organization "IfcOpenShell" id "IfcOpenShell" description "IfcOpenShell is an open source software library that helps users and software developers to work with IFC data." (roles: "CONTRIBUTOR"; telecom address "WEBPAGE": web page "https://ifcopenshell.org")
  Owner history of Person "ryan@openingdesign.com" of Organization (no name given) | application "Autodesk Revit 2020 (ENU)" version "2020" identifier "Revit" by Organization "Autodesk Revit 2020 (ENU)" | change MODIFIED | created 1646055635 (2022-02-28T13:40:35Z) | last modified 1646151956 (2022-03-01T16:25:56Z) by Person "ryan@openingdesign.com" of Organization (no name given) with "BlenderBIM Add-on" version "0.0.220218" identifier "BlenderBIM" by Organization "IfcOpenShell" id "IfcOpenShell" description "IfcOpenShell is an open source software library that helps users and software developers to work with IFC data." (roles: "CONTRIBUTOR"; telecom address "WEBPAGE": web page "https://ifcopenshell.org")

Units
  LENGTHUNIT: FOOT (conversion based)
  AREAUNIT: SQUARE FOOT (conversion based)
  VOLUMEUNIT: CUBIC FOOT (conversion based)
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  MOMENTOFINERTIAUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"
  LINEARFORCEUNIT: derived
  PLANARFORCEUNIT: derived

Spatial structure
IFCPROJECT "Project Number" | long name "CHRISTESON RESIDENCE" | phase "Project Status"
  IFCSITE "Default" | latitude 42° 21′ 30.344238″ | longitude -71° 3′ 35.194702″ | elevation above sea level 100.
    IFCBUILDING | postal address: "2154 COLLADY POINT DRIVE", "<Default>"
      IFCBUILDINGSTOREY "1ST FLOOR" | long name "1ST FLOOR" | object type "Level:Project Base Point" | elevation -1.41137169430094E-27
        contains 145 elements
          1 x IFCWALL | type IFCWALLTYPE "Walls 39:Walls 26" | object type "Walls 39:Walls 26" | names: "Walls 39:Walls 26:4520732" | material: "1/2" CDX PLYWOOD" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 43:Walls 26" | object type "Walls 43:Walls 26" | names: "Walls 43:Walls 26:4521567" | material: "1/2" CDX PLYWOOD" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 42:Walls 26" | object type "Walls 42:Walls 26" | names: "Walls 42:Walls 26:4521661" | material: "THERMALLY MODIFIED WOOD (VENT TOP AND BOTTOM)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 48:Walls 26" | object type "Walls 48:Walls 26" | names: "Walls 48:Walls 26:4523590" | material: "BUILDING WRAP" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 52:Walls 26" | object type "Walls 52:Walls 26" | names: "Walls 52:Walls 26:4525555" | material: "STEEL I BEAM JOISTS 24" O.C. - WEB(10") - FLANGE (2.75") - GAUGE (.125" ESTIMATED)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 53:Walls 26" | object type "Walls 53:Walls 26" | names: "Walls 53:Walls 26:4531899" | material: "STEEL C CHANNEL HDG PRE-DRILLED" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 54:Walls 26" | object type "Walls 54:Walls 26" | names: "Walls 54:Walls 26:4532146" | material: "1/2" CDX PLYWOOD" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 55:Walls 26" | object type "Walls 55:Walls 26" | names: "Walls 55:Walls 26:4532445" | material: "2X6 DOUBLE STUD TOP PLATE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 57:Walls 26" | object type "Walls 57:Walls 26" | names: "Walls 57:Walls 26:4532514" | material: "2X6 DOUBLE STUD TOP PLATE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 58:Walls 26" | object type "Walls 58:Walls 26" | names: "Walls 58:Walls 26:4532539" | material: "2X6 DOUBLE STUD TOP PLATE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 59:Walls 26" | object type "Walls 59:Walls 26" | names: "Walls 59:Walls 26:4532576" | material: "2X6 DOUBLE STUD TOP PLATE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 60:Walls 26" | object type "Walls 60:Walls 26" | names: "Walls 60:Walls 26:4532608" | material: "METAL FLASHING (MATCH SS)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 61:Walls 26" | object type "Walls 61:Walls 26" | names: "Walls 61:Walls 26:4532953" | material: "BUILDING WRAP" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 62:Walls 26" | object type "Walls 62:Walls 26" | names: "Walls 62:Walls 26:4533159" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 63:Walls 26" | object type "Walls 63:Walls 26" | names: "Walls 63:Walls 26:4533697" | material: "CONCRETE WALL - (PATTERNED CONCRETE W/ VINYL FORMLINERS)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 64:Walls 26" | object type "Walls 64:Walls 26" | names: "Walls 64:Walls 26:4533765" | material: "5/8" GYP. BD" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 65:Walls 26" | object type "Walls 65:Walls 26" | names: "Walls 65:Walls 26:4533863" | material: "5/8" GYP. BD" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 66:Walls 26" | object type "Walls 66:Walls 26" | names: "Walls 66:Walls 26:4534169" | material: "THERMALLY MODIFIED WOOD (VENT TOP AND BOTTOM)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 67:Walls 26" | object type "Walls 67:Walls 26" | names: "Walls 67:Walls 26:4534370" | material: "AWNING WINDOW W/ INSULATED GLAZING" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 68:Walls 26" | object type "Walls 68:Walls 26" | names: "Walls 68:Walls 26:4534634" | material: "FILL CAVITY WITH BATT INSULATION" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 69:Walls 26" | object type "Walls 69:Walls 26" | names: "Walls 69:Walls 26:4534681" | material: "2" OF CLOSED POLYURETHANE CELL FOAM" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 70:Walls 26" | object type "Walls 70:Walls 26" | names: "Walls 70:Walls 26:4534749" | material: "2" OF CLOSED POLYURETHANE CELL FOAM" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 71:Walls 26" | object type "Walls 71:Walls 26" | names: "Walls 71:Walls 26:4535011" | material: "METAL FLASHING (MATCH SS)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 72:Walls 26" | object type "Walls 72:Walls 26" | names: "Walls 72:Walls 26:4535797" | material: "SEALANT (W/ BACKER ROD IF NECESSARY)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 74:Walls 26" | object type "Walls 74:Walls 26" | names: "Walls 74:Walls 26:4535903" | material: "2X6 DOUBLE STUD TOP PLATE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 75:Walls 26" | object type "Walls 75:Walls 26" | names: "Walls 75:Walls 26:4535938" | material: "2X6 DOUBLE STUD TOP PLATE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 76:Walls 26" | object type "Walls 76:Walls 26" | names: "Walls 76:Walls 26:4535974" | material: "2X BLOCKING" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 78:Walls 26" | object type "Walls 78:Walls 26" | names: "Walls 78:Walls 26:4536535" | material: "EXPANDING POLYURETHANE FOAM" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 79:Walls 26" | object type "Walls 79:Walls 26" | names: "Walls 79:Walls 26:4536695" | material: "EXPANDING POLYURETHANE FOAM" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 81:Walls 26" | object type "Walls 81:Walls 26" | names: "Walls 81:Walls 26:4537920" | material: "1/2" CDX PLYWOOD" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 82:Walls 26" | object type "Walls 82:Walls 26" | names: "Walls 82:Walls 26:4537997" | material: "1/2" CDX PLYWOOD" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 83:Walls 83" | object type "Walls 83:Walls 83" | names: "Walls 83:Walls 83:4538254" | material: "STANDING SEAM METAL WITH VARYING WIDTHS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 80:Walls 26" | object type "Walls 80:Walls 26" | names: "Walls 80:Walls 26:4538478" | material: "LVL(s) - SIZE T.B.D." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 84:Walls 26" | object type "Walls 84:Walls 26" | names: "Walls 84:Walls 26:4539002" | material: "2X WOOD STUDS W/ RIGID INSULATION" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 85:Walls 26" | object type "Walls 85:Walls 26" | names: "Walls 85:Walls 26:4539076" | material: "60 MIL EPDM MEMBRANE OVER 3/4" CDX OR OSB" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 86:Walls 26" | object type "Walls 86:Walls 26" | names: "Walls 86:Walls 26:4539585" | material: "60 MIL EPDM MEMBRANE OVER 3/4" CDX OR OSB" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 87:Walls 26" | object type "Walls 87:Walls 26" | names: "Walls 87:Walls 26:4540170" | material: "1/2" CDX PLYWOOD" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 91:Walls 26" | object type "Walls 91:Walls 26" | names: "Walls 91:Walls 26:4541630" | material: "TJI - SEE STRUCT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 92:Walls 26" | object type "Walls 92:Walls 26" | names: "Walls 92:Walls 26:4542177" | material: "1/2" CDX PLYWOOD" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 93:Walls 26" | object type "Walls 93:Walls 26" | names: "Walls 93:Walls 26:4542240" | material: "2X WOOD STUDS W/ RIGID INSULATION" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 117:Walls 26" | object type "Walls 117:Walls 26" | names: "Walls 117:Walls 26:4551371" | material: "THERMALLY MODIFIED WOOD (VENT TOP AND BOTTOM)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 162:Walls 162" | object type "Walls 162:Walls 162" | names: "Walls 162:Walls 162:4568244" | material: "TJI - SEE STRUCT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 163:Walls 162" | object type "Walls 163:Walls 162" | names: "Walls 163:Walls 162:4568312" | material: "2X BLOCKING" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 164:Walls 164" | object type "Walls 164:Walls 164" | names: "Walls 164:Walls 164:4569267" | material: "THERMALLY MODIFIED DECKING" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 165:Walls 164" | object type "Walls 165:Walls 164" | names: "Walls 165:Walls 164:4569367" | material: "3/4" CDX PLYWOOD" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 166:Walls 164" | object type "Walls 166:Walls 164" | names: "Walls 166:Walls 164:4569468" | material: "LVL(s) - SIZE T.B.D." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 167:Walls 164" | object type "Walls 167:Walls 164" | names: "Walls 167:Walls 164:4569554" | material: "1/2" CDX PLYWOOD" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 209:Walls 208" | object type "Walls 209:Walls 208" | names: "Walls 209:Walls 208:4586678" | material: "2X WOOD STUDS W/ 3" POLY ISO FOAM (NON-STRUCTURAL STUDS)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 210:Walls 208" | object type "Walls 210:Walls 208" | names: "Walls 210:Walls 208:4586721" | material: "5/8" GYP. BD" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 212:Walls 212" | object type "Walls 212:Walls 212" | names: "Walls 212:Walls 212:4587676" | material: "CRIPPLE STUD OR CLIP ANGLE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 225:Walls 26" | object type "Walls 225:Walls 26" | names: "Walls 225:Walls 26:4593571" | material: "2X BLOCKING" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 226:Walls 26" | object type "Walls 226:Walls 26" | names: "Walls 226:Walls 26:4593744" | material: "2X BLOCKING" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 227:Walls 26" | object type "Walls 227:Walls 26" | names: "Walls 227:Walls 26:4595654" | material: "3/4" CDX PLYWOOD" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 228:Walls 26" | object type "Walls 228:Walls 26" | names: "Walls 228:Walls 26:4595837" | material: "1/2" CDX PLYWOOD" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 229:Walls 26" | object type "Walls 229:Walls 26" | names: "Walls 229:Walls 26:4596372" | material: "METAL FLASHING (MATCH SS)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 230:Walls 26" | object type "Walls 230:Walls 26" | names: "Walls 230:Walls 26:4596814" | material: "2X BLOCKING" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 231:Walls 26" | object type "Walls 231:Walls 26" | names: "Walls 231:Walls 26:4596909" | material: "2X BLOCKING" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 73:Walls 26" | object type "Walls 73:Walls 26" | names: "Walls 73:Walls 26:4597481" | material: "SEALANT (W/ BACKER ROD IF NECESSARY)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 77:Walls 26" | object type "Walls 77:Walls 26" | names: "Walls 77:Walls 26:4597590" | material: "FILL REMAINING CAVITY WITH BLOWN-IN CELLULOSE INSULATION" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 232:Walls 26" | object type "Walls 232:Walls 26" | names: "Walls 232:Walls 26:4597890" | material: "2X BLOCKING" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 233:Walls 26" | object type "Walls 233:Walls 26" | names: "Walls 233:Walls 26:4598101" | material: "2X BLOCKING" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 234:Walls 26" | object type "Walls 234:Walls 26" | names: "Walls 234:Walls 26:4598146" | material: "2X BLOCKING" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 235:Walls 26" | object type "Walls 235:Walls 26" | names: "Walls 235:Walls 26:4598179" | material: "2X BLOCKING" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 236:Walls 236" | object type "Walls 236:Walls 236" | names: "Walls 236:Walls 236:4600287" | material: "EXPANDING POLYURETHANE FOAM" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 237:Walls 236" | object type "Walls 237:Walls 236" | names: "Walls 237:Walls 236:4600311" | material: "EXPANDING POLYURETHANE FOAM" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 238:Walls 238" | object type "Walls 238:Walls 238" | names: "Walls 238:Walls 238:4600397" | material: "SEALANT (W/ BACKER ROD IF NECESSARY)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 239:Walls 238" | object type "Walls 239:Walls 238" | names: "Walls 239:Walls 238:4600412" | material: "SEALANT (W/ BACKER ROD IF NECESSARY)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 241:Walls 26" | object type "Walls 241:Walls 26" | names: "Walls 241:Walls 26:4601395" | material: "SEALANT (W/ BACKER ROD IF NECESSARY)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 240:Walls 164" | object type "Walls 240:Walls 164" | names: "Walls 240:Walls 164:4602360" | material: "2X BLOCKING" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 243:Walls 164" | object type "Walls 243:Walls 164" | names: "Walls 243:Walls 164:4602858" | material: "BUILDING WRAP" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 172:Walls 162" | object type "Walls 172:Walls 162" | names: "Walls 172:Walls 162:4603314" | material: "TJI - SEE STRUCT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 242:Walls 164" | object type "Walls 242:Walls 164" | names: "Walls 242:Walls 164:4603476" | material: "2X BLOCKING" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 168:Walls 164" | object type "Walls 168:Walls 164" | names: "Walls 168:Walls 164:4603649" | material: "STANDING SEAM METAL WITH VARYING WIDTHS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 244:Walls 164" | object type "Walls 244:Walls 164" | names: "Walls 244:Walls 164:4605757" | material: "60 MIL EPDM MEMBRANE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 160:Walls 164" | object type "Walls 160:Walls 164" | names: "Walls 160:Walls 164:4610943" | material: "METAL FLASHING (MATCH SS)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 45:Walls 26" | object type "Walls 45:Walls 26" | names: "Walls 45:Walls 26:4613778" | material: "PRE-ENGINEERED TRUSS @ 24" O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 46:Walls 26" | object type "Walls 46:Walls 26" | names: "Walls 46:Walls 26:4614435" | material: "GUSSET PLATE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 247:Walls 26" | object type "Walls 247:Walls 26" | names: "Walls 247:Walls 26:4615210" | material: "2X BLOCKING" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 47:Walls 26" | object type "Walls 47:Walls 26" | names: "Walls 47:Walls 26:4615536" | material: "SELF ADHERED MEMBRANE - UNDER GUTTER AND ROOF FELT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 248:Walls 26" | object type "Walls 248:Walls 26" | names: "Walls 248:Walls 26:4615759" | material: "12 GA. METAL FLASHING (MATCH SS)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 251:Walls 26" | object type "Walls 251:Walls 26" | names: "Walls 251:Walls 26:4619909" | material: "1/2" CORE-E-VENT VENTED VERTICAL FURRING STRIPS 16" O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 252:Walls 26" | object type "Walls 252:Walls 26" | names: "Walls 252:Walls 26:4620008" | material: "BLOWN-IN INSULATION IN ENTIRE CAVITY" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 256:Walls 26" | object type "Walls 256:Walls 26" | names: "Walls 256:Walls 26:4625506" | material: "BUILDING WRAP" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 258:Walls 26" | object type "Walls 258:Walls 26" | names: "Walls 258:Walls 26:4625540" | material: "12 GA. METAL FLASHING (MATCH SS)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 259:Walls 26" | object type "Walls 259:Walls 26" | names: "Walls 259:Walls 26:4625562" | material: "12 GA. METAL FLASHING (MATCH SS)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 249:Walls 26" | object type "Walls 249:Walls 26" | names: "Walls 249:Walls 26:4627838" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 261:Walls 26" | object type "Walls 261:Walls 26" | names: "Walls 261:Walls 26:4629187" | material: "2X BLOCKING" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 245:Walls 26" | object type "Walls 245:Walls 26" | names: "Walls 245:Walls 26:4629686" | material: "EXPANDING POLYURETHANE FOAM" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 260:Walls 26" | object type "Walls 260:Walls 26" | names: "Walls 260:Walls 26:4629942" | material: "1/2" CORE-E-VENT BUG SCREEN" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 262:Walls 26" | object type "Walls 262:Walls 26" | names: "Walls 262:Walls 26:4630720" | material: "STANDING SEAM METAL WITH VARYING WIDTHS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 263:Walls 26" | object type "Walls 263:Walls 26" | names: "Walls 263:Walls 26:4631814" | material: "1/2" CORE-E-VENT VENTED VERTICAL FURRING STRIPS 16" O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 264:Walls 26" | object type "Walls 264:Walls 26" | names: "Walls 264:Walls 26:4631869" | material: "1/2" CORE-E-VENT BUG SCREEN" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 257:Walls 26" | object type "Walls 257:Walls 26" | names: "Walls 257:Walls 26:4632056" | material: "2X BLOCKING" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 265:Walls 26" | object type "Walls 265:Walls 26" | names: "Walls 265:Walls 26:4632132" | material: "GUSSET PLATE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 250:Walls 26" | object type "Walls 250:Walls 26" | names: "Walls 250:Walls 26:4632273" | material: "LVL RIM BOARD - SEE STRUCT. DWGS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 161:Walls 26" | object type "Walls 161:Walls 26" | names: "Walls 161:Walls 26:4632607" | material: "2X BLOCKING" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 267:Walls 26" | object type "Walls 267:Walls 26" | names: "Walls 267:Walls 26:4632655" | material: "2X BLOCKING" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 268:Walls 26" | object type "Walls 268:Walls 26" | names: "Walls 268:Walls 26:4632689" | material: "2X BLOCKING" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 269:Walls 26" | object type "Walls 269:Walls 26" | names: "Walls 269:Walls 26:4632740" | material: "2X BLOCKING" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 270:Walls 26" | object type "Walls 270:Walls 26" | names: "Walls 270:Walls 26:4633034" | material: "STEEL - SIZE TBD - PAINTED" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 271:Walls 26" | object type "Walls 271:Walls 26" | names: "Walls 271:Walls 26:4633437" | material: "2X WOOD STUD" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 266:Walls 26" | object type "Walls 266:Walls 26" | names: "Walls 266:Walls 26:4633517" | material: "LVL RIM BOARD(1 1/4") - SEE STRUCT. DWGS(1)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 272:Walls 26" | object type "Walls 272:Walls 26" | names: "Walls 272:Walls 26:4633555" | material: "2X BLOCKING" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 273:Walls 26" | object type "Walls 273:Walls 26" | names: "Walls 273:Walls 26:4633569" | material: "2X BLOCKING" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 274:Walls 26" | object type "Walls 274:Walls 26" | names: "Walls 274:Walls 26:4633583" | material: "2X BLOCKING" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 275:Walls 26" | object type "Walls 275:Walls 26" | names: "Walls 275:Walls 26:4633597" | material: "2X BLOCKING" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 276:Walls 26" | object type "Walls 276:Walls 26" | names: "Walls 276:Walls 26:4633611" | material: "2X BLOCKING" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 277:Walls 26" | object type "Walls 277:Walls 26" | names: "Walls 277:Walls 26:4634299" | material: "1/2" CDX PLYWOOD" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 278:Walls 26" | object type "Walls 278:Walls 26" | names: "Walls 278:Walls 26:4634348" | material: "1/2" CDX PLYWOOD" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 279:Walls 26" | object type "Walls 279:Walls 26" | names: "Walls 279:Walls 26:4634399" | material: "2X WOOD STUD" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 281:Walls 26" | object type "Walls 281:Walls 26" | names: "Walls 281:Walls 26:4634481" | material: "EXPANDING POLYURETHANE FOAM" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 282:Walls 26" | object type "Walls 282:Walls 26" | names: "Walls 282:Walls 26:4634801" | material: "TREATED 2X10's (NO. 1 GRADE) - STAINED - 10" O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 285:Walls 26" | object type "Walls 285:Walls 26" | names: "Walls 285:Walls 26:4635402" | material: "STEEL I BEAM JOISTS 24" O.C. - WEB(10") - FLANGE (2.75") - GAUGE (.125" ESTIMATED)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 288:Walls 26" | object type "Walls 288:Walls 26" | names: "Walls 288:Walls 26:4647088" | material: "1/2" CDX PLYWOOD" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 293:Walls 26" | object type "Walls 293:Walls 26" | names: "Walls 293:Walls 26:4647598" | material: "LVL(s) - SEE STRUCT. DWGS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 294:Walls 26" | object type "Walls 294:Walls 26" | names: "Walls 294:Walls 26:4648112" | material: "2X6s W/ 2" POLY ISO FOAM & 3.5" OF BLOWN-IN CELLULOSE INSULATION" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 295:Walls 26" | object type "Walls 295:Walls 26" | names: "Walls 295:Walls 26:4648219" | material: "5/8" GYP. BD" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 296:Walls 26" | object type "Walls 296:Walls 26" | names: "Walls 296:Walls 26:4648306" | material: "1/2" CORE-E-VENT BUG SCREEN" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 297:Walls 26" | object type "Walls 297:Walls 26" | names: "Walls 297:Walls 26:4648398" | material: "BUILDING WRAP" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 300:Walls 26" | object type "Walls 300:Walls 26" | names: "Walls 300:Walls 26:4649216" | material: "1/2" CORE-E-VENT VENTED VERTICAL FURRING STRIPS 16" O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 302:Walls 26" | object type "Walls 302:Walls 26" | names: "Walls 302:Walls 26:4649985" | material: "ALUM. STOREFRONT W/ TEMPERED INSULATED GLAZING" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 303:Walls 26" | object type "Walls 303:Walls 26" | names: "Walls 303:Walls 26:4650001" | material: "SEALANT (W/ BACKER ROD IF NECESSARY)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 304:Walls 26" | object type "Walls 304:Walls 26" | names: "Walls 304:Walls 26:4650017" | material: "SEALANT (W/ BACKER ROD IF NECESSARY)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 305:Walls 26" | object type "Walls 305:Walls 26" | names: "Walls 305:Walls 26:4650033" | material: "EXPANDING POLYURETHANE FOAM" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 306:Walls 26" | object type "Walls 306:Walls 26" | names: "Walls 306:Walls 26:4650047" | material: "METAL FLASHING (MATCH SS)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 290:Walls 26" | object type "Walls 290:Walls 26" | names: "Walls 290:Walls 26:4660223" | material: "2X BLOCKING" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 291:Walls 238" | object type "Walls 291:Walls 238" | names: "Walls 291:Walls 238:4660970" | material: "SEALANT (W/ BACKER ROD IF NECESSARY)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 307:Walls 26" | object type "Walls 307:Walls 26" | names: "Walls 307:Walls 26:4661124" | material: "1X4 WOOD TRIM" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 308:Walls 26" | object type "Walls 308:Walls 26" | names: "Walls 308:Walls 26:4662985" | material: "5/8" GYP. BD" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 309:Walls 26" | object type "Walls 309:Walls 26" | names: "Walls 309:Walls 26:4663285" | material: "2X BLOCKING" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 310:Walls 26" | object type "Walls 310:Walls 26" | names: "Walls 310:Walls 26:4663343" | material: "2X BLOCKING" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 312:Walls 26" | object type "Walls 312:Walls 26" | names: "Walls 312:Walls 26:4671875" | material: "SHIMS AS NECESSARY W/ EXPANDING POLYURETHANE FOAM(1)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 314:Walls 26" | object type "Walls 314:Walls 26" | names: "Walls 314:Walls 26:4672917" | material: "2X BLOCKING 24" O.C. BRACE TO FLOOR TRUSS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 315:Walls 26" | object type "Walls 315:Walls 26" | names: "Walls 315:Walls 26:4673435" | material: "2X WOOD STUD" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 44:Walls 26" | object type "Walls 44:Walls 26" | names: "Walls 44:Walls 26:4673466" | material: "2X WOOD STUD" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 246:Walls 26" | object type "Walls 246:Walls 26" | names: "Walls 246:Walls 26:4673489" | material: "2X WOOD STUD" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 311:Walls 26" | object type "Walls 311:Walls 26" | names: "Walls 311:Walls 26:4673513" | material: "2X WOOD STUD" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 280:Walls 26" | object type "Walls 280:Walls 26" | names: "Walls 280:Walls 26:4673574" | material: "2X WOOD STUD" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 313:Walls 26" | object type "Walls 313:Walls 26" | names: "Walls 313:Walls 26:4673599" | material: "2X WOOD STUD" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 255:Walls 26" | object type "Walls 255:Walls 26" | names: "Walls 255:Walls 26:4673638" | material: "TREATED 2X10 LEDGER - STAINED" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 316:Walls 26" | object type "Walls 316:Walls 26" | names: "Walls 316:Walls 26:4674203" | material: "2X WOOD STUD" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 317:Walls 26" | object type "Walls 317:Walls 26" | names: "Walls 317:Walls 26:4675234" | material: "2X BLOCKING 24" O.C. BRACE TO FLOOR TRUSS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 318:Walls 26" | object type "Walls 318:Walls 26" | names: "Walls 318:Walls 26:4675257" | material: "2X WOOD STUD" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 320:Walls 26" | object type "Walls 320:Walls 26" | names: "Walls 320:Walls 26:4676309" | material: "(3) GALV. WASHERS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 322:Walls 26" | object type "Walls 322:Walls 26" | names: "Walls 322:Walls 26:4677502" | material: "J BEAD DRYWALL TRIM" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
      IFCBUILDINGSTOREY "2ND FLOOR" | long name "2ND FLOOR" | object type "Level:Project Base Point" | elevation 12.
        contains 108 elements
          1 x IFCWALL | type IFCWALLTYPE "Walls 2:Walls 26" | object type "Walls 2:Walls 26" | names: "Walls 2:Walls 26:4502543" | material: "2X6 DOUBLE STUD TOP PLATE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 13:Walls 26" | object type "Walls 13:Walls 26" | names: "Walls 13:Walls 26:4502933" | material: "5/8" GYP. BD" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 1:Walls 26" | object type "Walls 1:Walls 26" | names: "Walls 1:Walls 26:4503730" | material: "2X6 DOUBLE STUD TOP PLATE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 3:Walls 26" | object type "Walls 3:Walls 26" | names: "Walls 3:Walls 26:4503751" | material: "ALUM. STOREFRONT W/ TEMPERED INSULATED GLAZING" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 12:Walls 26" | object type "Walls 12:Walls 26" | names: "Walls 12:Walls 26:4503866" | material: "5/8" GYP. BD" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 4:Walls 26" | object type "Walls 4:Walls 26" | names: "Walls 4:Walls 26:4506407" | material: "SEALANT (W/ BACKER ROD IF NECESSARY)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 6:Walls 26" | object type "Walls 6:Walls 26" | names: "Walls 6:Walls 26:4506786" | material: "PRE-ENGINEERED TRUSS @ 24" O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 14:Walls 26" | object type "Walls 14:Walls 26" | names: "Walls 14:Walls 26:4508068" | material: "LVL(s) - SIZE T.B.D." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "050523 - Metal fastenings - Joist Hanger - Generic:ROOF TRUSS HANGER - TYPE 1" | object type "050523 - Metal fastenings - Joist Hanger - Generic:ROOF TRUSS HANGER - TYPE 1" | names: "050523 - Metal fastenings - Joist Hanger - Generic:ROOF TRUSS HANGER - TYPE 1:4511454" | material: materials ("ROOF JOIST HANGER - TYPE 1", "ROOF JOIST HANGER - TYPE 1", "ROOF JOIST HANGER - TYPE 1", "ROOF JOIST HANGER - TYPE 1") | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ProvisionForVoid
          1 x IFCWALL | type IFCWALLTYPE "Walls 19:Walls 26" | object type "Walls 19:Walls 26" | names: "Walls 19:Walls 26:4511916" | material: "1/2" CDX PLYWOOD" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 31:Walls 26" | object type "Walls 31:Walls 26" | names: "Walls 31:Walls 26:4515613" | material: "GALV. STANDING SEAM METAL ROOF" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 33:Walls 26" | object type "Walls 33:Walls 26" | names: "Walls 33:Walls 26:4515660" | material: "BUILDING WRAP" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 20:Walls 26" | object type "Walls 20:Walls 26" | names: "Walls 20:Walls 26:4516105" | material: "METAL FLASHING (MATCH SS)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 23:Walls 26" | object type "Walls 23:Walls 26" | names: "Walls 23:Walls 26:4517552" | material: "METAL FLASHING (MATCH SS)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 34:Walls 26" | object type "Walls 34:Walls 26" | names: "Walls 34:Walls 26:4517857" | material: "EXPANDING POLYURETHANE FOAM" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 25:Walls 26" | object type "Walls 25:Walls 26" | names: "Walls 25:Walls 26:4517912" | material: "5/8" GYP. BD" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 35:Walls 26" | object type "Walls 35:Walls 26" | names: "Walls 35:Walls 26:4518029" | material: "2X6 DOUBLE STUD TOP PLATE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 26:Walls 26" | object type "Walls 26:Walls 26" | names: "Walls 26:Walls 26:4518158" | material: "BLOCKING - SIZE AS NEC." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 36:Walls 26" | object type "Walls 36:Walls 26" | names: "Walls 36:Walls 26:4518278" | material: "ROOF BATT. INSULATION (R-49) OVER 6 MIL VAPOR BARRIER" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 30:Walls 26" | object type "Walls 30:Walls 26" | names: "Walls 30:Walls 26:4520480" | material: "CURTAIN WALL W/ GLAZED ASSEMBLIES" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 40:Walls 26" | object type "Walls 40:Walls 26" | names: "Walls 40:Walls 26:4520976" | material: "3/4" CDX PLYWOOD" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 49:Walls 26" | object type "Walls 49:Walls 26" | names: "Walls 49:Walls 26:4523968" | material: "SEALANT (W/ BACKER ROD IF NECESSARY)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 50:Walls 26" | object type "Walls 50:Walls 26" | names: "Walls 50:Walls 26:4524940" | material: "EXPANDING POLYURETHANE FOAM" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 51:Walls 26" | object type "Walls 51:Walls 26" | names: "Walls 51:Walls 26:4525075" | material: "SEALANT (W/ BACKER ROD IF NECESSARY)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCBEAM | type IFCBEAMTYPE "061753 - Shop-Fabricated Wood Trusses - Generic1:24"" | object type "061753 - Shop-Fabricated Wood Trusses - Generic1:24"" | names: "061753 - Shop-Fabricated Wood Trusses - Generic1:24":4531829" | material: materials ("CUSTOM FLOOR TRUSS - SISTERED 2X4", "CUSTOM FLOOR TRUSS - SISTERED 2X4", "CUSTOM FLOOR TRUSS - SISTERED 2X4", "CUSTOM FLOOR TRUSS - SISTERED 2X4", "CUSTOM FLOOR TRUSS - SISTERED 2X4", "CUSTOM FLOOR TRUSS - SISTERED 2X4", "CUSTOM FLOOR TRUSS - SISTERED 2X4", "CUSTOM FLOOR TRUSS - SISTERED 2X4", "CUSTOM FLOOR TRUSS - SISTERED 2X4", "CUSTOM FLOOR TRUSS - SISTERED 2X4", "CUSTOM FLOOR TRUSS - SISTERED 2X4", "CUSTOM FLOOR TRUSS - SISTERED 2X4") | property sets: Pset_BeamCommon, Pset_ManufacturerTypeInformation, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfBeam
          1 x IFCWALL | type IFCWALLTYPE "Walls 88:Walls 26" | object type "Walls 88:Walls 26" | names: "Walls 88:Walls 26:4540279" | material: "60 MIL EPDM MEMBRANE OVER 3/4" CDX OR OSB" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 89:Walls 26" | object type "Walls 89:Walls 26" | names: "Walls 89:Walls 26:4540812" | material: "60 MIL EPDM MEMBRANE OVER 3/4" CDX OR OSB" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 90:Walls 26" | object type "Walls 90:Walls 26" | names: "Walls 90:Walls 26:4541221" | material: "THERMALLY MODIFIED WOOD (VENT TOP AND BOTTOM)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 95:Walls 95" | object type "Walls 95:Walls 95" | names: "Walls 95:Walls 95:4543350" | material: "STANDING SEAM METAL WITH VARYING WIDTHS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 96:Walls 96" | object type "Walls 96:Walls 96" | names: "Walls 96:Walls 96:4544207" | material: "PREFABRICATED ROOF SCISSOR TRUSS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 102:Walls 26" | object type "Walls 102:Walls 26" | names: "Walls 102:Walls 26:4547133" | material: "1/2" CDX PLYWOOD" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 105:Walls 26" | object type "Walls 105:Walls 26" | names: "Walls 105:Walls 26:4547947" | material: "ALUM. STOREFRONT W/ TEMPERED INSULATED GLAZING" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 107:Walls 26" | object type "Walls 107:Walls 26" | names: "Walls 107:Walls 26:4548189" | material: "LVL(s) - SIZE T.B.D." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 108:Walls 26" | object type "Walls 108:Walls 26" | names: "Walls 108:Walls 26:4548257" | material: "2X BLOCKING" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 109:Walls 26" | object type "Walls 109:Walls 26" | names: "Walls 109:Walls 26:4548306" | material: "5/8" GYP. BD @ CEILING" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 110:Walls 26" | object type "Walls 110:Walls 26" | names: "Walls 110:Walls 26:4548367" | material: "FILL ENTIRE CAVITY W/ CLOSED POLYURETHANE CELL FOAM(R-49MIN.)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 114:Walls 26" | object type "Walls 114:Walls 26" | names: "Walls 114:Walls 26:4550868" | material: "SEALANT (W/ BACKER ROD IF NECESSARY)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 115:Walls 26" | object type "Walls 115:Walls 26" | names: "Walls 115:Walls 26:4551167" | material: "SEALANT (W/ BACKER ROD IF NECESSARY)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 116:Walls 26" | object type "Walls 116:Walls 26" | names: "Walls 116:Walls 26:4551202" | material: "EXPANDING POLYURETHANE FOAM" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 119:Walls 26" | object type "Walls 119:Walls 26" | names: "Walls 119:Walls 26:4552563" | material: "LVL(s) - SIZE T.B.D." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 120:Walls 26" | object type "Walls 120:Walls 26" | names: "Walls 120:Walls 26:4552589" | material: "LVL(s) - SIZE T.B.D." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 121:Walls 26" | object type "Walls 121:Walls 26" | names: "Walls 121:Walls 26:4552997" | material: "5/8" GYP. BD" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 122:Walls 26" | object type "Walls 122:Walls 26" | names: "Walls 122:Walls 26:4553025" | material: "5/8" GYP. BD" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 137:Walls 26" | object type "Walls 137:Walls 26" | names: "Walls 137:Walls 26:4555142" | material: "TJI JOIST W/POLY ISO FOAM (ENTIRE CAVITY)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 138:Walls 26" | object type "Walls 138:Walls 26" | names: "Walls 138:Walls 26:4555224" | material: "TJI JOIST W/POLY ISO FOAM (ENTIRE CAVITY)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 140:Walls 26" | object type "Walls 140:Walls 26" | names: "Walls 140:Walls 26:4555316" | material: "5/8" GYP. BD @ CEILING" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 141:Walls 26" | object type "Walls 141:Walls 26" | names: "Walls 141:Walls 26:4555386" | material: "5/8" GYP. BD @ CEILING" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 154:Walls 26" | object type "Walls 154:Walls 26" | names: "Walls 154:Walls 26:4563886" | material: "5/8" GYP. BD" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 169:Walls 169" | object type "Walls 169:Walls 169" | names: "Walls 169:Walls 169:4571454" | material: "RAILING POST" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 170:Walls 170" | object type "Walls 170:Walls 170" | names: "Walls 170:Walls 170:4571627" | material: "WOOD RAILING (MAPLE, OR BIRCH) - W/ WALL RETURNS AT ENDS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 171:Walls 171" | object type "Walls 171:Walls 171" | names: "Walls 171:Walls 171:4571901" | material: "S.S. CABLE RAILING (3" O.C.)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 175:Walls 173" | object type "Walls 175:Walls 173" | names: "Walls 175:Walls 173:4573502" | material: "5/8" GYP. BD" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 183:Walls 183" | object type "Walls 183:Walls 183" | names: "Walls 183:Walls 183:4578917" | material: "LVL(s) - SIZE T.B.D." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 184:Walls 173" | object type "Walls 184:Walls 173" | names: "Walls 184:Walls 173:4578954" | material: "5/8" GYP. BD @ CEILING" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 185:Walls 185" | object type "Walls 185:Walls 185" | names: "Walls 185:Walls 185:4579223" | material: "TJI JOIST W/POLY ISO FOAM (ENTIRE CAVITY)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 190:Walls 190" | object type "Walls 190:Walls 190" | names: "Walls 190:Walls 190:4581242" | material: "1/2" CDX PLYWOOD" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 191:Walls 191" | object type "Walls 191:Walls 191" | names: "Walls 191:Walls 191:4581360" | material: "ALUM. STOREFRONT W/ TEMPERED INSULATED GLAZING" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 192:Walls 190" | object type "Walls 192:Walls 190" | names: "Walls 192:Walls 190:4581442" | material: "THERMALLY MODIFIED WOOD (VENT TOP AND BOTTOM)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 193:Walls 193" | object type "Walls 193:Walls 193" | names: "Walls 193:Walls 193:4581688" | material: "TJI - SEE STRUCT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 199:Walls 194" | object type "Walls 199:Walls 194" | names: "Walls 199:Walls 194:4582300" | material: "5/8" GYP. BD @ CEILING" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 200:Walls 194" | object type "Walls 200:Walls 194" | names: "Walls 200:Walls 194:4582345" | material: "FILL ENTIRE CAVITY W/ CLOSED POLYURETHANE CELL FOAM(R-49MIN.)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 201:Walls 201" | object type "Walls 201:Walls 201" | names: "Walls 201:Walls 201:4583247" | material: "BUILDING WRAP(AT WOOD SIDING)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 204:Walls 204" | object type "Walls 204:Walls 204" | names: "Walls 204:Walls 204:4585125" | material: "SEALANT (W/ BACKER ROD IF NECESSARY)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 205:Walls 205" | object type "Walls 205:Walls 205" | names: "Walls 205:Walls 205:4585316" | material: "EXPANDING POLYURETHANE FOAM" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 206:Walls 204" | object type "Walls 206:Walls 204" | names: "Walls 206:Walls 204:4585331" | material: "SEALANT (W/ BACKER ROD IF NECESSARY)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 207:Walls 207" | object type "Walls 207:Walls 207" | names: "Walls 207:Walls 207:4585723" | material: "METAL FLASHING (MATCH SS)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 213:Walls 198" | object type "Walls 213:Walls 198" | names: "Walls 213:Walls 198:4588394" | material: "2X BLOCKING" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 214:Walls 198" | object type "Walls 214:Walls 198" | names: "Walls 214:Walls 198:4588531" | material: "2X BLOCKING" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 215:Walls 190" | object type "Walls 215:Walls 190" | names: "Walls 215:Walls 190:4588560" | material: "2X BLOCKING" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 217:Walls 190" | object type "Walls 217:Walls 190" | names: "Walls 217:Walls 190:4588978" | material: "1/2" CORE-E-VENT BUG SCREEN" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 197:Walls 190" | object type "Walls 197:Walls 190" | names: "Walls 197:Walls 190:4589991" | material: "1/2" CORE-E-VENT VENTED VERTICAL FURRING STRIPS 16" O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 218:Walls 26" | object type "Walls 218:Walls 26" | names: "Walls 218:Walls 26:4590111" | material: "2X BLOCKING" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 219:Walls 26" | object type "Walls 219:Walls 26" | names: "Walls 219:Walls 26:4590241" | material: "SEALANT (W/ BACKER ROD IF NECESSARY)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 118:Walls 26" | object type "Walls 118:Walls 26" | names: "Walls 118:Walls 26:4591350" | material: "METAL FLASHING (MATCH SS)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 222:Walls 26" | object type "Walls 222:Walls 26" | names: "Walls 222:Walls 26:4591904" | material: "1/2" CORE-E-VENT BUG SCREEN" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 223:Walls 26" | object type "Walls 223:Walls 26" | names: "Walls 223:Walls 26:4592124" | material: "1/2" CORE-E-VENT VENTED VERTICAL FURRING STRIPS 16" O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "060523 - W_P_C - Fastenings - Generic:1/2" x 3"" | object type "060523 - W_P_C - Fastenings - Generic:1/2" x 3"" | names: "060523 - W_P_C - Fastenings - Generic:1/2" x 3":4619225" | material: materials ("<Unnamed>", "<Unnamed>", "1/2" DIA. A325 BOLT AT EACH PURLIN", "1/2" DIA. A325 BOLT AT EACH PURLIN") | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ProvisionForVoid
          1 x IFCWALL | type IFCWALLTYPE "Walls 253:Walls 26" | object type "Walls 253:Walls 26" | names: "Walls 253:Walls 26:4620724" | material: "ACOUSTICAL MAT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 254:Walls 26" | object type "Walls 254:Walls 26" | names: "Walls 254:Walls 26:4620811" | material: "LVT - SPEC TBD" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "060523 - W_P_C - Fastenings - Generic:Lag - .7500 - 3/4" | object type "060523 - W_P_C - Fastenings - Generic:Lag - .7500 - 3/4" | names: "060523 - W_P_C - Fastenings - Generic:Lag - .7500 - 3/4:4629918" | material: materials ("AT SILL - FASTENER AT 24" O.C.", "<Unnamed>") | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ProvisionForVoid
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "060523 - W_P_C - Fastenings - Generic:Lag - .7500 - 3/4" | object type "060523 - W_P_C - Fastenings - Generic:Lag - .7500 - 3/4" | names: "060523 - W_P_C - Fastenings - Generic:Lag - .7500 - 3/4:4632966" | material: materials ("AT SILL - FASTENER AT 24" O.C.", "<Unnamed>") | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ProvisionForVoid
          1 x IFCWALL | type IFCWALLTYPE "Walls 283:Walls 26" | object type "Walls 283:Walls 26" | names: "Walls 283:Walls 26:4635156" | material: "2X WOOD STUD" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 284:Walls 26" | object type "Walls 284:Walls 26" | names: "Walls 284:Walls 26:4635288" | material: "5/8" GYP. BD" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "060523 - W_P_C - Fastenings - Generic:Screw - .220 - #12" | object type "060523 - W_P_C - Fastenings - Generic:Screw - .220 - #12" | names: "060523 - W_P_C - Fastenings - Generic:Screw - .220 - #12:4635709" | material: "AT SILL - FASTENER AT 24" O.C." | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ProvisionForVoid
          1 x IFCWALL | type IFCWALLTYPE "Walls 103:Walls 26" | object type "Walls 103:Walls 26" | names: "Walls 103:Walls 26:4641658" | material: "BUILDING WRAP" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 287:Walls 26" | object type "Walls 287:Walls 26" | names: "Walls 287:Walls 26:4646270" | material: "ALUM. STOREFRONT W/ TEMPERED INSULATED GLAZING" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 289:Walls 26" | object type "Walls 289:Walls 26" | names: "Walls 289:Walls 26:4647175" | material: "2X BLOCKING" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 292:Walls 26" | object type "Walls 292:Walls 26" | names: "Walls 292:Walls 26:4647467" | material: "EXPANDING POLYURETHANE FOAM" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 298:Walls 26" | object type "Walls 298:Walls 26" | names: "Walls 298:Walls 26:4648461" | material: "SELF ADHERED MEMBRANE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 299:Walls 26" | object type "Walls 299:Walls 26" | names: "Walls 299:Walls 26:4648660" | material: "METAL FLASHING (MATCH SS)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 301:Walls 26" | object type "Walls 301:Walls 26" | names: "Walls 301:Walls 26:4649470" | material: "SEALANT (W/ BACKER ROD IF NECESSARY)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "060523 - W_P_C - Fastenings - Generic:Thru-Bolt - .6250 - 5/8" | object type "060523 - W_P_C - Fastenings - Generic:Thru-Bolt - .6250 - 5/8" | names: "060523 - W_P_C - Fastenings - Generic:Thru-Bolt - .6250 - 5/8:4656071" | material: materials ("<Unnamed>", "<Unnamed>", "AT SILL - FASTENER AT 24" O.C.", "AT SILL - FASTENER AT 24" O.C.", "AT SILL - FASTENER AT 24" O.C.") | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ProvisionForVoid
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "060523 - W_P_C - Fastenings - Generic:Thru-Bolt - .5000 - 1/2" | object type "060523 - W_P_C - Fastenings - Generic:Thru-Bolt - .5000 - 1/2" | names: "060523 - W_P_C - Fastenings - Generic:Thru-Bolt - .5000 - 1/2:4657463" | material: materials ("<Unnamed>", "<Unnamed>", "AT SILL - FASTENER AT 24" O.C.", "AT SILL - FASTENER AT 24" O.C.", "AT SILL - FASTENER AT 24" O.C.") | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ProvisionForVoid
          1 x IFCWALL | type IFCWALLTYPE "Walls 38:Walls 26" | object type "Walls 38:Walls 26" | names: "Walls 38:Walls 26:4659557" | material: "SEALANT (W/ BACKER ROD IF NECESSARY)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          2 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "060523 - W_P_C - Fastenings - Generic:Thru-Bolt - .6250 - 5/8" | object type "060523 - W_P_C - Fastenings - Generic:Thru-Bolt - .6250 - 5/8" | names: "060523 - W_P_C - Fastenings - Generic:Thru-Bolt - .6250 - 5/8:4672578", "060523 - W_P_C - Fastenings - Generic:Thru-Bolt - .6250 - 5/8:4676112" | material: materials ("<Unnamed>", "<Unnamed>", "AT SILL - FASTENER AT 24" O.C.", "AT SILL - FASTENER AT 24" O.C.", "AT SILL - FASTENER AT 24" O.C."); materials ("<Unnamed>", "AT SILL - FASTENER AT 24" O.C.") | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ProvisionForVoid
          2 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "060523 - W_P_C - Fastenings - Generic:Thru-Bolt - .6250 - 5/8" | object type "060523 - W_P_C - Fastenings - Generic:Thru-Bolt - .6250 - 5/8" | names: "060523 - W_P_C - Fastenings - Generic:Thru-Bolt - .6250 - 5/8:4673212", "060523 - W_P_C - Fastenings - Generic:Thru-Bolt - .6250 - 5/8:4675933" | material: materials ("<Unnamed>", "<Unnamed>", "AT SILL - FASTENER AT 24" O.C.", "AT SILL - FASTENER AT 24" O.C.", "AT SILL - FASTENER AT 24" O.C."); materials ("<Unnamed>", "AT SILL - FASTENER AT 24" O.C.") | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ProvisionForVoid
          2 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "060523 - W_P_C - Fastenings - Generic:Thru-Bolt - .5000 - 1/2" | object type "060523 - W_P_C - Fastenings - Generic:Thru-Bolt - .5000 - 1/2" | names: "060523 - W_P_C - Fastenings - Generic:Thru-Bolt - .5000 - 1/2:4673234", "060523 - W_P_C - Fastenings - Generic:Thru-Bolt - .5000 - 1/2:4675249" | material: materials ("<Unnamed>", "<Unnamed>", "AT SILL - FASTENER AT 24" O.C.", "AT SILL - FASTENER AT 24" O.C.", "AT SILL - FASTENER AT 24" O.C."); materials ("<Unnamed>", "AT SILL - FASTENER AT 24" O.C.") | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ProvisionForVoid
          4 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "060523 - W_P_C - Fastenings - Generic:Thru-Bolt - .5000 - 1/2" | object type "060523 - W_P_C - Fastenings - Generic:Thru-Bolt - .5000 - 1/2" | names: "060523 - W_P_C - Fastenings - Generic:Thru-Bolt - .5000 - 1/2:4673374", "060523 - W_P_C - Fastenings - Generic:Thru-Bolt - .5000 - 1/2:4673393", "060523 - W_P_C - Fastenings - Generic:Thru-Bolt - .5000 - 1/2:4675251" (+1 more) | material: materials ("<Unnamed>", "<Unnamed>", "AT SILL - FASTENER AT 24" O.C.", "AT SILL - FASTENER AT 24" O.C.", "AT SILL - FASTENER AT 24" O.C."); materials ("<Unnamed>", "AT SILL - FASTENER AT 24" O.C.") | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ProvisionForVoid
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "060523 - W_P_C - Fastenings - Generic:Lag - .7500 - 3/4" | object type "060523 - W_P_C - Fastenings - Generic:Lag - .7500 - 3/4" | names: "060523 - W_P_C - Fastenings - Generic:Lag - .7500 - 3/4:4673831" | material: materials ("AT SILL - FASTENER AT 24" O.C.", "<Unnamed>") | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ProvisionForVoid
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "060523 - W_P_C - Fastenings - Generic:Screw - .220 - #12" | object type "060523 - W_P_C - Fastenings - Generic:Screw - .220 - #12" | names: "060523 - W_P_C - Fastenings - Generic:Screw - .220 - #12:4674140" | material: "AT SILL - FASTENER AT 24" O.C." | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ProvisionForVoid
          1 x IFCWALL | type IFCWALLTYPE "Walls 319:Walls 26" | object type "Walls 319:Walls 26" | names: "Walls 319:Walls 26:4675533" | material: "1X4 WOOD TRIM" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 321:Walls 26" | object type "Walls 321:Walls 26" | names: "Walls 321:Walls 26:4677127" | material: "J BEAD DRYWALL TRIM" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
      IFCBUILDINGSTOREY "FLAT ROOF" | long name "FLAT ROOF" | object type "Level:Project Base Point" | elevation 21.1041666666667
        contains 57 elements
          1 x IFCWALL | type IFCWALLTYPE "Walls 18:Walls 26" | object type "Walls 18:Walls 26" | names: "Walls 18:Walls 26:4511666" | material: "3/4" CDX OR OSB" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 21:Walls 26" | object type "Walls 21:Walls 26" | names: "Walls 21:Walls 26:4512264" | material: "GALV. STANDING SEAM METAL ROOF" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 24:Walls 26" | object type "Walls 24:Walls 26" | names: "Walls 24:Walls 26:4512840" | material: "GALV. STANDING SEAM METAL ROOF" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 27:Walls 26" | object type "Walls 27:Walls 26" | names: "Walls 27:Walls 26:4513000" | material: "GALV. STANDING SEAM METAL ROOF" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 28:Walls 26" | object type "Walls 28:Walls 26" | names: "Walls 28:Walls 26:4513287" | material: "30LB ROOFING FELT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 29:Walls 26" | object type "Walls 29:Walls 26" | names: "Walls 29:Walls 26:4513562" | material: "GALV. CUSTOM GUTTER" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 32:Walls 26" | object type "Walls 32:Walls 26" | names: "Walls 32:Walls 26:4514458" | material: "GALV. STANDING SEAM METAL ROOF" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 11:Walls 26" | object type "Walls 11:Walls 26" | names: "Walls 11:Walls 26:4515833" | material: "(2) 3/4" COR-A-VENT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 17:Walls 26" | object type "Walls 17:Walls 26" | names: "Walls 17:Walls 26:4515910" | material: "(2) 3/4" COR-A-VENT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 22:Walls 26" | object type "Walls 22:Walls 26" | names: "Walls 22:Walls 26:4516929" | material: "GUTTER BRACKET" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 37:Walls 26" | object type "Walls 37:Walls 26" | names: "Walls 37:Walls 26:4519602" | material: "INSULATION BAFFLE BETWEEN TRUSSES" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 104:Walls 26" | object type "Walls 104:Walls 26" | names: "Walls 104:Walls 26:4548017" | material: "1/2" CDX PLYWOOD" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 106:Walls 26" | object type "Walls 106:Walls 26" | names: "Walls 106:Walls 26:4548118" | material: "3/4" CDX PLYWOOD" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 112:Walls 26" | object type "Walls 112:Walls 26" | names: "Walls 112:Walls 26:4548455" | material: "METAL COPING - MATCH SS ROOFING" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 113:Walls 26" | object type "Walls 113:Walls 26" | names: "Walls 113:Walls 26:4549155" | material: "EPS RIGID INSULATION (1/4"/12" MIN. SLOPE TO DRAINS)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 111:Walls 26" | object type "Walls 111:Walls 26" | names: "Walls 111:Walls 26:4549335" | material: "SELF ADHERED MEMBRANE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 124:Walls 26" | object type "Walls 124:Walls 26" | names: "Walls 124:Walls 26:4553102" | material: "2X BLOCKING" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 129:Walls 26" | object type "Walls 129:Walls 26" | names: "Walls 129:Walls 26:4554351" | material: "2X BLOCKING" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 130:Walls 26" | object type "Walls 130:Walls 26" | names: "Walls 130:Walls 26:4554523" | material: "2X BLOCKING" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 133:Walls 26" | object type "Walls 133:Walls 26" | names: "Walls 133:Walls 26:4554685" | material: "3/4" CDX PLYWOOD" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 134:Walls 26" | object type "Walls 134:Walls 26" | names: "Walls 134:Walls 26:4554787" | material: "1/2" CDX PLYWOOD" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 135:Walls 26" | object type "Walls 135:Walls 26" | names: "Walls 135:Walls 26:4554982" | material: "2X6s W/ 2" POLY ISO FOAM & 3.5" OF BLOWN-IN CELLULOSE INSULATION" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 136:Walls 26" | object type "Walls 136:Walls 26" | names: "Walls 136:Walls 26:4555074" | material: "EPS RIGID INSULATION (1/4"/12" MIN. SLOPE TO DRAINS)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 139:Walls 26" | object type "Walls 139:Walls 26" | names: "Walls 139:Walls 26:4555279" | material: "2X6s W/ 2" POLY ISO FOAM & 3.5" OF BLOWN-IN CELLULOSE INSULATION" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 142:Walls 26" | object type "Walls 142:Walls 26" | names: "Walls 142:Walls 26:4555442" | material: "1/2" CDX PLYWOOD" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 143:Walls 26" | object type "Walls 143:Walls 26" | names: "Walls 143:Walls 26:4555487" | material: "METAL FLASHING (MATCH SS)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 144:Walls 26" | object type "Walls 144:Walls 26" | names: "Walls 144:Walls 26:4556956" | material: "LINEAR SKYLIGHT - INSULATED TEMPERED GLAZING" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 145:Walls 26" | object type "Walls 145:Walls 26" | names: "Walls 145:Walls 26:4559582" | material: "60 MIL EPDM MEMBRANE (1/4"/12" MIN. SLOPE)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 147:Walls 26" | object type "Walls 147:Walls 26" | names: "Walls 147:Walls 26:4560115" | material: "SEALANT (W/ BACKER ROD IF NECESSARY)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 148:Walls 26" | object type "Walls 148:Walls 26" | names: "Walls 148:Walls 26:4560560" | material: "EXPANDING POLYURETHANE FOAM" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 149:Walls 26" | object type "Walls 149:Walls 26" | names: "Walls 149:Walls 26:4561939" | material: "METAL FLASHING (MATCH SS)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 150:Walls 26" | object type "Walls 150:Walls 26" | names: "Walls 150:Walls 26:4563084" | material: "60 MIL EPDM MEMBRANE (1/4"/12" MIN. SLOPE)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 152:Walls 26" | object type "Walls 152:Walls 26" | names: "Walls 152:Walls 26:4563566" | material: "3/4" CDX PLYWOOD" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 153:Walls 26" | object type "Walls 153:Walls 26" | names: "Walls 153:Walls 26:4563634" | material: "EPS RIGID INSULATION (1/4"/12" MIN. SLOPE TO DRAINS)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 173:Walls 173" | object type "Walls 173:Walls 173" | names: "Walls 173:Walls 173:4573262" | material: "1/2" CDX PLYWOOD" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 174:Walls 173" | object type "Walls 174:Walls 173" | names: "Walls 174:Walls 173:4573330" | material: "2X6s W/ 2" POLY ISO FOAM & 3.5" OF BLOWN-IN CELLULOSE INSULATION" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 176:Walls 176" | object type "Walls 176:Walls 176" | names: "Walls 176:Walls 176:4574004" | material: "2X BLOCKING" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 177:Walls 177" | object type "Walls 177:Walls 177" | names: "Walls 177:Walls 177:4575253" | material: "SKYLIGHTS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 178:Walls 178" | object type "Walls 178:Walls 178" | names: "Walls 178:Walls 178:4576521" | material: "METAL FLASHING (MATCH SS)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 179:Walls 179" | object type "Walls 179:Walls 179" | names: "Walls 179:Walls 179:4577746" | material: "BUILDING WRAP" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 180:Walls 180" | object type "Walls 180:Walls 180" | names: "Walls 180:Walls 180:4578067" | material: "60 MIL EPDM MEMBRANE (1/4"/12" MIN. SLOPE)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 181:Walls 180" | object type "Walls 181:Walls 180" | names: "Walls 181:Walls 180:4578299" | material: "EPS RIGID INSULATION (1/4"/12" MIN. SLOPE TO DRAINS)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 182:Walls 180" | object type "Walls 182:Walls 180" | names: "Walls 182:Walls 180:4578600" | material: "3/4" CDX PLYWOOD" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 186:Walls 186" | object type "Walls 186:Walls 186" | names: "Walls 186:Walls 186:4579996" | material: "SEALANT (W/ BACKER ROD IF NECESSARY)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 187:Walls 187" | object type "Walls 187:Walls 187" | names: "Walls 187:Walls 187:4580674" | material: "5/8" GYP. BD" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 189:Walls 189" | object type "Walls 189:Walls 189" | names: "Walls 189:Walls 189:4581009" | material: "EXPANDING POLYURETHANE FOAM" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 194:Walls 194" | object type "Walls 194:Walls 194" | names: "Walls 194:Walls 194:4581781" | material: "3/4" CDX PLYWOOD" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 195:Walls 195" | object type "Walls 195:Walls 195" | names: "Walls 195:Walls 195:4581849" | material: "1/2" CDX PLYWOOD" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 196:Walls 196" | object type "Walls 196:Walls 196" | names: "Walls 196:Walls 196:4582048" | material: "EPS RIGID INSULATION (1/4"/12" MIN. SLOPE TO DRAINS)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 198:Walls 198" | object type "Walls 198:Walls 198" | names: "Walls 198:Walls 198:4582257" | material: "2X BLOCKING" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 203:Walls 203" | object type "Walls 203:Walls 203" | names: "Walls 203:Walls 203:4584080" | material: "METAL COPING - MATCH SS ROOFING" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 216:Walls 190" | object type "Walls 216:Walls 190" | names: "Walls 216:Walls 190:4588790" | material: "1/2" CORE-E-VENT BUG SCREEN" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 220:Walls 26" | object type "Walls 220:Walls 26" | names: "Walls 220:Walls 26:4590324" | material: "2X BLOCKING" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 221:Walls 26" | object type "Walls 221:Walls 26" | names: "Walls 221:Walls 26:4590349" | material: "2X BLOCKING" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 224:Walls 26" | object type "Walls 224:Walls 26" | names: "Walls 224:Walls 26:4592390" | material: "60 MIL EPDM MEMBRANE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 286:Walls 201" | object type "Walls 286:Walls 201" | names: "Walls 286:Walls 201:4642479" | material: "60 MIL EPDM MEMBRANE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 202:Walls 201" | object type "Walls 202:Walls 201" | names: "Walls 202:Walls 201:4642801" | material: "METAL FLASHING (MATCH SS)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
      IFCBUILDINGSTOREY "ATTIC" | long name "ATTIC" | object type "Level:Project Base Point" | elevation 22.3229166666667
        contains 15 elements
          1 x IFCWALL | type IFCWALLTYPE "Walls 94:Walls 94" | object type "Walls 94:Walls 94" | names: "Walls 94:Walls 94:4542696" | material: "STANDING SEAM METAL WITH VARYING WIDTHS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 99:Walls 99" | object type "Walls 99:Walls 99" | names: "Walls 99:Walls 99:4544997" | material: "3/4" CDX PLYWOOD" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 100:Walls 100" | object type "Walls 100:Walls 100" | names: "Walls 100:Walls 100:4545920" | material: "60 MIL EPDM MEMBRANE OVER 3/4" CDX OR OSB" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 101:Walls 101" | object type "Walls 101:Walls 101" | names: "Walls 101:Walls 101:4546464" | material: "2X6s W/ 2" POLY ISO FOAM & 3.5" OF BLOWN-IN CELLULOSE INSULATION" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 128:Walls 26" | object type "Walls 128:Walls 26" | names: "Walls 128:Walls 26:4554034" | material: "INSULATED GLAZING" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 131:Walls 26" | object type "Walls 131:Walls 26" | names: "Walls 131:Walls 26:4554555" | material: "2X BLOCKING" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 132:Walls 26" | object type "Walls 132:Walls 26" | names: "Walls 132:Walls 26:4554607" | material: "2X BLOCKING" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 146:Walls 26" | object type "Walls 146:Walls 26" | names: "Walls 146:Walls 26:4557915" | material: "LINEAR SKYLIGHT - INSULATED TEMPERED GLAZING" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 151:Walls 26" | object type "Walls 151:Walls 26" | names: "Walls 151:Walls 26:4563414" | material: "EXPANDING POLYURETHANE FOAM" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 155:Walls 155" | object type "Walls 155:Walls 155" | names: "Walls 155:Walls 155:4564557" | material: "TJI - SEE STRUCT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 156:Walls 156" | object type "Walls 156:Walls 156" | names: "Walls 156:Walls 156:4565023" | material: "3/4" CDX PLYWOOD" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 157:Walls 157" | object type "Walls 157:Walls 157" | names: "Walls 157:Walls 157:4565312" | material: "BUILDING WRAP" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 158:Walls 158" | object type "Walls 158:Walls 158" | names: "Walls 158:Walls 158:4565681" | material: "1/2" CDX PLYWOOD" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 159:Walls 159" | object type "Walls 159:Walls 159" | names: "Walls 159:Walls 159:4566041" | material: "STANDING SEAM METAL WITH VARYING WIDTHS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 188:Walls 188" | object type "Walls 188:Walls 188" | names: "Walls 188:Walls 188:4580936" | material: "SILL PLATE GASKET" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon

Types
  IFCWALLTYPE "Walls 39:Walls 26" | 1 occurrence | material: "1/2" CDX PLYWOOD" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 43:Walls 26" | 1 occurrence | material: "1/2" CDX PLYWOOD" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 42:Walls 26" | 1 occurrence | material: "THERMALLY MODIFIED WOOD (VENT TOP AND BOTTOM)" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 48:Walls 26" | 1 occurrence | material: "BUILDING WRAP" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 52:Walls 26" | 1 occurrence | material: "STEEL I BEAM JOISTS 24" O.C. - WEB(10") - FLANGE (2.75") - GAUGE (.125" ESTIMATED)" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 53:Walls 26" | 1 occurrence | material: "STEEL C CHANNEL HDG PRE-DRILLED" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 54:Walls 26" | 1 occurrence | material: "1/2" CDX PLYWOOD" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 55:Walls 26" | 1 occurrence | material: "2X6 DOUBLE STUD TOP PLATE" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 57:Walls 26" | 1 occurrence | material: "2X6 DOUBLE STUD TOP PLATE" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 58:Walls 26" | 1 occurrence | material: "2X6 DOUBLE STUD TOP PLATE" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 59:Walls 26" | 1 occurrence | material: "2X6 DOUBLE STUD TOP PLATE" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 60:Walls 26" | 1 occurrence | material: "METAL FLASHING (MATCH SS)" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 61:Walls 26" | 1 occurrence | material: "BUILDING WRAP" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 62:Walls 26" | 1 occurrence | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 63:Walls 26" | 1 occurrence | material: "CONCRETE WALL - (PATTERNED CONCRETE W/ VINYL FORMLINERS)" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 64:Walls 26" | 1 occurrence | material: "5/8" GYP. BD" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 65:Walls 26" | 1 occurrence | material: "5/8" GYP. BD" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 66:Walls 26" | 1 occurrence | material: "THERMALLY MODIFIED WOOD (VENT TOP AND BOTTOM)" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 67:Walls 26" | 1 occurrence | material: "AWNING WINDOW W/ INSULATED GLAZING" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 68:Walls 26" | 1 occurrence | material: "FILL CAVITY WITH BATT INSULATION" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 69:Walls 26" | 1 occurrence | material: "2" OF CLOSED POLYURETHANE CELL FOAM" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 70:Walls 26" | 1 occurrence | material: "2" OF CLOSED POLYURETHANE CELL FOAM" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 71:Walls 26" | 1 occurrence | material: "METAL FLASHING (MATCH SS)" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 72:Walls 26" | 1 occurrence | material: "SEALANT (W/ BACKER ROD IF NECESSARY)" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 74:Walls 26" | 1 occurrence | material: "2X6 DOUBLE STUD TOP PLATE" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 75:Walls 26" | 1 occurrence | material: "2X6 DOUBLE STUD TOP PLATE" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 76:Walls 26" | 1 occurrence | material: "2X BLOCKING" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 78:Walls 26" | 1 occurrence | material: "EXPANDING POLYURETHANE FOAM" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 79:Walls 26" | 1 occurrence | material: "EXPANDING POLYURETHANE FOAM" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 81:Walls 26" | 1 occurrence | material: "1/2" CDX PLYWOOD" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 82:Walls 26" | 1 occurrence | material: "1/2" CDX PLYWOOD" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 83:Walls 83" | 1 occurrence | material: "STANDING SEAM METAL WITH VARYING WIDTHS" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 80:Walls 26" | 1 occurrence | material: "LVL(s) - SIZE T.B.D." | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 84:Walls 26" | 1 occurrence | material: "2X WOOD STUDS W/ RIGID INSULATION" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 85:Walls 26" | 1 occurrence | material: "60 MIL EPDM MEMBRANE OVER 3/4" CDX OR OSB" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 86:Walls 26" | 1 occurrence | material: "60 MIL EPDM MEMBRANE OVER 3/4" CDX OR OSB" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 87:Walls 26" | 1 occurrence | material: "1/2" CDX PLYWOOD" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 91:Walls 26" | 1 occurrence | material: "TJI - SEE STRUCT" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 92:Walls 26" | 1 occurrence | material: "1/2" CDX PLYWOOD" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 93:Walls 26" | 1 occurrence | material: "2X WOOD STUDS W/ RIGID INSULATION" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 117:Walls 26" | 1 occurrence | material: "THERMALLY MODIFIED WOOD (VENT TOP AND BOTTOM)" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 162:Walls 162" | 1 occurrence | material: "TJI - SEE STRUCT" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 163:Walls 162" | 1 occurrence | material: "2X BLOCKING" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 164:Walls 164" | 1 occurrence | material: "THERMALLY MODIFIED DECKING" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 165:Walls 164" | 1 occurrence | material: "3/4" CDX PLYWOOD" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 166:Walls 164" | 1 occurrence | material: "LVL(s) - SIZE T.B.D." | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 167:Walls 164" | 1 occurrence | material: "1/2" CDX PLYWOOD" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 209:Walls 208" | 1 occurrence | material: "2X WOOD STUDS W/ 3" POLY ISO FOAM (NON-STRUCTURAL STUDS)" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 210:Walls 208" | 1 occurrence | material: "5/8" GYP. BD" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 212:Walls 212" | 1 occurrence | material: "CRIPPLE STUD OR CLIP ANGLE" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 225:Walls 26" | 1 occurrence | material: "2X BLOCKING" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 226:Walls 26" | 1 occurrence | material: "2X BLOCKING" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 227:Walls 26" | 1 occurrence | material: "3/4" CDX PLYWOOD" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 228:Walls 26" | 1 occurrence | material: "1/2" CDX PLYWOOD" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 229:Walls 26" | 1 occurrence | material: "METAL FLASHING (MATCH SS)" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 230:Walls 26" | 1 occurrence | material: "2X BLOCKING" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 231:Walls 26" | 1 occurrence | material: "2X BLOCKING" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 73:Walls 26" | 1 occurrence | material: "SEALANT (W/ BACKER ROD IF NECESSARY)" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 77:Walls 26" | 1 occurrence | material: "FILL REMAINING CAVITY WITH BLOWN-IN CELLULOSE INSULATION" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 232:Walls 26" | 1 occurrence | material: "2X BLOCKING" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 233:Walls 26" | 1 occurrence | material: "2X BLOCKING" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 234:Walls 26" | 1 occurrence | material: "2X BLOCKING" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 235:Walls 26" | 1 occurrence | material: "2X BLOCKING" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 236:Walls 236" | 1 occurrence | material: "EXPANDING POLYURETHANE FOAM" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 237:Walls 236" | 1 occurrence | material: "EXPANDING POLYURETHANE FOAM" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 238:Walls 238" | 1 occurrence | material: "SEALANT (W/ BACKER ROD IF NECESSARY)" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 239:Walls 238" | 1 occurrence | material: "SEALANT (W/ BACKER ROD IF NECESSARY)" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 241:Walls 26" | 1 occurrence | material: "SEALANT (W/ BACKER ROD IF NECESSARY)" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 240:Walls 164" | 1 occurrence | material: "2X BLOCKING" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 243:Walls 164" | 1 occurrence | material: "BUILDING WRAP" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 172:Walls 162" | 1 occurrence | material: "TJI - SEE STRUCT" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 242:Walls 164" | 1 occurrence | material: "2X BLOCKING" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 168:Walls 164" | 1 occurrence | material: "STANDING SEAM METAL WITH VARYING WIDTHS" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 244:Walls 164" | 1 occurrence | material: "60 MIL EPDM MEMBRANE" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 160:Walls 164" | 1 occurrence | material: "METAL FLASHING (MATCH SS)" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 45:Walls 26" | 1 occurrence | material: "PRE-ENGINEERED TRUSS @ 24" O.C." | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 46:Walls 26" | 1 occurrence | material: "GUSSET PLATE" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 247:Walls 26" | 1 occurrence | material: "2X BLOCKING" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 47:Walls 26" | 1 occurrence | material: "SELF ADHERED MEMBRANE - UNDER GUTTER AND ROOF FELT" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 248:Walls 26" | 1 occurrence | material: "12 GA. METAL FLASHING (MATCH SS)" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 251:Walls 26" | 1 occurrence | material: "1/2" CORE-E-VENT VENTED VERTICAL FURRING STRIPS 16" O.C." | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 252:Walls 26" | 1 occurrence | material: "BLOWN-IN INSULATION IN ENTIRE CAVITY" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 256:Walls 26" | 1 occurrence | material: "BUILDING WRAP" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 258:Walls 26" | 1 occurrence | material: "12 GA. METAL FLASHING (MATCH SS)" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 259:Walls 26" | 1 occurrence | material: "12 GA. METAL FLASHING (MATCH SS)" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 249:Walls 26" | 1 occurrence | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 261:Walls 26" | 1 occurrence | material: "2X BLOCKING" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 245:Walls 26" | 1 occurrence | material: "EXPANDING POLYURETHANE FOAM" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 260:Walls 26" | 1 occurrence | material: "1/2" CORE-E-VENT BUG SCREEN" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 262:Walls 26" | 1 occurrence | material: "STANDING SEAM METAL WITH VARYING WIDTHS" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 263:Walls 26" | 1 occurrence | material: "1/2" CORE-E-VENT VENTED VERTICAL FURRING STRIPS 16" O.C." | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 264:Walls 26" | 1 occurrence | material: "1/2" CORE-E-VENT BUG SCREEN" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 257:Walls 26" | 1 occurrence | material: "2X BLOCKING" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 265:Walls 26" | 1 occurrence | material: "GUSSET PLATE" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 250:Walls 26" | 1 occurrence | material: "LVL RIM BOARD - SEE STRUCT. DWGS" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 161:Walls 26" | 1 occurrence | material: "2X BLOCKING" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 267:Walls 26" | 1 occurrence | material: "2X BLOCKING" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 268:Walls 26" | 1 occurrence | material: "2X BLOCKING" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 269:Walls 26" | 1 occurrence | material: "2X BLOCKING" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 270:Walls 26" | 1 occurrence | material: "STEEL - SIZE TBD - PAINTED" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 271:Walls 26" | 1 occurrence | material: "2X WOOD STUD" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 266:Walls 26" | 1 occurrence | material: "LVL RIM BOARD(1 1/4") - SEE STRUCT. DWGS(1)" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 272:Walls 26" | 1 occurrence | material: "2X BLOCKING" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 273:Walls 26" | 1 occurrence | material: "2X BLOCKING" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 274:Walls 26" | 1 occurrence | material: "2X BLOCKING" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 275:Walls 26" | 1 occurrence | material: "2X BLOCKING" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 276:Walls 26" | 1 occurrence | material: "2X BLOCKING" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 277:Walls 26" | 1 occurrence | material: "1/2" CDX PLYWOOD" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 278:Walls 26" | 1 occurrence | material: "1/2" CDX PLYWOOD" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 279:Walls 26" | 1 occurrence | material: "2X WOOD STUD" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 281:Walls 26" | 1 occurrence | material: "EXPANDING POLYURETHANE FOAM" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 282:Walls 26" | 1 occurrence | material: "TREATED 2X10's (NO. 1 GRADE) - STAINED - 10" O.C." | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 285:Walls 26" | 1 occurrence | material: "STEEL I BEAM JOISTS 24" O.C. - WEB(10") - FLANGE (2.75") - GAUGE (.125" ESTIMATED)" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 288:Walls 26" | 1 occurrence | material: "1/2" CDX PLYWOOD" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 293:Walls 26" | 1 occurrence | material: "LVL(s) - SEE STRUCT. DWGS" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 294:Walls 26" | 1 occurrence | material: "2X6s W/ 2" POLY ISO FOAM & 3.5" OF BLOWN-IN CELLULOSE INSULATION" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 295:Walls 26" | 1 occurrence | material: "5/8" GYP. BD" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 296:Walls 26" | 1 occurrence | material: "1/2" CORE-E-VENT BUG SCREEN" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 297:Walls 26" | 1 occurrence | material: "BUILDING WRAP" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 300:Walls 26" | 1 occurrence | material: "1/2" CORE-E-VENT VENTED VERTICAL FURRING STRIPS 16" O.C." | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 302:Walls 26" | 1 occurrence | material: "ALUM. STOREFRONT W/ TEMPERED INSULATED GLAZING" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 303:Walls 26" | 1 occurrence | material: "SEALANT (W/ BACKER ROD IF NECESSARY)" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 304:Walls 26" | 1 occurrence | material: "SEALANT (W/ BACKER ROD IF NECESSARY)" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 305:Walls 26" | 1 occurrence | material: "EXPANDING POLYURETHANE FOAM" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 306:Walls 26" | 1 occurrence | material: "METAL FLASHING (MATCH SS)" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 290:Walls 26" | 1 occurrence | material: "2X BLOCKING" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 291:Walls 238" | 1 occurrence | material: "SEALANT (W/ BACKER ROD IF NECESSARY)" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 307:Walls 26" | 1 occurrence | material: "1X4 WOOD TRIM" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 308:Walls 26" | 1 occurrence | material: "5/8" GYP. BD" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 309:Walls 26" | 1 occurrence | material: "2X BLOCKING" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 310:Walls 26" | 1 occurrence | material: "2X BLOCKING" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 312:Walls 26" | 1 occurrence | material: "SHIMS AS NECESSARY W/ EXPANDING POLYURETHANE FOAM(1)" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 314:Walls 26" | 1 occurrence | material: "2X BLOCKING 24" O.C. BRACE TO FLOOR TRUSS" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 315:Walls 26" | 1 occurrence | material: "2X WOOD STUD" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 44:Walls 26" | 1 occurrence | material: "2X WOOD STUD" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 246:Walls 26" | 1 occurrence | material: "2X WOOD STUD" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 311:Walls 26" | 1 occurrence | material: "2X WOOD STUD" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 280:Walls 26" | 1 occurrence | material: "2X WOOD STUD" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 313:Walls 26" | 1 occurrence | material: "2X WOOD STUD" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 255:Walls 26" | 1 occurrence | material: "TREATED 2X10 LEDGER - STAINED" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 316:Walls 26" | 1 occurrence | material: "2X WOOD STUD" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 317:Walls 26" | 1 occurrence | material: "2X BLOCKING 24" O.C. BRACE TO FLOOR TRUSS" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 318:Walls 26" | 1 occurrence | material: "2X WOOD STUD" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 320:Walls 26" | 1 occurrence | material: "(3) GALV. WASHERS" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 322:Walls 26" | 1 occurrence | material: "J BEAD DRYWALL TRIM" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 2:Walls 26" | 1 occurrence | material: "2X6 DOUBLE STUD TOP PLATE" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 13:Walls 26" | 1 occurrence | material: "5/8" GYP. BD" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 1:Walls 26" | 1 occurrence | material: "2X6 DOUBLE STUD TOP PLATE" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 3:Walls 26" | 1 occurrence | material: "ALUM. STOREFRONT W/ TEMPERED INSULATED GLAZING" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 12:Walls 26" | 1 occurrence | material: "5/8" GYP. BD" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 4:Walls 26" | 1 occurrence | material: "SEALANT (W/ BACKER ROD IF NECESSARY)" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 6:Walls 26" | 1 occurrence | material: "PRE-ENGINEERED TRUSS @ 24" O.C." | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 14:Walls 26" | 1 occurrence | material: "LVL(s) - SIZE T.B.D." | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCBUILDINGELEMENTPROXYTYPE "050523 - Metal fastenings - Joist Hanger - Generic:ROOF TRUSS HANGER - TYPE 1" | 1 occurrence | material: materials ("ROOF JOIST HANGER - TYPE 1", "ROOF JOIST HANGER - TYPE 1", "ROOF JOIST HANGER - TYPE 1", "ROOF JOIST HANGER - TYPE 1") | property sets: Pset_ProductRequirements
  IFCWALLTYPE "Walls 19:Walls 26" | 1 occurrence | material: "1/2" CDX PLYWOOD" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 31:Walls 26" | 1 occurrence | material: "GALV. STANDING SEAM METAL ROOF" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 33:Walls 26" | 1 occurrence | material: "BUILDING WRAP" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 20:Walls 26" | 1 occurrence | material: "METAL FLASHING (MATCH SS)" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 23:Walls 26" | 1 occurrence | material: "METAL FLASHING (MATCH SS)" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 34:Walls 26" | 1 occurrence | material: "EXPANDING POLYURETHANE FOAM" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 25:Walls 26" | 1 occurrence | material: "5/8" GYP. BD" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 35:Walls 26" | 1 occurrence | material: "2X6 DOUBLE STUD TOP PLATE" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 26:Walls 26" | 1 occurrence | material: "BLOCKING - SIZE AS NEC." | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 36:Walls 26" | 1 occurrence | material: "ROOF BATT. INSULATION (R-49) OVER 6 MIL VAPOR BARRIER" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 30:Walls 26" | 1 occurrence | material: "CURTAIN WALL W/ GLAZED ASSEMBLIES" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 40:Walls 26" | 1 occurrence | material: "3/4" CDX PLYWOOD" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 49:Walls 26" | 1 occurrence | material: "SEALANT (W/ BACKER ROD IF NECESSARY)" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 50:Walls 26" | 1 occurrence | material: "EXPANDING POLYURETHANE FOAM" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 51:Walls 26" | 1 occurrence | material: "SEALANT (W/ BACKER ROD IF NECESSARY)" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCBEAMTYPE "061753 - Shop-Fabricated Wood Trusses - Generic1:24"" | BEAM | 1 occurrence | material: materials ("CUSTOM FLOOR TRUSS - SISTERED 2X4", "CUSTOM FLOOR TRUSS - SISTERED 2X4", "CUSTOM FLOOR TRUSS - SISTERED 2X4", "CUSTOM FLOOR TRUSS - SISTERED 2X4", "CUSTOM FLOOR TRUSS - SISTERED 2X4", "CUSTOM FLOOR TRUSS - SISTERED 2X4", "CUSTOM FLOOR TRUSS - SISTERED 2X4", "CUSTOM FLOOR TRUSS - SISTERED 2X4", "CUSTOM FLOOR TRUSS - SISTERED 2X4", "CUSTOM FLOOR TRUSS - SISTERED 2X4", "CUSTOM FLOOR TRUSS - SISTERED 2X4", "CUSTOM FLOOR TRUSS - SISTERED 2X4") | property sets: Pset_BeamCommon, Pset_ManufacturerTypeInformation, Pset_ProductRequirements, Pset_ReinforcementBarPitchOfBeam
  IFCWALLTYPE "Walls 88:Walls 26" | 1 occurrence | material: "60 MIL EPDM MEMBRANE OVER 3/4" CDX OR OSB" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 89:Walls 26" | 1 occurrence | material: "60 MIL EPDM MEMBRANE OVER 3/4" CDX OR OSB" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 90:Walls 26" | 1 occurrence | material: "THERMALLY MODIFIED WOOD (VENT TOP AND BOTTOM)" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 95:Walls 95" | 1 occurrence | material: "STANDING SEAM METAL WITH VARYING WIDTHS" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 96:Walls 96" | 1 occurrence | material: "PREFABRICATED ROOF SCISSOR TRUSS" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 102:Walls 26" | 1 occurrence | material: "1/2" CDX PLYWOOD" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 105:Walls 26" | 1 occurrence | material: "ALUM. STOREFRONT W/ TEMPERED INSULATED GLAZING" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 107:Walls 26" | 1 occurrence | material: "LVL(s) - SIZE T.B.D." | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 108:Walls 26" | 1 occurrence | material: "2X BLOCKING" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 109:Walls 26" | 1 occurrence | material: "5/8" GYP. BD @ CEILING" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 110:Walls 26" | 1 occurrence | material: "FILL ENTIRE CAVITY W/ CLOSED POLYURETHANE CELL FOAM(R-49MIN.)" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 114:Walls 26" | 1 occurrence | material: "SEALANT (W/ BACKER ROD IF NECESSARY)" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 115:Walls 26" | 1 occurrence | material: "SEALANT (W/ BACKER ROD IF NECESSARY)" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 116:Walls 26" | 1 occurrence | material: "EXPANDING POLYURETHANE FOAM" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 119:Walls 26" | 1 occurrence | material: "LVL(s) - SIZE T.B.D." | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 120:Walls 26" | 1 occurrence | material: "LVL(s) - SIZE T.B.D." | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 121:Walls 26" | 1 occurrence | material: "5/8" GYP. BD" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 122:Walls 26" | 1 occurrence | material: "5/8" GYP. BD" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 137:Walls 26" | 1 occurrence | material: "TJI JOIST W/POLY ISO FOAM (ENTIRE CAVITY)" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 138:Walls 26" | 1 occurrence | material: "TJI JOIST W/POLY ISO FOAM (ENTIRE CAVITY)" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 140:Walls 26" | 1 occurrence | material: "5/8" GYP. BD @ CEILING" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 141:Walls 26" | 1 occurrence | material: "5/8" GYP. BD @ CEILING" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 154:Walls 26" | 1 occurrence | material: "5/8" GYP. BD" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 169:Walls 169" | 1 occurrence | material: "RAILING POST" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 170:Walls 170" | 1 occurrence | material: "WOOD RAILING (MAPLE, OR BIRCH) - W/ WALL RETURNS AT ENDS" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 171:Walls 171" | 1 occurrence | material: "S.S. CABLE RAILING (3" O.C.)" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 175:Walls 173" | 1 occurrence | material: "5/8" GYP. BD" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 183:Walls 183" | 1 occurrence | material: "LVL(s) - SIZE T.B.D." | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 184:Walls 173" | 1 occurrence | material: "5/8" GYP. BD @ CEILING" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 185:Walls 185" | 1 occurrence | material: "TJI JOIST W/POLY ISO FOAM (ENTIRE CAVITY)" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 190:Walls 190" | 1 occurrence | material: "1/2" CDX PLYWOOD" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 191:Walls 191" | 1 occurrence | material: "ALUM. STOREFRONT W/ TEMPERED INSULATED GLAZING" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 192:Walls 190" | 1 occurrence | material: "THERMALLY MODIFIED WOOD (VENT TOP AND BOTTOM)" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 193:Walls 193" | 1 occurrence | material: "TJI - SEE STRUCT" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 199:Walls 194" | 1 occurrence | material: "5/8" GYP. BD @ CEILING" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 200:Walls 194" | 1 occurrence | material: "FILL ENTIRE CAVITY W/ CLOSED POLYURETHANE CELL FOAM(R-49MIN.)" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 201:Walls 201" | 1 occurrence | material: "BUILDING WRAP(AT WOOD SIDING)" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 204:Walls 204" | 1 occurrence | material: "SEALANT (W/ BACKER ROD IF NECESSARY)" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 205:Walls 205" | 1 occurrence | material: "EXPANDING POLYURETHANE FOAM" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 206:Walls 204" | 1 occurrence | material: "SEALANT (W/ BACKER ROD IF NECESSARY)" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 207:Walls 207" | 1 occurrence | material: "METAL FLASHING (MATCH SS)" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 213:Walls 198" | 1 occurrence | material: "2X BLOCKING" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 214:Walls 198" | 1 occurrence | material: "2X BLOCKING" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 215:Walls 190" | 1 occurrence | material: "2X BLOCKING" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 217:Walls 190" | 1 occurrence | material: "1/2" CORE-E-VENT BUG SCREEN" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 197:Walls 190" | 1 occurrence | material: "1/2" CORE-E-VENT VENTED VERTICAL FURRING STRIPS 16" O.C." | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 218:Walls 26" | 1 occurrence | material: "2X BLOCKING" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 219:Walls 26" | 1 occurrence | material: "SEALANT (W/ BACKER ROD IF NECESSARY)" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 118:Walls 26" | 1 occurrence | material: "METAL FLASHING (MATCH SS)" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 222:Walls 26" | 1 occurrence | material: "1/2" CORE-E-VENT BUG SCREEN" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 223:Walls 26" | 1 occurrence | material: "1/2" CORE-E-VENT VENTED VERTICAL FURRING STRIPS 16" O.C." | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCBUILDINGELEMENTPROXYTYPE "060523 - W_P_C - Fastenings - Generic:1/2" x 3"" | 1 occurrence | material: materials ("<Unnamed>", "<Unnamed>", "1/2" DIA. A325 BOLT AT EACH PURLIN", "1/2" DIA. A325 BOLT AT EACH PURLIN") | property sets: Pset_ProductRequirements, Pset_ProvisionForVoid
  IFCWALLTYPE "Walls 253:Walls 26" | 1 occurrence | material: "ACOUSTICAL MAT" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 254:Walls 26" | 1 occurrence | material: "LVT - SPEC TBD" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCBUILDINGELEMENTPROXYTYPE "060523 - W_P_C - Fastenings - Generic:Lag - .7500 - 3/4" | 1 occurrence | material: materials ("AT SILL - FASTENER AT 24" O.C.", "<Unnamed>") | property sets: Pset_ProductRequirements, Pset_ProvisionForVoid
  IFCBUILDINGELEMENTPROXYTYPE "060523 - W_P_C - Fastenings - Generic:Lag - .7500 - 3/4" | 1 occurrence | material: materials ("AT SILL - FASTENER AT 24" O.C.", "<Unnamed>") | property sets: Pset_ProductRequirements, Pset_ProvisionForVoid
  IFCWALLTYPE "Walls 283:Walls 26" | 1 occurrence | material: "2X WOOD STUD" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 284:Walls 26" | 1 occurrence | material: "5/8" GYP. BD" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCBUILDINGELEMENTPROXYTYPE "060523 - W_P_C - Fastenings - Generic:Screw - .220 - #12" | 1 occurrence | material: materials ("AT SILL - FASTENER AT 24" O.C.", "<Unnamed>") | property sets: Pset_ProductRequirements, Pset_ProvisionForVoid
  IFCWALLTYPE "Walls 103:Walls 26" | 1 occurrence | material: "BUILDING WRAP" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 287:Walls 26" | 1 occurrence | material: "ALUM. STOREFRONT W/ TEMPERED INSULATED GLAZING" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 289:Walls 26" | 1 occurrence | material: "2X BLOCKING" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 292:Walls 26" | 1 occurrence | material: "EXPANDING POLYURETHANE FOAM" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 298:Walls 26" | 1 occurrence | material: "SELF ADHERED MEMBRANE" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 299:Walls 26" | 1 occurrence | material: "METAL FLASHING (MATCH SS)" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 301:Walls 26" | 1 occurrence | material: "SEALANT (W/ BACKER ROD IF NECESSARY)" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCBUILDINGELEMENTPROXYTYPE "060523 - W_P_C - Fastenings - Generic:Thru-Bolt - .6250 - 5/8" | 1 occurrence | material: materials ("<Unnamed>", "<Unnamed>", "AT SILL - FASTENER AT 24" O.C.", "AT SILL - FASTENER AT 24" O.C.", "AT SILL - FASTENER AT 24" O.C.") | property sets: Pset_ProductRequirements, Pset_ProvisionForVoid
  IFCBUILDINGELEMENTPROXYTYPE "060523 - W_P_C - Fastenings - Generic:Thru-Bolt - .5000 - 1/2" | 1 occurrence | material: materials ("<Unnamed>", "<Unnamed>", "AT SILL - FASTENER AT 24" O.C.", "AT SILL - FASTENER AT 24" O.C.", "AT SILL - FASTENER AT 24" O.C.") | property sets: Pset_ProductRequirements, Pset_ProvisionForVoid
  IFCWALLTYPE "Walls 38:Walls 26" | 1 occurrence | material: "SEALANT (W/ BACKER ROD IF NECESSARY)" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCBUILDINGELEMENTPROXYTYPE "060523 - W_P_C - Fastenings - Generic:Thru-Bolt - .6250 - 5/8" | 2 occurrences | material: materials ("<Unnamed>", "<Unnamed>", "AT SILL - FASTENER AT 24" O.C.", "AT SILL - FASTENER AT 24" O.C.", "AT SILL - FASTENER AT 24" O.C.") | property sets: Pset_ProductRequirements, Pset_ProvisionForVoid
  IFCBUILDINGELEMENTPROXYTYPE "060523 - W_P_C - Fastenings - Generic:Thru-Bolt - .6250 - 5/8" | 2 occurrences | material: materials ("<Unnamed>", "<Unnamed>", "AT SILL - FASTENER AT 24" O.C.", "AT SILL - FASTENER AT 24" O.C.", "AT SILL - FASTENER AT 24" O.C.") | property sets: Pset_ProductRequirements, Pset_ProvisionForVoid
  IFCBUILDINGELEMENTPROXYTYPE "060523 - W_P_C - Fastenings - Generic:Thru-Bolt - .5000 - 1/2" | 2 occurrences | material: materials ("<Unnamed>", "<Unnamed>", "AT SILL - FASTENER AT 24" O.C.", "AT SILL - FASTENER AT 24" O.C.", "AT SILL - FASTENER AT 24" O.C.") | property sets: Pset_ProductRequirements, Pset_ProvisionForVoid
  IFCBUILDINGELEMENTPROXYTYPE "060523 - W_P_C - Fastenings - Generic:Thru-Bolt - .5000 - 1/2" | 4 occurrences | material: materials ("<Unnamed>", "<Unnamed>", "AT SILL - FASTENER AT 24" O.C.", "AT SILL - FASTENER AT 24" O.C.", "AT SILL - FASTENER AT 24" O.C.") | property sets: Pset_ProductRequirements, Pset_ProvisionForVoid
  IFCBUILDINGELEMENTPROXYTYPE "060523 - W_P_C - Fastenings - Generic:Lag - .7500 - 3/4" | 1 occurrence | material: materials ("AT SILL - FASTENER AT 24" O.C.", "<Unnamed>") | property sets: Pset_ProductRequirements, Pset_ProvisionForVoid
  IFCBUILDINGELEMENTPROXYTYPE "060523 - W_P_C - Fastenings - Generic:Screw - .220 - #12" | 1 occurrence | material: materials ("AT SILL - FASTENER AT 24" O.C.", "<Unnamed>") | property sets: Pset_ProductRequirements, Pset_ProvisionForVoid
  IFCWALLTYPE "Walls 319:Walls 26" | 1 occurrence | material: "1X4 WOOD TRIM" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 321:Walls 26" | 1 occurrence | material: "J BEAD DRYWALL TRIM" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 18:Walls 26" | 1 occurrence | material: "3/4" CDX OR OSB" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 21:Walls 26" | 1 occurrence | material: "GALV. STANDING SEAM METAL ROOF" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 24:Walls 26" | 1 occurrence | material: "GALV. STANDING SEAM METAL ROOF" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 27:Walls 26" | 1 occurrence | material: "GALV. STANDING SEAM METAL ROOF" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 28:Walls 26" | 1 occurrence | material: "30LB ROOFING FELT" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 29:Walls 26" | 1 occurrence | material: "GALV. CUSTOM GUTTER" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 32:Walls 26" | 1 occurrence | material: "GALV. STANDING SEAM METAL ROOF" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 11:Walls 26" | 1 occurrence | material: "(2) 3/4" COR-A-VENT" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 17:Walls 26" | 1 occurrence | material: "(2) 3/4" COR-A-VENT" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 22:Walls 26" | 1 occurrence | material: "GUTTER BRACKET" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 37:Walls 26" | 1 occurrence | material: "INSULATION BAFFLE BETWEEN TRUSSES" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 104:Walls 26" | 1 occurrence | material: "1/2" CDX PLYWOOD" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 106:Walls 26" | 1 occurrence | material: "3/4" CDX PLYWOOD" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 112:Walls 26" | 1 occurrence | material: "METAL COPING - MATCH SS ROOFING" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 113:Walls 26" | 1 occurrence | material: "EPS RIGID INSULATION (1/4"/12" MIN. SLOPE TO DRAINS)" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 111:Walls 26" | 1 occurrence | material: "SELF ADHERED MEMBRANE" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 124:Walls 26" | 1 occurrence | material: "2X BLOCKING" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 129:Walls 26" | 1 occurrence | material: "2X BLOCKING" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 130:Walls 26" | 1 occurrence | material: "2X BLOCKING" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 133:Walls 26" | 1 occurrence | material: "3/4" CDX PLYWOOD" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 134:Walls 26" | 1 occurrence | material: "1/2" CDX PLYWOOD" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 135:Walls 26" | 1 occurrence | material: "2X6s W/ 2" POLY ISO FOAM & 3.5" OF BLOWN-IN CELLULOSE INSULATION" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 136:Walls 26" | 1 occurrence | material: "EPS RIGID INSULATION (1/4"/12" MIN. SLOPE TO DRAINS)" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 139:Walls 26" | 1 occurrence | material: "2X6s W/ 2" POLY ISO FOAM & 3.5" OF BLOWN-IN CELLULOSE INSULATION" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 142:Walls 26" | 1 occurrence | material: "1/2" CDX PLYWOOD" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 143:Walls 26" | 1 occurrence | material: "METAL FLASHING (MATCH SS)" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 144:Walls 26" | 1 occurrence | material: "LINEAR SKYLIGHT - INSULATED TEMPERED GLAZING" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 145:Walls 26" | 1 occurrence | material: "60 MIL EPDM MEMBRANE (1/4"/12" MIN. SLOPE)" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 147:Walls 26" | 1 occurrence | material: "SEALANT (W/ BACKER ROD IF NECESSARY)" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 148:Walls 26" | 1 occurrence | material: "EXPANDING POLYURETHANE FOAM" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 149:Walls 26" | 1 occurrence | material: "METAL FLASHING (MATCH SS)" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 150:Walls 26" | 1 occurrence | material: "60 MIL EPDM MEMBRANE (1/4"/12" MIN. SLOPE)" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 152:Walls 26" | 1 occurrence | material: "3/4" CDX PLYWOOD" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 153:Walls 26" | 1 occurrence | material: "EPS RIGID INSULATION (1/4"/12" MIN. SLOPE TO DRAINS)" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 173:Walls 173" | 1 occurrence | material: "1/2" CDX PLYWOOD" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 174:Walls 173" | 1 occurrence | material: "2X6s W/ 2" POLY ISO FOAM & 3.5" OF BLOWN-IN CELLULOSE INSULATION" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 176:Walls 176" | 1 occurrence | material: "2X BLOCKING" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 177:Walls 177" | 1 occurrence | material: "SKYLIGHTS" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 178:Walls 178" | 1 occurrence | material: "METAL FLASHING (MATCH SS)" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 179:Walls 179" | 1 occurrence | material: "BUILDING WRAP" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 180:Walls 180" | 1 occurrence | material: "60 MIL EPDM MEMBRANE (1/4"/12" MIN. SLOPE)" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 181:Walls 180" | 1 occurrence | material: "EPS RIGID INSULATION (1/4"/12" MIN. SLOPE TO DRAINS)" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 182:Walls 180" | 1 occurrence | material: "3/4" CDX PLYWOOD" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 186:Walls 186" | 1 occurrence | material: "SEALANT (W/ BACKER ROD IF NECESSARY)" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 187:Walls 187" | 1 occurrence | material: "5/8" GYP. BD" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 189:Walls 189" | 1 occurrence | material: "EXPANDING POLYURETHANE FOAM" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 194:Walls 194" | 1 occurrence | material: "3/4" CDX PLYWOOD" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 195:Walls 195" | 1 occurrence | material: "1/2" CDX PLYWOOD" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 196:Walls 196" | 1 occurrence | material: "EPS RIGID INSULATION (1/4"/12" MIN. SLOPE TO DRAINS)" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 198:Walls 198" | 1 occurrence | material: "2X BLOCKING" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 203:Walls 203" | 1 occurrence | material: "METAL COPING - MATCH SS ROOFING" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 216:Walls 190" | 1 occurrence | material: "1/2" CORE-E-VENT BUG SCREEN" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 220:Walls 26" | 1 occurrence | material: "2X BLOCKING" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 221:Walls 26" | 1 occurrence | material: "2X BLOCKING" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 224:Walls 26" | 1 occurrence | material: "60 MIL EPDM MEMBRANE" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 286:Walls 201" | 1 occurrence | material: "60 MIL EPDM MEMBRANE" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 202:Walls 201" | 1 occurrence | material: "METAL FLASHING (MATCH SS)" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 94:Walls 94" | 1 occurrence | material: "STANDING SEAM METAL WITH VARYING WIDTHS" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 99:Walls 99" | 1 occurrence | material: "3/4" CDX PLYWOOD" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 100:Walls 100" | 1 occurrence | material: "60 MIL EPDM MEMBRANE OVER 3/4" CDX OR OSB" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 101:Walls 101" | 1 occurrence | material: "2X6s W/ 2" POLY ISO FOAM & 3.5" OF BLOWN-IN CELLULOSE INSULATION" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 128:Walls 26" | 1 occurrence | material: "INSULATED GLAZING" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 131:Walls 26" | 1 occurrence | material: "2X BLOCKING" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 132:Walls 26" | 1 occurrence | material: "2X BLOCKING" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 146:Walls 26" | 1 occurrence | material: "LINEAR SKYLIGHT - INSULATED TEMPERED GLAZING" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 151:Walls 26" | 1 occurrence | material: "EXPANDING POLYURETHANE FOAM" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 155:Walls 155" | 1 occurrence | material: "TJI - SEE STRUCT" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 156:Walls 156" | 1 occurrence | material: "3/4" CDX PLYWOOD" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 157:Walls 157" | 1 occurrence | material: "BUILDING WRAP" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 158:Walls 158" | 1 occurrence | material: "1/2" CDX PLYWOOD" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 159:Walls 159" | 1 occurrence | material: "STANDING SEAM METAL WITH VARYING WIDTHS" | property sets: Pset_ProductRequirements, Pset_WallCommon
  IFCWALLTYPE "Walls 188:Walls 188" | 1 occurrence | material: "SILL PLATE GASKET" | property sets: Pset_ProductRequirements, Pset_WallCommon

Property sets
  Pset_ProductRequirements | properties | on 309 objects (305 IFCWALL, 4 IFCOPENINGELEMENT) | on 305 type objects
    Category = "Walls" (IFCLABEL)
  Pset_ProductRequirements | properties | on 18 objects (18 IFCBUILDINGELEMENTPROXY) | on 12 type objects
    Category = "Structural Connections" (IFCLABEL)
  Pset_ProductRequirements | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY) | on 1 type object
    Category = "Generic Models" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBEAM) | on 1 type object
    Category = "Structural Framing" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Name = "HIGH WATER MARK" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Name = "2ND FLOOR" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Name = "FLAT ROOF" (IFCLABEL)
  Pset_ProductRequirements: 1 more content on 1 objects not shown
  Pset_QuantityTakeOff | properties | on 231 objects (228 IFCWALL, 3 IFCOPENINGELEMENT)
    Reference = "Walls 26" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 10 objects (10 IFCWALL)
    Reference = "Walls 164" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 7 objects (7 IFCBUILDINGELEMENTPROXY)
    Reference = "Thru-Bolt - .5000 - 1/2" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 6 objects (6 IFCWALL)
    Reference = "Walls 190" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 5 objects (5 IFCBUILDINGELEMENTPROXY)
    Reference = "Thru-Bolt - .6250 - 5/8" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 4 objects (4 IFCWALL)
    Reference = "Walls 173" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 3 objects (3 IFCWALL)
    Reference = "Walls 162" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 3 objects (3 IFCWALL)
    Reference = "Walls 180" (IFCIDENTIFIER)
  Pset_QuantityTakeOff: 45 more contents on 60 objects not shown
  Pset_ReinforcementBarPitchOfWall | properties | on 228 objects (228 IFCWALL)
    Reference = "Walls 26" (IFCLABEL)
  Pset_ReinforcementBarPitchOfWall | properties | on 10 objects (10 IFCWALL)
    Reference = "Walls 164" (IFCLABEL)
  Pset_ReinforcementBarPitchOfWall | properties | on 6 objects (6 IFCWALL)
    Reference = "Walls 190" (IFCLABEL)
  Pset_ReinforcementBarPitchOfWall | properties | on 4 objects (4 IFCWALL)
    Reference = "Walls 173" (IFCLABEL)
  Pset_ReinforcementBarPitchOfWall | properties | on 3 objects (3 IFCWALL)
    Reference = "Walls 162" (IFCLABEL)
  Pset_ReinforcementBarPitchOfWall | properties | on 3 objects (3 IFCWALL)
    Reference = "Walls 180" (IFCLABEL)
  Pset_ReinforcementBarPitchOfWall | properties | on 3 objects (3 IFCWALL)
    Reference = "Walls 194" (IFCLABEL)
  Pset_ReinforcementBarPitchOfWall | properties | on 3 objects (3 IFCWALL)
    Reference = "Walls 198" (IFCLABEL)
  Pset_ReinforcementBarPitchOfWall: 38 more contents on 45 objects not shown
  Pset_WallCommon | properties | on 228 objects (228 IFCWALL)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Walls 26" (IFCIDENTIFIER)
  Pset_WallCommon | properties | on 10 objects (10 IFCWALL)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Walls 164" (IFCIDENTIFIER)
  Pset_WallCommon | properties | on 6 objects (6 IFCWALL)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Walls 190" (IFCIDENTIFIER)
  Pset_WallCommon | properties | on 4 objects (4 IFCWALL)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Walls 173" (IFCIDENTIFIER)
  Pset_WallCommon | properties | on 3 objects (3 IFCWALL)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Walls 162" (IFCIDENTIFIER)
  Pset_WallCommon | properties | on 3 objects (3 IFCWALL)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Walls 180" (IFCIDENTIFIER)
  Pset_WallCommon | properties | on 3 objects (3 IFCWALL)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Walls 194" (IFCIDENTIFIER)
  Pset_WallCommon | properties | on 3 objects (3 IFCWALL)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Walls 198" (IFCIDENTIFIER)
  Pset_WallCommon: 39 more contents on 45 objects not shown
  Pset_BuildingElementProxyCommon | properties | on 7 objects (7 IFCBUILDINGELEMENTPROXY)
    Reference = "Thru-Bolt - .5000 - 1/2" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 5 objects (5 IFCBUILDINGELEMENTPROXY)
    Reference = "Thru-Bolt - .6250 - 5/8" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 3 objects (3 IFCBUILDINGELEMENTPROXY)
    Reference = "Lag - .7500 - 3/4" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 2 objects (2 IFCBUILDINGELEMENTPROXY)
    Reference = "Screw - .220 - #12" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Reference = "ROOF TRUSS HANGER - TYPE 1" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Reference = "1/2" x 3"" (IFCIDENTIFIER)
  Pset_ProvisionForVoid | properties | on 4 objects (4 IFCBUILDINGELEMENTPROXY) | on 3 type objects
    Diameter = 0.04296875 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
  Pset_ProvisionForVoid | properties | on 3 objects (3 IFCBUILDINGELEMENTPROXY) | on 3 type objects
    Diameter = 0.0641276041666667 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
  Pset_ProvisionForVoid | properties | on 2 objects (2 IFCBUILDINGELEMENTPROXY) | on 3 type objects
    Diameter = 0.0533854166666667 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
  Pset_ProvisionForVoid | properties | on 2 objects (2 IFCBUILDINGELEMENTPROXY) | on 2 type objects
    Diameter = 0.0183333333333333 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
  Pset_ProvisionForVoid | properties | on 2 objects (2 IFCBUILDINGELEMENTPROXY)
    Depth = 0.25091194885748 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
    Diameter = 0.0533854166666667 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
    Width = 0.25091194885748 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
  Pset_ProvisionForVoid | properties | on 2 objects (2 IFCBUILDINGELEMENTPROXY)
    Depth = 0.554257812500785 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
    Diameter = 0.04296875 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
    Width = 0.554257812500785 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
  Pset_ProvisionForVoid | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Depth = 0.00520833333333333 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
    Height = 0.125000000000064 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
    Width = 0.00520833333333333 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
  Pset_ProvisionForVoid | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Depth = 0.392074220206723 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
    Diameter = 0.0416666666666667 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
    Width = 0.392074220206723 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
  Pset_ProvisionForVoid: 3 more contents on 2 objects not shown
  Pset_BeamCommon | properties | on 1 object (1 IFCBEAM)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "24"" (IFCIDENTIFIER)
    Slope = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Span = 8.8348828031958 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
  Pset_BeamCommon | properties | on 1 type object
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
  Pset_ManufacturerTypeInformation | properties | on 1 object (1 IFCBEAM) | on 1 type object
    Manufacturer = "RedBuilt™" (IFCLABEL)
  Pset_ReinforcementBarPitchOfBeam | properties | on 1 object (1 IFCBEAM)
    Description = "Joist" (IFCTEXT)
    Reference = "24"" (IFCLABEL)
  Pset_ReinforcementBarPitchOfBeam | properties | on 1 type object
    Description = "Joist" (IFCTEXT)
  Pset_OpeningElementCommon | properties | on 3 objects (3 IFCOPENINGELEMENT)
    Reference = "Walls 26" (IFCIDENTIFIER)
  Pset_OpeningElementCommon | properties | on 1 object (1 IFCOPENINGELEMENT)
    Reference = "Walls 169" (IFCIDENTIFIER)
  Pset_AirSideSystemInformation | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Name = "HIGH WATER MARK" (IFCLABEL)
  Pset_AirSideSystemInformation | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Name = "2ND FLOOR" (IFCLABEL)
  Pset_AirSideSystemInformation | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Name = "FLAT ROOF" (IFCLABEL)
  Pset_AirSideSystemInformation | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Name = "ATTIC" (IFCLABEL)
  Pset_BuildingStoreyCommon | properties | on 4 objects (4 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    IsLandmarked = UNKNOWN (IFCLOGICAL)
    NumberOfStoreys = 4 (IFCINTEGER)