IFC building model
Schema: "IFC4"
Description: "ViewDefinition [DesignTransferView_V1.0]"
File name: "Project Number"
Time stamp: "2022-11-08T17:55:49"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.07 : 28 Aug 2013"
Originating system: "20200210_1400(x64) - Exporter 20.3.3.0 - Alternate UI 20.3.3.0"
Application: "Autodesk Revit 2020 (ENU)" version "2020" identifier "Revit" by Organization "Autodesk Revit 2020 (ENU)"

People and organizations
  Person "ryan@openingdesign.com" of Organization (no name given)
  Owner history of Person "ryan@openingdesign.com" of Organization (no name given) | application "Autodesk Revit 2020 (ENU)" version "2020" identifier "Revit" by Organization "Autodesk Revit 2020 (ENU)" | change NOCHANGE | created 1667951619 (2022-11-08T23:53:39Z)

Units
  LENGTHUNIT: FOOT (conversion based)
  AREAUNIT: SQUARE FOOT (conversion based)
  VOLUMEUNIT: CUBIC FOOT (conversion based)
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  MOMENTOFINERTIAUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"
  LINEARFORCEUNIT: derived
  PLANARFORCEUNIT: derived

Spatial structure
IFCPROJECT "Project Number" | long name "MARCO POLO - 101 W 33RD STREET - CITY OF BRYAN TOWNSITE, BLOCK 96, LOT 3-5 & PT OF 6 & PT OF ALLEY" | phase "Project Status"
  IFCSITE "Default" | latitude 42° 21′ 30.344238″ | longitude -71° 3′ 35.194702″ | elevation above sea level 100.
    IFCBUILDING | postal address: "BRYAN, TX 77803", "<Default>"
      IFCBUILDINGSTOREY "BASEMENT" | long name "BASEMENT" | object type "Level:Project Base Point" | elevation -12.6666666666667
        contains 231 elements
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Surface:614023" | names: "Surface:614023" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 129:Generic Models 1" | object type "Generic Models 129:Generic Models 1" | names: "Generic Models 129:Generic Models 1:609995" | material: "EXISTING SLAB" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 8:Generic Models 1" | object type "Generic Models 8:Generic Models 1" | names: "Generic Models 8:Generic Models 1:826903" | material: "CONCRETE (3000 PSI CONCRETE)" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 141:Generic Models 1" | object type "Generic Models 141:Generic Models 1" | names: "Generic Models 141:Generic Models 1:830973" | material: "#4 CONT. STEEL REBAR" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 144:Generic Models 1" | object type "Generic Models 144:Generic Models 1" | names: "Generic Models 144:Generic Models 1:830994" | material: "#10 6x6 WIRE MESH" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 145:Generic Models 1" | object type "Generic Models 145:Generic Models 1" | names: "Generic Models 145:Generic Models 1:831218" | material: "6 MIL VAPOR BARRIER" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 150:Generic Models 1" | object type "Generic Models 150:Generic Models 1" | names: "Generic Models 150:Generic Models 1:831484" | material: "6" COMPACTED CRUSHED STONE" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 151:Generic Models 1" | object type "Generic Models 151:Generic Models 1" | names: "Generic Models 151:Generic Models 1:832637" | material: "GRADE (SLOPE 2% MIN AWAY FROM BUILDING)_grass" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 183:Generic Models 1" | object type "Generic Models 183:Generic Models 1" | names: "Generic Models 183:Generic Models 1:854474" | material: "STRUCTURAL WOOD COLUMN - SIZE TBD" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 177:Generic Models 1" | object type "Generic Models 177:Generic Models 1" | names: "Generic Models 177:Generic Models 1:856630" | material: "STRUCTURAL WOOD COLUMN - SIZE TBD" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 178:Generic Models 155" | object type "Generic Models 178:Generic Models 155" | names: "Generic Models 178:Generic Models 155:856646" | material: "CONCRETE (3000 PSI CONCRETE)" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 184:Generic Models 184" | object type "Generic Models 184:Generic Models 184" | names: "Generic Models 184:Generic Models 184:858653" | material: "GRADE" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          2 x IFCWALL | type IFCWALLTYPE "Basic Wall:GRADE BEAM - PERIMETER" | object type "Basic Wall:GRADE BEAM - PERIMETER" | names: "Basic Wall:GRADE BEAM - PERIMETER:1246038", "Basic Wall:GRADE BEAM - PERIMETER:1246039" | material: layers "Basic Wall:GRADE BEAM - PERIMETER" ("CONCRETE GRADE BEAM POURED WITH CONCRETE SLAB - SEE STRUCT DWGS" 1.5) | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCFOOTING | type IFCFOOTINGTYPE "Wall Foundation:12"X24"" | object type "Wall Foundation:12"X24"" | STRIP_FOOTING | names: "Wall Foundation:12"X24":1246153" | material: "CONCRETE FOOTING - 12"X24"" | property sets: Pset_EnvironmentalImpactIndicators, Pset_FootingCommon, Pset_ReinforcementBarCountOfIndependentFooting, Pset_ReinforcementBarPitchOfContinuousFooting
          1 x IFCFOOTING | type IFCFOOTINGTYPE "Wall Foundation:12"X24"" | object type "Wall Foundation:12"X24"" | STRIP_FOOTING | names: "Wall Foundation:12"X24":1246173" | material: "CONCRETE FOOTING - 12"X24"" | property sets: Pset_EnvironmentalImpactIndicators, Pset_FootingCommon, Pset_ReinforcementBarCountOfIndependentFooting, Pset_ReinforcementBarPitchOfContinuousFooting
          1 x IFCSLAB | type IFCSLABTYPE "Foundation Slab:6" Foundation Slab" | object type "Foundation Slab:6" Foundation Slab" | BASESLAB | names: "Foundation Slab:6" Foundation Slab:1247143" | material: layers "Foundation Slab:6" Foundation Slab" ("6" CONCRETE SLAB (3000PSI MIN.) W/ #10 6X6 OVER 6 MIL POLYETHYLENE VAPOR BARRIER" 0.5) | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Slab Edge:Thickened 24" x 12"" | object type "Slab Edge:Thickened 24" x 12"" | names: "Slab Edge:Thickened 24" x 12":1247150" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCSLAB | type IFCSLABTYPE "Floor:6" COMPACTED CRUSHED STONE" | object type "Floor:6" COMPACTED CRUSHED STONE" | FLOOR | names: "Floor:6" COMPACTED CRUSHED STONE:1247194" | material: layers "Floor:6" COMPACTED CRUSHED STONE" ("6" COMPACTED CRUSHED STONE" 0.5) | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Surface:1313663" | names: "Surface:1313663" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Surface:1313665" | names: "Surface:1313665" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCSLAB | type IFCSLABTYPE "Pad:GENERIC PAD" | object type "Pad:GENERIC PAD" | FLOOR | names: "Pad:GENERIC PAD:1313666" | material: layers "Pad:GENERIC PAD" ("PAD (TURNED OFF)" 0.5) | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 269:Generic Models 263" | object type "Generic Models 269:Generic Models 263" | names: "Generic Models 269:Generic Models 263:1381148" | material: "CONCRETE CURB" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 270:Generic Models 263" | object type "Generic Models 270:Generic Models 263" | names: "Generic Models 270:Generic Models 263:1381912" | material: "CONCRETE CURB" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 271:Generic Models 263" | object type "Generic Models 271:Generic Models 263" | names: "Generic Models 271:Generic Models 263:1382304" | material: "PAVEMENT" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 274:Generic Models 263" | object type "Generic Models 274:Generic Models 263" | names: "Generic Models 274:Generic Models 263:1384626" | material: "8" CRUSHED 1.25" AGGREGATE BASE COURSE (COMPACTED)" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 275:Generic Models 263" | object type "Generic Models 275:Generic Models 263" | names: "Generic Models 275:Generic Models 263:1384752" | material: "COMPACTED SUBGRADE" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 277:Generic Models 263" | object type "Generic Models 277:Generic Models 263" | names: "Generic Models 277:Generic Models 263:1385057" | material: "PAVING SURFACE (TYP.) SEE PLANS" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 278:Generic Models 263" | object type "Generic Models 278:Generic Models 263" | names: "Generic Models 278:Generic Models 263:1385167" | material: "5" MIN. COMPACTED BASE AGGREGATE UNDER CURB" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 279:Generic Models 263" | object type "Generic Models 279:Generic Models 263" | names: "Generic Models 279:Generic Models 263:1385327" | material: "PAVING SURFACE (TYP.) SEE PLANS" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 280:Generic Models 263" | object type "Generic Models 280:Generic Models 263" | names: "Generic Models 280:Generic Models 263:1385413" | material: "5" MIN. COMPACTED BASE AGGREGATE UNDER CURB" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 281:Generic Models 263" | object type "Generic Models 281:Generic Models 263" | names: "Generic Models 281:Generic Models 263:1385588" | material: "3" TO 6" WASHED OR CLEAR STONE" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 286:Generic Models 263" | object type "Generic Models 286:Generic Models 263" | names: "Generic Models 286:Generic Models 263:1386677" | material: "6" CRUSHED AGGREGATE BASE COURSE" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 292:Generic Models 263" | object type "Generic Models 292:Generic Models 263" | names: "Generic Models 292:Generic Models 263:1388713" | material: "CONCRETE CURB" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 294:Generic Models 263" | object type "Generic Models 294:Generic Models 263" | names: "Generic Models 294:Generic Models 263:1388734" | material: "PAVING SURFACE (TYP.) SEE PLANS" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 295:Generic Models 263" | object type "Generic Models 295:Generic Models 263" | names: "Generic Models 295:Generic Models 263:1388746" | material: "CRUSHED AGGREGATE BASE COURSE" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 289:Generic Models 263" | object type "Generic Models 289:Generic Models 263" | names: "Generic Models 289:Generic Models 263:1394121" | material: "7" CONC. DRIVE APPROACH" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 297:Generic Models 263" | object type "Generic Models 297:Generic Models 263" | names: "Generic Models 297:Generic Models 263:1394272" | material: "SLOPED - 7" CONC." | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 298:Generic Models 263" | object type "Generic Models 298:Generic Models 263" | names: "Generic Models 298:Generic Models 263:1394399" | material: "SEE SITE PLAN FOR LANDSCAPING" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 299:Generic Models 263" | object type "Generic Models 299:Generic Models 263" | names: "Generic Models 299:Generic Models 263:1395691" | material: "CONCRETE CURB" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 300:Generic Models 263" | object type "Generic Models 300:Generic Models 263" | names: "Generic Models 300:Generic Models 263:1395728" | material: "CONCRETE CURB" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 282:Generic Models 263" | object type "Generic Models 282:Generic Models 263" | names: "Generic Models 282:Generic Models 263:1398156" | material: "CONCRETE CURB" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 301:Generic Models 263" | object type "Generic Models 301:Generic Models 263" | names: "Generic Models 301:Generic Models 263:1398203" | material: "CONCRETE CURB" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 290:Generic Models 263" | object type "Generic Models 290:Generic Models 263" | names: "Generic Models 290:Generic Models 263:1399522" | material: "GRADED BACKFILL" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 291:Generic Models 263" | object type "Generic Models 291:Generic Models 263" | names: "Generic Models 291:Generic Models 263:1399720" | material: "GRADED BACKFILL" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 306:Generic Models 263" | object type "Generic Models 306:Generic Models 263" | names: "Generic Models 306:Generic Models 263:1399821" | material: "EXISTING GRADE" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 307:Generic Models 263" | object type "Generic Models 307:Generic Models 263" | names: "Generic Models 307:Generic Models 263:1400379" | material: "CONCRETE PAVEMENT HEAVY DUTY" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 310:Generic Models 263" | object type "Generic Models 310:Generic Models 263" | names: "Generic Models 310:Generic Models 263:1400408" | material: "8" CRUSHED 1.25" AGGREGATE BASE COURSE (COMPACTED)" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 311:Generic Models 263" | object type "Generic Models 311:Generic Models 263" | names: "Generic Models 311:Generic Models 263:1400420" | material: "COMPACTED SUBGRADE" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 309:Generic Models 263" | object type "Generic Models 309:Generic Models 263" | names: "Generic Models 309:Generic Models 263:1400637" | material: "EPOXY COATED 6 X 6 X W2.9 X W2.9, PLACED 3" ABOVE SLAB BASE" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 283:Generic Models 263" | object type "Generic Models 283:Generic Models 263" | names: "Generic Models 283:Generic Models 263:1403684" | material: "SLOPED - 7" CONC." | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 284:Generic Models 263" | object type "Generic Models 284:Generic Models 263" | names: "Generic Models 284:Generic Models 263:1403706" | material: "SEE SITE PLAN FOR LANDSCAPING" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 276:Generic Models 263" | object type "Generic Models 276:Generic Models 263" | names: "Generic Models 276:Generic Models 263:1405189" | material: "1" EXPANSION JOINT" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Basic Wall:RATED - 1 HR" | object type "Basic Wall:RATED - 1 HR" | names: "Basic Wall:RATED - 1 HR:1417669" | material: layers "Basic Wall:RATED - 1 HR" ("Default Wall" 0.666666666666667) | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCSLAB | type IFCSLABTYPE "316600 - Special Foundations - Diamond Pier - Generic:316600 - Special Foundations - Diamond Pier - Generic" | object type "316600 - Special Foundations - Diamond Pier - Generic:316600 - Special Foundations - Diamond Pier - Generic" | BASESLAB | names: "316600 - Special Foundations - Diamond Pier - Generic:316600 - Special Foundations - Diamond Pier - Generic:1417714" | material: "DIAMOND PIER DP-50/50 - (3300# B.L.C. AT 1500PSF SOILS, 4400# B.L.C. AT 2000PSF SOILS)" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCSLAB | type IFCSLABTYPE "316600 - Special Foundations - Diamond Pier - Generic:316600 - Special Foundations - Diamond Pier - Generic" | object type "316600 - Special Foundations - Diamond Pier - Generic:316600 - Special Foundations - Diamond Pier - Generic" | BASESLAB | names: "316600 - Special Foundations - Diamond Pier - Generic:316600 - Special Foundations - Diamond Pier - Generic:1417716" | material: "DIAMOND PIER DP-50/50 - (3300# B.L.C. AT 1500PSF SOILS, 4400# B.L.C. AT 2000PSF SOILS)" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCSLAB | type IFCSLABTYPE "316600 - Special Foundations - Diamond Pier - Generic:316600 - Special Foundations - Diamond Pier - Generic" | object type "316600 - Special Foundations - Diamond Pier - Generic:316600 - Special Foundations - Diamond Pier - Generic" | BASESLAB | names: "316600 - Special Foundations - Diamond Pier - Generic:316600 - Special Foundations - Diamond Pier - Generic:1417718" | material: "DIAMOND PIER DP-50/50 - (3300# B.L.C. AT 1500PSF SOILS, 4400# B.L.C. AT 2000PSF SOILS)" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "Timber-Column:6x6" | object type "Timber-Column:6x6" | COLUMN | names: "Timber-Column:6x6:1424465" | material: profiles "6x6" ("6x6": "STRUCTURAL WOOD COLUMN - SIZE TBD") | property sets: Pset_ColumnCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "Timber-Column:6x6" | object type "Timber-Column:6x6" | COLUMN | names: "Timber-Column:6x6:1424805" | material: profiles "6x6" ("6x6": "STRUCTURAL WOOD COLUMN - SIZE TBD") | property sets: Pset_ColumnCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "Timber-Column:6x6" | object type "Timber-Column:6x6" | COLUMN | names: "Timber-Column:6x6:1424882" | material: profiles "6x6" ("6x6": "STRUCTURAL WOOD COLUMN - SIZE TBD") | property sets: Pset_ColumnCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfColumn
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 299:Generic Models 263" | object type "Generic Models 299:Generic Models 263" | names: "Generic Models 299:Generic Models 263:1451698" | material: "CONCRETE CURB" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 299:Generic Models 263" | object type "Generic Models 299:Generic Models 263" | names: "Generic Models 299:Generic Models 263:1451928" | material: "CONCRETE CURB" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 349:Generic Models 1" | object type "Generic Models 349:Generic Models 1" | names: "Generic Models 349:Generic Models 1:1464038" | material: "STRUCTURAL FLOOR - SEE STRUCT. DWGS" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 414:Generic Models 1" | object type "Generic Models 414:Generic Models 1" | names: "Generic Models 414:Generic Models 1:1506002" | material: "5/8" GYP. BD @ CEILING" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 423:Generic Models 1" | object type "Generic Models 423:Generic Models 1" | names: "Generic Models 423:Generic Models 1:1507139" | material: "7/8" FURRING CHANNELS @ 16" O.C." | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 424:Generic Models 1" | object type "Generic Models 424:Generic Models 1" | names: "Generic Models 424:Generic Models 1:1507163" | material: "7/8" FURRING CHANNELS @ 16" O.C." | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 425:Generic Models 1" | object type "Generic Models 425:Generic Models 1" | names: "Generic Models 425:Generic Models 1:1507183" | material: "7/8" FURRING CHANNELS @ 16" O.C." | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 428:Generic Models 1" | object type "Generic Models 428:Generic Models 1" | names: "Generic Models 428:Generic Models 1:1507428" | material: "R-19 BATT INSULATION" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Ground Rod:Ground Rod" | object type "Ground Rod:Ground Rod" | names: "Ground Rod:Ground Rod:1515191" | material: "5/8" x 8' GROUND ROD" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Light Pole Base Plate1:Light Pole Base Plate" | object type "Light Pole Base Plate1:Light Pole Base Plate" | names: "Light Pole Base Plate1:Light Pole Base Plate:1515308" | material: "(4) VERTICAL #6 REBAR" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Light Pole Base Plate2:Light Pole Base Plate" | object type "Light Pole Base Plate2:Light Pole Base Plate" | names: "Light Pole Base Plate2:Light Pole Base Plate:1516878" | material: "STEEL BASE PLATE" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 126:Walls 126" | object type "Walls 126:Walls 126" | names: "Walls 126:Walls 126:1518668" | material: "24" DIA. CONCRETE POLE BASE WITH THOROSEAL FINISH" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 127:Walls 126" | object type "Walls 127:Walls 126" | names: "Walls 127:Walls 126:1519197" | material: "Earth" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 500:Generic Models 1" | object type "Generic Models 500:Generic Models 1" | names: "Generic Models 500:Generic Models 1:1577429" | material: "STRUCTURAL FLOOR - SEE STRUCT. DWGS" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 11:Generic Models 1" | object type "Generic Models 11:Generic Models 1" | names: "Generic Models 11:Generic Models 1:1577503" | material: "STRUCTURAL FLOOR - SEE STRUCT. DWGS" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 28:Generic Models 1" | object type "Generic Models 28:Generic Models 1" | names: "Generic Models 28:Generic Models 1:1577522" | material: "STRUCTURAL FLOOR - SEE STRUCT. DWGS" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 238:Generic Models 1" | object type "Generic Models 238:Generic Models 1" | names: "Generic Models 238:Generic Models 1:1577541" | material: "STRUCTURAL FLOOR - SEE STRUCT. DWGS" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 446:Generic Models 1" | object type "Generic Models 446:Generic Models 1" | names: "Generic Models 446:Generic Models 1:1577560" | material: "STRUCTURAL FLOOR - SEE STRUCT. DWGS" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 26:Generic Models 1" | object type "Generic Models 26:Generic Models 1" | names: "Generic Models 26:Generic Models 1:1577677" | material: "OTHER WALL TYPE" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 514:Generic Models 1" | object type "Generic Models 514:Generic Models 1" | names: "Generic Models 514:Generic Models 1:1578074" | material: "STRUCTURAL FLOOR - SEE STRUCT. DWGS" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 537:Generic Models 1" | object type "Generic Models 537:Generic Models 1" | names: "Generic Models 537:Generic Models 1:1579530" | material: "STRUCTURAL FLOOR - SEE STRUCT. DWGS" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Light Pole Base Plate3:Light Pole Base Plate" | object type "Light Pole Base Plate3:Light Pole Base Plate" | names: "Light Pole Base Plate3:Light Pole Base Plate:1586248" | material: "1 1/2" GAVL. STEEL (RGS) CONDUIT" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Light Pole Base Plate4:Light Pole Base Plate" | object type "Light Pole Base Plate4:Light Pole Base Plate" | names: "Light Pole Base Plate4:Light Pole Base Plate:1586650" | material: "1 1/2" GAVL. STEEL (RGS) CONDUIT" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Model Text:OD_Very Large" | object type "Model Text:OD_Very Large" | names: "Model Text:OD_Very Large:1595839" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Model Text:OD_Very Large" | object type "Model Text:OD_Very Large" | names: "Model Text:OD_Very Large:1595840" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Model Text:OD_Very Large" | object type "Model Text:OD_Very Large" | names: "Model Text:OD_Very Large:1595841" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Model Text:OD_Very Large" | object type "Model Text:OD_Very Large" | names: "Model Text:OD_Very Large:1595842" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Model Text:OD_Very Large" | object type "Model Text:OD_Very Large" | names: "Model Text:OD_Very Large:1595843" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Model Text:OD_Very Large" | object type "Model Text:OD_Very Large" | names: "Model Text:OD_Very Large:1595992" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 44:Generic Models 1" | object type "Generic Models 44:Generic Models 1" | names: "Generic Models 44:Generic Models 1:1601268" | material: "OPEN WEB WOOD TRUSS" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 40:Generic Models 1" | object type "Generic Models 40:Generic Models 1" | names: "Generic Models 40:Generic Models 1:1601430" | material: "OPEN WEB WOOD TRUSS" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 45:Generic Models 1" | object type "Generic Models 45:Generic Models 1" | names: "Generic Models 45:Generic Models 1:1601478" | material: "OPEN WEB WOOD TRUSS" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 50:Generic Models 1" | object type "Generic Models 50:Generic Models 1" | names: "Generic Models 50:Generic Models 1:1601574" | material: "OPEN WEB WOOD TRUSS" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 54:Generic Models 1" | object type "Generic Models 54:Generic Models 1" | names: "Generic Models 54:Generic Models 1:1601706" | material: "OPEN WEB WOOD TRUSS" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 8:Generic Models 1" | object type "Generic Models 8:Generic Models 1" | names: "Generic Models 8:Generic Models 1:1622703" | material: "CONCRETE (3000 PSI CONCRETE)" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 141:Generic Models 1" | object type "Generic Models 141:Generic Models 1" | names: "Generic Models 141:Generic Models 1:1622735" | material: "#4 CONT. STEEL REBAR" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 144:Generic Models 1" | object type "Generic Models 144:Generic Models 1" | names: "Generic Models 144:Generic Models 1:1622740" | material: "#10 6x6 WIRE MESH" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 213:Generic Models 1" | object type "Generic Models 213:Generic Models 1" | names: "Generic Models 213:Generic Models 1:1633830" | material: "5/8" GYP. BD (SHALL BEAR THE UL CERTIFICATION MARK)" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 216:Generic Models 1" | object type "Generic Models 216:Generic Models 1" | names: "Generic Models 216:Generic Models 1:1633848" | material: "7/8" FURRING CHANNELS @ 16" O.C." | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 217:Generic Models 1" | object type "Generic Models 217:Generic Models 1" | names: "Generic Models 217:Generic Models 1:1633858" | material: "7/8" FURRING CHANNELS @ 16" O.C." | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 218:Generic Models 1" | object type "Generic Models 218:Generic Models 1" | names: "Generic Models 218:Generic Models 1:1633868" | material: "7/8" FURRING CHANNELS @ 12" O.C." | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 221:Generic Models 1" | object type "Generic Models 221:Generic Models 1" | names: "Generic Models 221:Generic Models 1:1633899" | material: "R-19 BATT INSULATION" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 223:Generic Models 1" | object type "Generic Models 223:Generic Models 1" | names: "Generic Models 223:Generic Models 1:1633925" | material: "OPEN WEB WOOD TRUSS" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 224:Generic Models 1" | object type "Generic Models 224:Generic Models 1" | names: "Generic Models 224:Generic Models 1:1633938" | material: "OPEN WEB WOOD TRUSS" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 225:Generic Models 1" | object type "Generic Models 225:Generic Models 1" | names: "Generic Models 225:Generic Models 1:1633951" | material: "OPEN WEB WOOD TRUSS" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 226:Generic Models 1" | object type "Generic Models 226:Generic Models 1" | names: "Generic Models 226:Generic Models 1:1633964" | material: "OPEN WEB WOOD TRUSS" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 229:Generic Models 1" | object type "Generic Models 229:Generic Models 1" | names: "Generic Models 229:Generic Models 1:1633990" | material: "OPEN WEB WOOD TRUSS" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 230:Generic Models 1" | object type "Generic Models 230:Generic Models 1" | names: "Generic Models 230:Generic Models 1:1634117" | material: "5/8" GYP. BD (SHALL BEAR THE UL CERTIFICATION MARK)" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 231:Generic Models 1" | object type "Generic Models 231:Generic Models 1" | names: "Generic Models 231:Generic Models 1:1634198" | material: "5/8" GYP. BD @ CEILING (SHALL BEAR THE UL CERTIFICATION MARK)" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 430:Generic Models 1" | object type "Generic Models 430:Generic Models 1" | names: "Generic Models 430:Generic Models 1:1651556" | material: "NOMINAL 3/4" THICK, 48" WIDE GYPSUM BOARD - SEE UL LISTING FOR ADDITIONAL INFORMATION" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 797:Generic Models 1" | object type "Generic Models 797:Generic Models 1" | names: "Generic Models 797:Generic Models 1:1651582" | material: "GLASS FIBER OR MINERAL WOOL INSULATION BEARING THE UL CLASSIFICATION MARKING AS TO SURFACE BURNING CHARACTERISTICS AND/OR FIRE RESISTANCE - SEE UL LISTING FOR ADDITIONAL INFORMATION - FILL CAVITY" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 431:Generic Models 1" | object type "Generic Models 431:Generic Models 1" | names: "Generic Models 431:Generic Models 1:1651595" | material: "FORMED FROM MIN. 25 MSG GALV. STEEL SPACED MAX 24" O.C. PERPENDICULAR TO JOISTS - SEE UL LISTING FOR ADDITIONAL INFORMATION" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 433:Generic Models 1" | object type "Generic Models 433:Generic Models 1" | names: "Generic Models 433:Generic Models 1:1651607" | material: "EXISTING - 2X WOOD JOISTS" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 796:Generic Models 1" | object type "Generic Models 796:Generic Models 1" | names: "Generic Models 796:Generic Models 1:1651622" | material: "RESILIENT SOUND ISOLATION ACCESSORY SHALL BE USED AT EACH ATTACHMENT POINT OF THE RESILIENT CHANNELS AND SPACED MAX 16" O.C. - SEE UL LISTING FOR ADDITIONAL INFORMATION" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 421:Generic Models 1" | object type "Generic Models 421:Generic Models 1" | names: "Generic Models 421:Generic Models 1:1651662" | material: "RESILIENT SOUND ISOLATION ACCESSORY SHALL BE USED AT EACH ATTACHMENT POINT OF THE RESILIENT CHANNELS AND SPACED MAX 16" O.C. - SEE UL LISTING FOR ADDITIONAL INFORMATION" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 422:Generic Models 1" | object type "Generic Models 422:Generic Models 1" | names: "Generic Models 422:Generic Models 1:1651685" | material: "RESILIENT SOUND ISOLATION ACCESSORY SHALL BE USED AT EACH ATTACHMENT POINT OF THE RESILIENT CHANNELS AND SPACED MAX 16" O.C. - SEE UL LISTING FOR ADDITIONAL INFORMATION" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 233:Generic Models 1" | object type "Generic Models 233:Generic Models 1" | names: "Generic Models 233:Generic Models 1:1651709" | material: "EXISTING - 2X WOOD JOISTS" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 234:Generic Models 1" | object type "Generic Models 234:Generic Models 1" | names: "Generic Models 234:Generic Models 1:1651722" | material: "EXISTING - 2X WOOD JOISTS" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 235:Generic Models 1" | object type "Generic Models 235:Generic Models 1" | names: "Generic Models 235:Generic Models 1:1651751" | material: "ACOUSTICAL MATERIAL - SEE UL LISTING FOR RANGE OF OPTIONS" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 237:Generic Models 1" | object type "Generic Models 237:Generic Models 1" | names: "Generic Models 237:Generic Models 1:1651777" | material: "GLASS FIBER OR MINERAL WOOL INSULATION BEARING THE UL CLASSIFICATION MARKING AS TO SURFACE BURNING CHARACTERISTICS AND/OR FIRE RESISTANCE - SEE UL LISTING FOR ADDITIONAL INFORMATION - FILL CAVITY" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 239:Generic Models 1" | object type "Generic Models 239:Generic Models 1" | names: "Generic Models 239:Generic Models 1:1651794" | material: "EXISTING - 2X WOOD JOISTS" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 240:Generic Models 1" | object type "Generic Models 240:Generic Models 1" | names: "Generic Models 240:Generic Models 1:1651807" | material: "EXISTING - 2X WOOD JOISTS" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 241:Generic Models 1" | object type "Generic Models 241:Generic Models 1" | names: "Generic Models 241:Generic Models 1:1651820" | material: "EXISTING - 2X WOOD JOISTS" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 244:Generic Models 1" | object type "Generic Models 244:Generic Models 1" | names: "Generic Models 244:Generic Models 1:1651835" | material: "GALV. STEEL WITH TOTAL AREA OF DUCT OPENING NOT TO EXCEED 113 SQ. IN. PER 100 SQ. FT. OF CEILING AREA, AREA OF INDIVIDUAL DUCT OPENING NOT TO EXCEED 113 SQ. IN. MAX. DIMENSION OF OPENING 12" - SEE UL ..." | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 249:Generic Models 1" | object type "Generic Models 249:Generic Models 1" | names: "Generic Models 249:Generic Models 1:1651856" | material: "NO. 12 SWG GALV. STEEL WIRE, SUPPORTED FROM 16D NAILS DRIVEN THROUGH WOOD JOISTS 5" FROM BOTTOM OF JOISTS AND BENT UPWARD AT BOTH ENDS FOR POSITIVE SUPPORT - SEE UL LISTING FOR ADDITIONAL INFORMATION" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 253:Generic Models 1" | object type "Generic Models 253:Generic Models 1" | names: "Generic Models 253:Generic Models 1:1651877" | material: "20" X 48"/60" OR 24" X 48" - MAX OF 16 SQ FT PER 100 SQ FT OF CEILING AREA - OR - INCANDESCENT LAMP TYPE 6.5" DIA. X 7-1/2" HIGH - (4) FIXTURES PER 100 SQ FT OF CEILING AREA (USE FIXTURE" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 254:Generic Models 1" | object type "Generic Models 254:Generic Models 1" | names: "Generic Models 254:Generic Models 1:1651918" | material: "EXISTING - FLOOR BRIDGING" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 255:Generic Models 1" | object type "Generic Models 255:Generic Models 1" | names: "Generic Models 255:Generic Models 1:1651932" | material: "NO. 12 SWG GALV. STEEL WIRE, SUPPORTED FROM 16D NAILS DRIVEN THROUGH WOOD JOISTS 5" FROM BOTTOM OF JOISTS AND BENT UPWARD AT BOTH ENDS FOR POSITIVE SUPPORT - SEE UL LISTING FOR ADDITIONAL INFORMATION" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 256:Generic Models 1" | object type "Generic Models 256:Generic Models 1" | names: "Generic Models 256:Generic Models 1:1651956" | material: "EXISTING - FLOOR BRIDGING" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 257:Generic Models 1" | object type "Generic Models 257:Generic Models 1" | names: "Generic Models 257:Generic Models 1:1651969" | material: "ACOUSTICAL MATERIAL - SEE UL LISTING FOR RANGE OF OPTIONS" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 258:Generic Models 1" | object type "Generic Models 258:Generic Models 1" | names: "Generic Models 258:Generic Models 1:1651985" | material: "NOM 2 BY 4 IN. INSTALLED BETWEEN AND PERPENDICULAR TO WOOD JOISTS, AND CENTERED 5 IN. BELOW SUBFLOORING." | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 259:Generic Models 1" | object type "Generic Models 259:Generic Models 1" | names: "Generic Models 259:Generic Models 1:1651998" | material: "NO. 12 SWG GALV. STEEL WIRE, SUPPORTED FROM 16D NAILS DRIVEN THROUGH WOOD JOISTS 5" FROM BOTTOM OF JOISTS AND BENT UPWARD AT BOTH ENDS FOR POSITIVE SUPPORT - SEE UL LISTING FOR ADDITIONAL INFORMATION" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 260:Generic Models 1" | object type "Generic Models 260:Generic Models 1" | names: "Generic Models 260:Generic Models 1:1652050" | material: "STEEL FRAMING MEMBERS - SEE UL LISTING FOR RANGE OF OPTIONS" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 261:Generic Models 1" | object type "Generic Models 261:Generic Models 1" | names: "Generic Models 261:Generic Models 1:1652062" | material: "FIXTURE PROTECTION (IF NON-RATED FIXTURE) - SEE UL LISTING FOR SPECIFICS" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 262:Generic Models 1" | object type "Generic Models 262:Generic Models 1" | names: "Generic Models 262:Generic Models 1:1652080" | material: "GYPSUM BOARD — 5/8" X 4 FT WIDE GYPSUM BOARD, INSTALLED WITH LONG DIMENSION PERPENDICULAR TO CROSS TEES WITH SIDE JOINTS CENTERED ALONG MAIN RUNNERS." | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 265:Generic Models 1" | object type "Generic Models 265:Generic Models 1" | names: "Generic Models 265:Generic Models 1:1652106" | material: "GLASS FIBER OR MINERAL WOOL INSULATION BEARING THE UL CLASSIFICATION MARKING AS TO SURFACE BURNING CHARACTERISTICS AND/OR FIRE RESISTANCE - SEE UL LISTING FOR ADDITIONAL INFORMATION - FILL CAVITY" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 266:Generic Models 1" | object type "Generic Models 266:Generic Models 1" | names: "Generic Models 266:Generic Models 1:1652123" | material: "EXISTING - 2X WOOD JOISTS" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 267:Generic Models 1" | object type "Generic Models 267:Generic Models 1" | names: "Generic Models 267:Generic Models 1:1652136" | material: "EXISTING - 2X WOOD JOISTS" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 268:Generic Models 1" | object type "Generic Models 268:Generic Models 1" | names: "Generic Models 268:Generic Models 1:1652149" | material: "EXISTING - 2X WOOD JOISTS" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 296:Generic Models 1" | object type "Generic Models 296:Generic Models 1" | names: "Generic Models 296:Generic Models 1:1652164" | material: "AIR DUCT — MIN 0.029 IN. THICK (22 GAUGE) GALV STEEL AIR DUCT. TOTAL AREA OF DUCT OPENINGS NOT TO EXCEED 114 SQ IN. PER EACH 100 SQ FT OF CEILING AREA." | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 302:Generic Models 1" | object type "Generic Models 302:Generic Models 1" | names: "Generic Models 302:Generic Models 1:1652185" | material: "NO. 12 SWG GALV. STEEL WIRE, SUPPORTED FROM 16D NAILS DRIVEN THROUGH WOOD JOISTS 5" FROM BOTTOM OF JOISTS AND BENT UPWARD AT BOTH ENDS FOR POSITIVE SUPPORT - SEE UL LISTING FOR ADDITIONAL INFORMATION" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 303:Generic Models 1" | object type "Generic Models 303:Generic Models 1" | names: "Generic Models 303:Generic Models 1:1652206" | material: "2' x 4' RECESSED LIGHT FIXTURE WITH STEEL HOUSING AND 'FIXTURE PROTECTION' - SPACED TO NOT EXCEED 24 SQ FT PER 100 SQ FT OF CEILING AREA - SEE UL LISTING FOR MORE INFORMATION" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 305:Generic Models 1" | object type "Generic Models 305:Generic Models 1" | names: "Generic Models 305:Generic Models 1:1652247" | material: "EXISTING - FLOOR BRIDGING" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 313:Generic Models 1" | object type "Generic Models 313:Generic Models 1" | names: "Generic Models 313:Generic Models 1:1652261" | material: "NO. 12 SWG GALV. STEEL WIRE, SUPPORTED FROM 16D NAILS DRIVEN THROUGH WOOD JOISTS 5" FROM BOTTOM OF JOISTS AND BENT UPWARD AT BOTH ENDS FOR POSITIVE SUPPORT - SEE UL LISTING FOR ADDITIONAL INFORMATION" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 314:Generic Models 1" | object type "Generic Models 314:Generic Models 1" | names: "Generic Models 314:Generic Models 1:1652285" | material: "EXISTING - FLOOR BRIDGING" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 315:Generic Models 1" | object type "Generic Models 315:Generic Models 1" | names: "Generic Models 315:Generic Models 1:1652301" | material: "NOM 2 BY 4 IN. INSTALLED BETWEEN AND PERPENDICULAR TO WOOD JOISTS, AND CENTERED 5 IN. BELOW SUBFLOORING." | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 316:Generic Models 1" | object type "Generic Models 316:Generic Models 1" | names: "Generic Models 316:Generic Models 1:1652314" | material: "NO. 12 SWG GALV. STEEL WIRE, SUPPORTED FROM 16D NAILS DRIVEN THROUGH WOOD JOISTS 5" FROM BOTTOM OF JOISTS AND BENT UPWARD AT BOTH ENDS FOR POSITIVE SUPPORT - SEE UL LISTING FOR ADDITIONAL INFORMATION" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 317:Generic Models 1" | object type "Generic Models 317:Generic Models 1" | names: "Generic Models 317:Generic Models 1:1652367" | material: "FIXTURE PROTECTION (IF NON-RATED FIXTURE) - SEE UL LISTING FOR SPECIFICS" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 318:Generic Models 1" | object type "Generic Models 318:Generic Models 1" | names: "Generic Models 318:Generic Models 1:1652390" | material: "STEEL FRAMING MEMBERS - SEE UL LISTING FOR RANGE OF OPTIONS" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 404:Generic Models 1" | object type "Generic Models 404:Generic Models 1" | names: "Generic Models 404:Generic Models 1:1659546" | material: "CONCRETE FOUNDATION - (SEE 'WALL TAG' FOR SIZE & REBAR)" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 321:Generic Models 1" | object type "Generic Models 321:Generic Models 1" | names: "Generic Models 321:Generic Models 1:1659594" | material: "WALL REINFORCING - SEE PLAN SCHEDULES FOR SIZE/LOCATION" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 322:Generic Models 1" | object type "Generic Models 322:Generic Models 1" | names: "Generic Models 322:Generic Models 1:1659680" | material: "BREAK EVERY OTHER REBAR AT JOINT (TOP AND BOTTOM REBAR TO BE CONT.)" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 319:Generic Models 1" | object type "Generic Models 319:Generic Models 1" | names: "Generic Models 319:Generic Models 1:1660588" | material: "3/4" DEEP NOTCH AT EACH SIDE OF WALL (SPACE APART - 25FT MIN.)" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 555:Generic Models 1" | object type "Generic Models 555:Generic Models 1" | names: "Generic Models 555:Generic Models 1:1713008" | material: "STRUCTURAL FLOOR - SEE STRUCT. DWGS" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 204:Generic Models 1" | object type "Generic Models 204:Generic Models 1" | names: "Generic Models 204:Generic Models 1:1773316" | material: "STRUCTURAL FLOOR - SEE STRUCT. DWGS" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 206:Generic Models 1" | object type "Generic Models 206:Generic Models 1" | names: "Generic Models 206:Generic Models 1:1773499" | material: "STRUCTURAL FLOOR - SEE STRUCT. DWGS" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 208:Generic Models 1" | object type "Generic Models 208:Generic Models 1" | names: "Generic Models 208:Generic Models 1:1773613" | material: "STRUCTURAL FLOOR - SEE STRUCT. DWGS" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 210:Generic Models 1" | object type "Generic Models 210:Generic Models 1" | names: "Generic Models 210:Generic Models 1:1773717" | material: "STRUCTURAL FLOOR - SEE STRUCT. DWGS" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 596:Generic Models 1" | object type "Generic Models 596:Generic Models 1" | names: "Generic Models 596:Generic Models 1:1818276" | material: "STRUCTURAL FLOOR - SEE STRUCT. DWGS" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 57:Generic Models 1" | object type "Generic Models 57:Generic Models 1" | names: "Generic Models 57:Generic Models 1:1824687" | material: "STRUCTURAL FLOOR - SEE STRUCT. DWGS" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 58:Generic Models 1" | object type "Generic Models 58:Generic Models 1" | names: "Generic Models 58:Generic Models 1:1824706" | material: "STRUCTURAL FLOOR - SEE STRUCT. DWGS" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 61:Generic Models 1" | object type "Generic Models 61:Generic Models 1" | names: "Generic Models 61:Generic Models 1:1848231" | material: "5/8" GYP. BD @ CEILING" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 63:Generic Models 1" | object type "Generic Models 63:Generic Models 1" | names: "Generic Models 63:Generic Models 1:1848259" | material: "7/8" FURRING CHANNELS @ 16" O.C." | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 68:Generic Models 1" | object type "Generic Models 68:Generic Models 1" | names: "Generic Models 68:Generic Models 1:1848300" | material: "FILL CAVITY WITH BATT INSULATION" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 70:Generic Models 1" | object type "Generic Models 70:Generic Models 1" | names: "Generic Models 70:Generic Models 1:1848326" | material: "OPEN WEB WOOD TRUSS" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 71:Generic Models 1" | object type "Generic Models 71:Generic Models 1" | names: "Generic Models 71:Generic Models 1:1848339" | material: "OPEN WEB WOOD TRUSS" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 72:Generic Models 1" | object type "Generic Models 72:Generic Models 1" | names: "Generic Models 72:Generic Models 1:1848352" | material: "OPEN WEB WOOD TRUSS" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 73:Generic Models 1" | object type "Generic Models 73:Generic Models 1" | names: "Generic Models 73:Generic Models 1:1848365" | material: "OPEN WEB WOOD TRUSS" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 211:Generic Models 1" | object type "Generic Models 211:Generic Models 1" | names: "Generic Models 211:Generic Models 1:1848391" | material: "OPEN WEB WOOD TRUSS" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 212:Generic Models 1" | object type "Generic Models 212:Generic Models 1" | names: "Generic Models 212:Generic Models 1:1848411" | material: "OPEN WEB WOOD TRUSS" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 214:Generic Models 1" | object type "Generic Models 214:Generic Models 1" | names: "Generic Models 214:Generic Models 1:1848424" | material: "OPEN WEB WOOD TRUSS" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 215:Generic Models 1" | object type "Generic Models 215:Generic Models 1" | names: "Generic Models 215:Generic Models 1:1848437" | material: "OPEN WEB WOOD TRUSS" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 345:Generic Models 1" | object type "Generic Models 345:Generic Models 1" | names: "Generic Models 345:Generic Models 1:1848797" | material: "5/8" GYP. BD" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 342:Generic Models 1" | object type "Generic Models 342:Generic Models 1" | names: "Generic Models 342:Generic Models 1:1848940" | material: "5/8" GYP. BD @ CEILING" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 64:Generic Models 1" | object type "Generic Models 64:Generic Models 1" | names: "Generic Models 64:Generic Models 1:1849353" | material: "CONDUIT/PIPE" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 344:Generic Models 1" | object type "Generic Models 344:Generic Models 1" | names: "Generic Models 344:Generic Models 1:1849507" | material: "DOUBLE 2X WOOD TOP PLATE" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 348:Generic Models 1" | object type "Generic Models 348:Generic Models 1" | names: "Generic Models 348:Generic Models 1:1849566" | material: "DOUBLE 2X WOOD TOP PLATE" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 351:Generic Models 1" | object type "Generic Models 351:Generic Models 1" | names: "Generic Models 351:Generic Models 1:1849596" | material: "DOUBLE 2X WOOD TOP PLATE" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 353:Generic Models 1" | object type "Generic Models 353:Generic Models 1" | names: "Generic Models 353:Generic Models 1:1849609" | material: "DOUBLE 2X WOOD TOP PLATE" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 354:Generic Models 1" | object type "Generic Models 354:Generic Models 1" | names: "Generic Models 354:Generic Models 1:1850205" | material: "3" CONCRETE TOPPING" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 387:Generic Models 1" | object type "Generic Models 387:Generic Models 1" | names: "Generic Models 387:Generic Models 1:1850257" | material: "PRECAST PLANK - SEE PRECAST SHOPS FOR SIZE" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 388:Generic Models 1" | object type "Generic Models 388:Generic Models 1" | names: "Generic Models 388:Generic Models 1:1850301" | material: "UL RATED FIRE STOP" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 389:Generic Models 1" | object type "Generic Models 389:Generic Models 1" | names: "Generic Models 389:Generic Models 1:1850411" | material: "SINGLE 2X WOOD SILL - TREATED IF CONCRETE" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 390:Generic Models 1" | object type "Generic Models 390:Generic Models 1" | names: "Generic Models 390:Generic Models 1:1850535" | material: "SINGLE 2X WOOD SILL - TREATED IF CONCRETE" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 391:Generic Models 1" | object type "Generic Models 391:Generic Models 1" | names: "Generic Models 391:Generic Models 1:1850568" | material: "2X WOOD STUDS BEYOND" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 392:Generic Models 1" | object type "Generic Models 392:Generic Models 1" | names: "Generic Models 392:Generic Models 1:1850653" | material: "2X WOOD STUDS BEYOND" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 399:Generic Models 1" | object type "Generic Models 399:Generic Models 1" | names: "Generic Models 399:Generic Models 1:1850846" | material: "7/8" FURRING CHANNELS @ 16" O.C." | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 62:Generic Models 1" | object type "Generic Models 62:Generic Models 1" | names: "Generic Models 62:Generic Models 1:1850876" | material: "7/8" FURRING CHANNELS @ 16" O.C." | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 400:Generic Models 1" | object type "Generic Models 400:Generic Models 1" | names: "Generic Models 400:Generic Models 1:1850894" | material: "7/8" FURRING CHANNELS @ 16" O.C." | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 401:Generic Models 1" | object type "Generic Models 401:Generic Models 1" | names: "Generic Models 401:Generic Models 1:1850912" | material: "CONDUIT/PIPE" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 405:Generic Models 1" | object type "Generic Models 405:Generic Models 1" | names: "Generic Models 405:Generic Models 1:1851094" | material: "UL RATED FIRE STOP" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 406:Generic Models 1" | object type "Generic Models 406:Generic Models 1" | names: "Generic Models 406:Generic Models 1:1851126" | material: "CONDUIT/PIPE" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 407:Generic Models 1" | object type "Generic Models 407:Generic Models 1" | names: "Generic Models 407:Generic Models 1:1851151" | material: "UL RATED FIRE STOP" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 409:Generic Models 1" | object type "Generic Models 409:Generic Models 1" | names: "Generic Models 409:Generic Models 1:1851602" | material: "FILL CAVITY WITH BATT INSULATION" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 352:Generic Models 1" | object type "Generic Models 352:Generic Models 1" | names: "Generic Models 352:Generic Models 1:1851677" | material: "5/8" GYP. BD" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 410:Generic Models 1" | object type "Generic Models 410:Generic Models 1" | names: "Generic Models 410:Generic Models 1:1851747" | material: "HATCHED AREA" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 411:Generic Models 1" | object type "Generic Models 411:Generic Models 1" | names: "Generic Models 411:Generic Models 1:1852408" | material: "FILL CAVITY WITH BATT INSULATION" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "Timber-Column:6x6" | object type "Timber-Column:6x6" | COLUMN | names: "Timber-Column:6x6:2169660" | material: profiles "6x6" ("6x6": "STRUCTURAL WOOD COLUMN - SIZE TBD") | property sets: Pset_ColumnCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "HSS-Round Hollow Structural Section-Column:HSS - 3.5" - SIZE TBD" | object type "HSS-Round Hollow Structural Section-Column:HSS - 3.5" - SIZE TBD" | COLUMN | names: "HSS-Round Hollow Structural Section-Column:HSS - 3.5" - SIZE TBD:2169678" | material: profiles "HSS - 3.5" - SIZE TBD" ("HSS - 3.5" - SIZE TBD": "STRUCTURAL STEEL COLUMN - SIZE TBD") | property sets: Pset_ColumnCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfColumn
          1 x IFCWALL | type IFCWALLTYPE "Basic Wall:W4BØD - (5/8 GYP - 2X4 WOOD(BATT) - 5/8 GYP)" | object type "Basic Wall:W4BØD - (5/8 GYP - 2X4 WOOD(BATT) - 5/8 GYP)" | names: "Basic Wall:W4BØD - (5/8 GYP - 2X4 WOOD(BATT) - 5/8 GYP):2236823" | material: layers "Basic Wall:W4BØD - (5/8 GYP - 2X4 WOOD(BATT) - 5/8 GYP)" ("5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" 0.0520833333333333, "2x6 STUDS 16" O.C. (R-19 BATT. INSULATION)" 0.291666666666667, "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" 0.0520833333333333) | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 561:Generic Models 1" | object type "Generic Models 561:Generic Models 1" | names: "Generic Models 561:Generic Models 1:2355825" | material: "STRUCTURAL FLOOR - SEE STRUCT. DWGS" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 453:Generic Models 1" | object type "Generic Models 453:Generic Models 1" | names: "Generic Models 453:Generic Models 1:2360995" | material: "STRUCTURAL FLOOR - SEE STRUCT. DWGS" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 502:Generic Models 1" | object type "Generic Models 502:Generic Models 1" | names: "Generic Models 502:Generic Models 1:2361008" | material: "OTHER WALL TYPE" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Compound Ceiling:GYP. BD - HUNG" | object type "Compound Ceiling:GYP. BD - HUNG" | CEILING | names: "Compound Ceiling:GYP. BD - HUNG:2575198" | material: layers "Compound Ceiling:GYP. BD - HUNG" ("CEILING GRID" 0.135416666666667, "5/8" GYP. BD" 0.0520833333333333) | property sets: Pset_CoveringCommon, Pset_EnvironmentalImpactIndicators
          2 x IFCLIGHTFIXTURE | type IFCLIGHTFIXTURETYPE "Troffer - 2x4 Parabolic:2' x 4' (2 Lamps)" | object type "Troffer - 2x4 Parabolic:2' x 4' (2 Lamps)" | names: "Troffer - 2x4 Parabolic:2' x 4' (2 Lamps):2575204", "Troffer - 2x4 Parabolic:2' x 4' (2 Lamps):2891963" | material: "<Unnamed>" | property sets: Pset_EnvironmentalImpactIndicators, Pset_LightFixtureTypeCommon
          2 x IFCLIGHTFIXTURE | type IFCLIGHTFIXTURETYPE "Troffer - 2x2 Parabolic:2' x 2' (2 Lamps)" | object type "Troffer - 2x2 Parabolic:2' x 2' (2 Lamps)" | names: "Troffer - 2x2 Parabolic:2' x 2' (2 Lamps):2575205", "Troffer - 2x2 Parabolic:2' x 2' (2 Lamps):2891964" | material: "<Unnamed>" | property sets: Pset_EnvironmentalImpactIndicators, Pset_LightFixtureTypeCommon
          2 x IFCLIGHTFIXTURE | type IFCLIGHTFIXTURETYPE "Troffer - Lens:2' x 4' (2 Lamps)" | object type "Troffer - Lens:2' x 4' (2 Lamps)" | names: "Troffer - Lens:2' x 4' (2 Lamps):2575206", "Troffer - Lens:2' x 4' (2 Lamps):2891965" | material: "<Unnamed>" | property sets: Pset_EnvironmentalImpactIndicators, Pset_LightFixtureTypeCommon
          1 x IFCLIGHTFIXTURE | type IFCLIGHTFIXTURETYPE "Ceiling - Linear Box:2' x 4' - 2 Lamp" | object type "Ceiling - Linear Box:2' x 4' - 2 Lamp" | names: "Ceiling - Linear Box:2' x 4' - 2 Lamp:2575207" | material: "<Unnamed>" | property sets: Pset_EnvironmentalImpactIndicators, Pset_LightFixtureTypeCommon
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Compound Ceiling:GYP. BD - HUNG" | object type "Compound Ceiling:GYP. BD - HUNG" | CEILING | names: "Compound Ceiling:GYP. BD - HUNG:2579780" | material: layers "Compound Ceiling:GYP. BD - HUNG" ("CEILING GRID" 0.135416666666667, "5/8" GYP. BD" 0.0520833333333333) | property sets: Pset_CoveringCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Compound Ceiling:GYP. BD - HUNG" | object type "Compound Ceiling:GYP. BD - HUNG" | CEILING | names: "Compound Ceiling:GYP. BD - HUNG:2579864" | material: layers "Compound Ceiling:GYP. BD - HUNG" ("CEILING GRID" 0.135416666666667, "5/8" GYP. BD" 0.0520833333333333) | property sets: Pset_CoveringCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Ceiling_Diffuser_-_Square_3882:24" x 24"" | object type "Ceiling_Diffuser_-_Square_3882:24" x 24"" | names: "Ceiling_Diffuser_-_Square_3882:24" x 24":2579870" | material: "<Unnamed>" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "211300 - Fire-Suppression Sprinkler Systems - Exposed Head:211300 - Fire-Suppression Sprinkler Systems - Exposed Head" | object type "211300 - Fire-Suppression Sprinkler Systems - Exposed Head:211300 - Fire-Suppression Sprinkler Systems - Exposed Head" | names: "211300 - Fire-Suppression Sprinkler Systems - Exposed Head:211300 - Fire-Suppression Sprinkler Systems - Exposed Head:2580784" | material: "EXISTING SPRINKLER HEADS TO REMAIN" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCLIGHTFIXTURE | type IFCLIGHTFIXTURETYPE "Lighting_Fixture-Lutron-Recessed-Finire-4in-Round-Downlight:Not a Type - Load Type Catalog" | object type "Lighting_Fixture-Lutron-Recessed-Finire-4in-Round-Downlight:Not a Type - Load Type Catalog" | names: "Lighting_Fixture-Lutron-Recessed-Finire-4in-Round-Downlight:Not a Type - Load Type Catalog:2580831" | material: constituents "MaterialConstituentSet" ("Steel - Lutron - Galvanized": "Steel - Lutron - Galvanized", "Steel - Lutron - Clear Bright Alzak": "Steel - Lutron - Clear Bright Alzak", "Steel - Lutron - Galvanized Black": "Steel - Lutron - Galvanized Black", "Steel - Lutron - Stainless Steel": "Steel - Lutron - Stainless Steel") | property sets: Pset_ElectricalDeviceCommon, Pset_EnvironmentalImpactIndicators, Pset_LightFixtureTypeCommon, Pset_ManufacturerTypeInformation
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 530:Generic Models 1" | object type "Generic Models 530:Generic Models 1" | names: "Generic Models 530:Generic Models 1:2713353" | material: "STRUCTURAL FLOOR - SEE STRUCT. DWGS" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 15:Walls 15" | object type "Walls 15:Walls 15" | names: "Walls 15:Walls 15:2891257" | material: "CONCRETE WALL" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 5:Walls 15" | object type "Walls 5:Walls 15" | names: "Walls 5:Walls 15:2891798" | material: "PLAM-1" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 6:Walls 15" | object type "Walls 6:Walls 15" | names: "Walls 6:Walls 15:2891858" | material: "PLAM-1" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 7:Walls 15" | object type "Walls 7:Walls 15" | names: "Walls 7:Walls 15:2891917" | material: "PLAM-1" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Compound Ceiling:GYP. BD - HUNG" | object type "Compound Ceiling:GYP. BD - HUNG" | CEILING | names: "Compound Ceiling:GYP. BD - HUNG:2891958" | material: layers "Compound Ceiling:GYP. BD - HUNG" ("CEILING GRID" 0.135416666666667, "5/8" GYP. BD" 0.0520833333333333) | property sets: Pset_CoveringCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCFLOWTERMINAL | type IFCDISTRIBUTIONELEMENTTYPE "224000 - Plumbing Fixtures - Water Closet - Generic:ADA" | object type "224000 - Plumbing Fixtures - Water Closet - Generic:ADA" | names: "224000 - Plumbing Fixtures - Water Closet - Generic:ADA:2892032" | material: constituents "MaterialConstituentSet" ("FLOOR MOUNTED TOILET": "FLOOR MOUNTED TOILET", "<Unnamed>": "<Unnamed>", "GRAB BARS - AT ADA RESTROOMS ONLY": "GRAB BARS - AT ADA RESTROOMS ONLY", "NAPKIN DIPENSER (IF WOMEN'S)": "NAPKIN DIPENSER (IF WOMEN'S)", "TOILET PAPER DISPENSER": "TOILET PAPER DISPENSER") | property sets: Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Walls 8:Walls 15" | object type "Walls 8:Walls 15" | names: "Walls 8:Walls 15:2892098" | material: constituents "MaterialConstituentSet" ("CONCRETE WALL": "CONCRETE WALL", "PLAM-1": "PLAM-1") | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Walls 9:Walls 15" | object type "Walls 9:Walls 15" | names: "Walls 9:Walls 15:2892149" | material: constituents "MaterialConstituentSet" ("CONCRETE WALL": "CONCRETE WALL", "PLAM-1": "PLAM-1") | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Walls 10:Walls 15" | object type "Walls 10:Walls 15" | names: "Walls 10:Walls 15:2892178" | material: constituents "MaterialConstituentSet" ("CONCRETE WALL": "CONCRETE WALL", "PLAM-1": "PLAM-1") | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCROOF | object type "Basic Roof:STANDING SEAM - FOAM - GYP" | names: "Basic Roof:STANDING SEAM - FOAM - GYP:3044596" | parts: 1 IFCSLAB | property sets: Pset_EnvironmentalImpactIndicators, Pset_RoofCommon
          1 x IFCROOF | object type "Basic Roof:STANDING SEAM - RAFTER" | names: "Basic Roof:STANDING SEAM - RAFTER:3045972" | parts: 1 IFCSLAB | property sets: Pset_EnvironmentalImpactIndicators, Pset_RoofCommon
          1 x IFCROOF | object type "Basic Roof:SHINGLES - FOAM - GYP" | names: "Basic Roof:SHINGLES - FOAM - GYP:3046033" | parts: 1 IFCSLAB | property sets: Pset_EnvironmentalImpactIndicators, Pset_RoofCommon
          1 x IFCROOF | object type "Basic Roof:SHINGLES - RAFTER" | names: "Basic Roof:SHINGLES - RAFTER:3046341" | parts: 1 IFCSLAB | property sets: Pset_EnvironmentalImpactIndicators, Pset_RoofCommon
          1 x IFCSLAB | type IFCSLABTYPE "Footing-Cylindrical:20"WX42"D" | object type "Footing-Cylindrical:20"WX42"D" | BASESLAB | names: "Footing-Cylindrical:20"WX42"D:4346499" | material: "CYLINDRICAL CONCRETE PIER - 20"Øx4'-0" - (4) # 4 VERTICALS - (3) #3 TIES @ 2" OC - REST @ 12" OC" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
      IFCBUILDINGSTOREY "1ST FLOOR" | long name "1ST FLOOR" | object type "Level:Project Base Point" | elevation 0.
        contains 1537 elements
          3 x IFCWALL | type IFCWALLTYPE "Basic Wall:GRADE BEAM - PERIMETER" | object type "Basic Wall:GRADE BEAM - PERIMETER" | names: "Basic Wall:GRADE BEAM - PERIMETER:340460", "Basic Wall:GRADE BEAM - PERIMETER:340461", "Basic Wall:GRADE BEAM - PERIMETER:637968" | material: layers "Basic Wall:GRADE BEAM - PERIMETER" ("CONCRETE GRADE BEAM POURED WITH CONCRETE SLAB - SEE STRUCT DWGS" 1.5) | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCFLOWTERMINAL | type IFCDISTRIBUTIONELEMENTTYPE "224000 - Plumbing Fixtures - Water Closet - Generic:ADA" | object type "224000 - Plumbing Fixtures - Water Closet - Generic:ADA" | names: "224000 - Plumbing Fixtures - Water Closet - Generic:ADA:395407" | material: constituents "MaterialConstituentSet" ("FLOOR MOUNTED TOILET": "FLOOR MOUNTED TOILET", "<Unnamed>": "<Unnamed>", "GRAB BARS - AT ADA RESTROOMS ONLY": "GRAB BARS - AT ADA RESTROOMS ONLY", "NAPKIN DIPENSER (IF WOMEN'S)": "NAPKIN DIPENSER (IF WOMEN'S)", "TOILET PAPER DISPENSER": "TOILET PAPER DISPENSER") | property sets: Pset_EnvironmentalImpactIndicators
          1 x IFCFLOWTERMINAL | type IFCDISTRIBUTIONELEMENTTYPE "Plbg-Sink Wall Mounted-UH:Sink" | object type "Plbg-Sink Wall Mounted-UH:Sink" | names: "Plbg-Sink Wall Mounted-UH:Sink:403462" | material: constituents "MaterialConstituentSet" ("<Unnamed>": "<Unnamed>", "BOTTLE TRAP": "BOTTLE TRAP", "FRAMELESS MIRROR": "FRAMELESS MIRROR", "SINK": "SINK") | property sets: Pset_EnvironmentalImpactIndicators
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 15:Generic Models 1" | object type "Generic Models 15:Generic Models 1" | names: "Generic Models 15:Generic Models 1:426780" | material: "METAL RUNNER CHANNEL; FASTEN @ 24" O.C." | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 17:Generic Models 1" | object type "Generic Models 17:Generic Models 1" | names: "Generic Models 17:Generic Models 1:426800" | material: "ACOUSTICAL SEALANT OR FIRE SEALANT, IF RATED WALL" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 20:Generic Models 1" | object type "Generic Models 20:Generic Models 1" | names: "Generic Models 20:Generic Models 1:426834" | material: "WALL BASE AS SCHEDULED" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 23:Generic Models 1" | object type "Generic Models 23:Generic Models 1" | names: "Generic Models 23:Generic Models 1:426865" | material: "DEEP LEG OF DEFLECTION TRACK (2" MIN. DEFLECTION)" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 24:Generic Models 1" | object type "Generic Models 24:Generic Models 1" | names: "Generic Models 24:Generic Models 1:426875" | material: "ACOUSTICAL SEALANT OR FIRE SEALANT, IF RATED WALL" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          15 x IFCWALL | type IFCWALLTYPE "Basic Wall:RATED - 0.5 HR" | object type "Basic Wall:RATED - 0.5 HR" | names: "Basic Wall:RATED - 0.5 HR:577630", "Basic Wall:RATED - 0.5 HR:2148277", "Basic Wall:RATED - 0.5 HR:2148281" (+12 more) | material: layers "Basic Wall:RATED - 0.5 HR" ("<Unnamed>" 0.666666666666667) | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          5 x IFCWALL | type IFCWALLTYPE "Basic Wall:RATED - 1 HR" | object type "Basic Wall:RATED - 1 HR" | names: "Basic Wall:RATED - 1 HR:578097", "Basic Wall:RATED - 1 HR:2168407", "Basic Wall:RATED - 1 HR:2168771" (+2 more) | material: layers "Basic Wall:RATED - 1 HR" ("Default Wall" 0.666666666666667) | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Basic Wall:RATED - 1.5 HR" | object type "Basic Wall:RATED - 1.5 HR" | names: "Basic Wall:RATED - 1.5 HR:578128" | material: layers "Basic Wall:RATED - 1.5 HR" ("<Unnamed>" 0.666666666666667) | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Basic Wall:RATED - 2 HR" | object type "Basic Wall:RATED - 2 HR" | names: "Basic Wall:RATED - 2 HR:578136" | material: layers "Basic Wall:RATED - 2 HR" ("<Unnamed>" 0.666666666666667) | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Basic Wall:RATED - 3 HR" | object type "Basic Wall:RATED - 3 HR" | names: "Basic Wall:RATED - 3 HR:578144" | material: layers "Basic Wall:RATED - 3 HR" ("<Unnamed>" 0.666666666666667) | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Basic Wall:RATED - 4 HR" | object type "Basic Wall:RATED - 4 HR" | names: "Basic Wall:RATED - 4 HR:578154" | material: layers "Basic Wall:RATED - 4 HR" ("<Unnamed>" 0.666666666666667) | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1:Generic Models 1" | object type "Generic Models 1:Generic Models 1" | names: "Generic Models 1:Generic Models 1:582123" | material: "2X WOOD SILL - TREATED IF ON CONCRETE" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 2:Generic Models 1" | object type "Generic Models 2:Generic Models 1" | names: "Generic Models 2:Generic Models 1:582133" | material: "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 3:Generic Models 1" | object type "Generic Models 3:Generic Models 1" | names: "Generic Models 3:Generic Models 1:582143" | material: "ACOUSTICAL SEALANT" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 5:Generic Models 1" | object type "Generic Models 5:Generic Models 1" | names: "Generic Models 5:Generic Models 1:582163" | material: "WALL BASE AS SCHEDULED" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 14:Generic Models 1" | object type "Generic Models 14:Generic Models 1" | names: "Generic Models 14:Generic Models 1:582243" | material: "CEILING TRACK AS SCHEDULED" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 41:Generic Models 1" | object type "Generic Models 41:Generic Models 1" | names: "Generic Models 41:Generic Models 1:582283" | material: "ACOUSTICAL SEALANT" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 42:Generic Models 1" | object type "Generic Models 42:Generic Models 1" | names: "Generic Models 42:Generic Models 1:582293" | material: "MATCH EXISTING BASE" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 49:Generic Models 1" | object type "Generic Models 49:Generic Models 1" | names: "Generic Models 49:Generic Models 1:582363" | material: "CEILING AS SCHEDULED" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 52:Generic Models 65" | object type "Generic Models 52:Generic Models 65" | names: "Generic Models 52:Generic Models 65:587734" | material: "2X WOOD STUD" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 19:Generic Models 65" | object type "Generic Models 19:Generic Models 65" | names: "Generic Models 19:Generic Models 65:588926" | material: "METAL STUD" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          5 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Egress - Path of Travel:Egress - Path of Travel" | object type "Egress - Path of Travel:Egress - Path of Travel" | names: "Egress - Path of Travel:Egress - Path of Travel:593791", "Egress - Path of Travel:Egress - Path of Travel:593830", "Egress - Path of Travel:Egress - Path of Travel:2149321" (+2 more) | material: "<Unnamed>" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 122:Generic Models 1" | object type "Generic Models 122:Generic Models 1" | names: "Generic Models 122:Generic Models 1:609975" | material: "TOP METAL STUD TRACK" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 128:Generic Models 1" | object type "Generic Models 128:Generic Models 1" | names: "Generic Models 128:Generic Models 1:609985" | material: "STRUCTURAL DECK" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 132:Generic Models 1" | object type "Generic Models 132:Generic Models 1" | names: "Generic Models 132:Generic Models 1:610005" | material: "METAL STUD - (SEE 'WALL TAG' & 'LAYER MATERIAL SCHEDULE' FOR SIZE, SPACING, & INSULATION)" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 134:Generic Models 1" | object type "Generic Models 134:Generic Models 1" | names: "Generic Models 134:Generic Models 1:610015" | material: "CEILING TRACK TO MATCH EXISTING" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 136:Generic Models 1" | object type "Generic Models 136:Generic Models 1" | names: "Generic Models 136:Generic Models 1:610020" | material: "METAL RUNNER CHANNEL; FASTEN @ 24" O.C." | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 142:Generic Models 1" | object type "Generic Models 142:Generic Models 1" | names: "Generic Models 142:Generic Models 1:610035" | material: "CEILING TRACK TO MATCH EXISTING" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 143:Generic Models 1" | object type "Generic Models 143:Generic Models 1" | names: "Generic Models 143:Generic Models 1:610045" | material: "CEILING AS SCHEDULED" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 146:Generic Models 1" | object type "Generic Models 146:Generic Models 1" | names: "Generic Models 146:Generic Models 1:610055" | material: "CEILING AS SCHEDULED" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 147:Generic Models 65" | object type "Generic Models 147:Generic Models 65" | names: "Generic Models 147:Generic Models 65:610068" | material: "METAL STUD (16" O.C.)" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 149:Generic Models 1" | object type "Generic Models 149:Generic Models 1" | names: "Generic Models 149:Generic Models 1:610088" | material: "ALUM. STOREFRONT W/ TEMPERED SINGLE GLAZING" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 83:Generic Models 1" | object type "Generic Models 83:Generic Models 1" | names: "Generic Models 83:Generic Models 1:610098" | material: "DEEP LEG OF DEFLECTION TRACK (2" MIN. DEFLECTION)" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 94:Generic Models 65" | object type "Generic Models 94:Generic Models 65" | names: "Generic Models 94:Generic Models 65:610108" | material: "DIAGONAL BRACING AS NECESSARY - ATTACH TO STRUCTURAL DECK" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 97:Generic Models 46" | object type "Generic Models 97:Generic Models 46" | names: "Generic Models 97:Generic Models 46:610121" | material: "BLOCKING - SIZE AS NEC." | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 98:Generic Models 1" | object type "Generic Models 98:Generic Models 1" | names: "Generic Models 98:Generic Models 1:610131" | material: "SEALANT (W/ BACKER ROD IF NECESSARY)" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 124:Generic Models 1" | object type "Generic Models 124:Generic Models 1" | names: "Generic Models 124:Generic Models 1:610141" | material: "SEALANT (W/ BACKER ROD IF NECESSARY)" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 126:Generic Models 46" | object type "Generic Models 126:Generic Models 46" | names: "Generic Models 126:Generic Models 46:610159" | material: "BLOCKING - SIZE AS NEC." | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 135:Generic Models 1" | object type "Generic Models 135:Generic Models 1" | names: "Generic Models 135:Generic Models 1:610170" | material: "SEALANT (W/ BACKER ROD IF NECESSARY)" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 137:Generic Models 1" | object type "Generic Models 137:Generic Models 1" | names: "Generic Models 137:Generic Models 1:610180" | material: "SEALANT (W/ BACKER ROD IF NECESSARY)" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 138:Generic Models 1" | object type "Generic Models 138:Generic Models 1" | names: "Generic Models 138:Generic Models 1:637141" | material: "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 16:Generic Models 1" | object type "Generic Models 16:Generic Models 1" | names: "Generic Models 16:Generic Models 1:637269" | material: "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Basic Wall:M6RØD - (6" CMU)" | object type "Basic Wall:M6RØD - (6" CMU)" | names: "Basic Wall:M6RØD - (6" CMU):638762" | material: layers "Basic Wall:M6RØD - (6" CMU)" ("CMU (SEE 'WALL TAG' FOR SIZE)" 0.46875) | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Basic Wall:FURR - W2CØFA - (5/8 GYP - 2X2 WOOD)" | object type "Basic Wall:FURR - W2CØFA - (5/8 GYP - 2X2 WOOD)" | names: "Basic Wall:FURR - W2CØFA - (5/8 GYP - 2X2 WOOD):639323" | material: layers "Basic Wall:FURR - W2CØFA - (5/8 GYP - 2X2 WOOD)" ("2X WOOD STUD" 0.125, "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" 0.0520833333333333) | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Basic Wall:FURR - W2EØFD - (5/8 GYP - 2X2 WOOD(RIGID INSULATION))" | object type "Basic Wall:FURR - W2EØFD - (5/8 GYP - 2X2 WOOD(RIGID INSULATION))" | names: "Basic Wall:FURR - W2EØFD - (5/8 GYP - 2X2 WOOD(RIGID INSULATION)):639326" | material: layers "Basic Wall:FURR - W2EØFD - (5/8 GYP - 2X2 WOOD(RIGID INSULATION))" ("2X WOOD STUDS W/ RIGID INSULATION" 0.125, "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" 0.0520833333333333) | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 34:Generic Models 1" | object type "Generic Models 34:Generic Models 1" | names: "Generic Models 34:Generic Models 1:828799" | material: "2X WOOD SILL - TREATED IF ON CONCRETE" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 43:Generic Models 65" | object type "Generic Models 43:Generic Models 65" | names: "Generic Models 43:Generic Models 65:829101" | material: "2X6s WOOD JOISTS - 16" O.C." | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 46:Generic Models 1" | object type "Generic Models 46:Generic Models 1" | names: "Generic Models 46:Generic Models 1:829188" | material: "1/2" CDX PLYWOOD" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 51:Generic Models 1" | object type "Generic Models 51:Generic Models 1" | names: "Generic Models 51:Generic Models 1:829284" | material: "VINYL SIDING OVER AIR & MOISTURE BARRIER" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 140:Generic Models 1" | object type "Generic Models 140:Generic Models 1" | names: "Generic Models 140:Generic Models 1:829357" | material: "2x6 STUDS 16" O.C. (R-19 BATT. INSULATION)" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 139:Generic Models 1" | object type "Generic Models 139:Generic Models 1" | names: "Generic Models 139:Generic Models 1:829521" | material: "#4 CONT. STEEL REBAR" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 152:Generic Models 1" | object type "Generic Models 152:Generic Models 1" | names: "Generic Models 152:Generic Models 1:833476" | material: "1/2" GYP. BD" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 153:Generic Models 1" | object type "Generic Models 153:Generic Models 1" | names: "Generic Models 153:Generic Models 1:852181" | material: "SILL PLATE GASKET" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 181:Generic Models 65" | object type "Generic Models 181:Generic Models 65" | names: "Generic Models 181:Generic Models 65:854445" | material: "HORIZONTAL 1X6 CEDAR PLANKS W/ CLEAR WOOD SEALER" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 154:Generic Models 1" | object type "Generic Models 154:Generic Models 1" | names: "Generic Models 154:Generic Models 1:855166" | material: "VERTICAL 1X6 CEDAR PLANKS W/ CLEAR WOOD SEALER" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 158:Generic Models 1" | object type "Generic Models 158:Generic Models 1" | names: "Generic Models 158:Generic Models 1:855467" | material: "VERTICAL 1X6 CEDAR PLANKS W/ CLEAR WOOD SEALER" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 159:Generic Models 1" | object type "Generic Models 159:Generic Models 1" | names: "Generic Models 159:Generic Models 1:855498" | material: "VERTICAL 1X6 CEDAR PLANKS W/ CLEAR WOOD SEALER" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 160:Generic Models 1" | object type "Generic Models 160:Generic Models 1" | names: "Generic Models 160:Generic Models 1:855513" | material: "VERTICAL 1X6 CEDAR PLANKS W/ CLEAR WOOD SEALER" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 161:Generic Models 1" | object type "Generic Models 161:Generic Models 1" | names: "Generic Models 161:Generic Models 1:855528" | material: "VERTICAL 1X6 CEDAR PLANKS W/ CLEAR WOOD SEALER" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 162:Generic Models 1" | object type "Generic Models 162:Generic Models 1" | names: "Generic Models 162:Generic Models 1:855543" | material: "VERTICAL 1X6 CEDAR PLANKS W/ CLEAR WOOD SEALER" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 163:Generic Models 1" | object type "Generic Models 163:Generic Models 1" | names: "Generic Models 163:Generic Models 1:855558" | material: "VERTICAL 1X6 CEDAR PLANKS W/ CLEAR WOOD SEALER" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 164:Generic Models 1" | object type "Generic Models 164:Generic Models 1" | names: "Generic Models 164:Generic Models 1:855573" | material: "VERTICAL 1X6 CEDAR PLANKS W/ CLEAR WOOD SEALER" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 165:Generic Models 1" | object type "Generic Models 165:Generic Models 1" | names: "Generic Models 165:Generic Models 1:855588" | material: "VERTICAL 1X6 CEDAR PLANKS W/ CLEAR WOOD SEALER" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 166:Generic Models 1" | object type "Generic Models 166:Generic Models 1" | names: "Generic Models 166:Generic Models 1:855603" | material: "VERTICAL 1X6 CEDAR PLANKS W/ CLEAR WOOD SEALER" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 167:Generic Models 1" | object type "Generic Models 167:Generic Models 1" | names: "Generic Models 167:Generic Models 1:855618" | material: "VERTICAL 1X6 CEDAR PLANKS W/ CLEAR WOOD SEALER" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 168:Generic Models 1" | object type "Generic Models 168:Generic Models 1" | names: "Generic Models 168:Generic Models 1:855633" | material: "VERTICAL 1X6 CEDAR PLANKS W/ CLEAR WOOD SEALER" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 169:Generic Models 1" | object type "Generic Models 169:Generic Models 1" | names: "Generic Models 169:Generic Models 1:855648" | material: "VERTICAL 1X6 CEDAR PLANKS W/ CLEAR WOOD SEALER" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 170:Generic Models 1" | object type "Generic Models 170:Generic Models 1" | names: "Generic Models 170:Generic Models 1:855663" | material: "VERTICAL 1X6 CEDAR PLANKS W/ CLEAR WOOD SEALER" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 171:Generic Models 1" | object type "Generic Models 171:Generic Models 1" | names: "Generic Models 171:Generic Models 1:855678" | material: "VERTICAL 1X6 CEDAR PLANKS W/ CLEAR WOOD SEALER" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 172:Generic Models 1" | object type "Generic Models 172:Generic Models 1" | names: "Generic Models 172:Generic Models 1:855693" | material: "VERTICAL 1X6 CEDAR PLANKS W/ CLEAR WOOD SEALER" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 173:Generic Models 1" | object type "Generic Models 173:Generic Models 1" | names: "Generic Models 173:Generic Models 1:855708" | material: "VERTICAL 1X6 CEDAR PLANKS W/ CLEAR WOOD SEALER" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 174:Generic Models 1" | object type "Generic Models 174:Generic Models 1" | names: "Generic Models 174:Generic Models 1:855723" | material: "VERTICAL 1X6 CEDAR PLANKS W/ CLEAR WOOD SEALER" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 175:Generic Models 1" | object type "Generic Models 175:Generic Models 1" | names: "Generic Models 175:Generic Models 1:855738" | material: "VERTICAL 1X6 CEDAR PLANKS W/ CLEAR WOOD SEALER" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 176:Generic Models 1" | object type "Generic Models 176:Generic Models 1" | names: "Generic Models 176:Generic Models 1:855753" | material: "VERTICAL 1X6 CEDAR PLANKS W/ CLEAR WOOD SEALER" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 179:Generic Models 1" | object type "Generic Models 179:Generic Models 1" | names: "Generic Models 179:Generic Models 1:855824" | material: "VERTICAL 1X6 CEDAR PLANKS W/ CLEAR WOOD SEALER" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 180:Generic Models 65" | object type "Generic Models 180:Generic Models 65" | names: "Generic Models 180:Generic Models 65:856122" | material: "HORIZONTAL 1X6 CEDAR PLANKS W/ CLEAR WOOD SEALER" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 197:Generic Models 1" | object type "Generic Models 197:Generic Models 1" | names: "Generic Models 197:Generic Models 1:1181065" | material: "2X BLOCKING - LOCATED AT GRAB BARS, WALL HUNG CABINETS, ETC.)" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCBEAM | type IFCBEAMTYPE "Dimension Lumber - Canted Ends:2x8" | object type "Dimension Lumber - Canted Ends:2x8" | BEAM | names: "Dimension Lumber - Canted Ends:2x8:1232599" | material: profiles "2x8" ("2x8": "PRE-ENGINEERED TRUSS @ 24" O.C.") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "Dimension Lumber - Truncated:2x8" | object type "Dimension Lumber - Truncated:2x8" | BEAM | names: "Dimension Lumber - Truncated:2x8:1234426" | material: profiles "2x8" ("2x8": "Softwood, Lumber - hortz") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCCURTAINWALL | type IFCCURTAINWALLTYPE "Curtain Wall:FRAMELESS GLASS" | object type "Curtain Wall:FRAMELESS GLASS" | names: "Curtain Wall:FRAMELESS GLASS:1235803" | parts: 10 IFCMEMBER, 5 IFCPLATE | property sets: Pset_CurtainWallCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCCURTAINWALL | type IFCCURTAINWALLTYPE "Curtain Wall:EMPTY - PANEL" | object type "Curtain Wall:EMPTY - PANEL" | names: "Curtain Wall:EMPTY - PANEL:1235913" | parts: 22 IFCMEMBER | property sets: Pset_CurtainWallCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCCURTAINWALL | type IFCCURTAINWALLTYPE "Curtain Wall:POLYCARBONATE WALL" | object type "Curtain Wall:POLYCARBONATE WALL" | names: "Curtain Wall:POLYCARBONATE WALL:1237256" | parts: 4 IFCMEMBER, 1 IFCCURTAINWALL | property sets: Pset_CurtainWallCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCFURNITURE | type IFCFURNITURETYPE "OD_CW_Closet:OD_CW_Closet" | object type "OD_CW_Closet:OD_CW_Closet" | names: "OD_CW_Closet:OD_CW_Closet:1245669" | material: "CASEWORK" | property sets: Pset_EnvironmentalImpactIndicators, Pset_FurnitureTypeCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "A_Revit_Suv_3d_car_5231:A_Revit_Suv_3d_car_5231" | object type "A_Revit_Suv_3d_car_5231:A_Revit_Suv_3d_car_5231" | names: "A_Revit_Suv_3d_car_5231:A_Revit_Suv_3d_car_5231:1284122" | material: constituents "MaterialConstituentSet" ("dark gray": "dark gray", "Tire": "Tire", "Wheel": "Wheel", "Red Light": "Red Light", "yellow": "yellow", "NEW WINDOWS THROUGHOUT": "NEW WINDOWS THROUGHOUT", "white": "white", "blue": "blue", "r-suv1 body": "r-suv1 body") | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Land_Rover_Evoque_-_SUV_Car_Vehicle_Automobile_13067:Land_Rover_Evoque_-_SUV_Car_Vehicle_Automobile_13067" | object type "Land_Rover_Evoque_-_SUV_Car_Vehicle_Automobile_13067:Land_Rover_Evoque_-_SUV_Car_Vehicle_Automobile_13067" | names: "Land_Rover_Evoque_-_SUV_Car_Vehicle_Automobile_13067:Land_Rover_Evoque_-_SUV_Car_Vehicle_Automobile_13067:1284194" | material: "<Unnamed>" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          8 x IFCWALL | type IFCWALLTYPE "Basic Wall:W4BØD - (5/8 GYP - 2X4 WOOD(BATT) - 5/8 GYP)" | object type "Basic Wall:W4BØD - (5/8 GYP - 2X4 WOOD(BATT) - 5/8 GYP)" | names: "Basic Wall:W4BØD - (5/8 GYP - 2X4 WOOD(BATT) - 5/8 GYP):1314187", "Basic Wall:W4BØD - (5/8 GYP - 2X4 WOOD(BATT) - 5/8 GYP):2168577", "Basic Wall:W4BØD - (5/8 GYP - 2X4 WOOD(BATT) - 5/8 GYP):2170693" (+5 more) | material: layers "Basic Wall:W4BØD - (5/8 GYP - 2X4 WOOD(BATT) - 5/8 GYP)" ("5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" 0.0520833333333333, "2x6 STUDS 16" O.C. (R-19 BATT. INSULATION)" 0.291666666666667, "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" 0.0520833333333333) | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 272:Generic Models 263" | object type "Generic Models 272:Generic Models 263" | names: "Generic Models 272:Generic Models 263:1384116" | material: "1.50" ASPHALT SURFACE COURSE (E-0.3)" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 273:Generic Models 263" | object type "Generic Models 273:Generic Models 263" | names: "Generic Models 273:Generic Models 263:1384314" | material: "INSTALL TACK COAT PER WDOT SPECIFICATIONS IF LAYERS ARE NOT INSTALLED AT THE SAME TIME" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 263:Generic Models 263" | object type "Generic Models 263:Generic Models 263" | names: "Generic Models 263:Generic Models 263:1384500" | material: "1.50" ASPHALT BINDER COURSE (E-0.3)" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 288:Generic Models 263" | object type "Generic Models 288:Generic Models 263" | names: "Generic Models 288:Generic Models 263:1387393" | material: "7" CONC. SIDE WALK, IF PRESENT (SEE SITE PLAN)" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 304:Generic Models 263" | object type "Generic Models 304:Generic Models 263" | names: "Generic Models 304:Generic Models 263:1396625" | material: "1" EXPANSION JOINT" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 308:Generic Models 263" | object type "Generic Models 308:Generic Models 263" | names: "Generic Models 308:Generic Models 263:1400384" | material: "MEDIUM BROOM FINISH" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 312:Generic Models 263" | object type "Generic Models 312:Generic Models 263" | names: "Generic Models 312:Generic Models 263:1402220" | material: "SEE SITE PLAN FOR LANDSCAPING" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 285:Generic Models 263" | object type "Generic Models 285:Generic Models 263" | names: "Generic Models 285:Generic Models 263:1403728" | material: "SEE SITE PLAN FOR LANDSCAPING" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          2 x IFCBEAM | type IFCBEAMTYPE "061100 - Wood Framing:2x10 - RIM JOIST" | object type "061100 - Wood Framing:2x10 - RIM JOIST" | BEAM | names: "061100 - Wood Framing:2x10 - RIM JOIST:1417680", "061100 - Wood Framing:2x10 - RIM JOIST:1417684" | material: profiles "2x10 - RIM JOIST" ("2x10 - RIM JOIST": "TREATED 2X10 RIM JOIST") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "061100 - Wood Framing:2x10 - RIM JOIST" | object type "061100 - Wood Framing:2x10 - RIM JOIST" | BEAM | names: "061100 - Wood Framing:2x10 - RIM JOIST:1417686" | material: profiles "2x10 - RIM JOIST" ("2x10 - RIM JOIST": "TREATED 2X10 RIM JOIST") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          3 x IFCBEAM | type IFCBEAMTYPE "061100 - Wood Framing:2x10 - BEAM" | object type "061100 - Wood Framing:2x10 - BEAM" | BEAM | names: "061100 - Wood Framing:2x10 - BEAM:1417749", "061100 - Wood Framing:2x10 - BEAM:1417751", "061100 - Wood Framing:2x10 - BEAM:1430713" | material: profiles "2x10 - BEAM" ("2x10 - BEAM": "(3) SISTERED 2X10s AT BEAM") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "061100 - Wood Framing:2x10 - LEDGER" | object type "061100 - Wood Framing:2x10 - LEDGER" | BEAM | names: "061100 - Wood Framing:2x10 - LEDGER:1417846" | material: profiles "2x10 - LEDGER" ("2x10 - LEDGER": "TREATED 2X10 RIM JOIST") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          2 x IFCBEAM | type IFCBEAMTYPE "Dimension Lumber - Canted Ends:6x6 - LATERAL BRACING" | object type "Dimension Lumber - Canted Ends:6x6 - LATERAL BRACING" | BEAM | names: "Dimension Lumber - Canted Ends:6x6 - LATERAL BRACING:1427857", "Dimension Lumber - Canted Ends:6x6 - LATERAL BRACING:1431593" | material: profiles "6x6 - LATERAL BRACING" ("6x6 - LATERAL BRACING": "6X6 TREATED LATERAL BRACE") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          2 x IFCBEAM | type IFCBEAMTYPE "Dimension Lumber - Canted Ends:6x6 - LATERAL BRACING" | object type "Dimension Lumber - Canted Ends:6x6 - LATERAL BRACING" | BEAM | names: "Dimension Lumber - Canted Ends:6x6 - LATERAL BRACING:1431474", "Dimension Lumber - Canted Ends:6x6 - LATERAL BRACING:1431531" | material: profiles "6x6 - LATERAL BRACING" ("6x6 - LATERAL BRACING": "6X6 TREATED LATERAL BRACE") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 285:Generic Models 263" | object type "Generic Models 285:Generic Models 263" | names: "Generic Models 285:Generic Models 263:1451950" | material: "SEE SITE PLAN FOR LANDSCAPING" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 356:Generic Models 65" | object type "Generic Models 356:Generic Models 65" | names: "Generic Models 356:Generic Models 65:1460408" | material: "MORTAR JOINT" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 360:Generic Models 65" | object type "Generic Models 360:Generic Models 65" | names: "Generic Models 360:Generic Models 65:1460526" | material: "MORTAR JOINT" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 366:Generic Models 65" | object type "Generic Models 366:Generic Models 65" | names: "Generic Models 366:Generic Models 65:1460740" | material: "MORTAR JOINT" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 384:Generic Models 1" | object type "Generic Models 384:Generic Models 1" | names: "Generic Models 384:Generic Models 1:1461889" | material: "STRUCTURAL DECK" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Continuous Angle1:Continuous Angle" | object type "Continuous Angle1:Continuous Angle" | names: "Continuous Angle1:Continuous Angle:1463390" | material: "L6X4X1/2 W/ 4" SLOT IN VERT. LOG FOR KWIK BOLT CENTER IN BLOCK (1/2" DIA. KWIK BOLT EXPANSION ANCHOR 2.25" EMBEDMENT AT 4FT O.C.)" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Dowel:Dowel" | object type "Dowel:Dowel" | names: "Dowel:Dowel:1463972" | material: "6" CMU WALL W/#4 VERT. BARS AT 32" O.C. (TYP.)" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Dowel1:Dowel" | object type "Dowel1:Dowel" | names: "Dowel1:Dowel:1464093" | material: "6" CMU WALL W/#4 VERT. BARS AT 32" O.C. (TYP.)" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCFURNITURE | type IFCFURNITURETYPE "Entertainment_Center_14771:Entertainment_Center_14771" | object type "Entertainment_Center_14771:Entertainment_Center_14771" | names: "Entertainment_Center_14771:Entertainment_Center_14771:1465371" | material: constituents "MaterialConstituentSet" ("TV - Black": "TV - Black", "TV - Glass": "TV - Glass", "SOLID CORE WOOD DOOR": "SOLID CORE WOOD DOOR") | property sets: Pset_EnvironmentalImpactIndicators, Pset_FurnitureTypeCommon
          1 x IFCFURNITURE | type IFCFURNITURETYPE "Couch-Both_Arms-Generic:1" | object type "Couch-Both_Arms-Generic:1" | names: "Couch-Both_Arms-Generic:1:1465372" | material: "<Unnamed>" | property sets: Pset_EnvironmentalImpactIndicators, Pset_FurnitureTypeCommon, Pset_ManufacturerTypeInformation
          1 x IFCFURNITURE | type IFCFURNITURETYPE "Table-Coffee:one" | object type "Table-Coffee:one" | names: "Table-Coffee:one:1465373" | material: "_WOOD" | property sets: Pset_EnvironmentalImpactIndicators, Pset_FurnitureTypeCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 426:Generic Models 1" | object type "Generic Models 426:Generic Models 1" | names: "Generic Models 426:Generic Models 1:1507267" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 427:Generic Models 1" | object type "Generic Models 427:Generic Models 1" | names: "Generic Models 427:Generic Models 1:1507317" | material: "SOUND MAT" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 429:Generic Models 1" | object type "Generic Models 429:Generic Models 1" | names: "Generic Models 429:Generic Models 1:1507517" | material: "3/4" GYP. CRETE" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Pole:Pole" | object type "Pole:Pole" | names: "Pole:Pole:1510851" | material: "STEEL LIGHT POLE" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Light Pole Base Plate:Light Pole Base Plate" | object type "Light Pole Base Plate:Light Pole Base Plate" | names: "Light Pole Base Plate:Light Pole Base Plate:1510904" | material: "STEEL BASE PLATE" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "321723 - Pavement Markings - Parking - Angled:PARKING" | object type "321723 - Pavement Markings - Parking - Angled:PARKING" | names: "321723 - Pavement Markings - Parking - Angled:PARKING:1529638" | material: constituents "MaterialConstituentSet" ("<Unnamed>": "<Unnamed>", "ADA AISLE": "ADA AISLE") | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCWALL | type IFCWALLTYPE "Basic Wall:W6BØD - (5/8 GYP - 2X6 WOOD(BATT) - 5/8 GYP)" | object type "Basic Wall:W6BØD - (5/8 GYP - 2X6 WOOD(BATT) - 5/8 GYP)" | names: "Basic Wall:W6BØD - (5/8 GYP - 2X6 WOOD(BATT) - 5/8 GYP):1535833" | material: layers "Basic Wall:W6BØD - (5/8 GYP - 2X6 WOOD(BATT) - 5/8 GYP)" ("5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" 0.0520833333333333, "2x6 STUDS 16" O.C. (R-19 BATT. INSULATION)" 0.458333333333333, "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" 0.0520833333333333) | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Basic Wall:W8BØD - (5/8 GYP - 2X8 WOOD(BATT) - 5/8 GYP)" | object type "Basic Wall:W8BØD - (5/8 GYP - 2X8 WOOD(BATT) - 5/8 GYP)" | names: "Basic Wall:W8BØD - (5/8 GYP - 2X8 WOOD(BATT) - 5/8 GYP):1539141" | material: layers "Basic Wall:W8BØD - (5/8 GYP - 2X8 WOOD(BATT) - 5/8 GYP)" ("5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" 0.0520833333333333, "2x6 STUDS 16" O.C. (R-19 BATT. INSULATION)" 0.604166666666667, "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" 0.0520833333333333) | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 32:Generic Models 1" | object type "Generic Models 32:Generic Models 1" | names: "Generic Models 32:Generic Models 1:1563609" | material: "WALL BASE AS SCHEDULED" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 287:Generic Models 65" | object type "Generic Models 287:Generic Models 65" | names: "Generic Models 287:Generic Models 65:1564528" | material: "MORTAR JOINT" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 293:Generic Models 65" | object type "Generic Models 293:Generic Models 65" | names: "Generic Models 293:Generic Models 65:1565394" | material: "MORTAR JOINT" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 346:Generic Models 65" | object type "Generic Models 346:Generic Models 65" | names: "Generic Models 346:Generic Models 65:1565428" | material: "MORTAR JOINT" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 350:Generic Models 65" | object type "Generic Models 350:Generic Models 65" | names: "Generic Models 350:Generic Models 65:1565497" | material: "MORTAR JOINT" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 355:Generic Models 65" | object type "Generic Models 355:Generic Models 65" | names: "Generic Models 355:Generic Models 65:1565531" | material: "MORTAR JOINT" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 358:Generic Models 1" | object type "Generic Models 358:Generic Models 1" | names: "Generic Models 358:Generic Models 1:1566354" | material: "STANDARD 9-GAUGE (MW11), LADDER-SHAPED WIRE FABRICATED WITH BUTT-WELDED CROSS-RODS SPACED 406-MM (16-IN.) ON CENTER (OC)" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 155:Generic Models 1" | object type "Generic Models 155:Generic Models 1" | names: "Generic Models 155:Generic Models 1:1566670" | material: "DOUBLE 2X WOOD TOP PLATE" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 157:Generic Models 1" | object type "Generic Models 157:Generic Models 1" | names: "Generic Models 157:Generic Models 1:1566688" | material: "METAL STUD - (SEE 'WALL TAG' & 'LAYER MATERIAL SCHEDULE' FOR SIZE, SPACING, & INSULATION)" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 18:Generic Models 1" | object type "Generic Models 18:Generic Models 1" | names: "Generic Models 18:Generic Models 1:1566854" | material: "2x6 STUDS 16" O.C. (R-19 BATT. INSULATION)" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 6:Generic Models 1" | object type "Generic Models 6:Generic Models 1" | names: "Generic Models 6:Generic Models 1:1566942" | material: "DOUBLE 2X WOOD TOP PLATE" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 10:Generic Models 1" | object type "Generic Models 10:Generic Models 1" | names: "Generic Models 10:Generic Models 1:1567002" | material: "ACOUSTICAL SEALANT" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 12:Generic Models 1" | object type "Generic Models 12:Generic Models 1" | names: "Generic Models 12:Generic Models 1:1567081" | material: "ACOUSTICAL SEALANT" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 9:Generic Models 1" | object type "Generic Models 9:Generic Models 1" | names: "Generic Models 9:Generic Models 1:1567282" | material: "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 13:Generic Models 1" | object type "Generic Models 13:Generic Models 1" | names: "Generic Models 13:Generic Models 1:1567312" | material: "2X WOOD SILL - TREATED IF ON CONCRETE" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 25:Generic Models 1" | object type "Generic Models 25:Generic Models 1" | names: "Generic Models 25:Generic Models 1:1567317" | material: "5/8" GYP. BD" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 228:Generic Models 1" | object type "Generic Models 228:Generic Models 1" | names: "Generic Models 228:Generic Models 1:1567337" | material: "WALL BASE AS SCHEDULED" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 243:Generic Models 1" | object type "Generic Models 243:Generic Models 1" | names: "Generic Models 243:Generic Models 1:1567367" | material: "ATTACH GYPSUM BOARD TO STUDS AND NOT TO TOP TRACK" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 245:Generic Models 1" | object type "Generic Models 245:Generic Models 1" | names: "Generic Models 245:Generic Models 1:1567372" | material: "METAL RUNNER CHANNEL; FASTEN @ 24" O.C." | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 246:Generic Models 1" | object type "Generic Models 246:Generic Models 1" | names: "Generic Models 246:Generic Models 1:1567387" | material: "ACOUSTICAL SEALANT" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 247:Generic Models 1" | object type "Generic Models 247:Generic Models 1" | names: "Generic Models 247:Generic Models 1:1567397" | material: "MATCH EXISTING BASE" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 248:Generic Models 1" | object type "Generic Models 248:Generic Models 1" | names: "Generic Models 248:Generic Models 1:1567407" | material: "ATTACH GYPSUM BOARD TO STUDS AND NOT TO TOP TRACK" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 359:Generic Models 1" | object type "Generic Models 359:Generic Models 1" | names: "Generic Models 359:Generic Models 1:1567464" | material: "DOUBLE 2X WOOD TOP PLATE" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 361:Generic Models 1" | object type "Generic Models 361:Generic Models 1" | names: "Generic Models 361:Generic Models 1:1567469" | material: "2x6 STUDS 16" O.C. (R-19 BATT. INSULATION)" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 364:Generic Models 1" | object type "Generic Models 364:Generic Models 1" | names: "Generic Models 364:Generic Models 1:1567501" | material: "DOUBLE 2X WOOD TOP PLATE" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 365:Generic Models 1" | object type "Generic Models 365:Generic Models 1" | names: "Generic Models 365:Generic Models 1:1567512" | material: "CONTINUOUS FIRE RATED SEALANT EACH SIDE." | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 368:Generic Models 1" | object type "Generic Models 368:Generic Models 1" | names: "Generic Models 368:Generic Models 1:1567528" | material: "WOOD STRUCTURAL PANEL (WSP) - SEE STRUCT DWGS" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 370:Generic Models 1" | object type "Generic Models 370:Generic Models 1" | names: "Generic Models 370:Generic Models 1:1567562" | material: "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 371:Generic Models 1" | object type "Generic Models 371:Generic Models 1" | names: "Generic Models 371:Generic Models 1:1567595" | material: "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 373:Generic Models 1" | object type "Generic Models 373:Generic Models 1" | names: "Generic Models 373:Generic Models 1:1567700" | material: "CONTINUOUS FIRE RATED SEALANT EACH SIDE." | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 367:Generic Models 1" | object type "Generic Models 367:Generic Models 1" | names: "Generic Models 367:Generic Models 1:1567716" | material: "CONTINUOUS FIRE RATED SEALANT EACH SIDE." | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 374:Generic Models 1" | object type "Generic Models 374:Generic Models 1" | names: "Generic Models 374:Generic Models 1:1567726" | material: "CONTINUOUS FIRE RATED SEALANT EACH SIDE." | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 375:Generic Models 1" | object type "Generic Models 375:Generic Models 1" | names: "Generic Models 375:Generic Models 1:1567753" | material: "CONTINUOUS FIRE RATED SEALANT EACH SIDE." | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 376:Generic Models 1" | object type "Generic Models 376:Generic Models 1" | names: "Generic Models 376:Generic Models 1:1567763" | material: "CONTINUOUS FIRE RATED SEALANT EACH SIDE." | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 377:Generic Models 1" | object type "Generic Models 377:Generic Models 1" | names: "Generic Models 377:Generic Models 1:1567773" | material: "CONTINUOUS FIRE RATED SEALANT EACH SIDE." | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 378:Generic Models 1" | object type "Generic Models 378:Generic Models 1" | names: "Generic Models 378:Generic Models 1:1567783" | material: "CONTINUOUS FIRE RATED SEALANT EACH SIDE." | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 29:Generic Models 1" | object type "Generic Models 29:Generic Models 1" | names: "Generic Models 29:Generic Models 1:1567832" | material: "25 GA. RESILIENT CHANNEL - 24" O.C." | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 362:Generic Models 1" | object type "Generic Models 362:Generic Models 1" | names: "Generic Models 362:Generic Models 1:1568068" | material: "LADDER TRUSS - SEE STRUCT DWGS" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 380:Generic Models 1" | object type "Generic Models 380:Generic Models 1" | names: "Generic Models 380:Generic Models 1:1568122" | material: "2X WOOD STUD" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 252:Generic Models 1" | object type "Generic Models 252:Generic Models 1" | names: "Generic Models 252:Generic Models 1:1568456" | material: "LADDER TRUSS - SEE STRUCT DWGS" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 379:Generic Models 1" | object type "Generic Models 379:Generic Models 1" | names: "Generic Models 379:Generic Models 1:1568544" | material: "LADDER TRUSS - SEE STRUCT DWGS" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 382:Generic Models 1" | object type "Generic Models 382:Generic Models 1" | names: "Generic Models 382:Generic Models 1:1568585" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 381:Generic Models 1" | object type "Generic Models 381:Generic Models 1" | names: "Generic Models 381:Generic Models 1:1568658" | material: "2X WOOD SILL" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 383:Generic Models 1" | object type "Generic Models 383:Generic Models 1" | names: "Generic Models 383:Generic Models 1:1568679" | material: "1" GYP. CRETE" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 385:Generic Models 1" | object type "Generic Models 385:Generic Models 1" | names: "Generic Models 385:Generic Models 1:1568750" | material: "1" GYP. CRETE" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 434:Generic Models 1" | object type "Generic Models 434:Generic Models 1" | names: "Generic Models 434:Generic Models 1:1568846" | material: "5/8" GYP. BD @ CEILING" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 436:Generic Models 1" | object type "Generic Models 436:Generic Models 1" | names: "Generic Models 436:Generic Models 1:1568967" | material: "WOOD TRUSS - SEE STRUCT DWGS" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 437:Generic Models 1" | object type "Generic Models 437:Generic Models 1" | names: "Generic Models 437:Generic Models 1:1568984" | material: "WOOD TRUSS - SEE STRUCT DWGS" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 438:Generic Models 1" | object type "Generic Models 438:Generic Models 1" | names: "Generic Models 438:Generic Models 1:1569050" | material: "2X NAILER" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 439:Generic Models 1" | object type "Generic Models 439:Generic Models 1" | names: "Generic Models 439:Generic Models 1:1569101" | material: "2X NAILER" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 440:Generic Models 1" | object type "Generic Models 440:Generic Models 1" | names: "Generic Models 440:Generic Models 1:1569136" | material: "WOOD TRUSS - SEE STRUCT DWGS" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 441:Generic Models 1" | object type "Generic Models 441:Generic Models 1" | names: "Generic Models 441:Generic Models 1:1569178" | material: "25 GA. RESILIENT CHANNEL - 24" O.C." | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 442:Generic Models 1" | object type "Generic Models 442:Generic Models 1" | names: "Generic Models 442:Generic Models 1:1569205" | material: "METAL STUD - (SEE 'WALL TAG' & 'LAYER MATERIAL SCHEDULE' FOR SIZE, SPACING, & INSULATION)" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 443:Generic Models 1" | object type "Generic Models 443:Generic Models 1" | names: "Generic Models 443:Generic Models 1:1569271" | material: "25 GA. RESILIENT CHANNEL - 24" O.C." | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 372:Generic Models 1" | object type "Generic Models 372:Generic Models 1" | names: "Generic Models 372:Generic Models 1:1569322" | material: "5/8" GYP. BD @ CEILING" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 435:Generic Models 1" | object type "Generic Models 435:Generic Models 1" | names: "Generic Models 435:Generic Models 1:1569461" | material: "2X WOOD SILL - TREATED IF ON CONCRETE" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 444:Generic Models 1" | object type "Generic Models 444:Generic Models 1" | names: "Generic Models 444:Generic Models 1:1569466" | material: "5/8" GYP. BD" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 445:Generic Models 1" | object type "Generic Models 445:Generic Models 1" | names: "Generic Models 445:Generic Models 1:1569476" | material: "WALL BASE AS SCHEDULED" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 449:Generic Models 1" | object type "Generic Models 449:Generic Models 1" | names: "Generic Models 449:Generic Models 1:1569511" | material: "METAL RUNNER CHANNEL; FASTEN @ 24" O.C." | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 450:Generic Models 1" | object type "Generic Models 450:Generic Models 1" | names: "Generic Models 450:Generic Models 1:1569526" | material: "ACOUSTICAL SEALANT" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 451:Generic Models 1" | object type "Generic Models 451:Generic Models 1" | names: "Generic Models 451:Generic Models 1:1569536" | material: "MATCH EXISTING BASE" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 456:Generic Models 1" | object type "Generic Models 456:Generic Models 1" | names: "Generic Models 456:Generic Models 1:1569594" | material: "2x6 STUDS 16" O.C. (R-19 BATT. INSULATION)" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 457:Generic Models 1" | object type "Generic Models 457:Generic Models 1" | names: "Generic Models 457:Generic Models 1:1569615" | material: "DOUBLE 2X WOOD TOP PLATE" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 460:Generic Models 1" | object type "Generic Models 460:Generic Models 1" | names: "Generic Models 460:Generic Models 1:1569645" | material: "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 461:Generic Models 1" | object type "Generic Models 461:Generic Models 1" | names: "Generic Models 461:Generic Models 1:1569658" | material: "1/2" GYP. BD. OR FINISH PLYWOOD (SEE INTERIOR ELEVATIONS)" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 465:Generic Models 1" | object type "Generic Models 465:Generic Models 1" | names: "Generic Models 465:Generic Models 1:1569706" | material: "CONTINUOUS FIRE RATED SEALANT EACH SIDE." | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 466:Generic Models 1" | object type "Generic Models 466:Generic Models 1" | names: "Generic Models 466:Generic Models 1:1569716" | material: "CONTINUOUS FIRE RATED SEALANT EACH SIDE." | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 467:Generic Models 1" | object type "Generic Models 467:Generic Models 1" | names: "Generic Models 467:Generic Models 1:1569726" | material: "CONTINUOUS FIRE RATED SEALANT EACH SIDE." | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 468:Generic Models 1" | object type "Generic Models 468:Generic Models 1" | names: "Generic Models 468:Generic Models 1:1569736" | material: "CONTINUOUS FIRE RATED SEALANT EACH SIDE." | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 469:Generic Models 1" | object type "Generic Models 469:Generic Models 1" | names: "Generic Models 469:Generic Models 1:1569746" | material: "25 GA. RESILIENT CHANNEL - 24" O.C." | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 471:Generic Models 1" | object type "Generic Models 471:Generic Models 1" | names: "Generic Models 471:Generic Models 1:1569762" | material: "2X WOOD STUD" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 475:Generic Models 1" | object type "Generic Models 475:Generic Models 1" | names: "Generic Models 475:Generic Models 1:1569824" | material: "2X WOOD SILL" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 476:Generic Models 1" | object type "Generic Models 476:Generic Models 1" | names: "Generic Models 476:Generic Models 1:1569829" | material: "19"/32" FINISH GRADE PLYWOOD" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 477:Generic Models 1" | object type "Generic Models 477:Generic Models 1" | names: "Generic Models 477:Generic Models 1:1569842" | material: "1" GYP. CRETE" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 478:Generic Models 1" | object type "Generic Models 478:Generic Models 1" | names: "Generic Models 478:Generic Models 1:1569855" | material: "2X WOOD STUD" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 486:Generic Models 1" | object type "Generic Models 486:Generic Models 1" | names: "Generic Models 486:Generic Models 1:1569950" | material: "WOOD TRUSS FLOOR ASSEMBLY - (FILL CAVITY W/ CELLULOSE BLOWN-IN INSULATION) (UL - L521 FLOOR ASSEMBLY)" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 487:Generic Models 1" | object type "Generic Models 487:Generic Models 1" | names: "Generic Models 487:Generic Models 1:1569974" | material: "25 GA. RESILIENT CHANNEL - 24" O.C." | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 488:Generic Models 1" | object type "Generic Models 488:Generic Models 1" | names: "Generic Models 488:Generic Models 1:1569981" | material: "5/8" GYP. BD @ CEILING" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 459:Generic Models 1" | object type "Generic Models 459:Generic Models 1" | names: "Generic Models 459:Generic Models 1:1570040" | material: "5/8" GYP. BD" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 489:Generic Models 1" | object type "Generic Models 489:Generic Models 1" | names: "Generic Models 489:Generic Models 1:1571359" | material: "3.5" X 6" LVLs - 32" O.C. - EXPOSED - NO WOOD STAMPS - SEE STRUCT FOR DEPTH" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 490:Generic Models 1" | object type "Generic Models 490:Generic Models 1" | names: "Generic Models 490:Generic Models 1:1571399" | material: "3.5" X 6" LVLs BLOCKING BETWEEN LVL JOISTS" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 491:Generic Models 1" | object type "Generic Models 491:Generic Models 1" | names: "Generic Models 491:Generic Models 1:1571538" | material: "SOUND MAT" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 492:Generic Models 1" | object type "Generic Models 492:Generic Models 1" | names: "Generic Models 492:Generic Models 1:1571583" | material: "19"/32" OSB PLYWOOD BONDED W/ EXT. GLUE" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 474:Generic Models 1" | object type "Generic Models 474:Generic Models 1" | names: "Generic Models 474:Generic Models 1:1571647" | material: "19"/32" OSB PLYWOOD BONDED W/ EXT. GLUE - NO STAMPS - EXPOSED TO FINISH SPACE" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 470:Generic Models 1" | object type "Generic Models 470:Generic Models 1" | names: "Generic Models 470:Generic Models 1:1571758" | material: "WOOD TRUSS - SEE STRUCT DWGS" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 493:Generic Models 1" | object type "Generic Models 493:Generic Models 1" | names: "Generic Models 493:Generic Models 1:1571806" | material: "LVL RIM BOARD - SEE STRUCT. DWGS" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 472:Generic Models 1" | object type "Generic Models 472:Generic Models 1" | names: "Generic Models 472:Generic Models 1:1571883" | material: "WOOD TRUSS - SEE STRUCT DWGS" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 473:Generic Models 1" | object type "Generic Models 473:Generic Models 1" | names: "Generic Models 473:Generic Models 1:1571933" | material: "WOOD TRUSS - SEE STRUCT DWGS" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 448:Generic Models 1" | object type "Generic Models 448:Generic Models 1" | names: "Generic Models 448:Generic Models 1:1572049" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 452:Generic Models 1" | object type "Generic Models 452:Generic Models 1" | names: "Generic Models 452:Generic Models 1:1572213" | material: "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 458:Generic Models 1" | object type "Generic Models 458:Generic Models 1" | names: "Generic Models 458:Generic Models 1:1572226" | material: "5/8" GYP. BD" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 462:Generic Models 1" | object type "Generic Models 462:Generic Models 1" | names: "Generic Models 462:Generic Models 1:1572298" | material: "5/8" GYP. BD" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 463:Generic Models 1" | object type "Generic Models 463:Generic Models 1" | names: "Generic Models 463:Generic Models 1:1572311" | material: "1/2" GYP. BD. OR FINISH PLYWOOD (SEE INTERIOR ELEVATIONS)" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 464:Generic Models 1" | object type "Generic Models 464:Generic Models 1" | names: "Generic Models 464:Generic Models 1:1572359" | material: "25 GA. RESILIENT CHANNEL - 24" O.C." | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 455:Generic Models 1" | object type "Generic Models 455:Generic Models 1" | names: "Generic Models 455:Generic Models 1:1572450" | material: "DOUBLE 2X WOOD TOP PLATE" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 479:Generic Models 1" | object type "Generic Models 479:Generic Models 1" | names: "Generic Models 479:Generic Models 1:1572503" | material: "25 GA. RESILIENT CHANNEL - 24" O.C." | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 480:Generic Models 1" | object type "Generic Models 480:Generic Models 1" | names: "Generic Models 480:Generic Models 1:1572521" | material: "SOUND MAT" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 481:Generic Models 1" | object type "Generic Models 481:Generic Models 1" | names: "Generic Models 481:Generic Models 1:1572564" | material: "FLOOR FINISH T.B.D" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 482:Generic Models 1" | object type "Generic Models 482:Generic Models 1" | names: "Generic Models 482:Generic Models 1:1572617" | material: "WALL BASE AS SCHEDULED" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 483:Generic Models 1" | object type "Generic Models 483:Generic Models 1" | names: "Generic Models 483:Generic Models 1:1572641" | material: "WALL BASE AS SCHEDULED" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 484:Generic Models 1" | object type "Generic Models 484:Generic Models 1" | names: "Generic Models 484:Generic Models 1:1572705" | material: "CONTINUOUS FIRE RATED SEALANT EACH SIDE." | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 485:Generic Models 1" | object type "Generic Models 485:Generic Models 1" | names: "Generic Models 485:Generic Models 1:1572715" | material: "CONTINUOUS FIRE RATED SEALANT EACH SIDE." | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 494:Generic Models 1" | object type "Generic Models 494:Generic Models 1" | names: "Generic Models 494:Generic Models 1:1572795" | material: "CONTINUOUS FIRE RATED SEALANT EACH SIDE." | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 495:Generic Models 1" | object type "Generic Models 495:Generic Models 1" | names: "Generic Models 495:Generic Models 1:1572805" | material: "CONTINUOUS FIRE RATED SEALANT EACH SIDE." | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 496:Generic Models 1" | object type "Generic Models 496:Generic Models 1" | names: "Generic Models 496:Generic Models 1:1574821" | material: "METAL STUD - (SEE 'WALL TAG' & 'LAYER MATERIAL SCHEDULE' FOR SIZE, SPACING, & INSULATION)" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 21:Generic Models 1" | object type "Generic Models 21:Generic Models 1" | names: "Generic Models 21:Generic Models 1:1575228" | material: "WOOD TRUSS FLOOR ASSEMBLY - (FILL CAVITY W/ CELLULOSE BLOWN-IN INSULATION) (UL - L521 FLOOR ASSEMBLY)" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 35:Generic Models 1" | object type "Generic Models 35:Generic Models 1" | names: "Generic Models 35:Generic Models 1:1575271" | material: "WOOD TRUSS FLOOR ASSEMBLY - (FILL CAVITY W/ CELLULOSE BLOWN-IN INSULATION) (UL - L521 FLOOR ASSEMBLY)" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 36:Generic Models 1" | object type "Generic Models 36:Generic Models 1" | names: "Generic Models 36:Generic Models 1:1576960" | material: "2X WOOD SILL - TREATED IF ON CONCRETE" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 67:Generic Models 1" | object type "Generic Models 67:Generic Models 1" | names: "Generic Models 67:Generic Models 1:1576965" | material: "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 242:Generic Models 1" | object type "Generic Models 242:Generic Models 1" | names: "Generic Models 242:Generic Models 1:1576975" | material: "ACOUSTICAL SEALANT" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 251:Generic Models 1" | object type "Generic Models 251:Generic Models 1" | names: "Generic Models 251:Generic Models 1:1576985" | material: "WALL BASE AS SCHEDULED" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 454:Generic Models 1" | object type "Generic Models 454:Generic Models 1" | names: "Generic Models 454:Generic Models 1:1577005" | material: "CEILING TRACK AS SCHEDULED" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 503:Generic Models 1" | object type "Generic Models 503:Generic Models 1" | names: "Generic Models 503:Generic Models 1:1577075" | material: "CEILING AS SCHEDULED" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 504:Generic Models 65" | object type "Generic Models 504:Generic Models 65" | names: "Generic Models 504:Generic Models 65:1577086" | material: "2X WOOD STUD" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 505:Generic Models 1" | object type "Generic Models 505:Generic Models 1" | names: "Generic Models 505:Generic Models 1:1577112" | material: "DOUBLE 2X WOOD TOP PLATE" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 506:Generic Models 1" | object type "Generic Models 506:Generic Models 1" | names: "Generic Models 506:Generic Models 1:1577117" | material: "2x6 STUDS 16" O.C. (R-19 BATT. INSULATION)" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 508:Generic Models 1" | object type "Generic Models 508:Generic Models 1" | names: "Generic Models 508:Generic Models 1:1577149" | material: "DOUBLE 2X WOOD TOP PLATE" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 509:Generic Models 1" | object type "Generic Models 509:Generic Models 1" | names: "Generic Models 509:Generic Models 1:1577160" | material: "ACOUSTICAL SEALANT" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 499:Generic Models 1" | object type "Generic Models 499:Generic Models 1" | names: "Generic Models 499:Generic Models 1:1577281" | material: "UNDERSIDE OF FLOOR ASSEMBLY - SEE STRUCT. DWGS" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 7:Generic Models 1" | object type "Generic Models 7:Generic Models 1" | names: "Generic Models 7:Generic Models 1:1577398" | material: "UNDERSIDE OF FLOOR ASSEMBLY - SEE STRUCT. DWGS" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 447:Generic Models 1" | object type "Generic Models 447:Generic Models 1" | names: "Generic Models 447:Generic Models 1:1577634" | material: "UNDERSIDE OF FLOOR ASSEMBLY - SEE STRUCT. DWGS" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 501:Generic Models 65" | object type "Generic Models 501:Generic Models 65" | names: "Generic Models 501:Generic Models 65:1577857" | material: "MORTAR JOINT" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 507:Generic Models 65" | object type "Generic Models 507:Generic Models 65" | names: "Generic Models 507:Generic Models 65:1577891" | material: "MORTAR JOINT" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 511:Generic Models 65" | object type "Generic Models 511:Generic Models 65" | names: "Generic Models 511:Generic Models 65:1577960" | material: "MORTAR JOINT" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 512:Generic Models 65" | object type "Generic Models 512:Generic Models 65" | names: "Generic Models 512:Generic Models 65:1577994" | material: "MORTAR JOINT" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 513:Generic Models 1" | object type "Generic Models 513:Generic Models 1" | names: "Generic Models 513:Generic Models 1:1578028" | material: "STRUCTURAL DECK" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Continuous Angle2:Continuous Angle" | object type "Continuous Angle2:Continuous Angle" | names: "Continuous Angle2:Continuous Angle:1578039" | material: "3" X 3" X 8" L. CLIP ANGLES @ 4'-0" O.C. MECH. FASTENED TO UNDERSIDE OF STRUCTURE OR SLAB - BOTH SIDES OF WALL" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Continuous Angle3:Continuous Angle" | object type "Continuous Angle3:Continuous Angle" | names: "Continuous Angle3:Continuous Angle:1578050" | material: "3" X 3" X 8" L. CLIP ANGLES @ 4'-0" O.C. MECH. FASTENED TO UNDERSIDE OF STRUCTURE OR SLAB - BOTH SIDES OF WALL" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 515:Generic Models 65" | object type "Generic Models 515:Generic Models 65" | names: "Generic Models 515:Generic Models 65:1578102" | material: "MORTAR JOINT" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 516:Generic Models 65" | object type "Generic Models 516:Generic Models 65" | names: "Generic Models 516:Generic Models 65:1578139" | material: "MORTAR JOINT" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 517:Generic Models 65" | object type "Generic Models 517:Generic Models 65" | names: "Generic Models 517:Generic Models 65:1578173" | material: "MORTAR JOINT" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 519:Generic Models 65" | object type "Generic Models 519:Generic Models 65" | names: "Generic Models 519:Generic Models 65:1578242" | material: "MORTAR JOINT" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 520:Generic Models 65" | object type "Generic Models 520:Generic Models 65" | names: "Generic Models 520:Generic Models 65:1578276" | material: "MORTAR JOINT" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 521:Generic Models 1" | object type "Generic Models 521:Generic Models 1" | names: "Generic Models 521:Generic Models 1:1578306" | material: "STANDARD 9-GAUGE (MW11), LADDER-SHAPED WIRE FABRICATED WITH BUTT-WELDED CROSS-RODS SPACED 406-MM (16-IN.) ON CENTER (OC)" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 347:Generic Models 65" | object type "Generic Models 347:Generic Models 65" | names: "Generic Models 347:Generic Models 65:1578448" | material: "MORTAR JOINT" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 363:Generic Models 65" | object type "Generic Models 363:Generic Models 65" | names: "Generic Models 363:Generic Models 65:1578492" | material: "MORTAR JOINT" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 510:Generic Models 65" | object type "Generic Models 510:Generic Models 65" | names: "Generic Models 510:Generic Models 65:1578542" | material: "MORTAR JOINT" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 518:Generic Models 65" | object type "Generic Models 518:Generic Models 65" | names: "Generic Models 518:Generic Models 65:1578630" | material: "MORTAR JOINT" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 33:Generic Models 1" | object type "Generic Models 33:Generic Models 1" | names: "Generic Models 33:Generic Models 1:1579126" | material: "ACOUSTICAL SEALANT OR FIRE SEALANT, IF RATED WALL" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 31:Generic Models 1" | object type "Generic Models 31:Generic Models 1" | names: "Generic Models 31:Generic Models 1:1579142" | material: "ACOUSTICAL SEALANT OR FIRE SEALANT, IF RATED WALL" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 522:Generic Models 1" | object type "Generic Models 522:Generic Models 1" | names: "Generic Models 522:Generic Models 1:1579361" | material: "METAL RUNNER CHANNEL; FASTEN @ 24" O.C." | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 523:Generic Models 1" | object type "Generic Models 523:Generic Models 1" | names: "Generic Models 523:Generic Models 1:1579371" | material: "ACOUSTICAL SEALANT OR FIRE SEALANT, IF RATED WALL" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 524:Generic Models 1" | object type "Generic Models 524:Generic Models 1" | names: "Generic Models 524:Generic Models 1:1579381" | material: "WALL BASE AS SCHEDULED" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 525:Generic Models 1" | object type "Generic Models 525:Generic Models 1" | names: "Generic Models 525:Generic Models 1:1579391" | material: "DEEP LEG OF DEFLECTION TRACK (2" MIN. DEFLECTION)" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 526:Generic Models 1" | object type "Generic Models 526:Generic Models 1" | names: "Generic Models 526:Generic Models 1:1579401" | material: "ACOUSTICAL SEALANT OR FIRE SEALANT, IF RATED WALL" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 531:Generic Models 65" | object type "Generic Models 531:Generic Models 65" | names: "Generic Models 531:Generic Models 65:1579452" | material: "METAL STUD" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 532:Generic Models 1" | object type "Generic Models 532:Generic Models 1" | names: "Generic Models 532:Generic Models 1:1579457" | material: "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 533:Generic Models 1" | object type "Generic Models 533:Generic Models 1" | names: "Generic Models 533:Generic Models 1:1579462" | material: "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 534:Generic Models 1" | object type "Generic Models 534:Generic Models 1" | names: "Generic Models 534:Generic Models 1:1579472" | material: "2X BLOCKING - LOCATED AT GRAB BARS, WALL HUNG CABINETS, ETC.)" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 535:Generic Models 1" | object type "Generic Models 535:Generic Models 1" | names: "Generic Models 535:Generic Models 1:1579509" | material: "WALL BASE AS SCHEDULED" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 536:Generic Models 1" | object type "Generic Models 536:Generic Models 1" | names: "Generic Models 536:Generic Models 1:1579514" | material: "METAL STUD - (SEE 'WALL TAG' & 'LAYER MATERIAL SCHEDULE' FOR SIZE, SPACING, & INSULATION)" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 538:Generic Models 1" | object type "Generic Models 538:Generic Models 1" | names: "Generic Models 538:Generic Models 1:1579544" | material: "UNDERSIDE OF FLOOR ASSEMBLY - SEE STRUCT. DWGS" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 539:Generic Models 1" | object type "Generic Models 539:Generic Models 1" | names: "Generic Models 539:Generic Models 1:1579563" | material: "ACOUSTICAL SEALANT OR FIRE SEALANT, IF RATED WALL" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 540:Generic Models 1" | object type "Generic Models 540:Generic Models 1" | names: "Generic Models 540:Generic Models 1:1579573" | material: "ACOUSTICAL SEALANT OR FIRE SEALANT, IF RATED WALL" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 541:Generic Models 1" | object type "Generic Models 541:Generic Models 1" | names: "Generic Models 541:Generic Models 1:1579600" | material: "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 542:Generic Models 1" | object type "Generic Models 542:Generic Models 1" | names: "Generic Models 542:Generic Models 1:1579655" | material: "25 GA. RESILIENT CHANNEL - 24" O.C." | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 543:Generic Models 1" | object type "Generic Models 543:Generic Models 1" | names: "Generic Models 543:Generic Models 1:1579695" | material: "ACOUSTICAL SEALANT OR FIRE SEALANT, IF RATED WALL" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 544:Generic Models 1" | object type "Generic Models 544:Generic Models 1" | names: "Generic Models 544:Generic Models 1:1579725" | material: "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 545:Generic Models 1" | object type "Generic Models 545:Generic Models 1" | names: "Generic Models 545:Generic Models 1:1579771" | material: "ACOUSTICAL SEALANT OR FIRE SEALANT, IF RATED WALL" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 546:Generic Models 1" | object type "Generic Models 546:Generic Models 1" | names: "Generic Models 546:Generic Models 1:1579861" | material: "ACOUSTICAL SEALANT OR FIRE SEALANT, IF RATED WALL" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 547:Generic Models 1" | object type "Generic Models 547:Generic Models 1" | names: "Generic Models 547:Generic Models 1:1579890" | material: "ACOUSTICAL SEALANT OR FIRE SEALANT, IF RATED WALL" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 548:Generic Models 1" | object type "Generic Models 548:Generic Models 1" | names: "Generic Models 548:Generic Models 1:1579970" | material: "25 GA. RESILIENT CHANNEL - 24" O.C." | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 549:Generic Models 1" | object type "Generic Models 549:Generic Models 1" | names: "Generic Models 549:Generic Models 1:1582866" | material: "BOND BEAM W/ (1) CONT. #5 BAR CONT." | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 369:Generic Models 1" | object type "Generic Models 369:Generic Models 1" | names: "Generic Models 369:Generic Models 1:1583302" | material: "FILL CORE IF APPLICABLE - SEE STRUCTURAL DWGS FOR DETAILS" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 53:Generic Models 1" | object type "Generic Models 53:Generic Models 1" | names: "Generic Models 53:Generic Models 1:1601636" | material: "OPEN WEB WOOD TRUSS" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Dowel5:Dowel" | object type "Dowel5:Dowel" | names: "Dowel5:Dowel:1614630" | material: "PRECAST PLANK - SEE PRECAST SHOPS FOR SIZE" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 78:Generic Models 1" | object type "Generic Models 78:Generic Models 1" | names: "Generic Models 78:Generic Models 1:1614654" | material: "BEARING STRIP" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Dowel7:Dowel" | object type "Dowel7:Dowel" | names: "Dowel7:Dowel:1614828" | material: "#4 x 16" BAR @ 2-0" O.C. MAX. DRILL THRU HOLLOWCORE OR KEYWAY & INTO CIP WALL W/ 4" MIN. EMBED" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 91:Generic Models 1" | object type "Generic Models 91:Generic Models 1" | names: "Generic Models 91:Generic Models 1:1614869" | material: "3" CONCRETE TOPPING" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 96:Generic Models 1" | object type "Generic Models 96:Generic Models 1" | names: "Generic Models 96:Generic Models 1:1614983" | material: "CONCRETE WALL" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 75:Generic Models 1" | object type "Generic Models 75:Generic Models 1" | names: "Generic Models 75:Generic Models 1:1615730" | material: "TREATED 2X SILL PLATE - SEE STRUCT. SCHEDULES FOR SIZE - ATTACH WITH" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 76:Generic Models 1" | object type "Generic Models 76:Generic Models 1" | names: "Generic Models 76:Generic Models 1:1615830" | material: "#4 CONT. STEEL REBAR IN TOPPING SLAB" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Dowel6:Dowel" | object type "Dowel6:Dowel" | names: "Dowel6:Dowel:1615883" | material: "#4 VERTICAL U-SHAPED HAIRPINS AT 18" O.C. - 36" LONG" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 77:Generic Models 1" | object type "Generic Models 77:Generic Models 1" | names: "Generic Models 77:Generic Models 1:1616055" | material: "#4 VERTICAL U-SHAPED HAIRPINS AT 18" O.C. - 36" LONG" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 79:Generic Models 1" | object type "Generic Models 79:Generic Models 1" | names: "Generic Models 79:Generic Models 1:1616415" | material: "#4 HORZ. U-SHAPED HAIRPINS - 36" LONG - LOOP AROUND VERT. HAIRPIN" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 80:Generic Models 1" | object type "Generic Models 80:Generic Models 1" | names: "Generic Models 80:Generic Models 1:1616542" | material: "WALL REINFORCING - SEE PLAN SCHEDULES FOR SIZE/LOCATION" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 81:Generic Models 1" | object type "Generic Models 81:Generic Models 1" | names: "Generic Models 81:Generic Models 1:1616646" | material: "WALL REINFORCING - SEE PLAN SCHEDULES FOR SIZE/LOCATION" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 82:Generic Models 1" | object type "Generic Models 82:Generic Models 1" | names: "Generic Models 82:Generic Models 1:1616792" | material: "WALL REINFORCING - SEE PLAN SCHEDULES FOR SIZE/LOCATION" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 84:Generic Models 1" | object type "Generic Models 84:Generic Models 1" | names: "Generic Models 84:Generic Models 1:1616808" | material: "WALL REINFORCING - SEE PLAN SCHEDULES FOR SIZE/LOCATION" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          2 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "050523 - W_P_C - Fastenings - Bent Anchor Bolt:5/8"" | object type "050523 - W_P_C - Fastenings - Bent Anchor Bolt:5/8"" | names: "050523 - W_P_C - Fastenings - Bent Anchor Bolt:5/8":1617861", "050523 - W_P_C - Fastenings - Bent Anchor Bolt:5/8":1618148" | material: "5/8” GALV. BENT ANCHOR BOLT @ 4’ O.C. (WITHIN 8” OF EVERY CORNER) 7” MIN. EMBEDMENT" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCWALL | type IFCWALLTYPE "Dowel8:Dowel" | object type "Dowel8:Dowel" | names: "Dowel8:Dowel:1617962" | material: "PRECAST PLANK - SEE PRECAST SHOPS FOR SIZE" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 85:Generic Models 1" | object type "Generic Models 85:Generic Models 1" | names: "Generic Models 85:Generic Models 1:1617969" | material: "BEARING STRIP" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Dowel9:Dowel" | object type "Dowel9:Dowel" | names: "Dowel9:Dowel:1617989" | material: "#4 x 16" BAR @ 2-0" O.C. MAX. DRILL THRU HOLLOWCORE OR KEYWAY & INTO CIP WALL W/ 4" MIN. EMBED" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 86:Generic Models 1" | object type "Generic Models 86:Generic Models 1" | names: "Generic Models 86:Generic Models 1:1617996" | material: "3" CONCRETE TOPPING" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 87:Generic Models 1" | object type "Generic Models 87:Generic Models 1" | names: "Generic Models 87:Generic Models 1:1618017" | material: "CONCRETE WALL" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 88:Generic Models 1" | object type "Generic Models 88:Generic Models 1" | names: "Generic Models 88:Generic Models 1:1618032" | material: "TREATED 2X SILL PLATE - SEE STRUCT. SCHEDULES FOR SIZE - ATTACH WITH" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 89:Generic Models 1" | object type "Generic Models 89:Generic Models 1" | names: "Generic Models 89:Generic Models 1:1618045" | material: "#4 CONT. STEEL REBAR IN TOPPING SLAB" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Dowel10:Dowel" | object type "Dowel10:Dowel" | names: "Dowel10:Dowel:1618061" | material: "#4 VERTICAL U-SHAPED HAIRPINS AT 18" O.C. - 36" LONG" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 90:Generic Models 1" | object type "Generic Models 90:Generic Models 1" | names: "Generic Models 90:Generic Models 1:1618070" | material: "#4 VERTICAL U-SHAPED HAIRPINS AT 18" O.C. - 36" LONG" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 92:Generic Models 1" | object type "Generic Models 92:Generic Models 1" | names: "Generic Models 92:Generic Models 1:1618083" | material: "#4 HORZ. U-SHAPED HAIRPINS - 36" LONG - LOOP AROUND VERT. HAIRPIN" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 95:Generic Models 1" | object type "Generic Models 95:Generic Models 1" | names: "Generic Models 95:Generic Models 1:1618109" | material: "WALL REINFORCING - SEE PLAN SCHEDULES FOR SIZE/LOCATION" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 99:Generic Models 1" | object type "Generic Models 99:Generic Models 1" | names: "Generic Models 99:Generic Models 1:1618126" | material: "WALL REINFORCING - SEE PLAN SCHEDULES FOR SIZE/LOCATION" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 100:Generic Models 1" | object type "Generic Models 100:Generic Models 1" | names: "Generic Models 100:Generic Models 1:1618136" | material: "WALL REINFORCING - SEE PLAN SCHEDULES FOR SIZE/LOCATION" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 101:Generic Models 1" | object type "Generic Models 101:Generic Models 1" | names: "Generic Models 101:Generic Models 1:1618681" | material: "2X WOOD STUDS - SEE STRUCT SCHEDULE FOR SIZE" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 102:Generic Models 1" | object type "Generic Models 102:Generic Models 1" | names: "Generic Models 102:Generic Models 1:1618883" | material: "2X WOOD STUDS - SEE STRUCT SCHEDULE FOR SIZE" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 103:Generic Models 1" | object type "Generic Models 103:Generic Models 1" | names: "Generic Models 103:Generic Models 1:1619141" | material: "4x4 - W4.0xW4.0 WWM - OVERLAP 8" AT SPLICES" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 104:Generic Models 1" | object type "Generic Models 104:Generic Models 1" | names: "Generic Models 104:Generic Models 1:1619290" | material: "4x4 - W4.0xW4.0 WWM - OVERLAP 8" AT SPLICES" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 105:Generic Models 1" | object type "Generic Models 105:Generic Models 1" | names: "Generic Models 105:Generic Models 1:1619338" | material: "FILL CORE IF APPLICABLE - SEE STRUCTURAL DWGS FOR DETAILS" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 113:Generic Models 65" | object type "Generic Models 113:Generic Models 65" | names: "Generic Models 113:Generic Models 65:1619487" | material: "MORTAR JOINT" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 114:Generic Models 65" | object type "Generic Models 114:Generic Models 65" | names: "Generic Models 114:Generic Models 65:1619509" | material: "CMU (SEE 'WALL TAG' FOR SIZE)" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Dowel13:Dowel" | object type "Dowel13:Dowel" | names: "Dowel13:Dowel:1619577" | material: "WALL REINFORCING - SEE PLAN SCHEDULES FOR SIZE/LOCATION" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 118:Generic Models 65" | object type "Generic Models 118:Generic Models 65" | names: "Generic Models 118:Generic Models 65:1619584" | material: "MORTAR JOINT" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 119:Generic Models 65" | object type "Generic Models 119:Generic Models 65" | names: "Generic Models 119:Generic Models 65:1619606" | material: "CMU (SEE 'WALL TAG' FOR SIZE)" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 120:Generic Models 1" | object type "Generic Models 120:Generic Models 1" | names: "Generic Models 120:Generic Models 1:1619618" | material: "REINFORCEMENT GROUTED INTO BROKEN CORE" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 106:Generic Models 65" | object type "Generic Models 106:Generic Models 65" | names: "Generic Models 106:Generic Models 65:1619787" | material: "CMU (SEE 'WALL TAG' FOR SIZE)" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 108:Generic Models 65" | object type "Generic Models 108:Generic Models 65" | names: "Generic Models 108:Generic Models 65:1619799" | material: "MORTAR JOINT" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 109:Generic Models 65" | object type "Generic Models 109:Generic Models 65" | names: "Generic Models 109:Generic Models 65:1619830" | material: "CMU (SEE 'WALL TAG' FOR SIZE)" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 110:Generic Models 65" | object type "Generic Models 110:Generic Models 65" | names: "Generic Models 110:Generic Models 65:1619842" | material: "MORTAR JOINT" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 111:Generic Models 65" | object type "Generic Models 111:Generic Models 65" | names: "Generic Models 111:Generic Models 65:1619877" | material: "CMU (SEE 'WALL TAG' FOR SIZE)" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 107:Generic Models 65" | object type "Generic Models 107:Generic Models 65" | names: "Generic Models 107:Generic Models 65:1620157" | material: "CMU (SEE 'WALL TAG' FOR SIZE)" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 112:Generic Models 65" | object type "Generic Models 112:Generic Models 65" | names: "Generic Models 112:Generic Models 65:1620169" | material: "MORTAR JOINT" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 115:Generic Models 65" | object type "Generic Models 115:Generic Models 65" | names: "Generic Models 115:Generic Models 65:1620201" | material: "CMU (SEE 'WALL TAG' FOR SIZE)" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 116:Generic Models 65" | object type "Generic Models 116:Generic Models 65" | names: "Generic Models 116:Generic Models 65:1620213" | material: "MORTAR JOINT" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 117:Generic Models 1" | object type "Generic Models 117:Generic Models 1" | names: "Generic Models 117:Generic Models 1:1620261" | material: "PRECAST PLANK - SEE PRECAST SHOPS FOR SIZE" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 121:Generic Models 1" | object type "Generic Models 121:Generic Models 1" | names: "Generic Models 121:Generic Models 1:1621614" | material: "3" CONCRETE TOPPING" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 123:Generic Models 1" | object type "Generic Models 123:Generic Models 1" | names: "Generic Models 123:Generic Models 1:1621813" | material: "#3 J's @ 24" O.C." | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 127:Generic Models 1" | object type "Generic Models 127:Generic Models 1" | names: "Generic Models 127:Generic Models 1:1622300" | material: "SEE SCHEDULE FOR FILLED CORES" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 130:Generic Models 65" | object type "Generic Models 130:Generic Models 65" | names: "Generic Models 130:Generic Models 65:1622309" | material: "MORTAR JOINT" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Dowel11:Dowel" | object type "Dowel11:Dowel" | names: "Dowel11:Dowel:1622333" | material: "PRECAST PLANK - SEE PRECAST SHOPS FOR SIZE" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 131:Generic Models 65" | object type "Generic Models 131:Generic Models 65" | names: "Generic Models 131:Generic Models 65:1622340" | material: "MORTAR JOINT" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 133:Generic Models 1" | object type "Generic Models 133:Generic Models 1" | names: "Generic Models 133:Generic Models 1:1622357" | material: "BEARING STRIP" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Dowel12:Dowel" | object type "Dowel12:Dowel" | names: "Dowel12:Dowel:1622372" | material: "#4 J's @ 24" O.C. - GROUTED IN PRECAST KEYS AND CORES" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 182:Generic Models 65" | object type "Generic Models 182:Generic Models 65" | names: "Generic Models 182:Generic Models 65:1622384" | material: "CMU (SEE 'WALL TAG' FOR SIZE)" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 185:Generic Models 1" | object type "Generic Models 185:Generic Models 1" | names: "Generic Models 185:Generic Models 1:1622400" | material: "SOLID CMU AS NEEDED" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 186:Generic Models 65" | object type "Generic Models 186:Generic Models 65" | names: "Generic Models 186:Generic Models 65:1622412" | material: "MORTAR JOINT" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 187:Generic Models 1" | object type "Generic Models 187:Generic Models 1" | names: "Generic Models 187:Generic Models 1:1622429" | material: "SOLID CMU AS NEEDED" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 188:Generic Models 65" | object type "Generic Models 188:Generic Models 65" | names: "Generic Models 188:Generic Models 65:1622441" | material: "MORTAR JOINT" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 189:Generic Models 65" | object type "Generic Models 189:Generic Models 65" | names: "Generic Models 189:Generic Models 65:1622463" | material: "CMU (SEE 'WALL TAG' FOR SIZE)" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 190:Generic Models 1" | object type "Generic Models 190:Generic Models 1" | names: "Generic Models 190:Generic Models 1:1622477" | material: "SEE SCHEDULE FOR FILLED CORES" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 191:Generic Models 65" | object type "Generic Models 191:Generic Models 65" | names: "Generic Models 191:Generic Models 65:1622486" | material: "MORTAR JOINT" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 192:Generic Models 65" | object type "Generic Models 192:Generic Models 65" | names: "Generic Models 192:Generic Models 65:1622508" | material: "CMU (SEE 'WALL TAG' FOR SIZE)" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Dowel14:Dowel" | object type "Dowel14:Dowel" | names: "Dowel14:Dowel:1622531" | material: "#4 REBARS @ 24" O.C." | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 193:Generic Models 65" | object type "Generic Models 193:Generic Models 65" | names: "Generic Models 193:Generic Models 65:1622538" | material: "MORTAR JOINT" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 194:Generic Models 65" | object type "Generic Models 194:Generic Models 65" | names: "Generic Models 194:Generic Models 65:1622560" | material: "CMU (SEE 'WALL TAG' FOR SIZE)" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 195:Generic Models 1" | object type "Generic Models 195:Generic Models 1" | names: "Generic Models 195:Generic Models 1:1622572" | material: "3" CONCRETE TOPPING" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 196:Generic Models 65" | object type "Generic Models 196:Generic Models 65" | names: "Generic Models 196:Generic Models 65:1622594" | material: "MORTAR JOINT" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 198:Generic Models 65" | object type "Generic Models 198:Generic Models 65" | names: "Generic Models 198:Generic Models 65:1622616" | material: "CONT. KNOCK OUT BOND BEAM" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 199:Generic Models 1" | object type "Generic Models 199:Generic Models 1" | names: "Generic Models 199:Generic Models 1:1622628" | material: "GROUT CORES AT REBAR" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 200:Generic Models 1" | object type "Generic Models 200:Generic Models 1" | names: "Generic Models 200:Generic Models 1:1622654" | material: "4x4 - W4.0xW4.0 WWM - OVERLAP 8" AT SPLICES" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 201:Generic Models 1" | object type "Generic Models 201:Generic Models 1" | names: "Generic Models 201:Generic Models 1:1622672" | material: "(2) #5's" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 202:Generic Models 1" | object type "Generic Models 202:Generic Models 1" | names: "Generic Models 202:Generic Models 1:1622682" | material: "CONT. KNOCK OUT BOND BEAM" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 203:Generic Models 1" | object type "Generic Models 203:Generic Models 1" | names: "Generic Models 203:Generic Models 1:1622696" | material: "(2) #5's" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 139:Generic Models 1" | object type "Generic Models 139:Generic Models 1" | names: "Generic Models 139:Generic Models 1:1622725" | material: "#4 CONT. STEEL REBAR" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 55:Generic Models 1" | object type "Generic Models 55:Generic Models 1" | names: "Generic Models 55:Generic Models 1:1622967" | material: "4x4 - W4.0xW4.0 WWM - OVERLAP 8" AT SPLICES" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 56:Generic Models 1" | object type "Generic Models 56:Generic Models 1" | names: "Generic Models 56:Generic Models 1:1623516" | material: "WALL REINFORCING - SEE PLAN SCHEDULES FOR SIZE/LOCATION" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 219:Generic Models 1" | object type "Generic Models 219:Generic Models 1" | names: "Generic Models 219:Generic Models 1:1633873" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 220:Generic Models 1" | object type "Generic Models 220:Generic Models 1" | names: "Generic Models 220:Generic Models 1:1633886" | material: "SOUND MAT" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 222:Generic Models 1" | object type "Generic Models 222:Generic Models 1" | names: "Generic Models 222:Generic Models 1:1633912" | material: "3/4" GYP. CRETE" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 227:Generic Models 1" | object type "Generic Models 227:Generic Models 1" | names: "Generic Models 227:Generic Models 1:1633977" | material: "OPEN WEB WOOD TRUSS" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "321723 - Pavement Markings - Parking - Angled:BIKE" | object type "321723 - Pavement Markings - Parking - Angled:BIKE" | names: "321723 - Pavement Markings - Parking - Angled:BIKE:1651115" | material: "<Unnamed>" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 232:Generic Models 1" | object type "Generic Models 232:Generic Models 1" | names: "Generic Models 232:Generic Models 1:1651569" | material: "EXISTING FLOOR SUBSTRATE - MIN 19/32 THICK WOOD STRUCTURAL PANELS" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 236:Generic Models 1" | object type "Generic Models 236:Generic Models 1" | names: "Generic Models 236:Generic Models 1:1651764" | material: "EXISTING FLOOR SUBSTRATE - 1 X 4 T&G LAID PERPENDICULAR TO JOISTS, OR 19/32" PLYWOOD WOOD STRUCTURAL PANELS" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 264:Generic Models 1" | object type "Generic Models 264:Generic Models 1" | names: "Generic Models 264:Generic Models 1:1652093" | material: "EXISTING FLOOR SUBSTRATE - 15/32" THICK PLYWOOD OR 7/16" THICK ORIENTATED STRAND BOARD (OSB) WOOD STRUCTURAL PANELS" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 320:Generic Models 1" | object type "Generic Models 320:Generic Models 1" | names: "Generic Models 320:Generic Models 1:1712872" | material: "2X WOOD SILL - TREATED IF ON CONCRETE" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 323:Generic Models 1" | object type "Generic Models 323:Generic Models 1" | names: "Generic Models 323:Generic Models 1:1712877" | material: "5/8" GYP. BD" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 324:Generic Models 1" | object type "Generic Models 324:Generic Models 1" | names: "Generic Models 324:Generic Models 1:1712887" | material: "ACOUSTICAL SEALANT OR FIRE SEALANT, IF RATED WALL" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 325:Generic Models 1" | object type "Generic Models 325:Generic Models 1" | names: "Generic Models 325:Generic Models 1:1712897" | material: "WALL BASE AS SCHEDULED" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 327:Generic Models 1" | object type "Generic Models 327:Generic Models 1" | names: "Generic Models 327:Generic Models 1:1712912" | material: "METAL RUNNER CHANNEL; FASTEN @ 24" O.C." | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 328:Generic Models 65" | object type "Generic Models 328:Generic Models 65" | names: "Generic Models 328:Generic Models 65:1712927" | material: "2X WOOD STUD" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 329:Generic Models 1" | object type "Generic Models 329:Generic Models 1" | names: "Generic Models 329:Generic Models 1:1712951" | material: "DOUBLE 2X WOOD TOP PLATE" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 330:Generic Models 1" | object type "Generic Models 330:Generic Models 1" | names: "Generic Models 330:Generic Models 1:1712956" | material: "2x6 STUDS 16" O.C. (R-19 BATT. INSULATION)" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 331:Generic Models 1" | object type "Generic Models 331:Generic Models 1" | names: "Generic Models 331:Generic Models 1:1712977" | material: "DOUBLE 2X WOOD TOP PLATE" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 332:Generic Models 1" | object type "Generic Models 332:Generic Models 1" | names: "Generic Models 332:Generic Models 1:1712988" | material: "ACOUSTICAL SEALANT OR FIRE SEALANT, IF RATED WALL" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 333:Generic Models 1" | object type "Generic Models 333:Generic Models 1" | names: "Generic Models 333:Generic Models 1:1712994" | material: "UNDERSIDE OF FLOOR ASSEMBLY - SEE STRUCT. DWGS" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 334:Generic Models 1" | object type "Generic Models 334:Generic Models 1" | names: "Generic Models 334:Generic Models 1:1713023" | material: "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 335:Generic Models 1" | object type "Generic Models 335:Generic Models 1" | names: "Generic Models 335:Generic Models 1:1713033" | material: "ACOUSTICAL SEALANT OR FIRE SEALANT, IF RATED WALL" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 336:Generic Models 1" | object type "Generic Models 336:Generic Models 1" | names: "Generic Models 336:Generic Models 1:1713051" | material: "ACOUSTICAL SEALANT OR FIRE SEALANT, IF RATED WALL" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 337:Generic Models 1" | object type "Generic Models 337:Generic Models 1" | names: "Generic Models 337:Generic Models 1:1713061" | material: "25 GA. RESILIENT CHANNEL - 24" O.C." | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 338:Generic Models 1" | object type "Generic Models 338:Generic Models 1" | names: "Generic Models 338:Generic Models 1:1713077" | material: "25 GA. RESILIENT CHANNEL - 24" O.C." | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 339:Generic Models 1" | object type "Generic Models 339:Generic Models 1" | names: "Generic Models 339:Generic Models 1:1713083" | material: "IF SHEAR WALL - WOOD STRUCTURAL PANEL (WSP) - SEE STRUCT DWGS" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 340:Generic Models 1" | object type "Generic Models 340:Generic Models 1" | names: "Generic Models 340:Generic Models 1:1713096" | material: "5/8" GYP. BD" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 341:Generic Models 1" | object type "Generic Models 341:Generic Models 1" | names: "Generic Models 341:Generic Models 1:1713106" | material: "ACOUSTICAL SEALANT OR FIRE SEALANT, IF RATED WALL" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 556:Generic Models 1" | object type "Generic Models 556:Generic Models 1" | names: "Generic Models 556:Generic Models 1:1713116" | material: "WALL BASE AS SCHEDULED" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 567:Generic Models 1" | object type "Generic Models 567:Generic Models 1" | names: "Generic Models 567:Generic Models 1:1713134" | material: "ACOUSTICAL SEALANT OR FIRE SEALANT, IF RATED WALL" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 571:Generic Models 1" | object type "Generic Models 571:Generic Models 1" | names: "Generic Models 571:Generic Models 1:1713139" | material: "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 577:Generic Models 1" | object type "Generic Models 577:Generic Models 1" | names: "Generic Models 577:Generic Models 1:1713149" | material: "ACOUSTICAL SEALANT OR FIRE SEALANT, IF RATED WALL" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 590:Generic Models 1" | object type "Generic Models 590:Generic Models 1" | names: "Generic Models 590:Generic Models 1:1713167" | material: "ACOUSTICAL SEALANT OR FIRE SEALANT, IF RATED WALL" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 558:Generic Models 1" | object type "Generic Models 558:Generic Models 1" | names: "Generic Models 558:Generic Models 1:1713172" | material: "IF SHEAR WALL - WOOD STRUCTURAL PANEL (WSP) - SEE STRUCT DWGS" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
        IFCSPACE "111" | long name "1BD-T1 - TYPE B" | SPACE
        IFCSPACE "112" | long name "STUDIO - T2 - TYPE B" | SPACE
          contains 1 element
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "085000 - Windows - Casement or Awning or Fixed:FIXED PICTURE - TYPE 1" | object type "085000 - Windows - Casement or Awning or Fixed:FIXED PICTURE - TYPE 1" | names: "085000 - Windows - Casement or Awning or Fixed:FIXED PICTURE - TYPE 1:4053208" | material: constituents "MaterialConstituentSet" ("DOUBLE HUNG WINDOWS - BLACK EXT/INT SASH - LIMIT BOTTOM SASH TO 4" MAX OPEN": "DOUBLE HUNG WINDOWS - BLACK EXT/INT SASH - LIMIT BOTTOM SASH TO 4" MAX OPEN", "GL - INSULATED - LOW-E": "GL - INSULATED - LOW-E", "<Unnamed>": "<Unnamed>") | property sets: Pset_EnvironmentalImpactIndicators, Pset_ManufacturerTypeInformation, Pset_OpeningElementCommon
        IFCSPACE "113" | long name "STUDIO - T1 - TYPE B" | SPACE
          contains 1 element
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "085000 - Windows - Casement or Awning or Fixed:FIXED PICTURE - TYPE 1" | object type "085000 - Windows - Casement or Awning or Fixed:FIXED PICTURE - TYPE 1" | names: "085000 - Windows - Casement or Awning or Fixed:FIXED PICTURE - TYPE 1:4054235" | material: constituents "MaterialConstituentSet" ("DOUBLE HUNG WINDOWS - BLACK EXT/INT SASH - LIMIT BOTTOM SASH TO 4" MAX OPEN": "DOUBLE HUNG WINDOWS - BLACK EXT/INT SASH - LIMIT BOTTOM SASH TO 4" MAX OPEN", "GL - INSULATED - LOW-E": "GL - INSULATED - LOW-E", "<Unnamed>": "<Unnamed>") | property sets: Pset_EnvironmentalImpactIndicators, Pset_ManufacturerTypeInformation, Pset_OpeningElementCommon
        IFCSPACE "114" | long name "STUDIO - T1 - TYPE A" | SPACE
          contains 1 element
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "085000 - Windows - Casement or Awning or Fixed:FIXED PICTURE - TYPE 1" | object type "085000 - Windows - Casement or Awning or Fixed:FIXED PICTURE - TYPE 1" | names: "085000 - Windows - Casement or Awning or Fixed:FIXED PICTURE - TYPE 1:4054258" | material: constituents "MaterialConstituentSet" ("DOUBLE HUNG WINDOWS - BLACK EXT/INT SASH - LIMIT BOTTOM SASH TO 4" MAX OPEN": "DOUBLE HUNG WINDOWS - BLACK EXT/INT SASH - LIMIT BOTTOM SASH TO 4" MAX OPEN", "GL - INSULATED - LOW-E": "GL - INSULATED - LOW-E", "<Unnamed>": "<Unnamed>") | property sets: Pset_EnvironmentalImpactIndicators, Pset_ManufacturerTypeInformation, Pset_OpeningElementCommon
        IFCSPACE "115" | long name "STUDIO - T2 - TYPE B" | SPACE
          contains 1 element
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "085000 - Windows - Casement or Awning or Fixed:FIXED PICTURE - TYPE 1" | object type "085000 - Windows - Casement or Awning or Fixed:FIXED PICTURE - TYPE 1" | names: "085000 - Windows - Casement or Awning or Fixed:FIXED PICTURE - TYPE 1:4054228" | material: constituents "MaterialConstituentSet" ("DOUBLE HUNG WINDOWS - BLACK EXT/INT SASH - LIMIT BOTTOM SASH TO 4" MAX OPEN": "DOUBLE HUNG WINDOWS - BLACK EXT/INT SASH - LIMIT BOTTOM SASH TO 4" MAX OPEN", "GL - INSULATED - LOW-E": "GL - INSULATED - LOW-E", "<Unnamed>": "<Unnamed>") | property sets: Pset_EnvironmentalImpactIndicators, Pset_ManufacturerTypeInformation, Pset_OpeningElementCommon
        IFCSPACE "116" | long name "1BD - T1 - TYPE B" | SPACE
      IFCBUILDINGSTOREY "2ND FLOOR" | long name "2ND FLOOR" | object type "Level:Project Base Point" | elevation 10.8020833333333
        contains 434 elements
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 74:Generic Models 1" | object type "Generic Models 74:Generic Models 1" | names: "Generic Models 74:Generic Models 1:1775660" | material: "UNDERSIDE OF FLOOR ASSEMBLY - SEE STRUCT. DWGS" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 93:Generic Models 1" | object type "Generic Models 93:Generic Models 1" | names: "Generic Models 93:Generic Models 1:1775673" | material: "STRUCTURAL FLOOR - SEE STRUCT. DWGS" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 12:Structural Framing 1" | object type "Structural Framing 12:Structural Framing 1" | names: "Structural Framing 12:Structural Framing 1:1775694" | material: "BEND DOWN FLANGE OF METAL TRACK - FASTENER PER MANU. REQUIREMENTS" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 13:Structural Framing 2" | object type "Structural Framing 13:Structural Framing 2" | names: "Structural Framing 13:Structural Framing 2:1775703" | material: "METAL STUD TRACK WELDED OR SCREWED PER MANU. REQUIREMENTS" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 14:Structural Framing 2" | object type "Structural Framing 14:Structural Framing 2" | names: "Structural Framing 14:Structural Framing 2:1775712" | material: "(2) BOXED STUDS - SAME SIZE AS WALL STUDS" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 15:Structural Framing 2" | object type "Structural Framing 15:Structural Framing 2" | names: "Structural Framing 15:Structural Framing 2:1775721" | material: "(2) BOXED STUDS - SAME SIZE AS WALL STUDS" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 16:Structural Framing 2" | object type "Structural Framing 16:Structural Framing 2" | names: "Structural Framing 16:Structural Framing 2:1775730" | material: "METAL STUD TRACK WELDED OR SCREWED PER MANU. REQUIREMENTS" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 17:Structural Framing 2" | object type "Structural Framing 17:Structural Framing 2" | names: "Structural Framing 17:Structural Framing 2:1775739" | material: "METAL STUD TRACK WELDED OR SCREWED PER MANU. REQUIREMENTS" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 18:Structural Framing 2" | object type "Structural Framing 18:Structural Framing 2" | names: "Structural Framing 18:Structural Framing 2:1775748" | material: "METAL STUD TRACK WELDED OR SCREWED PER MANU. REQUIREMENTS" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 19:Structural Framing 1" | object type "Structural Framing 19:Structural Framing 1" | names: "Structural Framing 19:Structural Framing 1:1775754" | material: "VERTICAL METAL CRIPPLE STUD BEYOND" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 21:Structural Framing 1" | object type "Structural Framing 21:Structural Framing 1" | names: "Structural Framing 21:Structural Framing 1:1775764" | material: "DOUBLE UP METAL STUDS @ JAMB" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 22:Structural Framing 1" | object type "Structural Framing 22:Structural Framing 1" | names: "Structural Framing 22:Structural Framing 1:1775774" | material: "DOUBLE UP METAL STUDS @ JAMB" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCSLAB | type IFCSLABTYPE "Floor:FLOOR TRUSS" | object type "Floor:FLOOR TRUSS" | FLOOR | names: "Floor:FLOOR TRUSS:3571459" | material: layers "Floor:FLOOR TRUSS" ("HARDWOOD FLOOR" 0.0625, "3/4" GYP. CRETE TOPPING" 0.0625, "1/8" SOUND MAT" 0.0104166666666667, "3/4" CDX/OSB PLYWOOD - SEE STRUCT DWGS" 0.0625, "WOOD TRUSS FLOOR ASSEMBLY - (FILL CAVITY W/ CELLULOSE BLOWN-IN INSULATION) (UL - L521 FLOOR ASSEMBLY)" 1.5, "25 GA. RESILIENT CHANNEL - 24" O.C." 0.0416666666666667, "5/8" GYP. BD @ CEILING" 0.0520833333333333) | property sets: Pset_EnvironmentalImpactIndicators, Pset_ManufacturerTypeInformation, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          10 x IFCCURTAINWALL | type IFCCURTAINWALLTYPE "Curtain Wall:HORSE 3" | object type "Curtain Wall:HORSE 3" | names: "Curtain Wall:HORSE 3:3623372", "Curtain Wall:HORSE 3:3623406", "Curtain Wall:HORSE 3:3623412" (+7 more) | parts: 90 IFCMEMBER, 34 IFCPLATE | property sets: Pset_CurtainWallCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCSLAB | type IFCSLABTYPE "Floor:FLOOR TRUSS" | object type "Floor:FLOOR TRUSS" | FLOOR | names: "Floor:FLOOR TRUSS:3647605" | material: layers "Floor:FLOOR TRUSS" ("HARDWOOD FLOOR" 0.0625, "3/4" GYP. CRETE TOPPING" 0.0625, "1/8" SOUND MAT" 0.0104166666666667, "3/4" CDX/OSB PLYWOOD - SEE STRUCT DWGS" 0.0625, "WOOD TRUSS FLOOR ASSEMBLY - (FILL CAVITY W/ CELLULOSE BLOWN-IN INSULATION) (UL - L521 FLOOR ASSEMBLY)" 1.5, "25 GA. RESILIENT CHANNEL - 24" O.C." 0.0416666666666667, "5/8" GYP. BD @ CEILING" 0.0520833333333333) | property sets: Pset_EnvironmentalImpactIndicators, Pset_ManufacturerTypeInformation, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCSLAB | type IFCSLABTYPE "Floor:FLOOR TRUSS" | object type "Floor:FLOOR TRUSS" | FLOOR | names: "Floor:FLOOR TRUSS:3647827" | material: layers "Floor:FLOOR TRUSS" ("HARDWOOD FLOOR" 0.0625, "3/4" GYP. CRETE TOPPING" 0.0625, "1/8" SOUND MAT" 0.0104166666666667, "3/4" CDX/OSB PLYWOOD - SEE STRUCT DWGS" 0.0625, "WOOD TRUSS FLOOR ASSEMBLY - (FILL CAVITY W/ CELLULOSE BLOWN-IN INSULATION) (UL - L521 FLOOR ASSEMBLY)" 1.5, "25 GA. RESILIENT CHANNEL - 24" O.C." 0.0416666666666667, "5/8" GYP. BD @ CEILING" 0.0520833333333333) | property sets: Pset_EnvironmentalImpactIndicators, Pset_ManufacturerTypeInformation, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCSLAB | type IFCSLABTYPE "Floor:FLOOR TRUSS" | object type "Floor:FLOOR TRUSS" | FLOOR | names: "Floor:FLOOR TRUSS:3647970" | material: layers "Floor:FLOOR TRUSS" ("HARDWOOD FLOOR" 0.0625, "3/4" GYP. CRETE TOPPING" 0.0625, "1/8" SOUND MAT" 0.0104166666666667, "3/4" CDX/OSB PLYWOOD - SEE STRUCT DWGS" 0.0625, "WOOD TRUSS FLOOR ASSEMBLY - (FILL CAVITY W/ CELLULOSE BLOWN-IN INSULATION) (UL - L521 FLOOR ASSEMBLY)" 1.5, "25 GA. RESILIENT CHANNEL - 24" O.C." 0.0416666666666667, "5/8" GYP. BD @ CEILING" 0.0520833333333333) | property sets: Pset_EnvironmentalImpactIndicators, Pset_ManufacturerTypeInformation, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCSLAB | type IFCSLABTYPE "Floor:FLOOR TRUSS" | object type "Floor:FLOOR TRUSS" | FLOOR | names: "Floor:FLOOR TRUSS:3648006" | material: layers "Floor:FLOOR TRUSS" ("HARDWOOD FLOOR" 0.0625, "3/4" GYP. CRETE TOPPING" 0.0625, "1/8" SOUND MAT" 0.0104166666666667, "3/4" CDX/OSB PLYWOOD - SEE STRUCT DWGS" 0.0625, "WOOD TRUSS FLOOR ASSEMBLY - (FILL CAVITY W/ CELLULOSE BLOWN-IN INSULATION) (UL - L521 FLOOR ASSEMBLY)" 1.5, "25 GA. RESILIENT CHANNEL - 24" O.C." 0.0416666666666667, "5/8" GYP. BD @ CEILING" 0.0520833333333333) | property sets: Pset_EnvironmentalImpactIndicators, Pset_ManufacturerTypeInformation, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCSLAB | type IFCSLABTYPE "Floor:FLOOR TRUSS" | object type "Floor:FLOOR TRUSS" | FLOOR | names: "Floor:FLOOR TRUSS:3648147" | material: layers "Floor:FLOOR TRUSS" ("HARDWOOD FLOOR" 0.0625, "3/4" GYP. CRETE TOPPING" 0.0625, "1/8" SOUND MAT" 0.0104166666666667, "3/4" CDX/OSB PLYWOOD - SEE STRUCT DWGS" 0.0625, "WOOD TRUSS FLOOR ASSEMBLY - (FILL CAVITY W/ CELLULOSE BLOWN-IN INSULATION) (UL - L521 FLOOR ASSEMBLY)" 1.5, "25 GA. RESILIENT CHANNEL - 24" O.C." 0.0416666666666667, "5/8" GYP. BD @ CEILING" 0.0520833333333333) | property sets: Pset_EnvironmentalImpactIndicators, Pset_ManufacturerTypeInformation, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          2 x IFCFURNITURE | type IFCFURNITURETYPE "125819 - Dining Tables and Chairs - Table - Rectangular:1" | object type "125819 - Dining Tables and Chairs - Table - Rectangular:1" | names: "125819 - Dining Tables and Chairs - Table - Rectangular:1:3658768", "125819 - Dining Tables and Chairs - Table - Rectangular:1:3705462" | material: constituents "MaterialConstituentSet" ("MET": "MET", "BASE CABINETS": "BASE CABINETS") | property sets: Pset_EnvironmentalImpactIndicators, Pset_FurnitureTypeCommon, Pset_ManufacturerTypeInformation
          4 x IFCFURNITURE | type IFCFURNITURETYPE "125819 - Dining Tables and Chairs - Chair - Deja:Type 1" | object type "125819 - Dining Tables and Chairs - Chair - Deja:Type 1" | names: "125819 - Dining Tables and Chairs - Chair - Deja:Type 1:3658769", "125819 - Dining Tables and Chairs - Chair - Deja:Type 1:3658772", "125819 - Dining Tables and Chairs - Chair - Deja:Type 1:3705463" (+1 more) | material: "STAINLESS STEEL - EQUIP." | property sets: Pset_EnvironmentalImpactIndicators, Pset_FurnitureTypeCommon, Pset_ManufacturerTypeInformation
          4 x IFCFURNITURE | type IFCFURNITURETYPE "125819 - Dining Tables and Chairs - Chair - Deja:Type 1" | object type "125819 - Dining Tables and Chairs - Chair - Deja:Type 1" | names: "125819 - Dining Tables and Chairs - Chair - Deja:Type 1:3658770", "125819 - Dining Tables and Chairs - Chair - Deja:Type 1:3658771", "125819 - Dining Tables and Chairs - Chair - Deja:Type 1:3705464" (+1 more) | material: "STAINLESS STEEL - EQUIP." | property sets: Pset_EnvironmentalImpactIndicators, Pset_FurnitureTypeCommon, Pset_ManufacturerTypeInformation
          1 x IFCFURNITURE | type IFCFURNITURETYPE "Seating-Setee-Teknion-BBMC_Metropolitan-R1:Lounge Settee 2" | object type "Seating-Setee-Teknion-BBMC_Metropolitan-R1:Lounge Settee 2" | names: "Seating-Setee-Teknion-BBMC_Metropolitan-R1:Lounge Settee 2:3658774" | material: constituents "MaterialConstituentSet" ("_DESIGN_FABRIC": "_DESIGN_FABRIC", "Metal - Teknion - C6 - Chrome": "Metal - Teknion - C6 - Chrome", "Plastic - Teknion - Z1 - Greystone": "Plastic - Teknion - Z1 - Greystone") | property sets: Pset_EnvironmentalImpactIndicators, Pset_FurnitureTypeCommon, Pset_ManufacturerTypeInformation
          1 x IFCFURNITURE | type IFCFURNITURETYPE "Table-Coffee-Teknion-STRTC_Cover-R1:38,25" w x 27,5" d x 15" h 2" | object type "Table-Coffee-Teknion-STRTC_Cover-R1:38,25" w x 27,5" d x 15" h 2" | names: "Table-Coffee-Teknion-STRTC_Cover-R1:38,25" w x 27,5" d x 15" h 2:3658775" | material: constituents "MaterialConstituentSet" ("STEEL STRUCTURE (HOT DIPPED GALV.)": "STEEL STRUCTURE (HOT DIPPED GALV.)", "BASE CABINETS": "BASE CABINETS") | property sets: Pset_EnvironmentalImpactIndicators, Pset_FurnitureTypeCommon, Pset_ManufacturerTypeInformation
          1 x IFCFURNITURE | type IFCFURNITURETYPE "Seating-Lounge_Chair-Teknion-BBMC_Metropolitan-R1:Lounge Chair" | object type "Seating-Lounge_Chair-Teknion-BBMC_Metropolitan-R1:Lounge Chair" | names: "Seating-Lounge_Chair-Teknion-BBMC_Metropolitan-R1:Lounge Chair:3658776" | material: constituents "MaterialConstituentSet" ("_DESIGN_FABRIC": "_DESIGN_FABRIC", "<Unnamed>": "<Unnamed>", "Metal - Teknion - C6 - Chrome": "Metal - Teknion - C6 - Chrome") | property sets: Pset_EnvironmentalImpactIndicators, Pset_FurnitureTypeCommon, Pset_ManufacturerTypeInformation
          1 x IFCFURNITURE | type IFCFURNITURETYPE "Seating-Setee-Teknion-BBMC_Metropolitan-R1:Lounge Settee 2" | object type "Seating-Setee-Teknion-BBMC_Metropolitan-R1:Lounge Settee 2" | names: "Seating-Setee-Teknion-BBMC_Metropolitan-R1:Lounge Settee 2:3658806" | material: constituents "MaterialConstituentSet" ("_DESIGN_FABRIC": "_DESIGN_FABRIC", "Metal - Teknion - C6 - Chrome": "Metal - Teknion - C6 - Chrome", "Plastic - Teknion - Z1 - Greystone": "Plastic - Teknion - Z1 - Greystone") | property sets: Pset_EnvironmentalImpactIndicators, Pset_FurnitureTypeCommon, Pset_ManufacturerTypeInformation
          1 x IFCFURNITURE | type IFCFURNITURETYPE "Table-Coffee-Teknion-STRTC_Cover-R1:38,25" w x 27,5" d x 15" h 2" | object type "Table-Coffee-Teknion-STRTC_Cover-R1:38,25" w x 27,5" d x 15" h 2" | names: "Table-Coffee-Teknion-STRTC_Cover-R1:38,25" w x 27,5" d x 15" h 2:3658807" | material: constituents "MaterialConstituentSet" ("STEEL STRUCTURE (HOT DIPPED GALV.)": "STEEL STRUCTURE (HOT DIPPED GALV.)", "BASE CABINETS": "BASE CABINETS") | property sets: Pset_EnvironmentalImpactIndicators, Pset_FurnitureTypeCommon, Pset_ManufacturerTypeInformation
          1 x IFCFURNITURE | type IFCFURNITURETYPE "Seating-Lounge_Chair-Teknion-BBMC_Metropolitan-R1:Lounge Chair" | object type "Seating-Lounge_Chair-Teknion-BBMC_Metropolitan-R1:Lounge Chair" | names: "Seating-Lounge_Chair-Teknion-BBMC_Metropolitan-R1:Lounge Chair:3658808" | material: constituents "MaterialConstituentSet" ("_DESIGN_FABRIC": "_DESIGN_FABRIC", "<Unnamed>": "<Unnamed>", "Metal - Teknion - C6 - Chrome": "Metal - Teknion - C6 - Chrome") | property sets: Pset_EnvironmentalImpactIndicators, Pset_FurnitureTypeCommon, Pset_ManufacturerTypeInformation
          2 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "GAS GRILL:one" | object type "GAS GRILL:one" | names: "GAS GRILL:one:3658819", "GAS GRILL:one:3658883" | material: constituents "MaterialConstituentSet" ("Danver Stainless Steel Lt-Rt": "Danver Stainless Steel Lt-Rt", "Stainless Steel, Brushed": "Stainless Steel, Brushed", "Wolf Outdoor - Glass, Cast, Gray": "Wolf Outdoor - Glass, Cast, Gray", "Steel, Polished": "Steel, Polished", "Danver Chrome Plated": "Danver Chrome Plated", "Danver Stainless Steel Up-Dn": "Danver Stainless Steel Up-Dn", "Plastic, Opaque Black": "Plastic, Opaque Black", "Danver Toe Kick": "Danver Toe Kick") | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators, Pset_ManufacturerTypeInformation
          4 x IFCCURTAINWALL | type IFCCURTAINWALLTYPE "Curtain Wall:SLOTTED WOOD FENCE" | object type "Curtain Wall:SLOTTED WOOD FENCE" | names: "Curtain Wall:SLOTTED WOOD FENCE:3658938", "Curtain Wall:SLOTTED WOOD FENCE:3660389", "Curtain Wall:SLOTTED WOOD FENCE:3663023" (+1 more) | parts: 500 IFCMEMBER, 200 IFCPLATE | property sets: Pset_CurtainWallCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Enscape AssetDefinition - Clark, Sitting:Enscape AssetDefinition - Clark, Sitting" | object type "Enscape AssetDefinition - Clark, Sitting:Enscape AssetDefinition - Clark, Sitting" | names: "Enscape AssetDefinition - Clark, Sitting:Enscape AssetDefinition - Clark, Sitting:3669938" | material: "<Unnamed>" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Enscape AssetDefinition - Allen Sitting:Enscape AssetDefinition - Allen Sitting" | object type "Enscape AssetDefinition - Allen Sitting:Enscape AssetDefinition - Allen Sitting" | names: "Enscape AssetDefinition - Allen Sitting:Enscape AssetDefinition - Allen Sitting:3703043" | material: "<Unnamed>" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          2 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Enscape AssetDefinition - Asya Sitting:Enscape AssetDefinition - Asya Sitting" | object type "Enscape AssetDefinition - Asya Sitting:Enscape AssetDefinition - Asya Sitting" | names: "Enscape AssetDefinition - Asya Sitting:Enscape AssetDefinition - Asya Sitting:3703045", "Enscape AssetDefinition - Asya Sitting:Enscape AssetDefinition - Asya Sitting:3705468" | material: "<Unnamed>" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Enscape AssetDefinition - Connor and Isabella, Standing 02:Enscape AssetDefinition - Connor and Isabella, Standing 02" | object type "Enscape AssetDefinition - Connor and Isabella, Standing 02:Enscape AssetDefinition - Connor and Isabella, Standing 02" | names: "Enscape AssetDefinition - Connor and Isabella, Standing 02:Enscape AssetDefinition - Connor and Isabella, Standing 02:3703047" | material: "<Unnamed>" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Enscape AssetDefinition - Elena, Standing 02:Enscape AssetDefinition - Elena, Standing 02" | object type "Enscape AssetDefinition - Elena, Standing 02:Enscape AssetDefinition - Elena, Standing 02" | names: "Enscape AssetDefinition - Elena, Standing 02:Enscape AssetDefinition - Elena, Standing 02:3703048" | material: "<Unnamed>" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Enscape AssetDefinition - Juliette, Standing 02:Enscape AssetDefinition - Juliette, Standing 02" | object type "Enscape AssetDefinition - Juliette, Standing 02:Enscape AssetDefinition - Juliette, Standing 02" | names: "Enscape AssetDefinition - Juliette, Standing 02:Enscape AssetDefinition - Juliette, Standing 02:3703049" | material: "<Unnamed>" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Enscape AssetDefinition - Daud, Sitting:Enscape AssetDefinition - Daud, Sitting" | object type "Enscape AssetDefinition - Daud, Sitting:Enscape AssetDefinition - Daud, Sitting" | names: "Enscape AssetDefinition - Daud, Sitting:Enscape AssetDefinition - Daud, Sitting:3703050" | material: "<Unnamed>" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Enscape AssetDefinition - Francine, Walking 03:Enscape AssetDefinition - Francine, Walking 03" | object type "Enscape AssetDefinition - Francine, Walking 03:Enscape AssetDefinition - Francine, Walking 03" | names: "Enscape AssetDefinition - Francine, Walking 03:Enscape AssetDefinition - Francine, Walking 03:3703051" | material: "<Unnamed>" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          2 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Enscape AssetDefinition - Maja Sitting:Enscape AssetDefinition - Maja Sitting" | object type "Enscape AssetDefinition - Maja Sitting:Enscape AssetDefinition - Maja Sitting" | names: "Enscape AssetDefinition - Maja Sitting:Enscape AssetDefinition - Maja Sitting:3703052", "Enscape AssetDefinition - Maja Sitting:Enscape AssetDefinition - Maja Sitting:3705469" | material: "<Unnamed>" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          3 x IFCWALL | type IFCWALLTYPE "Basic Wall:EXT 2b - batten board - 1HR" | object type "Basic Wall:EXT 2b - batten board - 1HR" | names: "Basic Wall:EXT 2b - batten board - 1HR:4023635", "Basic Wall:EXT 2b - batten board - 1HR:4023650", "Basic Wall:EXT 2b - batten board - 1HR:4023663" | material: layers "Basic Wall:EXT 2b - batten board - 1HR" ("FIBER CEMENT - BATTEN AND BOARD SIDING - COLOR (IRON GRAY) - 3/4"X2.5" BATTENS 12" O.C." 0.0833333333333333, "BUILDING WRAP (ASTM 2273) OVER FIBERGLASS MAT GYPSUM SHEATHING" 0.0416666666666667, "2x6 STUDS 16" O.C. (R-19 BATT. INSULATION)" 0.458333333333333, "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" 0.0520833333333333) | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4023636" | names: "4023636" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          3 x IFCWALL | type IFCWALLTYPE "Basic Wall:EXT 2 - corrugated metal - 1 hr - 2nd level" | object type "Basic Wall:EXT 2 - corrugated metal - 1 hr - 2nd level" | names: "Basic Wall:EXT 2 - corrugated metal - 1 hr - 2nd level:4023638", "Basic Wall:EXT 2 - corrugated metal - 1 hr - 2nd level:4023646", "Basic Wall:EXT 2 - corrugated metal - 1 hr - 2nd level:4024951" | material: layers "Basic Wall:EXT 2 - corrugated metal - 1 hr - 2nd level" ("RIBBED PBD METAL PANEL W/ EXPOSED FASTENERS - COLOR (CHARCOAL GRAY)" 0.0729166666666667, "BUILDING WRAP (ASTM 2273) OVER FIBERGLASS MAT GYPSUM SHEATHING" 0.0520833333333333, "2x6 STUDS 16" O.C. (R-19 BATT. INSULATION)" 0.458333333333333, "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" 0.0520833333333333) | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4023639" | names: "4023639" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4023647" | names: "4023647" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4023651" | names: "4023651" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4023665" | names: "4023665" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          30 x IFCWALL | type IFCWALLTYPE "Basic Wall:EXT 2 - corrugated metal" | object type "Basic Wall:EXT 2 - corrugated metal" | names: "Basic Wall:EXT 2 - corrugated metal:4023676", "Basic Wall:EXT 2 - corrugated metal:4023697", "Basic Wall:EXT 2 - corrugated metal:4028399" (+27 more) | material: layers "Basic Wall:EXT 2 - corrugated metal" ("RIBBED PBD METAL PANEL W/ EXPOSED FASTENERS - COLOR (CHARCOAL GRAY)" 0.0729166666666667, "DRAINAGE WRAP (ASTM E2273) OVER 1/2" CDX SHEATHING" 0.0416666666666667, "2x6 STUDS 16" O.C. (R-19 BATT. INSULATION)" 0.458333333333333, "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" 0.0520833333333333) | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4023678" | names: "4023678" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          31 x IFCWALL | type IFCWALLTYPE "Basic Wall:EXT 2b - batten board" | object type "Basic Wall:EXT 2b - batten board" | names: "Basic Wall:EXT 2b - batten board:4023681", "Basic Wall:EXT 2b - batten board:4023702", "Basic Wall:EXT 2b - batten board:4028388" (+28 more) | material: layers "Basic Wall:EXT 2b - batten board" ("FIBER CEMENT - BATTEN AND BOARD SIDING - COLOR (IRON GRAY) - 3/4"X2.5" BATTENS 12" O.C." 0.0833333333333333, "DRAINAGE WRAP (ASTM E2273) OVER 1/2" CDX SHEATHING" 0.0416666666666667, "2x6 STUDS 16" O.C. (R-19 BATT. INSULATION)" 0.458333333333333, "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" 0.0520833333333333) | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4023683" | names: "4023683" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4023699" | names: "4023699" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4023704" | names: "4023704" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4024953" | names: "4024953" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4028390" | names: "4028390" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4028401" | names: "4028401" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4031140" | names: "4031140" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4031151" | names: "4031151" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4031235" | names: "4031235" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4031246" | names: "4031246" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4031392" | names: "4031392" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4031546" | names: "4031546" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4032576" | names: "4032576" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4032587" | names: "4032587" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4032593" | names: "4032593" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4032604" | names: "4032604" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4032621" | names: "4032621" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4032638" | names: "4032638" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4032654" | names: "4032654" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4032665" | names: "4032665" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4032671" | names: "4032671" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4032682" | names: "4032682" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4032699" | names: "4032699" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4032716" | names: "4032716" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4032825" | names: "4032825" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4032836" | names: "4032836" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4032842" | names: "4032842" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4032853" | names: "4032853" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4032870" | names: "4032870" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4032887" | names: "4032887" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          2 x IFCWALL | type IFCWALLTYPE "Basic Wall:EXT 2b - batten board - shear" | object type "Basic Wall:EXT 2b - batten board - shear" | names: "Basic Wall:EXT 2b - batten board - shear:4034913", "Basic Wall:EXT 2b - batten board - shear:4035406" | material: layers "Basic Wall:EXT 2b - batten board - shear" ("FIBER CEMENT - BATTEN AND BOARD SIDING - COLOR (IRON GRAY) - 3/4"X2.5" BATTENS 12" O.C." 0.0833333333333333, "DRAINAGE WRAP (ASTM E2273) OVER 1/2" CDX SHEATHING" 0.0416666666666667, "2x6 STUDS 16" O.C. (R-19 BATT. INSULATION)" 0.458333333333333, "WOOD STRUCTURAL PANEL (WSP) - SEE STRUCT DWGS" 0.0416666666666667, "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" 0.0520833333333333) | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4034915" | names: "4034915" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          2 x IFCWALL | type IFCWALLTYPE "Basic Wall:EXT 2 - corrugated metal - shear - 2nd level" | object type "Basic Wall:EXT 2 - corrugated metal - shear - 2nd level" | names: "Basic Wall:EXT 2 - corrugated metal - shear - 2nd level:4034924", "Basic Wall:EXT 2 - corrugated metal - shear - 2nd level:4035417" | material: layers "Basic Wall:EXT 2 - corrugated metal - shear - 2nd level" ("RIBBED PBD METAL PANEL W/ EXPOSED FASTENERS - COLOR (CHARCOAL GRAY)" 0.0729166666666667, "DRAINAGE WRAP (ASTM E2273) OVER 1/2" CDX SHEATHING" 0.0416666666666667, "2x6 STUDS 16" O.C. (R-19 BATT. INSULATION)" 0.458333333333333, "WOOD STRUCTURAL PANEL (WSP) - SEE STRUCT DWGS" 0.0416666666666667, "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" 0.0520833333333333) | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4034926" | names: "4034926" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4035408" | names: "4035408" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4035419" | names: "4035419" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4035588" | names: "4035588" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4035591" | names: "4035591" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4035722" | names: "4035722" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4035725" | names: "4035725" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          4 x IFCDOOR | type IFCDOORTYPE "OD_SINGLE:SINGLE - LITE - MUNTINS - 3-0 x 6-8" | object type "OD_SINGLE:SINGLE - LITE - MUNTINS - 3-0 x 6-8" | DOOR | SINGLE_SWING_LEFT | names: "OD_SINGLE:SINGLE - LITE - MUNTINS - 3-0 x 6-8:4037908", "OD_SINGLE:SINGLE - LITE - MUNTINS - 3-0 x 6-8:4089449", "OD_SINGLE:SINGLE - LITE - MUNTINS - 3-0 x 6-8:4359956" (+1 more) | material: constituents "MaterialConstituentSet" ("GL - TEMPERED - INSULATED - LOW-E": "GL - TEMPERED - INSULATED - LOW-E", "CW - CLAD WOOD DOOR": "CW - CLAD WOOD DOOR") | property sets: Pset_DoorCommon, Pset_EnvironmentalImpactIndicators
          4 x IFCDOOR | type IFCDOORTYPE "OD_SINGLE:SINGLE - LITE - MUNTINS - 3-0 x 6-8" | object type "OD_SINGLE:SINGLE - LITE - MUNTINS - 3-0 x 6-8" | DOOR | SINGLE_SWING_RIGHT | names: "OD_SINGLE:SINGLE - LITE - MUNTINS - 3-0 x 6-8:4037909", "OD_SINGLE:SINGLE - LITE - MUNTINS - 3-0 x 6-8:4091060", "OD_SINGLE:SINGLE - LITE - MUNTINS - 3-0 x 6-8:4185402" (+1 more) | material: constituents "MaterialConstituentSet" ("GL - TEMPERED - INSULATED - LOW-E": "GL - TEMPERED - INSULATED - LOW-E", "CW - CLAD WOOD DOOR": "CW - CLAD WOOD DOOR") | property sets: Pset_DoorCommon, Pset_EnvironmentalImpactIndicators
          2 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "085000 - Windows - Casement or Awning or Fixed:FIXED PICTURE - TYPE 1" | object type "085000 - Windows - Casement or Awning or Fixed:FIXED PICTURE - TYPE 1" | names: "085000 - Windows - Casement or Awning or Fixed:FIXED PICTURE - TYPE 1:4054340", "085000 - Windows - Casement or Awning or Fixed:FIXED PICTURE - TYPE 1:4054749" | material: constituents "MaterialConstituentSet" ("DOUBLE HUNG WINDOWS - BLACK EXT/INT SASH - LIMIT BOTTOM SASH TO 4" MAX OPEN": "DOUBLE HUNG WINDOWS - BLACK EXT/INT SASH - LIMIT BOTTOM SASH TO 4" MAX OPEN", "GL - INSULATED - LOW-E": "GL - INSULATED - LOW-E", "<Unnamed>": "<Unnamed>") | property sets: Pset_EnvironmentalImpactIndicators, Pset_ManufacturerTypeInformation, Pset_OpeningElementCommon
          3 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "085000 - Windows - Casement or Awning or Fixed:FIXED PICTURE - TYPE 1" | object type "085000 - Windows - Casement or Awning or Fixed:FIXED PICTURE - TYPE 1" | names: "085000 - Windows - Casement or Awning or Fixed:FIXED PICTURE - TYPE 1:4054734", "085000 - Windows - Casement or Awning or Fixed:FIXED PICTURE - TYPE 1:4054739", "085000 - Windows - Casement or Awning or Fixed:FIXED PICTURE - TYPE 1:4200905" | material: constituents "MaterialConstituentSet" ("DOUBLE HUNG WINDOWS - BLACK EXT/INT SASH - LIMIT BOTTOM SASH TO 4" MAX OPEN": "DOUBLE HUNG WINDOWS - BLACK EXT/INT SASH - LIMIT BOTTOM SASH TO 4" MAX OPEN", "GL - INSULATED - LOW-E": "GL - INSULATED - LOW-E", "<Unnamed>": "<Unnamed>") | property sets: Pset_EnvironmentalImpactIndicators, Pset_ManufacturerTypeInformation, Pset_OpeningElementCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "085000 - Windows - Double Hung:SINGLE HUNG - TYPE 2 - TEMPERED" | object type "085000 - Windows - Double Hung:SINGLE HUNG - TYPE 2 - TEMPERED" | names: "085000 - Windows - Double Hung:SINGLE HUNG - TYPE 2 - TEMPERED:4056705" | material: constituents "MaterialConstituentSet" ("DOUBLE HUNG WINDOWS - BLACK EXT/INT SASH - LIMIT BOTTOM SASH TO 4" MAX OPEN": "DOUBLE HUNG WINDOWS - BLACK EXT/INT SASH - LIMIT BOTTOM SASH TO 4" MAX OPEN", "WINDOW SASH/TRIM": "WINDOW SASH/TRIM", "GL - INSULATED - LOW-E": "GL - INSULATED - LOW-E") | property sets: Pset_EnvironmentalImpactIndicators, Pset_ManufacturerTypeInformation, Pset_OpeningElementCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "085000 - Windows - Double Hung:SINGLE HUNG - TYPE 1 - TEMPERED" | object type "085000 - Windows - Double Hung:SINGLE HUNG - TYPE 1 - TEMPERED" | names: "085000 - Windows - Double Hung:SINGLE HUNG - TYPE 1 - TEMPERED:4056706" | material: constituents "MaterialConstituentSet" ("DOUBLE HUNG WINDOWS - BLACK EXT/INT SASH - LIMIT BOTTOM SASH TO 4" MAX OPEN": "DOUBLE HUNG WINDOWS - BLACK EXT/INT SASH - LIMIT BOTTOM SASH TO 4" MAX OPEN", "WINDOW SASH/TRIM": "WINDOW SASH/TRIM", "GL - INSULATED - LOW-E": "GL - INSULATED - LOW-E") | property sets: Pset_EnvironmentalImpactIndicators, Pset_ManufacturerTypeInformation, Pset_OpeningElementCommon
          2 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "085000 - Windows - Double Hung:SINGLE HUNG - TYPE 2 - TEMPERED" | object type "085000 - Windows - Double Hung:SINGLE HUNG - TYPE 2 - TEMPERED" | names: "085000 - Windows - Double Hung:SINGLE HUNG - TYPE 2 - TEMPERED:4056708", "085000 - Windows - Double Hung:SINGLE HUNG - TYPE 2 - TEMPERED:4056718" | material: constituents "MaterialConstituentSet" ("DOUBLE HUNG WINDOWS - BLACK EXT/INT SASH - LIMIT BOTTOM SASH TO 4" MAX OPEN": "DOUBLE HUNG WINDOWS - BLACK EXT/INT SASH - LIMIT BOTTOM SASH TO 4" MAX OPEN", "WINDOW SASH/TRIM": "WINDOW SASH/TRIM", "GL - INSULATED - LOW-E": "GL - INSULATED - LOW-E") | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators, Pset_ManufacturerTypeInformation
          6 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "085000 - Windows - Double Hung:SINGLE HUNG - TYPE 2" | object type "085000 - Windows - Double Hung:SINGLE HUNG - TYPE 2" | names: "085000 - Windows - Double Hung:SINGLE HUNG - TYPE 2:4056709", "085000 - Windows - Double Hung:SINGLE HUNG - TYPE 2:4056722", "085000 - Windows - Double Hung:SINGLE HUNG - TYPE 2:4186847" (+3 more) | material: constituents "MaterialConstituentSet" ("DOUBLE HUNG WINDOWS - BLACK EXT/INT SASH - LIMIT BOTTOM SASH TO 4" MAX OPEN": "DOUBLE HUNG WINDOWS - BLACK EXT/INT SASH - LIMIT BOTTOM SASH TO 4" MAX OPEN", "WINDOW SASH/TRIM": "WINDOW SASH/TRIM", "GL - INSULATED - LOW-E": "GL - INSULATED - LOW-E") | property sets: Pset_EnvironmentalImpactIndicators, Pset_ManufacturerTypeInformation, Pset_OpeningElementCommon
          3 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "085000 - Windows - Double Hung:SINGLE HUNG - TYPE 1" | object type "085000 - Windows - Double Hung:SINGLE HUNG - TYPE 1" | names: "085000 - Windows - Double Hung:SINGLE HUNG - TYPE 1:4056710", "085000 - Windows - Double Hung:SINGLE HUNG - TYPE 1:4186850", "085000 - Windows - Double Hung:SINGLE HUNG - TYPE 1:4461636" | material: constituents "MaterialConstituentSet" ("DOUBLE HUNG WINDOWS - BLACK EXT/INT SASH - LIMIT BOTTOM SASH TO 4" MAX OPEN": "DOUBLE HUNG WINDOWS - BLACK EXT/INT SASH - LIMIT BOTTOM SASH TO 4" MAX OPEN", "WINDOW SASH/TRIM": "WINDOW SASH/TRIM", "GL - INSULATED - LOW-E": "GL - INSULATED - LOW-E") | property sets: Pset_EnvironmentalImpactIndicators, Pset_ManufacturerTypeInformation, Pset_OpeningElementCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "085000 - Windows - Double Hung:SINGLE HUNG - TYPE 1" | object type "085000 - Windows - Double Hung:SINGLE HUNG - TYPE 1" | names: "085000 - Windows - Double Hung:SINGLE HUNG - TYPE 1:4056711" | material: constituents "MaterialConstituentSet" ("DOUBLE HUNG WINDOWS - BLACK EXT/INT SASH - LIMIT BOTTOM SASH TO 4" MAX OPEN": "DOUBLE HUNG WINDOWS - BLACK EXT/INT SASH - LIMIT BOTTOM SASH TO 4" MAX OPEN", "WINDOW SASH/TRIM": "WINDOW SASH/TRIM", "GL - INSULATED - LOW-E": "GL - INSULATED - LOW-E") | property sets: Pset_EnvironmentalImpactIndicators, Pset_ManufacturerTypeInformation, Pset_OpeningElementCommon
          2 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "085000 - Windows - Double Hung:SINGLE HUNG - TYPE 2" | object type "085000 - Windows - Double Hung:SINGLE HUNG - TYPE 2" | names: "085000 - Windows - Double Hung:SINGLE HUNG - TYPE 2:4056712", "085000 - Windows - Double Hung:SINGLE HUNG - TYPE 2:4056719" | material: constituents "MaterialConstituentSet" ("DOUBLE HUNG WINDOWS - BLACK EXT/INT SASH - LIMIT BOTTOM SASH TO 4" MAX OPEN": "DOUBLE HUNG WINDOWS - BLACK EXT/INT SASH - LIMIT BOTTOM SASH TO 4" MAX OPEN", "WINDOW SASH/TRIM": "WINDOW SASH/TRIM", "GL - INSULATED - LOW-E": "GL - INSULATED - LOW-E") | property sets: Pset_EnvironmentalImpactIndicators, Pset_ManufacturerTypeInformation, Pset_OpeningElementCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "085000 - Windows - Double Hung:SINGLE HUNG - TYPE 2" | object type "085000 - Windows - Double Hung:SINGLE HUNG - TYPE 2" | names: "085000 - Windows - Double Hung:SINGLE HUNG - TYPE 2:4056723" | material: constituents "MaterialConstituentSet" ("DOUBLE HUNG WINDOWS - BLACK EXT/INT SASH - LIMIT BOTTOM SASH TO 4" MAX OPEN": "DOUBLE HUNG WINDOWS - BLACK EXT/INT SASH - LIMIT BOTTOM SASH TO 4" MAX OPEN", "WINDOW SASH/TRIM": "WINDOW SASH/TRIM", "GL - INSULATED - LOW-E": "GL - INSULATED - LOW-E") | property sets: Pset_EnvironmentalImpactIndicators, Pset_ManufacturerTypeInformation, Pset_OpeningElementCommon
          1 x IFCSLAB | type IFCSLABTYPE "Floor:balc floor" | object type "Floor:balc floor" | FLOOR | names: "Floor:balc floor:4058513" | material: layers "Floor:balc floor" ("COMPOSITE DECKING" 0.0833333333333333) | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCSLAB | type IFCSLABTYPE "Floor:balc floor" | object type "Floor:balc floor" | FLOOR | names: "Floor:balc floor:4058728" | material: layers "Floor:balc floor" ("COMPOSITE DECKING" 0.0833333333333333) | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4185256" | names: "4185256" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4185259" | names: "4185259" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCWALL | type IFCWALLTYPE "Basic Wall:EXT 2 - corrugated metal - 2nd level" | object type "Basic Wall:EXT 2 - corrugated metal - 2nd level" | names: "Basic Wall:EXT 2 - corrugated metal - 2nd level:4185266" | material: layers "Basic Wall:EXT 2 - corrugated metal - 2nd level" ("RIBBED PBD METAL PANEL W/ EXPOSED FASTENERS - COLOR (CHARCOAL GRAY)" 0.0729166666666667, "DRAINAGE WRAP (ASTM E2273) OVER 1/2" CDX SHEATHING" 0.0416666666666667, "2x6 STUDS 16" O.C. (R-19 BATT. INSULATION)" 0.458333333333333, "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" 0.0520833333333333) | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4185267" | names: "4185267" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4185280" | names: "4185280" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4185298" | names: "4185298" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4185319" | names: "4185319" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4185329" | names: "4185329" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4185341" | names: "4185341" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4185352" | names: "4185352" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          2 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "085000 - Windows - Double Hung:SINGLE HUNG - TYPE 2" | object type "085000 - Windows - Double Hung:SINGLE HUNG - TYPE 2" | names: "085000 - Windows - Double Hung:SINGLE HUNG - TYPE 2:4186752", "085000 - Windows - Double Hung:SINGLE HUNG - TYPE 2:4186758" | material: constituents "MaterialConstituentSet" ("DOUBLE HUNG WINDOWS - BLACK EXT/INT SASH - LIMIT BOTTOM SASH TO 4" MAX OPEN": "DOUBLE HUNG WINDOWS - BLACK EXT/INT SASH - LIMIT BOTTOM SASH TO 4" MAX OPEN", "WINDOW SASH/TRIM": "WINDOW SASH/TRIM", "GL - INSULATED - LOW-E": "GL - INSULATED - LOW-E") | property sets: Pset_EnvironmentalImpactIndicators, Pset_ManufacturerTypeInformation, Pset_OpeningElementCommon
          2 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "085000 - Windows - Double Hung:SINGLE HUNG - TYPE 2" | object type "085000 - Windows - Double Hung:SINGLE HUNG - TYPE 2" | names: "085000 - Windows - Double Hung:SINGLE HUNG - TYPE 2:4186754", "085000 - Windows - Double Hung:SINGLE HUNG - TYPE 2:4186755" | material: constituents "MaterialConstituentSet" ("DOUBLE HUNG WINDOWS - BLACK EXT/INT SASH - LIMIT BOTTOM SASH TO 4" MAX OPEN": "DOUBLE HUNG WINDOWS - BLACK EXT/INT SASH - LIMIT BOTTOM SASH TO 4" MAX OPEN", "WINDOW SASH/TRIM": "WINDOW SASH/TRIM", "GL - INSULATED - LOW-E": "GL - INSULATED - LOW-E") | property sets: Pset_EnvironmentalImpactIndicators, Pset_ManufacturerTypeInformation, Pset_OpeningElementCommon
          2 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "085000 - Windows - Double Hung:SINGLE HUNG - TYPE 1" | object type "085000 - Windows - Double Hung:SINGLE HUNG - TYPE 1" | names: "085000 - Windows - Double Hung:SINGLE HUNG - TYPE 1:4186757", "085000 - Windows - Double Hung:SINGLE HUNG - TYPE 1:4186759" | material: constituents "MaterialConstituentSet" ("DOUBLE HUNG WINDOWS - BLACK EXT/INT SASH - LIMIT BOTTOM SASH TO 4" MAX OPEN": "DOUBLE HUNG WINDOWS - BLACK EXT/INT SASH - LIMIT BOTTOM SASH TO 4" MAX OPEN", "WINDOW SASH/TRIM": "WINDOW SASH/TRIM", "GL - INSULATED - LOW-E": "GL - INSULATED - LOW-E") | property sets: Pset_EnvironmentalImpactIndicators, Pset_ManufacturerTypeInformation, Pset_OpeningElementCommon
          2 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "085000 - Windows - Double Hung:SINGLE HUNG - TYPE 1" | object type "085000 - Windows - Double Hung:SINGLE HUNG - TYPE 1" | names: "085000 - Windows - Double Hung:SINGLE HUNG - TYPE 1:4186761", "085000 - Windows - Double Hung:SINGLE HUNG - TYPE 1:4461524" | material: constituents "MaterialConstituentSet" ("DOUBLE HUNG WINDOWS - BLACK EXT/INT SASH - LIMIT BOTTOM SASH TO 4" MAX OPEN": "DOUBLE HUNG WINDOWS - BLACK EXT/INT SASH - LIMIT BOTTOM SASH TO 4" MAX OPEN", "WINDOW SASH/TRIM": "WINDOW SASH/TRIM", "GL - INSULATED - LOW-E": "GL - INSULATED - LOW-E") | property sets: Pset_EnvironmentalImpactIndicators, Pset_ManufacturerTypeInformation, Pset_OpeningElementCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "085000 - Windows - Casement or Awning or Fixed:FIXED PICTURE - TYPE 1" | object type "085000 - Windows - Casement or Awning or Fixed:FIXED PICTURE - TYPE 1" | names: "085000 - Windows - Casement or Awning or Fixed:FIXED PICTURE - TYPE 1:4199508" | material: constituents "MaterialConstituentSet" ("DOUBLE HUNG WINDOWS - BLACK EXT/INT SASH - LIMIT BOTTOM SASH TO 4" MAX OPEN": "DOUBLE HUNG WINDOWS - BLACK EXT/INT SASH - LIMIT BOTTOM SASH TO 4" MAX OPEN", "GL - INSULATED - LOW-E": "GL - INSULATED - LOW-E", "<Unnamed>": "<Unnamed>") | property sets: Pset_EnvironmentalImpactIndicators, Pset_ManufacturerTypeInformation, Pset_OpeningElementCommon
          2 x IFCWALL | type IFCWALLTYPE "Basic Wall:SHEAR - W4H5D - (5/8 GYP - 1/2 WSP - 2X4 WOOD(BATT))" | object type "Basic Wall:SHEAR - W4H5D - (5/8 GYP - 1/2 WSP - 2X4 WOOD(BATT))" | names: "Basic Wall:SHEAR - W4H5D - (5/8 GYP - 1/2 WSP - 2X4 WOOD(BATT)):4250092", "Basic Wall:SHEAR - W4H5D - (5/8 GYP - 1/2 WSP - 2X4 WOOD(BATT)):4250136" | material: layers "Basic Wall:SHEAR - W4H5D - (5/8 GYP - 1/2 WSP - 2X4 WOOD(BATT))" ("AIR GAP" 0.0416666666666667, "2x4 STUDS (1ST FL @ 8" O.C. • 2ND FL @ 12" O.C. • 3RD FL @ 16" O.C.) - BATT. INSULATION AT STUD CAVITY" 0.291666666666667, "WOOD STRUCTURAL PANEL (WSP) - SEE STRUCT DWGS" 0.0416666666666667, "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" 0.0520833333333333) | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          8 x IFCWALL | type IFCWALLTYPE "Basic Wall:SHEAR - W4_5D - (5/8 GYP - 2X4 WOOD(BATT))" | object type "Basic Wall:SHEAR - W4_5D - (5/8 GYP - 2X4 WOOD(BATT))" | names: "Basic Wall:SHEAR - W4_5D - (5/8 GYP - 2X4 WOOD(BATT)):4250141", "Basic Wall:SHEAR - W4_5D - (5/8 GYP - 2X4 WOOD(BATT)):4250239", "Basic Wall:SHEAR - W4_5D - (5/8 GYP - 2X4 WOOD(BATT)):4250312" (+5 more) | material: layers "Basic Wall:SHEAR - W4_5D - (5/8 GYP - 2X4 WOOD(BATT))" ("AIR GAP" 0.0416666666666667, "2x4 STUDS (1ST FL @ 8" O.C. • 2ND FL @ 12" O.C. • 3RD FL @ 16" O.C.) - BATT. INSULATION AT STUD CAVITY" 0.291666666666667, "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" 0.0520833333333333) | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4303743" | names: "4303743" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4397244" | names: "4397244" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4397251" | names: "4397251" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4397357" | names: "4397357" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4397359" | names: "4397359" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4397378" | names: "4397378" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4397382" | names: "4397382" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4397406" | names: "4397406" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4397408" | names: "4397408" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4397412" | names: "4397412" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4397414" | names: "4397414" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4398211" | names: "4398211" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4398218" | names: "4398218" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4401981" | names: "4401981" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4401983" | names: "4401983" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4402003" | names: "4402003" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4402007" | names: "4402007" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4402039" | names: "4402039" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4402041" | names: "4402041" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4402045" | names: "4402045" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4402047" | names: "4402047" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4402233" | names: "4402233" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4402234" | names: "4402234" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4402235" | names: "4402235" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4408343" | names: "4408343" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4408344" | names: "4408344" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4408346" | names: "4408346" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4408348" | names: "4408348" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4408350" | names: "4408350" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4408356" | names: "4408356" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4408358" | names: "4408358" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4409468" | names: "4409468" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4409482" | names: "4409482" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4410307" | names: "4410307" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4410309" | names: "4410309" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4410311" | names: "4410311" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4410313" | names: "4410313" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4410329" | names: "4410329" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4410331" | names: "4410331" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4410333" | names: "4410333" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4410335" | names: "4410335" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4410340" | names: "4410340" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4410342" | names: "4410342" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4410344" | names: "4410344" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4410346" | names: "4410346" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4410362" | names: "4410362" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4410364" | names: "4410364" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4410366" | names: "4410366" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4410368" | names: "4410368" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4411077" | names: "4411077" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4411110" | names: "4411110" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4411112" | names: "4411112" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4411114" | names: "4411114" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4411117" | names: "4411117" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4411120" | names: "4411120" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4411122" | names: "4411122" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4412290" | names: "4412290" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4412307" | names: "4412307" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4413180" | names: "4413180" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4413182" | names: "4413182" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4413184" | names: "4413184" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4413186" | names: "4413186" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4413202" | names: "4413202" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4413204" | names: "4413204" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4413206" | names: "4413206" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4413208" | names: "4413208" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4413213" | names: "4413213" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4413215" | names: "4413215" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4413217" | names: "4413217" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4413219" | names: "4413219" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4413235" | names: "4413235" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4413237" | names: "4413237" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4413239" | names: "4413239" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4413241" | names: "4413241" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4416523" | names: "4416523" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4416524" | names: "4416524" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4416528" | names: "4416528" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4417423" | names: "4417423" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4417424" | names: "4417424" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4417783" | names: "4417783" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4417790" | names: "4417790" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4418876" | names: "4418876" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4418884" | names: "4418884" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4418888" | names: "4418888" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4418896" | names: "4418896" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4423443" | names: "4423443" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4423444" | names: "4423444" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4423827" | names: "4423827" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4423836" | names: "4423836" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4424940" | names: "4424940" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4424948" | names: "4424948" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4424952" | names: "4424952" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4424960" | names: "4424960" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          12 x IFCWALL | type IFCWALLTYPE "Basic Wall:shaft" | object type "Basic Wall:shaft" | names: "Basic Wall:shaft:4435569", "Basic Wall:shaft:4436193", "Basic Wall:shaft:4436483" (+9 more) | material: layers "Basic Wall:shaft" ("16 GA. PERFORATED GALV. STEEL PANEL" 0.0104166666666667, "METAL STUD - GALV. - 16" O.C." 0.166666666666667) | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Indoor Unit - Evaporator - Air_Conditioner-Single_Zone-Indoor-Daikin-FTKN_NMVJU:Indoor Unit - Evaporator - 1.5Ton_FTKN18NMVJU" | object type "Indoor Unit - Evaporator - Air_Conditioner-Single_Zone-Indoor-Daikin-FTKN_NMVJU:Indoor Unit - Evaporator - 1.5Ton_FTKN18NMVJU" | names: "Indoor Unit - Evaporator - Air_Conditioner-Single_Zone-Indoor-Daikin-FTKN_NMVJU:Indoor Unit - Evaporator - 1.5Ton_FTKN18NMVJU:4451707" | material: constituents "MaterialConstituentSet" ("Metal - Daikin - Galvanized Steel": "Metal - Daikin - Galvanized Steel", "Metal - Daikin - Copper": "Metal - Daikin - Copper") | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators, Pset_ManufacturerTypeInformation
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Indoor Unit - Evaporator - Air_Conditioner-Single_Zone-Indoor-Daikin-FTKN_NMVJU:Indoor Unit - Evaporator - 1.5Ton_FTKN18NMVJU" | object type "Indoor Unit - Evaporator - Air_Conditioner-Single_Zone-Indoor-Daikin-FTKN_NMVJU:Indoor Unit - Evaporator - 1.5Ton_FTKN18NMVJU" | names: "Indoor Unit - Evaporator - Air_Conditioner-Single_Zone-Indoor-Daikin-FTKN_NMVJU:Indoor Unit - Evaporator - 1.5Ton_FTKN18NMVJU:4451924" | material: constituents "MaterialConstituentSet" ("Metal - Daikin - Galvanized Steel": "Metal - Daikin - Galvanized Steel", "Metal - Daikin - Copper": "Metal - Daikin - Copper") | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators, Pset_ManufacturerTypeInformation
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4452184" | names: "4452184" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4454411" | names: "4454411" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4454415" | names: "4454415" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4454420" | names: "4454420" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4454424" | names: "4454424" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "085000 - Windows - Double Hung:SINGLE HUNG - TYPE 1" | object type "085000 - Windows - Double Hung:SINGLE HUNG - TYPE 1" | names: "085000 - Windows - Double Hung:SINGLE HUNG - TYPE 1:4460843" | material: constituents "MaterialConstituentSet" ("DOUBLE HUNG WINDOWS - BLACK EXT/INT SASH - LIMIT BOTTOM SASH TO 4" MAX OPEN": "DOUBLE HUNG WINDOWS - BLACK EXT/INT SASH - LIMIT BOTTOM SASH TO 4" MAX OPEN", "WINDOW SASH/TRIM": "WINDOW SASH/TRIM", "GL - INSULATED - LOW-E": "GL - INSULATED - LOW-E") | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators, Pset_ManufacturerTypeInformation
          30 x IFCPIPESEGMENT | type IFCPIPESEGMENTTYPE "Pipe Types:Default" | object type "Pipe Types:Default" | names: "Pipe Types:Default:4467499", "Pipe Types:Default:4467514", "Pipe Types:Default:4467540" (+27 more) | material: "GALV. PIPE WHERE EXPOSED - (EXPOSED LINE SETS, BEHIND PERFORATED PANEL)" | property sets: Pset_EnvironmentalImpactIndicators, Pset_PipeSegmentOccurrence, Pset_PipeSegmentTypeCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4472406" | names: "4472406" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4472461" | names: "4472461" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4473215" | names: "4473215" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4473218" | names: "4473218" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4473245" | names: "4473245" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4473248" | names: "4473248" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4473265" | names: "4473265" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4473268" | names: "4473268" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4475659" | names: "4475659" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4475737" | names: "4475737" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4475738" | names: "4475738" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4494545" | names: "4494545" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4494575" | names: "4494575" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4494578" | names: "4494578" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4494580" | names: "4494580" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4494582" | names: "4494582" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4494584" | names: "4494584" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4494585" | names: "4494585" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4494586" | names: "4494586" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4494588" | names: "4494588" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4496652" | names: "4496652" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4496654" | names: "4496654" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4496656" | names: "4496656" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4496658" | names: "4496658" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4496674" | names: "4496674" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4496676" | names: "4496676" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4496678" | names: "4496678" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4496680" | names: "4496680" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4496687" | names: "4496687" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4496689" | names: "4496689" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4496691" | names: "4496691" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4496707" | names: "4496707" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4496711" | names: "4496711" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4496713" | names: "4496713" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4536647" | names: "4536647" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          2 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "085000 - Windows - Double Hung:SINGLE HUNG - TYPE 1" | object type "085000 - Windows - Double Hung:SINGLE HUNG - TYPE 1" | names: "085000 - Windows - Double Hung:SINGLE HUNG - TYPE 1:4536650", "085000 - Windows - Double Hung:SINGLE HUNG - TYPE 1:4536651" | material: constituents "MaterialConstituentSet" ("DOUBLE HUNG WINDOWS - BLACK EXT/INT SASH - LIMIT BOTTOM SASH TO 4" MAX OPEN": "DOUBLE HUNG WINDOWS - BLACK EXT/INT SASH - LIMIT BOTTOM SASH TO 4" MAX OPEN", "WINDOW SASH/TRIM": "WINDOW SASH/TRIM", "GL - INSULATED - LOW-E": "GL - INSULATED - LOW-E") | property sets: Pset_EnvironmentalImpactIndicators, Pset_ManufacturerTypeInformation, Pset_OpeningElementCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4537816" | names: "4537816" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4537878" | names: "4537878" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4538102" | names: "4538102" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4538105" | names: "4538105" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          5 x IFCWALL | type IFCWALLTYPE "Basic Wall:FIRE SEPERATION IN CAVITY" | object type "Basic Wall:FIRE SEPERATION IN CAVITY" | names: "Basic Wall:FIRE SEPERATION IN CAVITY:4598216", "Basic Wall:FIRE SEPERATION IN CAVITY:4598291", "Basic Wall:FIRE SEPERATION IN CAVITY:4598362" (+2 more) | material: layers "Basic Wall:FIRE SEPERATION IN CAVITY" ("5/8" GYP. BD" 0.0520833333333333, "LVL RIM BOARD - SEE STRUCT. DWGS" 0.0833333333333333, "5/8" GYP. BD" 0.0520833333333333) | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCALARM | type IFCALARMTYPE "104416 - Fire Extinguishers - Wall:Class A - Light - 2A" | object type "104416 - Fire Extinguishers - Wall:Class A - Light - 2A" | names: "104416 - Fire Extinguishers - Wall:Class A - Light - 2A:4608990" | material: constituents "MaterialConstituentSet" ("FIRE EXTINGUISHER": "FIRE EXTINGUISHER", "Metal - Paint Finish - Black, Matte": "Metal - Paint Finish - Black, Matte", "<Unnamed>": "<Unnamed>") | property sets: Pset_EnvironmentalImpactIndicators, Pset_OpeningElementCommon
          1 x IFCALARM | type IFCALARMTYPE "104416 - Fire Extinguishers - Wall:Class A - Light - 2A" | object type "104416 - Fire Extinguishers - Wall:Class A - Light - 2A" | names: "104416 - Fire Extinguishers - Wall:Class A - Light - 2A:4609017" | material: constituents "MaterialConstituentSet" ("FIRE EXTINGUISHER": "FIRE EXTINGUISHER", "Metal - Paint Finish - Black, Matte": "Metal - Paint Finish - Black, Matte", "<Unnamed>": "<Unnamed>") | property sets: Pset_EnvironmentalImpactIndicators, Pset_OpeningElementCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Enscape AssetDefinition - Annouk and Maud, Standing 03:Enscape AssetDefinition - Annouk and Maud, Standing 03" | object type "Enscape AssetDefinition - Annouk and Maud, Standing 03:Enscape AssetDefinition - Annouk and Maud, Standing 03" | names: "Enscape AssetDefinition - Annouk and Maud, Standing 03:Enscape AssetDefinition - Annouk and Maud, Standing 03:4641127" | material: "<Unnamed>" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Enscape AssetDefinition - Bao, Standing 03:Enscape AssetDefinition - Bao, Standing 03" | object type "Enscape AssetDefinition - Bao, Standing 03:Enscape AssetDefinition - Bao, Standing 03" | names: "Enscape AssetDefinition - Bao, Standing 03:Enscape AssetDefinition - Bao, Standing 03:4641128" | material: "<Unnamed>" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCRAILING | type IFCRAILINGTYPE "Railings 9:Railings 1" | object type "Railings 9:Railings 1" | names: "Railings 9:Railings 1:4480940" | material: "WOOD RAILING (MAPLE, OR BIRCH) - W/ WALL RETURNS AT ENDS" | property sets: Pset_EnvironmentalImpactIndicators, Pset_RailingCommon
          1 x IFCRAILING | type IFCRAILINGTYPE "Railings 11:Railings 1" | object type "Railings 11:Railings 1" | names: "Railings 11:Railings 1:4480960" | material: "WOOD RAILING (MAPLE, OR BIRCH) - W/ WALL RETURNS AT ENDS" | property sets: Pset_EnvironmentalImpactIndicators, Pset_RailingCommon
          1 x IFCRAILING | type IFCRAILINGTYPE "Railings 12:Railings 1" | object type "Railings 12:Railings 1" | names: "Railings 12:Railings 1:4481044" | material: "WOOD RAILING (MAPLE, OR BIRCH) - W/ WALL RETURNS AT ENDS" | property sets: Pset_EnvironmentalImpactIndicators, Pset_RailingCommon
          1 x IFCRAILING | type IFCRAILINGTYPE "Railings 13:Railings 1" | object type "Railings 13:Railings 1" | names: "Railings 13:Railings 1:4481064" | material: "WOOD RAILING (MAPLE, OR BIRCH) - W/ WALL RETURNS AT ENDS" | property sets: Pset_EnvironmentalImpactIndicators, Pset_RailingCommon
        IFCSPACE "121" | long name "1BD-T1" | SPACE
        IFCSPACE "122" | long name "STUDIO - T2" | SPACE
        IFCSPACE "123" | long name "STUDIO - T1" | SPACE
        IFCSPACE "124" | long name "STUDIO - T1" | SPACE
        IFCSPACE "125" | long name "STUDIO - T2" | SPACE
        IFCSPACE "126" | long name "1BD-T1" | SPACE
      IFCBUILDINGSTOREY "3RD FLOOR" | long name "3RD FLOOR" | object type "Level:Project Base Point" | elevation 21.46875
        contains 418 elements
          1 x IFCWALL | type IFCWALLTYPE "Light Pole Luminaire:Light Pole Luminaire" | object type "Light Pole Luminaire:Light Pole Luminaire" | names: "Light Pole Luminaire:Light Pole Luminaire:1513850" | material: "LUMINAIRE HOUSING AS SPECIFIED" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Model Text:OD_Very Large" | object type "Model Text:OD_Very Large" | names: "Model Text:OD_Very Large:1594948" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Model Text:OD_Very Large" | object type "Model Text:OD_Very Large" | names: "Model Text:OD_Very Large:1594962" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Model Text:OD_Very Large" | object type "Model Text:OD_Very Large" | names: "Model Text:OD_Very Large:1594972" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Model Text:OD_Very Large" | object type "Model Text:OD_Very Large" | names: "Model Text:OD_Very Large:1594992" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Model Text:OD_Very Large" | object type "Model Text:OD_Very Large" | names: "Model Text:OD_Very Large:1595008" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Model Text:OD_Very Large" | object type "Model Text:OD_Very Large" | names: "Model Text:OD_Very Large:1596034" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCROOF | type IFCROOFTYPE "Basic Roof:BALC" | object type "Basic Roof:BALC" | names: "Basic Roof:BALC:3434157" | material: layers "Basic Roof:BALC" ("TPO ROOFING MEMBRANE" 0.0208333333333333, "TAPERED RIGID INSULATION FOR DRAINAGE" 0.25, "5/8" T1-11 WOOD PANELING - EXT. GRADE - STAIN-1 - SEE LIFE SAFETY DRAWINGS" 0.0625) | property sets: Pset_EnvironmentalImpactIndicators, Pset_RoofCommon
          1 x IFCSLAB | type IFCSLABTYPE "Floor:FLOOR TRUSS" | object type "Floor:FLOOR TRUSS" | FLOOR | names: "Floor:FLOOR TRUSS:3618028" | material: layers "Floor:FLOOR TRUSS" ("HARDWOOD FLOOR" 0.0625, "3/4" GYP. CRETE TOPPING" 0.0625, "1/8" SOUND MAT" 0.0104166666666667, "3/4" CDX/OSB PLYWOOD - SEE STRUCT DWGS" 0.0625, "WOOD TRUSS FLOOR ASSEMBLY - (FILL CAVITY W/ CELLULOSE BLOWN-IN INSULATION) (UL - L521 FLOOR ASSEMBLY)" 1.5, "25 GA. RESILIENT CHANNEL - 24" O.C." 0.0416666666666667, "5/8" GYP. BD @ CEILING" 0.0520833333333333) | property sets: Pset_EnvironmentalImpactIndicators, Pset_ManufacturerTypeInformation, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCSLAB | type IFCSLABTYPE "Floor:FLOOR TRUSS" | object type "Floor:FLOOR TRUSS" | FLOOR | names: "Floor:FLOOR TRUSS:3647875" | material: layers "Floor:FLOOR TRUSS" ("HARDWOOD FLOOR" 0.0625, "3/4" GYP. CRETE TOPPING" 0.0625, "1/8" SOUND MAT" 0.0104166666666667, "3/4" CDX/OSB PLYWOOD - SEE STRUCT DWGS" 0.0625, "WOOD TRUSS FLOOR ASSEMBLY - (FILL CAVITY W/ CELLULOSE BLOWN-IN INSULATION) (UL - L521 FLOOR ASSEMBLY)" 1.5, "25 GA. RESILIENT CHANNEL - 24" O.C." 0.0416666666666667, "5/8" GYP. BD @ CEILING" 0.0520833333333333) | property sets: Pset_EnvironmentalImpactIndicators, Pset_ManufacturerTypeInformation, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCSLAB | type IFCSLABTYPE "Floor:FLOOR TRUSS" | object type "Floor:FLOOR TRUSS" | FLOOR | names: "Floor:FLOOR TRUSS:3647982" | material: layers "Floor:FLOOR TRUSS" ("HARDWOOD FLOOR" 0.0625, "3/4" GYP. CRETE TOPPING" 0.0625, "1/8" SOUND MAT" 0.0104166666666667, "3/4" CDX/OSB PLYWOOD - SEE STRUCT DWGS" 0.0625, "WOOD TRUSS FLOOR ASSEMBLY - (FILL CAVITY W/ CELLULOSE BLOWN-IN INSULATION) (UL - L521 FLOOR ASSEMBLY)" 1.5, "25 GA. RESILIENT CHANNEL - 24" O.C." 0.0416666666666667, "5/8" GYP. BD @ CEILING" 0.0520833333333333) | property sets: Pset_EnvironmentalImpactIndicators, Pset_ManufacturerTypeInformation, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCSLAB | type IFCSLABTYPE "Floor:FLOOR TRUSS" | object type "Floor:FLOOR TRUSS" | FLOOR | names: "Floor:FLOOR TRUSS:3648052" | material: layers "Floor:FLOOR TRUSS" ("HARDWOOD FLOOR" 0.0625, "3/4" GYP. CRETE TOPPING" 0.0625, "1/8" SOUND MAT" 0.0104166666666667, "3/4" CDX/OSB PLYWOOD - SEE STRUCT DWGS" 0.0625, "WOOD TRUSS FLOOR ASSEMBLY - (FILL CAVITY W/ CELLULOSE BLOWN-IN INSULATION) (UL - L521 FLOOR ASSEMBLY)" 1.5, "25 GA. RESILIENT CHANNEL - 24" O.C." 0.0416666666666667, "5/8" GYP. BD @ CEILING" 0.0520833333333333) | property sets: Pset_EnvironmentalImpactIndicators, Pset_ManufacturerTypeInformation, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCSLAB | type IFCSLABTYPE "Floor:FLOOR TRUSS" | object type "Floor:FLOOR TRUSS" | FLOOR | names: "Floor:FLOOR TRUSS:3648159" | material: layers "Floor:FLOOR TRUSS" ("HARDWOOD FLOOR" 0.0625, "3/4" GYP. CRETE TOPPING" 0.0625, "1/8" SOUND MAT" 0.0104166666666667, "3/4" CDX/OSB PLYWOOD - SEE STRUCT DWGS" 0.0625, "WOOD TRUSS FLOOR ASSEMBLY - (FILL CAVITY W/ CELLULOSE BLOWN-IN INSULATION) (UL - L521 FLOOR ASSEMBLY)" 1.5, "25 GA. RESILIENT CHANNEL - 24" O.C." 0.0416666666666667, "5/8" GYP. BD @ CEILING" 0.0520833333333333) | property sets: Pset_EnvironmentalImpactIndicators, Pset_ManufacturerTypeInformation, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCROOF | type IFCROOFTYPE "Basic Roof:SOFFIT" | object type "Basic Roof:SOFFIT" | names: "Basic Roof:SOFFIT:3648652" | material: layers "Basic Roof:SOFFIT" ("2X FRAMING - SEE STRUCT DWGS" 0.604166666666667, "FIBER CEMENT - SOFFIT - COLOR (GOLDEN LEAVES)" 0.0625) | property sets: Pset_EnvironmentalImpactIndicators, Pset_RoofCommon
          16 x IFCCURTAINWALL | type IFCCURTAINWALLTYPE "Curtain Wall:HORSE 3" | object type "Curtain Wall:HORSE 3" | names: "Curtain Wall:HORSE 3:3653962", "Curtain Wall:HORSE 3:3900927", "Curtain Wall:HORSE 3:3900948" (+13 more) | parts: 144 IFCMEMBER, 60 IFCPLATE | property sets: Pset_CurtainWallCommon, Pset_EnvironmentalImpactIndicators
          4 x IFCCURTAINWALL | type IFCCURTAINWALLTYPE "Curtain Wall:SLOTTED WOOD FENCE" | object type "Curtain Wall:SLOTTED WOOD FENCE" | names: "Curtain Wall:SLOTTED WOOD FENCE:3662652", "Curtain Wall:SLOTTED WOOD FENCE:3662789", "Curtain Wall:SLOTTED WOOD FENCE:3663375" (+1 more) | parts: 500 IFCMEMBER, 200 IFCPLATE | property sets: Pset_CurtainWallCommon, Pset_EnvironmentalImpactIndicators
          2 x IFCFURNITURE | type IFCFURNITURETYPE "125819 - Dining Tables and Chairs - Table - Rectangular:1" | object type "125819 - Dining Tables and Chairs - Table - Rectangular:1" | names: "125819 - Dining Tables and Chairs - Table - Rectangular:1:3669909", "125819 - Dining Tables and Chairs - Table - Rectangular:1:3705420" | material: constituents "MaterialConstituentSet" ("MET": "MET", "BASE CABINETS": "BASE CABINETS") | property sets: Pset_EnvironmentalImpactIndicators, Pset_FurnitureTypeCommon, Pset_ManufacturerTypeInformation
          4 x IFCFURNITURE | type IFCFURNITURETYPE "125819 - Dining Tables and Chairs - Chair - Deja:Type 1" | object type "125819 - Dining Tables and Chairs - Chair - Deja:Type 1" | names: "125819 - Dining Tables and Chairs - Chair - Deja:Type 1:3669910", "125819 - Dining Tables and Chairs - Chair - Deja:Type 1:3669913", "125819 - Dining Tables and Chairs - Chair - Deja:Type 1:3705421" (+1 more) | material: "STAINLESS STEEL - EQUIP." | property sets: Pset_EnvironmentalImpactIndicators, Pset_FurnitureTypeCommon, Pset_ManufacturerTypeInformation
          4 x IFCFURNITURE | type IFCFURNITURETYPE "125819 - Dining Tables and Chairs - Chair - Deja:Type 1" | object type "125819 - Dining Tables and Chairs - Chair - Deja:Type 1" | names: "125819 - Dining Tables and Chairs - Chair - Deja:Type 1:3669911", "125819 - Dining Tables and Chairs - Chair - Deja:Type 1:3669912", "125819 - Dining Tables and Chairs - Chair - Deja:Type 1:3705422" (+1 more) | material: "STAINLESS STEEL - EQUIP." | property sets: Pset_EnvironmentalImpactIndicators, Pset_FurnitureTypeCommon, Pset_ManufacturerTypeInformation
          1 x IFCFURNITURE | type IFCFURNITURETYPE "Seating-Setee-Teknion-BBMC_Metropolitan-R1:Lounge Settee 2" | object type "Seating-Setee-Teknion-BBMC_Metropolitan-R1:Lounge Settee 2" | names: "Seating-Setee-Teknion-BBMC_Metropolitan-R1:Lounge Settee 2:3669915" | material: constituents "MaterialConstituentSet" ("_DESIGN_FABRIC": "_DESIGN_FABRIC", "Metal - Teknion - C6 - Chrome": "Metal - Teknion - C6 - Chrome", "Plastic - Teknion - Z1 - Greystone": "Plastic - Teknion - Z1 - Greystone") | property sets: Pset_EnvironmentalImpactIndicators, Pset_FurnitureTypeCommon, Pset_ManufacturerTypeInformation
          2 x IFCFURNITURE | type IFCFURNITURETYPE "Table-Coffee-Teknion-STRTC_Cover-R1:38,25" w x 27,5" d x 15" h 2" | object type "Table-Coffee-Teknion-STRTC_Cover-R1:38,25" w x 27,5" d x 15" h 2" | names: "Table-Coffee-Teknion-STRTC_Cover-R1:38,25" w x 27,5" d x 15" h 2:3669916", "Table-Coffee-Teknion-STRTC_Cover-R1:38,25" w x 27,5" d x 15" h 2:3705286" | material: constituents "MaterialConstituentSet" ("STEEL STRUCTURE (HOT DIPPED GALV.)": "STEEL STRUCTURE (HOT DIPPED GALV.)", "BASE CABINETS": "BASE CABINETS") | property sets: Pset_EnvironmentalImpactIndicators, Pset_FurnitureTypeCommon, Pset_ManufacturerTypeInformation
          2 x IFCFURNITURE | type IFCFURNITURETYPE "Seating-Lounge_Chair-Teknion-BBMC_Metropolitan-R1:Lounge Chair" | object type "Seating-Lounge_Chair-Teknion-BBMC_Metropolitan-R1:Lounge Chair" | names: "Seating-Lounge_Chair-Teknion-BBMC_Metropolitan-R1:Lounge Chair:3669917", "Seating-Lounge_Chair-Teknion-BBMC_Metropolitan-R1:Lounge Chair:3705287" | material: constituents "MaterialConstituentSet" ("_DESIGN_FABRIC": "_DESIGN_FABRIC", "<Unnamed>": "<Unnamed>", "Metal - Teknion - C6 - Chrome": "Metal - Teknion - C6 - Chrome") | property sets: Pset_EnvironmentalImpactIndicators, Pset_FurnitureTypeCommon, Pset_ManufacturerTypeInformation
          1 x IFCFURNITURE | type IFCFURNITURETYPE "Seating-Setee-Teknion-BBMC_Metropolitan-R1:Lounge Settee 2" | object type "Seating-Setee-Teknion-BBMC_Metropolitan-R1:Lounge Settee 2" | names: "Seating-Setee-Teknion-BBMC_Metropolitan-R1:Lounge Settee 2:3669919" | material: constituents "MaterialConstituentSet" ("_DESIGN_FABRIC": "_DESIGN_FABRIC", "Metal - Teknion - C6 - Chrome": "Metal - Teknion - C6 - Chrome", "Plastic - Teknion - Z1 - Greystone": "Plastic - Teknion - Z1 - Greystone") | property sets: Pset_EnvironmentalImpactIndicators, Pset_FurnitureTypeCommon, Pset_ManufacturerTypeInformation
          1 x IFCFURNITURE | type IFCFURNITURETYPE "Table-Coffee-Teknion-STRTC_Cover-R1:38,25" w x 27,5" d x 15" h 2" | object type "Table-Coffee-Teknion-STRTC_Cover-R1:38,25" w x 27,5" d x 15" h 2" | names: "Table-Coffee-Teknion-STRTC_Cover-R1:38,25" w x 27,5" d x 15" h 2:3669920" | material: constituents "MaterialConstituentSet" ("STEEL STRUCTURE (HOT DIPPED GALV.)": "STEEL STRUCTURE (HOT DIPPED GALV.)", "BASE CABINETS": "BASE CABINETS") | property sets: Pset_EnvironmentalImpactIndicators, Pset_FurnitureTypeCommon, Pset_ManufacturerTypeInformation
          2 x IFCFURNITURE | type IFCFURNITURETYPE "Seating-Lounge_Chair-Teknion-BBMC_Metropolitan-R1:Lounge Chair" | object type "Seating-Lounge_Chair-Teknion-BBMC_Metropolitan-R1:Lounge Chair" | names: "Seating-Lounge_Chair-Teknion-BBMC_Metropolitan-R1:Lounge Chair:3669921", "Seating-Lounge_Chair-Teknion-BBMC_Metropolitan-R1:Lounge Chair:3705331" | material: constituents "MaterialConstituentSet" ("_DESIGN_FABRIC": "_DESIGN_FABRIC", "<Unnamed>": "<Unnamed>", "Metal - Teknion - C6 - Chrome": "Metal - Teknion - C6 - Chrome") | property sets: Pset_EnvironmentalImpactIndicators, Pset_FurnitureTypeCommon, Pset_ManufacturerTypeInformation
          2 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "GAS GRILL:one" | object type "GAS GRILL:one" | names: "GAS GRILL:one:3669923", "GAS GRILL:one:3669924" | material: constituents "MaterialConstituentSet" ("Danver Stainless Steel Lt-Rt": "Danver Stainless Steel Lt-Rt", "Stainless Steel, Brushed": "Stainless Steel, Brushed", "Wolf Outdoor - Glass, Cast, Gray": "Wolf Outdoor - Glass, Cast, Gray", "Steel, Polished": "Steel, Polished", "Danver Chrome Plated": "Danver Chrome Plated", "Danver Stainless Steel Up-Dn": "Danver Stainless Steel Up-Dn", "Plastic, Opaque Black": "Plastic, Opaque Black", "Danver Toe Kick": "Danver Toe Kick") | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators, Pset_ManufacturerTypeInformation
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Enscape AssetDefinition - Connor and Isabella, Standing 02:Enscape AssetDefinition - Connor and Isabella, Standing 02" | object type "Enscape AssetDefinition - Connor and Isabella, Standing 02:Enscape AssetDefinition - Connor and Isabella, Standing 02" | names: "Enscape AssetDefinition - Connor and Isabella, Standing 02:Enscape AssetDefinition - Connor and Isabella, Standing 02:3705048" | material: "<Unnamed>" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Enscape AssetDefinition - Elena, Standing 02:Enscape AssetDefinition - Elena, Standing 02" | object type "Enscape AssetDefinition - Elena, Standing 02:Enscape AssetDefinition - Elena, Standing 02" | names: "Enscape AssetDefinition - Elena, Standing 02:Enscape AssetDefinition - Elena, Standing 02:3705049" | material: "<Unnamed>" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Enscape AssetDefinition - Juliette, Standing 02:Enscape AssetDefinition - Juliette, Standing 02" | object type "Enscape AssetDefinition - Juliette, Standing 02:Enscape AssetDefinition - Juliette, Standing 02" | names: "Enscape AssetDefinition - Juliette, Standing 02:Enscape AssetDefinition - Juliette, Standing 02:3705050" | material: "<Unnamed>" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Enscape AssetDefinition - Francine, Walking 03:Enscape AssetDefinition - Francine, Walking 03" | object type "Enscape AssetDefinition - Francine, Walking 03:Enscape AssetDefinition - Francine, Walking 03" | names: "Enscape AssetDefinition - Francine, Walking 03:Enscape AssetDefinition - Francine, Walking 03:3705052" | material: "<Unnamed>" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Enscape AssetDefinition - Allen Sitting:Enscape AssetDefinition - Allen Sitting" | object type "Enscape AssetDefinition - Allen Sitting:Enscape AssetDefinition - Allen Sitting" | names: "Enscape AssetDefinition - Allen Sitting:Enscape AssetDefinition - Allen Sitting:3705087" | material: "<Unnamed>" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Enscape AssetDefinition - Allen Sitting:Enscape AssetDefinition - Allen Sitting" | object type "Enscape AssetDefinition - Allen Sitting:Enscape AssetDefinition - Allen Sitting" | names: "Enscape AssetDefinition - Allen Sitting:Enscape AssetDefinition - Allen Sitting:3705289" | material: "<Unnamed>" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          2 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Enscape AssetDefinition - Daud, Sitting:Enscape AssetDefinition - Daud, Sitting" | object type "Enscape AssetDefinition - Daud, Sitting:Enscape AssetDefinition - Daud, Sitting" | names: "Enscape AssetDefinition - Daud, Sitting:Enscape AssetDefinition - Daud, Sitting:3705290", "Enscape AssetDefinition - Daud, Sitting:Enscape AssetDefinition - Daud, Sitting:3754230" | material: "<Unnamed>" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          39 x IFCWALL | type IFCWALLTYPE "Basic Wall:EXT 2 - corrugated metal at parapet" | object type "Basic Wall:EXT 2 - corrugated metal at parapet" | names: "Basic Wall:EXT 2 - corrugated metal at parapet:4028027", "Basic Wall:EXT 2 - corrugated metal at parapet:4180661", "Basic Wall:EXT 2 - corrugated metal at parapet:4180664" (+36 more) | material: layers "Basic Wall:EXT 2 - corrugated metal at parapet" ("RIBBED PBD METAL PANEL W/ EXPOSED FASTENERS - COLOR (CHARCOAL GRAY)" 0.0729166666666667, "DRAINAGE WRAP (ASTM E2273) OVER 1/2" CDX SHEATHING" 0.0416666666666667, "2x6 STUDS 16" O.C. (R-19 BATT. INSULATION)" 0.458333333333333, "DRAINAGE WRAP (ASTM E2273) OVER 1/2" CDX SHEATHING" 0.0416666666666667, "RIBBED PBD METAL PANEL W/ EXPOSED FASTENERS - COLOR (CHARCOAL GRAY)" 0.0729166666666667) | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          4 x IFCDOOR | type IFCDOORTYPE "OD_SINGLE:SINGLE - LITE - MUNTINS - 3-0 x 6-8" | object type "OD_SINGLE:SINGLE - LITE - MUNTINS - 3-0 x 6-8" | DOOR | SINGLE_SWING_RIGHT | names: "OD_SINGLE:SINGLE - LITE - MUNTINS - 3-0 x 6-8:4037910", "OD_SINGLE:SINGLE - LITE - MUNTINS - 3-0 x 6-8:4091057", "OD_SINGLE:SINGLE - LITE - MUNTINS - 3-0 x 6-8:4185408" (+1 more) | material: constituents "MaterialConstituentSet" ("GL - TEMPERED - INSULATED - LOW-E": "GL - TEMPERED - INSULATED - LOW-E", "CW - CLAD WOOD DOOR": "CW - CLAD WOOD DOOR") | property sets: Pset_DoorCommon, Pset_EnvironmentalImpactIndicators
          4 x IFCDOOR | type IFCDOORTYPE "OD_SINGLE:SINGLE - LITE - MUNTINS - 3-0 x 6-8" | object type "OD_SINGLE:SINGLE - LITE - MUNTINS - 3-0 x 6-8" | DOOR | SINGLE_SWING_LEFT | names: "OD_SINGLE:SINGLE - LITE - MUNTINS - 3-0 x 6-8:4037911", "OD_SINGLE:SINGLE - LITE - MUNTINS - 3-0 x 6-8:4089583", "OD_SINGLE:SINGLE - LITE - MUNTINS - 3-0 x 6-8:4359954" (+1 more) | material: constituents "MaterialConstituentSet" ("GL - TEMPERED - INSULATED - LOW-E": "GL - TEMPERED - INSULATED - LOW-E", "CW - CLAD WOOD DOOR": "CW - CLAD WOOD DOOR") | property sets: Pset_DoorCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCROOF | object type "Basic Roof:sloped roof" | names: "Basic Roof:sloped roof:4050974" | parts: 3 IFCSLAB | property sets: Pset_EnvironmentalImpactIndicators, Pset_RoofCommon
          1 x IFCROOF | type IFCROOFTYPE "Basic Roof:SOFFIT" | object type "Basic Roof:SOFFIT" | names: "Basic Roof:SOFFIT:4051603" | material: layers "Basic Roof:SOFFIT" ("2X FRAMING - SEE STRUCT DWGS" 0.604166666666667, "FIBER CEMENT - SOFFIT - COLOR (GOLDEN LEAVES)" 0.0625) | property sets: Pset_EnvironmentalImpactIndicators, Pset_RoofCommon
          1 x IFCROOF | type IFCROOFTYPE "Basic Roof:SOFFIT" | object type "Basic Roof:SOFFIT" | names: "Basic Roof:SOFFIT:4051697" | material: layers "Basic Roof:SOFFIT" ("2X FRAMING - SEE STRUCT DWGS" 0.604166666666667, "FIBER CEMENT - SOFFIT - COLOR (GOLDEN LEAVES)" 0.0625) | property sets: Pset_EnvironmentalImpactIndicators, Pset_RoofCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "085000 - Windows - Double Hung:SINGLE HUNG - TYPE 2" | object type "085000 - Windows - Double Hung:SINGLE HUNG - TYPE 2" | names: "085000 - Windows - Double Hung:SINGLE HUNG - TYPE 2:4056123" | material: constituents "MaterialConstituentSet" ("DOUBLE HUNG WINDOWS - BLACK EXT/INT SASH - LIMIT BOTTOM SASH TO 4" MAX OPEN": "DOUBLE HUNG WINDOWS - BLACK EXT/INT SASH - LIMIT BOTTOM SASH TO 4" MAX OPEN", "WINDOW SASH/TRIM": "WINDOW SASH/TRIM", "GL - INSULATED - LOW-E": "GL - INSULATED - LOW-E") | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators, Pset_ManufacturerTypeInformation
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "085000 - Windows - Double Hung:SINGLE HUNG - TYPE 1 - TEMPERED" | object type "085000 - Windows - Double Hung:SINGLE HUNG - TYPE 1 - TEMPERED" | names: "085000 - Windows - Double Hung:SINGLE HUNG - TYPE 1 - TEMPERED:4056136" | material: constituents "MaterialConstituentSet" ("DOUBLE HUNG WINDOWS - BLACK EXT/INT SASH - LIMIT BOTTOM SASH TO 4" MAX OPEN": "DOUBLE HUNG WINDOWS - BLACK EXT/INT SASH - LIMIT BOTTOM SASH TO 4" MAX OPEN", "WINDOW SASH/TRIM": "WINDOW SASH/TRIM", "GL - INSULATED - LOW-E": "GL - INSULATED - LOW-E") | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators, Pset_ManufacturerTypeInformation
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "085000 - Windows - Double Hung:SINGLE HUNG - TYPE 2 - TEMPERED" | object type "085000 - Windows - Double Hung:SINGLE HUNG - TYPE 2 - TEMPERED" | names: "085000 - Windows - Double Hung:SINGLE HUNG - TYPE 2 - TEMPERED:4056137" | material: constituents "MaterialConstituentSet" ("DOUBLE HUNG WINDOWS - BLACK EXT/INT SASH - LIMIT BOTTOM SASH TO 4" MAX OPEN": "DOUBLE HUNG WINDOWS - BLACK EXT/INT SASH - LIMIT BOTTOM SASH TO 4" MAX OPEN", "WINDOW SASH/TRIM": "WINDOW SASH/TRIM", "GL - INSULATED - LOW-E": "GL - INSULATED - LOW-E") | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators, Pset_ManufacturerTypeInformation
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "085000 - Windows - Double Hung:SINGLE HUNG - TYPE 2" | object type "085000 - Windows - Double Hung:SINGLE HUNG - TYPE 2" | names: "085000 - Windows - Double Hung:SINGLE HUNG - TYPE 2:4056138" | material: constituents "MaterialConstituentSet" ("DOUBLE HUNG WINDOWS - BLACK EXT/INT SASH - LIMIT BOTTOM SASH TO 4" MAX OPEN": "DOUBLE HUNG WINDOWS - BLACK EXT/INT SASH - LIMIT BOTTOM SASH TO 4" MAX OPEN", "WINDOW SASH/TRIM": "WINDOW SASH/TRIM", "GL - INSULATED - LOW-E": "GL - INSULATED - LOW-E") | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators, Pset_ManufacturerTypeInformation
          3 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "085000 - Windows - Double Hung:SINGLE HUNG - TYPE 1" | object type "085000 - Windows - Double Hung:SINGLE HUNG - TYPE 1" | names: "085000 - Windows - Double Hung:SINGLE HUNG - TYPE 1:4056141", "085000 - Windows - Double Hung:SINGLE HUNG - TYPE 1:4201057", "085000 - Windows - Double Hung:SINGLE HUNG - TYPE 1:4201060" | material: constituents "MaterialConstituentSet" ("DOUBLE HUNG WINDOWS - BLACK EXT/INT SASH - LIMIT BOTTOM SASH TO 4" MAX OPEN": "DOUBLE HUNG WINDOWS - BLACK EXT/INT SASH - LIMIT BOTTOM SASH TO 4" MAX OPEN", "WINDOW SASH/TRIM": "WINDOW SASH/TRIM", "GL - INSULATED - LOW-E": "GL - INSULATED - LOW-E") | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators, Pset_ManufacturerTypeInformation, Pset_OpeningElementCommon
          3 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "085000 - Windows - Double Hung:SINGLE HUNG - TYPE 2" | object type "085000 - Windows - Double Hung:SINGLE HUNG - TYPE 2" | names: "085000 - Windows - Double Hung:SINGLE HUNG - TYPE 2:4056142", "085000 - Windows - Double Hung:SINGLE HUNG - TYPE 2:4201058", "085000 - Windows - Double Hung:SINGLE HUNG - TYPE 2:4201059" | material: constituents "MaterialConstituentSet" ("DOUBLE HUNG WINDOWS - BLACK EXT/INT SASH - LIMIT BOTTOM SASH TO 4" MAX OPEN": "DOUBLE HUNG WINDOWS - BLACK EXT/INT SASH - LIMIT BOTTOM SASH TO 4" MAX OPEN", "WINDOW SASH/TRIM": "WINDOW SASH/TRIM", "GL - INSULATED - LOW-E": "GL - INSULATED - LOW-E") | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators, Pset_ManufacturerTypeInformation, Pset_OpeningElementCommon
          2 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "085000 - Windows - Double Hung:SINGLE HUNG - TYPE 2 - TEMPERED" | object type "085000 - Windows - Double Hung:SINGLE HUNG - TYPE 2 - TEMPERED" | names: "085000 - Windows - Double Hung:SINGLE HUNG - TYPE 2 - TEMPERED:4056145", "085000 - Windows - Double Hung:SINGLE HUNG - TYPE 2 - TEMPERED:4056147" | material: constituents "MaterialConstituentSet" ("DOUBLE HUNG WINDOWS - BLACK EXT/INT SASH - LIMIT BOTTOM SASH TO 4" MAX OPEN": "DOUBLE HUNG WINDOWS - BLACK EXT/INT SASH - LIMIT BOTTOM SASH TO 4" MAX OPEN", "WINDOW SASH/TRIM": "WINDOW SASH/TRIM", "GL - INSULATED - LOW-E": "GL - INSULATED - LOW-E") | property sets: Pset_EnvironmentalImpactIndicators, Pset_ManufacturerTypeInformation, Pset_OpeningElementCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "085000 - Windows - Double Hung:SINGLE HUNG - TYPE 1" | object type "085000 - Windows - Double Hung:SINGLE HUNG - TYPE 1" | names: "085000 - Windows - Double Hung:SINGLE HUNG - TYPE 1:4056146" | material: constituents "MaterialConstituentSet" ("DOUBLE HUNG WINDOWS - BLACK EXT/INT SASH - LIMIT BOTTOM SASH TO 4" MAX OPEN": "DOUBLE HUNG WINDOWS - BLACK EXT/INT SASH - LIMIT BOTTOM SASH TO 4" MAX OPEN", "WINDOW SASH/TRIM": "WINDOW SASH/TRIM", "GL - INSULATED - LOW-E": "GL - INSULATED - LOW-E") | property sets: Pset_EnvironmentalImpactIndicators, Pset_ManufacturerTypeInformation, Pset_OpeningElementCommon
          1 x IFCSLAB | type IFCSLABTYPE "Floor:balc floor" | object type "Floor:balc floor" | FLOOR | names: "Floor:balc floor:4058702" | material: layers "Floor:balc floor" ("COMPOSITE DECKING" 0.0833333333333333) | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCSLAB | type IFCSLABTYPE "Floor:balc floor" | object type "Floor:balc floor" | FLOOR | names: "Floor:balc floor:4058754" | material: layers "Floor:balc floor" ("COMPOSITE DECKING" 0.0833333333333333) | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Fascia:Fascia 1" | object type "Fascia:Fascia 1" | names: "Fascia:Fascia 1:4166240" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          2 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "085000 - Windows - Casement or Awning or Fixed:FIXED PICTURE - TYPE 1" | object type "085000 - Windows - Casement or Awning or Fixed:FIXED PICTURE - TYPE 1" | names: "085000 - Windows - Casement or Awning or Fixed:FIXED PICTURE - TYPE 1:4181960", "085000 - Windows - Casement or Awning or Fixed:FIXED PICTURE - TYPE 1:4182517" | material: constituents "MaterialConstituentSet" ("DOUBLE HUNG WINDOWS - BLACK EXT/INT SASH - LIMIT BOTTOM SASH TO 4" MAX OPEN": "DOUBLE HUNG WINDOWS - BLACK EXT/INT SASH - LIMIT BOTTOM SASH TO 4" MAX OPEN", "GL - INSULATED - LOW-E": "GL - INSULATED - LOW-E", "<Unnamed>": "<Unnamed>") | property sets: Pset_EnvironmentalImpactIndicators, Pset_ManufacturerTypeInformation, Pset_OpeningElementCommon
          3 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "085000 - Windows - Casement or Awning or Fixed:FIXED PICTURE - TYPE 1" | object type "085000 - Windows - Casement or Awning or Fixed:FIXED PICTURE - TYPE 1" | names: "085000 - Windows - Casement or Awning or Fixed:FIXED PICTURE - TYPE 1:4182574", "085000 - Windows - Casement or Awning or Fixed:FIXED PICTURE - TYPE 1:4182579", "085000 - Windows - Casement or Awning or Fixed:FIXED PICTURE - TYPE 1:4200904" | material: constituents "MaterialConstituentSet" ("DOUBLE HUNG WINDOWS - BLACK EXT/INT SASH - LIMIT BOTTOM SASH TO 4" MAX OPEN": "DOUBLE HUNG WINDOWS - BLACK EXT/INT SASH - LIMIT BOTTOM SASH TO 4" MAX OPEN", "GL - INSULATED - LOW-E": "GL - INSULATED - LOW-E", "<Unnamed>": "<Unnamed>") | property sets: Pset_EnvironmentalImpactIndicators, Pset_ManufacturerTypeInformation, Pset_OpeningElementCommon, Pset_BuildingElementProxyCommon
          1 x IFCROOF | type IFCROOFTYPE "Basic Roof:WOOD-FRAMED ROOF ABOVE 3RD FLOOR" | object type "Basic Roof:WOOD-FRAMED ROOF ABOVE 3RD FLOOR" | names: "Basic Roof:WOOD-FRAMED ROOF ABOVE 3RD FLOOR:4185221" | material: layers "Basic Roof:WOOD-FRAMED ROOF ABOVE 3RD FLOOR" ("TPO ROOFING MEMBRANE" 0.0208333333333333, "1" MIN. POLYISO INSULATION OVER UNDERLAYMENT (WRAP UP/OVER PARAPET)" 0.0833333333333333, "3/4" CDX/OSB PLYWOOD - SEE STRUCT DWGS" 0.0625, "TRAPEZOIDAL WOOD TRUSS ROOF ASSEMBLY - (FILL CAVITY W/ CELLULOSE BLOWN-IN INSULATION) (R-VALUE = 50)" 1.5, "5/8" GYP. BD @ CEILING" 0.0520833333333333) | property sets: Pset_EnvironmentalImpactIndicators, Pset_RoofCommon
          3 x IFCWALL | type IFCWALLTYPE "Basic Wall:EXT 2 - corrugated metal at parapet - 1HR" | object type "Basic Wall:EXT 2 - corrugated metal at parapet - 1HR" | names: "Basic Wall:EXT 2 - corrugated metal at parapet - 1HR:4198078", "Basic Wall:EXT 2 - corrugated metal at parapet - 1HR:4198223", "Basic Wall:EXT 2 - corrugated metal at parapet - 1HR:4417252" | material: layers "Basic Wall:EXT 2 - corrugated metal at parapet - 1HR" ("RIBBED PBD METAL PANEL W/ EXPOSED FASTENERS - COLOR (CHARCOAL GRAY)" 0.0729166666666667, "BUILDING WRAP (ASTM 2273) OVER FIBERGLASS MAT GYPSUM SHEATHING" 0.0416666666666667, "2x6 STUDS 16" O.C. (R-19 BATT. INSULATION)" 0.458333333333333, "BUILDING WRAP (ASTM 2273) OVER FIBERGLASS MAT GYPSUM SHEATHING" 0.0416666666666667, "RIBBED PBD METAL PANEL W/ EXPOSED FASTENERS - COLOR (CHARCOAL GRAY)" 0.0729166666666667) | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          4 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "085000 - Windows - Double Hung:SINGLE HUNG - TYPE 2" | object type "085000 - Windows - Double Hung:SINGLE HUNG - TYPE 2" | names: "085000 - Windows - Double Hung:SINGLE HUNG - TYPE 2:4199369", "085000 - Windows - Double Hung:SINGLE HUNG - TYPE 2:4199372", "085000 - Windows - Double Hung:SINGLE HUNG - TYPE 2:4199379" (+1 more) | material: constituents "MaterialConstituentSet" ("DOUBLE HUNG WINDOWS - BLACK EXT/INT SASH - LIMIT BOTTOM SASH TO 4" MAX OPEN": "DOUBLE HUNG WINDOWS - BLACK EXT/INT SASH - LIMIT BOTTOM SASH TO 4" MAX OPEN", "WINDOW SASH/TRIM": "WINDOW SASH/TRIM", "GL - INSULATED - LOW-E": "GL - INSULATED - LOW-E") | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators, Pset_ManufacturerTypeInformation, Pset_OpeningElementCommon
          4 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "085000 - Windows - Double Hung:SINGLE HUNG - TYPE 1" | object type "085000 - Windows - Double Hung:SINGLE HUNG - TYPE 1" | names: "085000 - Windows - Double Hung:SINGLE HUNG - TYPE 1:4199370", "085000 - Windows - Double Hung:SINGLE HUNG - TYPE 1:4199373", "085000 - Windows - Double Hung:SINGLE HUNG - TYPE 1:4199377" (+1 more) | material: constituents "MaterialConstituentSet" ("DOUBLE HUNG WINDOWS - BLACK EXT/INT SASH - LIMIT BOTTOM SASH TO 4" MAX OPEN": "DOUBLE HUNG WINDOWS - BLACK EXT/INT SASH - LIMIT BOTTOM SASH TO 4" MAX OPEN", "WINDOW SASH/TRIM": "WINDOW SASH/TRIM", "GL - INSULATED - LOW-E": "GL - INSULATED - LOW-E") | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators, Pset_ManufacturerTypeInformation, Pset_OpeningElementCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "085000 - Windows - Casement or Awning or Fixed:FIXED PICTURE - TYPE 1" | object type "085000 - Windows - Casement or Awning or Fixed:FIXED PICTURE - TYPE 1" | names: "085000 - Windows - Casement or Awning or Fixed:FIXED PICTURE - TYPE 1:4199380" | material: constituents "MaterialConstituentSet" ("DOUBLE HUNG WINDOWS - BLACK EXT/INT SASH - LIMIT BOTTOM SASH TO 4" MAX OPEN": "DOUBLE HUNG WINDOWS - BLACK EXT/INT SASH - LIMIT BOTTOM SASH TO 4" MAX OPEN", "GL - INSULATED - LOW-E": "GL - INSULATED - LOW-E", "<Unnamed>": "<Unnamed>") | property sets: Pset_EnvironmentalImpactIndicators, Pset_ManufacturerTypeInformation, Pset_OpeningElementCommon
          2 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "085000 - Windows - Double Hung:SINGLE HUNG - TYPE 2" | object type "085000 - Windows - Double Hung:SINGLE HUNG - TYPE 2" | names: "085000 - Windows - Double Hung:SINGLE HUNG - TYPE 2:4200969", "085000 - Windows - Double Hung:SINGLE HUNG - TYPE 2:4201019" | material: constituents "MaterialConstituentSet" ("DOUBLE HUNG WINDOWS - BLACK EXT/INT SASH - LIMIT BOTTOM SASH TO 4" MAX OPEN": "DOUBLE HUNG WINDOWS - BLACK EXT/INT SASH - LIMIT BOTTOM SASH TO 4" MAX OPEN", "WINDOW SASH/TRIM": "WINDOW SASH/TRIM", "GL - INSULATED - LOW-E": "GL - INSULATED - LOW-E") | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators, Pset_ManufacturerTypeInformation
          2 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "085000 - Windows - Double Hung:SINGLE HUNG - TYPE 1" | object type "085000 - Windows - Double Hung:SINGLE HUNG - TYPE 1" | names: "085000 - Windows - Double Hung:SINGLE HUNG - TYPE 1:4200970", "085000 - Windows - Double Hung:SINGLE HUNG - TYPE 1:4201020" | material: constituents "MaterialConstituentSet" ("DOUBLE HUNG WINDOWS - BLACK EXT/INT SASH - LIMIT BOTTOM SASH TO 4" MAX OPEN": "DOUBLE HUNG WINDOWS - BLACK EXT/INT SASH - LIMIT BOTTOM SASH TO 4" MAX OPEN", "WINDOW SASH/TRIM": "WINDOW SASH/TRIM", "GL - INSULATED - LOW-E": "GL - INSULATED - LOW-E") | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators, Pset_ManufacturerTypeInformation
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4201628" | names: "4201628" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4201630" | names: "4201630" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4201631" | names: "4201631" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4201632" | names: "4201632" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4201633" | names: "4201633" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4201634" | names: "4201634" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4201636" | names: "4201636" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4201637" | names: "4201637" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4201638" | names: "4201638" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4201639" | names: "4201639" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4201640" | names: "4201640" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4201641" | names: "4201641" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4201746" | names: "4201746" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4201747" | names: "4201747" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4201748" | names: "4201748" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4201749" | names: "4201749" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4201750" | names: "4201750" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4201760" | names: "4201760" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4201761" | names: "4201761" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4201762" | names: "4201762" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4201763" | names: "4201763" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4201764" | names: "4201764" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4201767" | names: "4201767" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4201768" | names: "4201768" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4201769" | names: "4201769" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4201770" | names: "4201770" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4201771" | names: "4201771" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4201781" | names: "4201781" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4201782" | names: "4201782" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4201783" | names: "4201783" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4201784" | names: "4201784" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4201785" | names: "4201785" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4206952" | names: "4206952" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4206953" | names: "4206953" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4206954" | names: "4206954" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4207058" | names: "4207058" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4207059" | names: "4207059" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4207060" | names: "4207060" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4207271" | names: "4207271" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4207557" | names: "4207557" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          2 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "085000 - Windows - Double Hung:SINGLE HUNG - TYPE 2" | object type "085000 - Windows - Double Hung:SINGLE HUNG - TYPE 2" | names: "085000 - Windows - Double Hung:SINGLE HUNG - TYPE 2:4207586", "085000 - Windows - Double Hung:SINGLE HUNG - TYPE 2:4207596" | material: constituents "MaterialConstituentSet" ("DOUBLE HUNG WINDOWS - BLACK EXT/INT SASH - LIMIT BOTTOM SASH TO 4" MAX OPEN": "DOUBLE HUNG WINDOWS - BLACK EXT/INT SASH - LIMIT BOTTOM SASH TO 4" MAX OPEN", "WINDOW SASH/TRIM": "WINDOW SASH/TRIM", "GL - INSULATED - LOW-E": "GL - INSULATED - LOW-E") | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators, Pset_ManufacturerTypeInformation
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "085000 - Windows - Double Hung:SINGLE HUNG - TYPE 1" | object type "085000 - Windows - Double Hung:SINGLE HUNG - TYPE 1" | names: "085000 - Windows - Double Hung:SINGLE HUNG - TYPE 1:4207587" | material: constituents "MaterialConstituentSet" ("DOUBLE HUNG WINDOWS - BLACK EXT/INT SASH - LIMIT BOTTOM SASH TO 4" MAX OPEN": "DOUBLE HUNG WINDOWS - BLACK EXT/INT SASH - LIMIT BOTTOM SASH TO 4" MAX OPEN", "WINDOW SASH/TRIM": "WINDOW SASH/TRIM", "GL - INSULATED - LOW-E": "GL - INSULATED - LOW-E") | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators, Pset_ManufacturerTypeInformation
          1 x IFCSLAB | type IFCSLABTYPE "Floor:FLOOR TRUSS" | object type "Floor:FLOOR TRUSS" | FLOOR | names: "Floor:FLOOR TRUSS:4211685" | material: layers "Floor:FLOOR TRUSS" ("HARDWOOD FLOOR" 0.0625, "3/4" GYP. CRETE TOPPING" 0.0625, "1/8" SOUND MAT" 0.0104166666666667, "3/4" CDX/OSB PLYWOOD - SEE STRUCT DWGS" 0.0625, "WOOD TRUSS FLOOR ASSEMBLY - (FILL CAVITY W/ CELLULOSE BLOWN-IN INSULATION) (UL - L521 FLOOR ASSEMBLY)" 1.5, "25 GA. RESILIENT CHANNEL - 24" O.C." 0.0416666666666667, "5/8" GYP. BD @ CEILING" 0.0520833333333333) | property sets: Pset_EnvironmentalImpactIndicators, Pset_ManufacturerTypeInformation, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          8 x IFCWALL | type IFCWALLTYPE "Basic Wall:SHEAR - W4_5D - (5/8 GYP - 2X4 WOOD(BATT))" | object type "Basic Wall:SHEAR - W4_5D - (5/8 GYP - 2X4 WOOD(BATT))" | names: "Basic Wall:SHEAR - W4_5D - (5/8 GYP - 2X4 WOOD(BATT)):4250174", "Basic Wall:SHEAR - W4_5D - (5/8 GYP - 2X4 WOOD(BATT)):4250240", "Basic Wall:SHEAR - W4_5D - (5/8 GYP - 2X4 WOOD(BATT)):4250313" (+5 more) | material: layers "Basic Wall:SHEAR - W4_5D - (5/8 GYP - 2X4 WOOD(BATT))" ("AIR GAP" 0.0416666666666667, "2x4 STUDS (1ST FL @ 8" O.C. • 2ND FL @ 12" O.C. • 3RD FL @ 16" O.C.) - BATT. INSULATION AT STUD CAVITY" 0.291666666666667, "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" 0.0520833333333333) | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          2 x IFCWALL | type IFCWALLTYPE "Basic Wall:SHEAR - W4H5D - (5/8 GYP - 1/2 WSP - 2X4 WOOD(BATT))" | object type "Basic Wall:SHEAR - W4H5D - (5/8 GYP - 1/2 WSP - 2X4 WOOD(BATT))" | names: "Basic Wall:SHEAR - W4H5D - (5/8 GYP - 1/2 WSP - 2X4 WOOD(BATT)):4250251", "Basic Wall:SHEAR - W4H5D - (5/8 GYP - 1/2 WSP - 2X4 WOOD(BATT)):4250305" | material: layers "Basic Wall:SHEAR - W4H5D - (5/8 GYP - 1/2 WSP - 2X4 WOOD(BATT))" ("AIR GAP" 0.0416666666666667, "2x4 STUDS (1ST FL @ 8" O.C. • 2ND FL @ 12" O.C. • 3RD FL @ 16" O.C.) - BATT. INSULATION AT STUD CAVITY" 0.291666666666667, "WOOD STRUCTURAL PANEL (WSP) - SEE STRUCT DWGS" 0.0416666666666667, "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" 0.0520833333333333) | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCROOF | type IFCROOFTYPE "Basic Roof:CRICKETS" | object type "Basic Roof:CRICKETS" | names: "Basic Roof:CRICKETS:4302797" | material: layers "Basic Roof:CRICKETS" ("TPO ROOFING MEMBRANE" 0.0208333333333333, "1" MIN. POLYISO INSULATION OVER UNDERLAYMENT (WRAP UP/OVER PARAPET)" 0.0833333333333333, "3/4" CDX/OSB PLYWOOD - SEE STRUCT DWGS" 0.0625) | property sets: Pset_EnvironmentalImpactIndicators, Pset_RoofCommon
          1 x IFCROOF | type IFCROOFTYPE "Basic Roof:WOOD-FRAMED ROOF ABOVE 3RD FLOOR" | object type "Basic Roof:WOOD-FRAMED ROOF ABOVE 3RD FLOOR" | names: "Basic Roof:WOOD-FRAMED ROOF ABOVE 3RD FLOOR:4303264" | material: layers "Basic Roof:WOOD-FRAMED ROOF ABOVE 3RD FLOOR" ("TPO ROOFING MEMBRANE" 0.0208333333333333, "1" MIN. POLYISO INSULATION OVER UNDERLAYMENT (WRAP UP/OVER PARAPET)" 0.0833333333333333, "3/4" CDX/OSB PLYWOOD - SEE STRUCT DWGS" 0.0625, "TRAPEZOIDAL WOOD TRUSS ROOF ASSEMBLY - (FILL CAVITY W/ CELLULOSE BLOWN-IN INSULATION) (R-VALUE = 50)" 1.5, "5/8" GYP. BD @ CEILING" 0.0520833333333333) | property sets: Pset_EnvironmentalImpactIndicators, Pset_RoofCommon
          1 x IFCROOF | type IFCROOFTYPE "Basic Roof:CRICKETS" | object type "Basic Roof:CRICKETS" | names: "Basic Roof:CRICKETS:4303304" | material: layers "Basic Roof:CRICKETS" ("TPO ROOFING MEMBRANE" 0.0208333333333333, "1" MIN. POLYISO INSULATION OVER UNDERLAYMENT (WRAP UP/OVER PARAPET)" 0.0833333333333333, "3/4" CDX/OSB PLYWOOD - SEE STRUCT DWGS" 0.0625) | property sets: Pset_EnvironmentalImpactIndicators, Pset_RoofCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4303746" | names: "4303746" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCROOF | type IFCROOFTYPE "Basic Roof:WOOD-FRAMED ROOF ABOVE 3RD FLOOR" | object type "Basic Roof:WOOD-FRAMED ROOF ABOVE 3RD FLOOR" | names: "Basic Roof:WOOD-FRAMED ROOF ABOVE 3RD FLOOR:4303980" | material: layers "Basic Roof:WOOD-FRAMED ROOF ABOVE 3RD FLOOR" ("TPO ROOFING MEMBRANE" 0.0208333333333333, "1" MIN. POLYISO INSULATION OVER UNDERLAYMENT (WRAP UP/OVER PARAPET)" 0.0833333333333333, "3/4" CDX/OSB PLYWOOD - SEE STRUCT DWGS" 0.0625, "TRAPEZOIDAL WOOD TRUSS ROOF ASSEMBLY - (FILL CAVITY W/ CELLULOSE BLOWN-IN INSULATION) (R-VALUE = 50)" 1.5, "5/8" GYP. BD @ CEILING" 0.0520833333333333) | property sets: Pset_EnvironmentalImpactIndicators, Pset_RoofCommon
          1 x IFCROOF | type IFCROOFTYPE "Basic Roof:CRICKETS" | object type "Basic Roof:CRICKETS" | names: "Basic Roof:CRICKETS:4303987" | material: layers "Basic Roof:CRICKETS" ("TPO ROOFING MEMBRANE" 0.0208333333333333, "1" MIN. POLYISO INSULATION OVER UNDERLAYMENT (WRAP UP/OVER PARAPET)" 0.0833333333333333, "3/4" CDX/OSB PLYWOOD - SEE STRUCT DWGS" 0.0625) | property sets: Pset_EnvironmentalImpactIndicators, Pset_RoofCommon
          1 x IFCROOF | type IFCROOFTYPE "Basic Roof:WOOD-FRAMED ROOF ABOVE 3RD FLOOR" | object type "Basic Roof:WOOD-FRAMED ROOF ABOVE 3RD FLOOR" | names: "Basic Roof:WOOD-FRAMED ROOF ABOVE 3RD FLOOR:4305892" | material: layers "Basic Roof:WOOD-FRAMED ROOF ABOVE 3RD FLOOR" ("TPO ROOFING MEMBRANE" 0.0208333333333333, "1" MIN. POLYISO INSULATION OVER UNDERLAYMENT (WRAP UP/OVER PARAPET)" 0.0833333333333333, "3/4" CDX/OSB PLYWOOD - SEE STRUCT DWGS" 0.0625, "TRAPEZOIDAL WOOD TRUSS ROOF ASSEMBLY - (FILL CAVITY W/ CELLULOSE BLOWN-IN INSULATION) (R-VALUE = 50)" 1.5, "5/8" GYP. BD @ CEILING" 0.0520833333333333) | property sets: Pset_EnvironmentalImpactIndicators, Pset_RoofCommon
          1 x IFCROOF | type IFCROOFTYPE "Basic Roof:CRICKETS" | object type "Basic Roof:CRICKETS" | names: "Basic Roof:CRICKETS:4305901" | material: layers "Basic Roof:CRICKETS" ("TPO ROOFING MEMBRANE" 0.0208333333333333, "1" MIN. POLYISO INSULATION OVER UNDERLAYMENT (WRAP UP/OVER PARAPET)" 0.0833333333333333, "3/4" CDX/OSB PLYWOOD - SEE STRUCT DWGS" 0.0625) | property sets: Pset_EnvironmentalImpactIndicators, Pset_RoofCommon
          1 x IFCROOF | type IFCROOFTYPE "Basic Roof:WOOD-FRAMED ROOF ABOVE 3RD FLOOR" | object type "Basic Roof:WOOD-FRAMED ROOF ABOVE 3RD FLOOR" | names: "Basic Roof:WOOD-FRAMED ROOF ABOVE 3RD FLOOR:4306691" | material: layers "Basic Roof:WOOD-FRAMED ROOF ABOVE 3RD FLOOR" ("TPO ROOFING MEMBRANE" 0.0208333333333333, "1" MIN. POLYISO INSULATION OVER UNDERLAYMENT (WRAP UP/OVER PARAPET)" 0.0833333333333333, "3/4" CDX/OSB PLYWOOD - SEE STRUCT DWGS" 0.0625, "TRAPEZOIDAL WOOD TRUSS ROOF ASSEMBLY - (FILL CAVITY W/ CELLULOSE BLOWN-IN INSULATION) (R-VALUE = 50)" 1.5, "5/8" GYP. BD @ CEILING" 0.0520833333333333) | property sets: Pset_EnvironmentalImpactIndicators, Pset_RoofCommon
          1 x IFCROOF | type IFCROOFTYPE "Basic Roof:CRICKETS" | object type "Basic Roof:CRICKETS" | names: "Basic Roof:CRICKETS:4306700" | material: layers "Basic Roof:CRICKETS" ("TPO ROOFING MEMBRANE" 0.0208333333333333, "1" MIN. POLYISO INSULATION OVER UNDERLAYMENT (WRAP UP/OVER PARAPET)" 0.0833333333333333, "3/4" CDX/OSB PLYWOOD - SEE STRUCT DWGS" 0.0625) | property sets: Pset_EnvironmentalImpactIndicators, Pset_RoofCommon
          1 x IFCROOF | type IFCROOFTYPE "Basic Roof:WOOD-FRAMED ROOF ABOVE 3RD FLOOR" | object type "Basic Roof:WOOD-FRAMED ROOF ABOVE 3RD FLOOR" | names: "Basic Roof:WOOD-FRAMED ROOF ABOVE 3RD FLOOR:4306779" | material: layers "Basic Roof:WOOD-FRAMED ROOF ABOVE 3RD FLOOR" ("TPO ROOFING MEMBRANE" 0.0208333333333333, "1" MIN. POLYISO INSULATION OVER UNDERLAYMENT (WRAP UP/OVER PARAPET)" 0.0833333333333333, "3/4" CDX/OSB PLYWOOD - SEE STRUCT DWGS" 0.0625, "TRAPEZOIDAL WOOD TRUSS ROOF ASSEMBLY - (FILL CAVITY W/ CELLULOSE BLOWN-IN INSULATION) (R-VALUE = 50)" 1.5, "5/8" GYP. BD @ CEILING" 0.0520833333333333) | property sets: Pset_EnvironmentalImpactIndicators, Pset_RoofCommon
          1 x IFCROOF | type IFCROOFTYPE "Basic Roof:CRICKETS" | object type "Basic Roof:CRICKETS" | names: "Basic Roof:CRICKETS:4306786" | material: layers "Basic Roof:CRICKETS" ("TPO ROOFING MEMBRANE" 0.0208333333333333, "1" MIN. POLYISO INSULATION OVER UNDERLAYMENT (WRAP UP/OVER PARAPET)" 0.0833333333333333, "3/4" CDX/OSB PLYWOOD - SEE STRUCT DWGS" 0.0625) | property sets: Pset_EnvironmentalImpactIndicators, Pset_RoofCommon
          2 x IFCFLOWTERMINAL | type IFCDISTRIBUTIONELEMENTTYPE "22142613 - Roof Drains - Type A:22142613 - Roof Drains - Type A" | object type "22142613 - Roof Drains - Type A:22142613 - Roof Drains - Type A" | names: "22142613 - Roof Drains - Type A:22142613 - Roof Drains - Type A:4364255", "22142613 - Roof Drains - Type A:22142613 - Roof Drains - Type A:4364637" | material: "ROOF DRAIN, TYP. (SEE PLUMB DWGS) - W/ INTEGRATED EMERGENCY OVERFLOW DRAIN" | property sets: Pset_EnvironmentalImpactIndicators
          4 x IFCFLOWTERMINAL | type IFCDISTRIBUTIONELEMENTTYPE "22142613 - Roof Drains - Type A:22142613 - Roof Drains - Type A" | object type "22142613 - Roof Drains - Type A:22142613 - Roof Drains - Type A" | names: "22142613 - Roof Drains - Type A:22142613 - Roof Drains - Type A:4364649", "22142613 - Roof Drains - Type A:22142613 - Roof Drains - Type A:4364650", "22142613 - Roof Drains - Type A:22142613 - Roof Drains - Type A:4364678" (+1 more) | material: "ROOF DRAIN, TYP. (SEE PLUMB DWGS) - W/ INTEGRATED EMERGENCY OVERFLOW DRAIN" | property sets: Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Hatch-Precision_Ladders-Roof_Hatch:PH-(A) 2’-6” X 3’-0”" | object type "Hatch-Precision_Ladders-Roof_Hatch:PH-(A) 2’-6” X 3’-0”" | names: "Hatch-Precision_Ladders-Roof_Hatch:PH-(A) 2’-6” X 3’-0”:4381049" | material: constituents "MaterialConstituentSet" ("Insulation -Precision Ladders LLC - Rigid Fiber": "Insulation -Precision Ladders LLC - Rigid Fiber", "ROOF HATCH": "ROOF HATCH") | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators, Pset_ManufacturerTypeInformation
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Egress - Path of Travel:Egress - Path of Travel" | object type "Egress - Path of Travel:Egress - Path of Travel" | names: "Egress - Path of Travel:Egress - Path of Travel:4384098" | material: "<Unnamed>" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Egress - Path of Travel:Egress - Path of Travel" | object type "Egress - Path of Travel:Egress - Path of Travel" | names: "Egress - Path of Travel:Egress - Path of Travel:4384487" | material: "<Unnamed>" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Egress - Path of Travel:Egress - Path of Travel" | object type "Egress - Path of Travel:Egress - Path of Travel" | names: "Egress - Path of Travel:Egress - Path of Travel:4384530" | material: "<Unnamed>" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Egress - Path of Travel:Egress - Path of Travel" | object type "Egress - Path of Travel:Egress - Path of Travel" | names: "Egress - Path of Travel:Egress - Path of Travel:4384569" | material: "<Unnamed>" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Egress - Path of Travel:Egress - Path of Travel" | object type "Egress - Path of Travel:Egress - Path of Travel" | names: "Egress - Path of Travel:Egress - Path of Travel:4384608" | material: "<Unnamed>" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Egress - Path of Travel:Egress - Path of Travel" | object type "Egress - Path of Travel:Egress - Path of Travel" | names: "Egress - Path of Travel:Egress - Path of Travel:4384647" | material: "<Unnamed>" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Egress - Path of Travel:Egress - Path of Travel" | object type "Egress - Path of Travel:Egress - Path of Travel" | names: "Egress - Path of Travel:Egress - Path of Travel:4384696" | material: "<Unnamed>" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          9 x IFCPUMP | type IFCPUMPTYPE "HVAC_Air-Conditioning_Fujitsu General_AOYG22-24KATA:AOYG22KATA" | object type "HVAC_Air-Conditioning_Fujitsu General_AOYG22-24KATA:AOYG22KATA" | names: "HVAC_Air-Conditioning_Fujitsu General_AOYG22-24KATA:AOYG22KATA:4390544", "HVAC_Air-Conditioning_Fujitsu General_AOYG22-24KATA:AOYG22KATA:4574048", "HVAC_Air-Conditioning_Fujitsu General_AOYG22-24KATA:AOYG22KATA:4606125" (+6 more) | material: constituents "MaterialConstituentSet" ("MINI SPLIT CONDENSER - REF. MECH. DWGS": "MINI SPLIT CONDENSER - REF. MECH. DWGS", "Color RGB 040-040-040": "Color RGB 040-040-040", "<Unnamed>": "<Unnamed>") | property sets: Pset_EnvironmentalImpactIndicators, Pset_ManufacturerTypeInformation, Pset_PumpTypeCommon
          9 x IFCPUMP | type IFCPUMPTYPE "HVAC_Air-Conditioning_Fujitsu General_AOYG22-24KATA:AOYG22KATA" | object type "HVAC_Air-Conditioning_Fujitsu General_AOYG22-24KATA:AOYG22KATA" | names: "HVAC_Air-Conditioning_Fujitsu General_AOYG22-24KATA:AOYG22KATA:4390566", "HVAC_Air-Conditioning_Fujitsu General_AOYG22-24KATA:AOYG22KATA:4573993", "HVAC_Air-Conditioning_Fujitsu General_AOYG22-24KATA:AOYG22KATA:4605992" (+6 more) | material: constituents "MaterialConstituentSet" ("MINI SPLIT CONDENSER - REF. MECH. DWGS": "MINI SPLIT CONDENSER - REF. MECH. DWGS", "Color RGB 040-040-040": "Color RGB 040-040-040", "<Unnamed>": "<Unnamed>") | property sets: Pset_EnvironmentalImpactIndicators, Pset_ManufacturerTypeInformation, Pset_PumpTypeCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4397245" | names: "4397245" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4397252" | names: "4397252" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4397358" | names: "4397358" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4397360" | names: "4397360" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4397379" | names: "4397379" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4397383" | names: "4397383" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4397407" | names: "4397407" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4397409" | names: "4397409" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4397413" | names: "4397413" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4397415" | names: "4397415" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4398212" | names: "4398212" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4398219" | names: "4398219" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4401982" | names: "4401982" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4401984" | names: "4401984" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4402004" | names: "4402004" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4402008" | names: "4402008" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4402040" | names: "4402040" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4402042" | names: "4402042" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4402046" | names: "4402046" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4402048" | names: "4402048" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4411108" | names: "4411108" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4411109" | names: "4411109" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4411111" | names: "4411111" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4411113" | names: "4411113" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4411115" | names: "4411115" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4411116" | names: "4411116" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4411121" | names: "4411121" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4411123" | names: "4411123" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4412291" | names: "4412291" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4412308" | names: "4412308" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4413181" | names: "4413181" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4413183" | names: "4413183" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4413185" | names: "4413185" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4413187" | names: "4413187" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4413203" | names: "4413203" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4413205" | names: "4413205" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4413207" | names: "4413207" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4413209" | names: "4413209" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4413216" | names: "4413216" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4413218" | names: "4413218" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4413220" | names: "4413220" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4413236" | names: "4413236" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4413240" | names: "4413240" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4413242" | names: "4413242" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4414297" | names: "4414297" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4414824" | names: "4414824" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4414826" | names: "4414826" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4414827" | names: "4414827" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4414828" | names: "4414828" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4414829" | names: "4414829" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4414830" | names: "4414830" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4414831" | names: "4414831" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4414832" | names: "4414832" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4414833" | names: "4414833" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4414834" | names: "4414834" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4414835" | names: "4414835" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4414836" | names: "4414836" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4414837" | names: "4414837" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4415168" | names: "4415168" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4415169" | names: "4415169" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4415170" | names: "4415170" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4415183" | names: "4415183" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4415184" | names: "4415184" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4415185" | names: "4415185" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4415732" | names: "4415732" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4415745" | names: "4415745" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4416242" | names: "4416242" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4416243" | names: "4416243" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4416244" | names: "4416244" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4416245" | names: "4416245" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4416246" | names: "4416246" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4416256" | names: "4416256" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4416257" | names: "4416257" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4416258" | names: "4416258" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4416259" | names: "4416259" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4416260" | names: "4416260" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4416263" | names: "4416263" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4416264" | names: "4416264" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4416265" | names: "4416265" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4416266" | names: "4416266" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4416267" | names: "4416267" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4416277" | names: "4416277" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4416278" | names: "4416278" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4416279" | names: "4416279" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4416280" | names: "4416280" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4416281" | names: "4416281" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4416525" | names: "4416525" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4416526" | names: "4416526" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4416527" | names: "4416527" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4416640" | names: "4416640" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4417253" | names: "4417253" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4417254" | names: "4417254" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4419410" | names: "4419410" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4419411" | names: "4419411" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4419782" | names: "4419782" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4419791" | names: "4419791" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4420943" | names: "4420943" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4420951" | names: "4420951" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4420955" | names: "4420955" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4420963" | names: "4420963" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          10 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Heat_Pump_Unit-Multi_Zone-Outdoor-Daikin-2MXL18QMVJU:1.5Ton_2MXL18QMVJUA" | object type "Heat_Pump_Unit-Multi_Zone-Outdoor-Daikin-2MXL18QMVJU:1.5Ton_2MXL18QMVJUA" | names: "Heat_Pump_Unit-Multi_Zone-Outdoor-Daikin-2MXL18QMVJU:1.5Ton_2MXL18QMVJUA:4425254", "Heat_Pump_Unit-Multi_Zone-Outdoor-Daikin-2MXL18QMVJU:1.5Ton_2MXL18QMVJUA:4428535", "Heat_Pump_Unit-Multi_Zone-Outdoor-Daikin-2MXL18QMVJU:1.5Ton_2MXL18QMVJUA:4428635" (+7 more) | material: constituents "MaterialConstituentSet" ("blue": "blue", "BLACK": "BLACK", "<Unnamed>": "<Unnamed>", "Metal - Daikin - Copper": "Metal - Daikin - Copper", "Metal - Daikin - Paint Finish - Ivory White": "Metal - Daikin - Paint Finish - Ivory White") | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators, Pset_ManufacturerTypeInformation
          2 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Heat_Pump_Unit-Multi_Zone-Outdoor-Daikin-2MXL18QMVJU:1.5Ton_2MXL18QMVJUA" | object type "Heat_Pump_Unit-Multi_Zone-Outdoor-Daikin-2MXL18QMVJU:1.5Ton_2MXL18QMVJUA" | names: "Heat_Pump_Unit-Multi_Zone-Outdoor-Daikin-2MXL18QMVJU:1.5Ton_2MXL18QMVJUA:4428943", "Heat_Pump_Unit-Multi_Zone-Outdoor-Daikin-2MXL18QMVJU:1.5Ton_2MXL18QMVJUA:4428944" | material: constituents "MaterialConstituentSet" ("blue": "blue", "BLACK": "BLACK", "<Unnamed>": "<Unnamed>", "Metal - Daikin - Copper": "Metal - Daikin - Copper", "Metal - Daikin - Paint Finish - Ivory White": "Metal - Daikin - Paint Finish - Ivory White") | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators, Pset_ManufacturerTypeInformation
          12 x IFCWALL | type IFCWALLTYPE "Basic Wall:shaft" | object type "Basic Wall:shaft" | names: "Basic Wall:shaft:4436573", "Basic Wall:shaft:4436575", "Basic Wall:shaft:4436578" (+9 more) | material: layers "Basic Wall:shaft" ("16 GA. PERFORATED GALV. STEEL PANEL" 0.0104166666666667, "METAL STUD - GALV. - 16" O.C." 0.166666666666667) | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Indoor Unit - Evaporator - Air_Conditioner-Single_Zone-Indoor-Daikin-FTKN_NMVJU:Indoor Unit - Evaporator - 1.5Ton_FTKN18NMVJU" | object type "Indoor Unit - Evaporator - Air_Conditioner-Single_Zone-Indoor-Daikin-FTKN_NMVJU:Indoor Unit - Evaporator - 1.5Ton_FTKN18NMVJU" | names: "Indoor Unit - Evaporator - Air_Conditioner-Single_Zone-Indoor-Daikin-FTKN_NMVJU:Indoor Unit - Evaporator - 1.5Ton_FTKN18NMVJU:4444213" | material: constituents "MaterialConstituentSet" ("Metal - Daikin - Galvanized Steel": "Metal - Daikin - Galvanized Steel", "Metal - Daikin - Copper": "Metal - Daikin - Copper") | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators, Pset_ManufacturerTypeInformation
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Indoor Unit - Evaporator - Air_Conditioner-Single_Zone-Indoor-Daikin-FTKN_NMVJU:Indoor Unit - Evaporator - 1.5Ton_FTKN18NMVJU" | object type "Indoor Unit - Evaporator - Air_Conditioner-Single_Zone-Indoor-Daikin-FTKN_NMVJU:Indoor Unit - Evaporator - 1.5Ton_FTKN18NMVJU" | names: "Indoor Unit - Evaporator - Air_Conditioner-Single_Zone-Indoor-Daikin-FTKN_NMVJU:Indoor Unit - Evaporator - 1.5Ton_FTKN18NMVJU:4451656" | material: constituents "MaterialConstituentSet" ("Metal - Daikin - Galvanized Steel": "Metal - Daikin - Galvanized Steel", "Metal - Daikin - Copper": "Metal - Daikin - Copper") | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators, Pset_ManufacturerTypeInformation
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4454413" | names: "4454413" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4454414" | names: "4454414" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4454422" | names: "4454422" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4454423" | names: "4454423" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4475739" | names: "4475739" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4478034" | names: "4478034" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4494576" | names: "4494576" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4494577" | names: "4494577" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4494579" | names: "4494579" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4494581" | names: "4494581" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4494583" | names: "4494583" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4494587" | names: "4494587" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4494589" | names: "4494589" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4494590" | names: "4494590" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4495778" | names: "4495778" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4495792" | names: "4495792" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4496653" | names: "4496653" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4496655" | names: "4496655" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4496657" | names: "4496657" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4496659" | names: "4496659" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4496675" | names: "4496675" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4496677" | names: "4496677" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4496679" | names: "4496679" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4496681" | names: "4496681" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4496686" | names: "4496686" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4496688" | names: "4496688" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4496690" | names: "4496690" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4496692" | names: "4496692" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4496708" | names: "4496708" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4496710" | names: "4496710" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4496712" | names: "4496712" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4496714" | names: "4496714" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4537880" | names: "4537880" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4537881" | names: "4537881" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4538107" | names: "4538107" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "4538108" | names: "4538108" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          5 x IFCWALL | type IFCWALLTYPE "Basic Wall:FIRE SEPERATION IN CAVITY" | object type "Basic Wall:FIRE SEPERATION IN CAVITY" | names: "Basic Wall:FIRE SEPERATION IN CAVITY:4598261", "Basic Wall:FIRE SEPERATION IN CAVITY:4598292", "Basic Wall:FIRE SEPERATION IN CAVITY:4598409" (+2 more) | material: layers "Basic Wall:FIRE SEPERATION IN CAVITY" ("5/8" GYP. BD" 0.0520833333333333, "LVL RIM BOARD - SEE STRUCT. DWGS" 0.0833333333333333, "5/8" GYP. BD" 0.0520833333333333) | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCALARM | type IFCALARMTYPE "104416 - Fire Extinguishers - Wall:Class A - Light - 2A" | object type "104416 - Fire Extinguishers - Wall:Class A - Light - 2A" | names: "104416 - Fire Extinguishers - Wall:Class A - Light - 2A:4609066" | material: constituents "MaterialConstituentSet" ("FIRE EXTINGUISHER": "FIRE EXTINGUISHER", "Metal - Paint Finish - Black, Matte": "Metal - Paint Finish - Black, Matte", "<Unnamed>": "<Unnamed>") | property sets: Pset_EnvironmentalImpactIndicators, Pset_OpeningElementCommon
          1 x IFCALARM | type IFCALARMTYPE "104416 - Fire Extinguishers - Wall:Class A - Light - 2A" | object type "104416 - Fire Extinguishers - Wall:Class A - Light - 2A" | names: "104416 - Fire Extinguishers - Wall:Class A - Light - 2A:4609067" | material: constituents "MaterialConstituentSet" ("FIRE EXTINGUISHER": "FIRE EXTINGUISHER", "Metal - Paint Finish - Black, Matte": "Metal - Paint Finish - Black, Matte", "<Unnamed>": "<Unnamed>") | property sets: Pset_EnvironmentalImpactIndicators, Pset_OpeningElementCommon
        IFCSPACE "131" | long name "1BD-T1" | SPACE
          contains 2 elements
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Egress - Path of Travel:Egress - Path of Travel" | object type "Egress - Path of Travel:Egress - Path of Travel" | names: "Egress - Path of Travel:Egress - Path of Travel:4383992" | material: "<Unnamed>" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Egress - Path of Travel:Egress - Path of Travel" | object type "Egress - Path of Travel:Egress - Path of Travel" | names: "Egress - Path of Travel:Egress - Path of Travel:4385058" | material: "<Unnamed>" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
        IFCSPACE "132" | long name "STUDIO - T2" | SPACE
        IFCSPACE "133" | long name "STUDIO - T1" | SPACE
        IFCSPACE "134" | long name "STUDIO - T1" | SPACE
        IFCSPACE "135" | long name "STUDIO - T2" | SPACE
        IFCSPACE "136" | long name "1BD-T1" | SPACE

Types
  IFCBUILDINGELEMENTPROXYTYPE "Surface:614023" | 1 occurrence
  IFCWALLTYPE "Generic Models 129:Generic Models 1" | 1 occurrence | material: "EXISTING SLAB" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 8:Generic Models 1" | 1 occurrence | material: "CONCRETE (3000 PSI CONCRETE)" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 141:Generic Models 1" | 1 occurrence | material: "#4 CONT. STEEL REBAR" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 144:Generic Models 1" | 1 occurrence | material: "#10 6x6 WIRE MESH" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 145:Generic Models 1" | 1 occurrence | material: "6 MIL VAPOR BARRIER" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 150:Generic Models 1" | 1 occurrence | material: "6" COMPACTED CRUSHED STONE" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 151:Generic Models 1" | 1 occurrence | material: "GRADE (SLOPE 2% MIN AWAY FROM BUILDING)_grass" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 183:Generic Models 1" | 1 occurrence | material: "STRUCTURAL WOOD COLUMN - SIZE TBD" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 177:Generic Models 1" | 1 occurrence | material: "STRUCTURAL WOOD COLUMN - SIZE TBD" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 178:Generic Models 155" | 1 occurrence | material: "CONCRETE (3000 PSI CONCRETE)" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 184:Generic Models 184" | 1 occurrence | material: "GRADE" | property sets: Pset_WallCommon
  IFCWALLTYPE "Basic Wall:GRADE BEAM - PERIMETER" | STANDARD | 5 occurrences | material: layers "Basic Wall:GRADE BEAM - PERIMETER" ("CONCRETE GRADE BEAM POURED WITH CONCRETE SLAB - SEE STRUCT DWGS" 1.5) | property sets: Pset_WallCommon
  IFCFOOTINGTYPE "Wall Foundation:12"X24"" | STRIP_FOOTING | 1 occurrence
  IFCFOOTINGTYPE "Wall Foundation:12"X24"" | STRIP_FOOTING | 1 occurrence
  IFCSLABTYPE "Foundation Slab:6" Foundation Slab" | BASESLAB | 1 occurrence | material: layers "Foundation Slab:6" Foundation Slab" ("6" CONCRETE SLAB (3000PSI MIN.) W/ #10 6X6 OVER 6 MIL POLYETHYLENE VAPOR BARRIER" 0.5) | property sets: Pset_SlabCommon
  IFCBUILDINGELEMENTPROXYTYPE "Slab Edge:Thickened 24" x 12"" | 1 occurrence | property sets: Pset_BuildingElementProxyCommon
  IFCSLABTYPE "Floor:6" COMPACTED CRUSHED STONE" | FLOOR | 1 occurrence | material: layers "Floor:6" COMPACTED CRUSHED STONE" ("6" COMPACTED CRUSHED STONE" 0.5) | property sets: Pset_SlabCommon
  IFCBUILDINGELEMENTPROXYTYPE "Surface:1313663" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "Surface:1313665" | 1 occurrence
  IFCSLABTYPE "Pad:GENERIC PAD" | FLOOR | 1 occurrence | material: layers "Pad:GENERIC PAD" ("PAD (TURNED OFF)" 0.5) | property sets: Pset_SlabCommon
  IFCWALLTYPE "Generic Models 269:Generic Models 263" | 1 occurrence | material: "CONCRETE CURB" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 270:Generic Models 263" | 1 occurrence | material: "CONCRETE CURB" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 271:Generic Models 263" | 1 occurrence | material: "PAVEMENT" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 274:Generic Models 263" | 1 occurrence | material: "8" CRUSHED 1.25" AGGREGATE BASE COURSE (COMPACTED)" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 275:Generic Models 263" | 1 occurrence | material: "COMPACTED SUBGRADE" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 277:Generic Models 263" | 1 occurrence | material: "PAVING SURFACE (TYP.) SEE PLANS" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 278:Generic Models 263" | 1 occurrence | material: "5" MIN. COMPACTED BASE AGGREGATE UNDER CURB" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 279:Generic Models 263" | 1 occurrence | material: "PAVING SURFACE (TYP.) SEE PLANS" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 280:Generic Models 263" | 1 occurrence | material: "5" MIN. COMPACTED BASE AGGREGATE UNDER CURB" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 281:Generic Models 263" | 1 occurrence | material: "3" TO 6" WASHED OR CLEAR STONE" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 286:Generic Models 263" | 1 occurrence | material: "6" CRUSHED AGGREGATE BASE COURSE" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 292:Generic Models 263" | 1 occurrence | material: "CONCRETE CURB" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 294:Generic Models 263" | 1 occurrence | material: "PAVING SURFACE (TYP.) SEE PLANS" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 295:Generic Models 263" | 1 occurrence | material: "CRUSHED AGGREGATE BASE COURSE" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 289:Generic Models 263" | 1 occurrence | material: "7" CONC. DRIVE APPROACH" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 297:Generic Models 263" | 1 occurrence | material: "SLOPED - 7" CONC." | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 298:Generic Models 263" | 1 occurrence | material: "SEE SITE PLAN FOR LANDSCAPING" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 299:Generic Models 263" | 1 occurrence | material: "CONCRETE CURB" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 300:Generic Models 263" | 1 occurrence | material: "CONCRETE CURB" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 282:Generic Models 263" | 1 occurrence | material: "CONCRETE CURB" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 301:Generic Models 263" | 1 occurrence | material: "CONCRETE CURB" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 290:Generic Models 263" | 1 occurrence | material: "GRADED BACKFILL" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 291:Generic Models 263" | 1 occurrence | material: "GRADED BACKFILL" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 306:Generic Models 263" | 1 occurrence | material: "EXISTING GRADE" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 307:Generic Models 263" | 1 occurrence | material: "CONCRETE PAVEMENT HEAVY DUTY" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 310:Generic Models 263" | 1 occurrence | material: "8" CRUSHED 1.25" AGGREGATE BASE COURSE (COMPACTED)" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 311:Generic Models 263" | 1 occurrence | material: "COMPACTED SUBGRADE" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 309:Generic Models 263" | 1 occurrence | material: "EPOXY COATED 6 X 6 X W2.9 X W2.9, PLACED 3" ABOVE SLAB BASE" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 283:Generic Models 263" | 1 occurrence | material: "SLOPED - 7" CONC." | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 284:Generic Models 263" | 1 occurrence | material: "SEE SITE PLAN FOR LANDSCAPING" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 276:Generic Models 263" | 1 occurrence | material: "1" EXPANSION JOINT" | property sets: Pset_WallCommon
  IFCWALLTYPE "Basic Wall:RATED - 1 HR" | STANDARD | 6 occurrences | material: layers "Basic Wall:RATED - 1 HR" ("Default Wall" 0.666666666666667) | property sets: Pset_WallCommon
  IFCSLABTYPE "316600 - Special Foundations - Diamond Pier - Generic:316600 - Special Foundations - Diamond Pier - Generic" | BASESLAB | 1 occurrence | material: "DIAMOND PIER DP-50/50 - (3300# B.L.C. AT 1500PSF SOILS, 4400# B.L.C. AT 2000PSF SOILS)" | property sets: Pset_SlabCommon
  IFCSLABTYPE "316600 - Special Foundations - Diamond Pier - Generic:316600 - Special Foundations - Diamond Pier - Generic" | BASESLAB | 1 occurrence | material: "DIAMOND PIER DP-50/50 - (3300# B.L.C. AT 1500PSF SOILS, 4400# B.L.C. AT 2000PSF SOILS)" | property sets: Pset_SlabCommon
  IFCSLABTYPE "316600 - Special Foundations - Diamond Pier - Generic:316600 - Special Foundations - Diamond Pier - Generic" | BASESLAB | 1 occurrence | material: "DIAMOND PIER DP-50/50 - (3300# B.L.C. AT 1500PSF SOILS, 4400# B.L.C. AT 2000PSF SOILS)" | property sets: Pset_SlabCommon
  IFCCOLUMNTYPE "Timber-Column:6x6" | COLUMN | 1 occurrence | material: profiles "6x6" ("6x6": "STRUCTURAL WOOD COLUMN - SIZE TBD") | property sets: Pset_ColumnCommon
  IFCCOLUMNTYPE "Timber-Column:6x6" | COLUMN | 1 occurrence | material: profiles "6x6" ("6x6": "STRUCTURAL WOOD COLUMN - SIZE TBD") | property sets: Pset_ColumnCommon
  IFCCOLUMNTYPE "Timber-Column:6x6" | COLUMN | 1 occurrence | material: profiles "6x6" ("6x6": "STRUCTURAL WOOD COLUMN - SIZE TBD") | property sets: Pset_ColumnCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 299:Generic Models 263" | 1 occurrence | material: "CONCRETE CURB" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 299:Generic Models 263" | 1 occurrence | material: "CONCRETE CURB" | property sets: Pset_BuildingElementProxyCommon
  IFCWALLTYPE "Generic Models 349:Generic Models 1" | 1 occurrence | material: "STRUCTURAL FLOOR - SEE STRUCT. DWGS" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 414:Generic Models 1" | 1 occurrence | material: "5/8" GYP. BD @ CEILING" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 423:Generic Models 1" | 1 occurrence | material: "7/8" FURRING CHANNELS @ 16" O.C." | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 424:Generic Models 1" | 1 occurrence | material: "7/8" FURRING CHANNELS @ 16" O.C." | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 425:Generic Models 1" | 1 occurrence | material: "7/8" FURRING CHANNELS @ 16" O.C." | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 428:Generic Models 1" | 1 occurrence | material: "R-19 BATT INSULATION" | property sets: Pset_WallCommon
  IFCWALLTYPE "Ground Rod:Ground Rod" | 1 occurrence | material: "5/8" x 8' GROUND ROD" | property sets: Pset_WallCommon
  IFCWALLTYPE "Light Pole Base Plate1:Light Pole Base Plate" | 1 occurrence | material: "(4) VERTICAL #6 REBAR" | property sets: Pset_WallCommon
  IFCWALLTYPE "Light Pole Base Plate2:Light Pole Base Plate" | 1 occurrence | material: "STEEL BASE PLATE" | property sets: Pset_WallCommon
  IFCWALLTYPE "Walls 126:Walls 126" | 1 occurrence | material: "24" DIA. CONCRETE POLE BASE WITH THOROSEAL FINISH" | property sets: Pset_WallCommon
  IFCWALLTYPE "Walls 127:Walls 126" | 1 occurrence | material: "Earth" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 500:Generic Models 1" | 1 occurrence | material: "STRUCTURAL FLOOR - SEE STRUCT. DWGS" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 11:Generic Models 1" | 1 occurrence | material: "STRUCTURAL FLOOR - SEE STRUCT. DWGS" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 28:Generic Models 1" | 1 occurrence | material: "STRUCTURAL FLOOR - SEE STRUCT. DWGS" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 238:Generic Models 1" | 1 occurrence | material: "STRUCTURAL FLOOR - SEE STRUCT. DWGS" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 446:Generic Models 1" | 1 occurrence | material: "STRUCTURAL FLOOR - SEE STRUCT. DWGS" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 26:Generic Models 1" | 1 occurrence | material: "OTHER WALL TYPE" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 514:Generic Models 1" | 1 occurrence | material: "STRUCTURAL FLOOR - SEE STRUCT. DWGS" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 537:Generic Models 1" | 1 occurrence | material: "STRUCTURAL FLOOR - SEE STRUCT. DWGS" | property sets: Pset_WallCommon
  IFCWALLTYPE "Light Pole Base Plate3:Light Pole Base Plate" | 1 occurrence | material: "1 1/2" GAVL. STEEL (RGS) CONDUIT" | property sets: Pset_WallCommon
  IFCWALLTYPE "Light Pole Base Plate4:Light Pole Base Plate" | 1 occurrence | material: "1 1/2" GAVL. STEEL (RGS) CONDUIT" | property sets: Pset_WallCommon
  IFCBUILDINGELEMENTPROXYTYPE "Model Text:OD_Very Large" | 1 occurrence | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Model Text:OD_Very Large" | 1 occurrence | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Model Text:OD_Very Large" | 1 occurrence | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Model Text:OD_Very Large" | 1 occurrence | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Model Text:OD_Very Large" | 1 occurrence | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Model Text:OD_Very Large" | 1 occurrence | property sets: Pset_BuildingElementProxyCommon
  IFCWALLTYPE "Generic Models 44:Generic Models 1" | 1 occurrence | material: "OPEN WEB WOOD TRUSS" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 40:Generic Models 1" | 1 occurrence | material: "OPEN WEB WOOD TRUSS" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 45:Generic Models 1" | 1 occurrence | material: "OPEN WEB WOOD TRUSS" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 50:Generic Models 1" | 1 occurrence | material: "OPEN WEB WOOD TRUSS" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 54:Generic Models 1" | 1 occurrence | material: "OPEN WEB WOOD TRUSS" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 8:Generic Models 1" | 1 occurrence | material: "CONCRETE (3000 PSI CONCRETE)" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 141:Generic Models 1" | 1 occurrence | material: "#4 CONT. STEEL REBAR" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 144:Generic Models 1" | 1 occurrence | material: "#10 6x6 WIRE MESH" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 213:Generic Models 1" | 1 occurrence | material: "5/8" GYP. BD (SHALL BEAR THE UL CERTIFICATION MARK)" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 216:Generic Models 1" | 1 occurrence | material: "7/8" FURRING CHANNELS @ 16" O.C." | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 217:Generic Models 1" | 1 occurrence | material: "7/8" FURRING CHANNELS @ 16" O.C." | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 218:Generic Models 1" | 1 occurrence | material: "7/8" FURRING CHANNELS @ 12" O.C." | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 221:Generic Models 1" | 1 occurrence | material: "R-19 BATT INSULATION" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 223:Generic Models 1" | 1 occurrence | material: "OPEN WEB WOOD TRUSS" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 224:Generic Models 1" | 1 occurrence | material: "OPEN WEB WOOD TRUSS" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 225:Generic Models 1" | 1 occurrence | material: "OPEN WEB WOOD TRUSS" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 226:Generic Models 1" | 1 occurrence | material: "OPEN WEB WOOD TRUSS" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 229:Generic Models 1" | 1 occurrence | material: "OPEN WEB WOOD TRUSS" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 230:Generic Models 1" | 1 occurrence | material: "5/8" GYP. BD (SHALL BEAR THE UL CERTIFICATION MARK)" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 231:Generic Models 1" | 1 occurrence | material: "5/8" GYP. BD @ CEILING (SHALL BEAR THE UL CERTIFICATION MARK)" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 430:Generic Models 1" | 1 occurrence | material: "NOMINAL 3/4" THICK, 48" WIDE GYPSUM BOARD - SEE UL LISTING FOR ADDITIONAL INFORMATION" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 797:Generic Models 1" | 1 occurrence | material: "GLASS FIBER OR MINERAL WOOL INSULATION BEARING THE UL CLASSIFICATION MARKING AS TO SURFACE BURNING CHARACTERISTICS AND/OR FIRE RESISTANCE - SEE UL LISTING FOR ADDITIONAL INFORMATION - FILL CAVITY" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 431:Generic Models 1" | 1 occurrence | material: "FORMED FROM MIN. 25 MSG GALV. STEEL SPACED MAX 24" O.C. PERPENDICULAR TO JOISTS - SEE UL LISTING FOR ADDITIONAL INFORMATION" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 433:Generic Models 1" | 1 occurrence | material: "EXISTING - 2X WOOD JOISTS" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 796:Generic Models 1" | 1 occurrence | material: "RESILIENT SOUND ISOLATION ACCESSORY SHALL BE USED AT EACH ATTACHMENT POINT OF THE RESILIENT CHANNELS AND SPACED MAX 16" O.C. - SEE UL LISTING FOR ADDITIONAL INFORMATION" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 421:Generic Models 1" | 1 occurrence | material: "RESILIENT SOUND ISOLATION ACCESSORY SHALL BE USED AT EACH ATTACHMENT POINT OF THE RESILIENT CHANNELS AND SPACED MAX 16" O.C. - SEE UL LISTING FOR ADDITIONAL INFORMATION" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 422:Generic Models 1" | 1 occurrence | material: "RESILIENT SOUND ISOLATION ACCESSORY SHALL BE USED AT EACH ATTACHMENT POINT OF THE RESILIENT CHANNELS AND SPACED MAX 16" O.C. - SEE UL LISTING FOR ADDITIONAL INFORMATION" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 233:Generic Models 1" | 1 occurrence | material: "EXISTING - 2X WOOD JOISTS" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 234:Generic Models 1" | 1 occurrence | material: "EXISTING - 2X WOOD JOISTS" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 235:Generic Models 1" | 1 occurrence | material: "ACOUSTICAL MATERIAL - SEE UL LISTING FOR RANGE OF OPTIONS" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 237:Generic Models 1" | 1 occurrence | material: "GLASS FIBER OR MINERAL WOOL INSULATION BEARING THE UL CLASSIFICATION MARKING AS TO SURFACE BURNING CHARACTERISTICS AND/OR FIRE RESISTANCE - SEE UL LISTING FOR ADDITIONAL INFORMATION - FILL CAVITY" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 239:Generic Models 1" | 1 occurrence | material: "EXISTING - 2X WOOD JOISTS" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 240:Generic Models 1" | 1 occurrence | material: "EXISTING - 2X WOOD JOISTS" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 241:Generic Models 1" | 1 occurrence | material: "EXISTING - 2X WOOD JOISTS" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 244:Generic Models 1" | 1 occurrence | material: "GALV. STEEL WITH TOTAL AREA OF DUCT OPENING NOT TO EXCEED 113 SQ. IN. PER 100 SQ. FT. OF CEILING AREA, AREA OF INDIVIDUAL DUCT OPENING NOT TO EXCEED 113 SQ. IN. MAX. DIMENSION OF OPENING 12" - SEE UL ..." | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 249:Generic Models 1" | 1 occurrence | material: "NO. 12 SWG GALV. STEEL WIRE, SUPPORTED FROM 16D NAILS DRIVEN THROUGH WOOD JOISTS 5" FROM BOTTOM OF JOISTS AND BENT UPWARD AT BOTH ENDS FOR POSITIVE SUPPORT - SEE UL LISTING FOR ADDITIONAL INFORMATION" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 253:Generic Models 1" | 1 occurrence | material: "20" X 48"/60" OR 24" X 48" - MAX OF 16 SQ FT PER 100 SQ FT OF CEILING AREA - OR - INCANDESCENT LAMP TYPE 6.5" DIA. X 7-1/2" HIGH - (4) FIXTURES PER 100 SQ FT OF CEILING AREA (USE FIXTURE" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 254:Generic Models 1" | 1 occurrence | material: "EXISTING - FLOOR BRIDGING" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 255:Generic Models 1" | 1 occurrence | material: "NO. 12 SWG GALV. STEEL WIRE, SUPPORTED FROM 16D NAILS DRIVEN THROUGH WOOD JOISTS 5" FROM BOTTOM OF JOISTS AND BENT UPWARD AT BOTH ENDS FOR POSITIVE SUPPORT - SEE UL LISTING FOR ADDITIONAL INFORMATION" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 256:Generic Models 1" | 1 occurrence | material: "EXISTING - FLOOR BRIDGING" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 257:Generic Models 1" | 1 occurrence | material: "ACOUSTICAL MATERIAL - SEE UL LISTING FOR RANGE OF OPTIONS" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 258:Generic Models 1" | 1 occurrence | material: "NOM 2 BY 4 IN. INSTALLED BETWEEN AND PERPENDICULAR TO WOOD JOISTS, AND CENTERED 5 IN. BELOW SUBFLOORING." | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 259:Generic Models 1" | 1 occurrence | material: "NO. 12 SWG GALV. STEEL WIRE, SUPPORTED FROM 16D NAILS DRIVEN THROUGH WOOD JOISTS 5" FROM BOTTOM OF JOISTS AND BENT UPWARD AT BOTH ENDS FOR POSITIVE SUPPORT - SEE UL LISTING FOR ADDITIONAL INFORMATION" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 260:Generic Models 1" | 1 occurrence | material: "STEEL FRAMING MEMBERS - SEE UL LISTING FOR RANGE OF OPTIONS" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 261:Generic Models 1" | 1 occurrence | material: "FIXTURE PROTECTION (IF NON-RATED FIXTURE) - SEE UL LISTING FOR SPECIFICS" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 262:Generic Models 1" | 1 occurrence | material: "GYPSUM BOARD — 5/8" X 4 FT WIDE GYPSUM BOARD, INSTALLED WITH LONG DIMENSION PERPENDICULAR TO CROSS TEES WITH SIDE JOINTS CENTERED ALONG MAIN RUNNERS." | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 265:Generic Models 1" | 1 occurrence | material: "GLASS FIBER OR MINERAL WOOL INSULATION BEARING THE UL CLASSIFICATION MARKING AS TO SURFACE BURNING CHARACTERISTICS AND/OR FIRE RESISTANCE - SEE UL LISTING FOR ADDITIONAL INFORMATION - FILL CAVITY" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 266:Generic Models 1" | 1 occurrence | material: "EXISTING - 2X WOOD JOISTS" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 267:Generic Models 1" | 1 occurrence | material: "EXISTING - 2X WOOD JOISTS" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 268:Generic Models 1" | 1 occurrence | material: "EXISTING - 2X WOOD JOISTS" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 296:Generic Models 1" | 1 occurrence | material: "AIR DUCT — MIN 0.029 IN. THICK (22 GAUGE) GALV STEEL AIR DUCT. TOTAL AREA OF DUCT OPENINGS NOT TO EXCEED 114 SQ IN. PER EACH 100 SQ FT OF CEILING AREA." | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 302:Generic Models 1" | 1 occurrence | material: "NO. 12 SWG GALV. STEEL WIRE, SUPPORTED FROM 16D NAILS DRIVEN THROUGH WOOD JOISTS 5" FROM BOTTOM OF JOISTS AND BENT UPWARD AT BOTH ENDS FOR POSITIVE SUPPORT - SEE UL LISTING FOR ADDITIONAL INFORMATION" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 303:Generic Models 1" | 1 occurrence | material: "2' x 4' RECESSED LIGHT FIXTURE WITH STEEL HOUSING AND 'FIXTURE PROTECTION' - SPACED TO NOT EXCEED 24 SQ FT PER 100 SQ FT OF CEILING AREA - SEE UL LISTING FOR MORE INFORMATION" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 305:Generic Models 1" | 1 occurrence | material: "EXISTING - FLOOR BRIDGING" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 313:Generic Models 1" | 1 occurrence | material: "NO. 12 SWG GALV. STEEL WIRE, SUPPORTED FROM 16D NAILS DRIVEN THROUGH WOOD JOISTS 5" FROM BOTTOM OF JOISTS AND BENT UPWARD AT BOTH ENDS FOR POSITIVE SUPPORT - SEE UL LISTING FOR ADDITIONAL INFORMATION" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 314:Generic Models 1" | 1 occurrence | material: "EXISTING - FLOOR BRIDGING" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 315:Generic Models 1" | 1 occurrence | material: "NOM 2 BY 4 IN. INSTALLED BETWEEN AND PERPENDICULAR TO WOOD JOISTS, AND CENTERED 5 IN. BELOW SUBFLOORING." | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 316:Generic Models 1" | 1 occurrence | material: "NO. 12 SWG GALV. STEEL WIRE, SUPPORTED FROM 16D NAILS DRIVEN THROUGH WOOD JOISTS 5" FROM BOTTOM OF JOISTS AND BENT UPWARD AT BOTH ENDS FOR POSITIVE SUPPORT - SEE UL LISTING FOR ADDITIONAL INFORMATION" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 317:Generic Models 1" | 1 occurrence | material: "FIXTURE PROTECTION (IF NON-RATED FIXTURE) - SEE UL LISTING FOR SPECIFICS" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 318:Generic Models 1" | 1 occurrence | material: "STEEL FRAMING MEMBERS - SEE UL LISTING FOR RANGE OF OPTIONS" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 404:Generic Models 1" | 1 occurrence | material: "CONCRETE FOUNDATION - (SEE 'WALL TAG' FOR SIZE & REBAR)" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 321:Generic Models 1" | 1 occurrence | material: "WALL REINFORCING - SEE PLAN SCHEDULES FOR SIZE/LOCATION" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 322:Generic Models 1" | 1 occurrence | material: "BREAK EVERY OTHER REBAR AT JOINT (TOP AND BOTTOM REBAR TO BE CONT.)" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 319:Generic Models 1" | 1 occurrence | material: "3/4" DEEP NOTCH AT EACH SIDE OF WALL (SPACE APART - 25FT MIN.)" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 555:Generic Models 1" | 1 occurrence | material: "STRUCTURAL FLOOR - SEE STRUCT. DWGS" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 204:Generic Models 1" | 1 occurrence | material: "STRUCTURAL FLOOR - SEE STRUCT. DWGS" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 206:Generic Models 1" | 1 occurrence | material: "STRUCTURAL FLOOR - SEE STRUCT. DWGS" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 208:Generic Models 1" | 1 occurrence | material: "STRUCTURAL FLOOR - SEE STRUCT. DWGS" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 210:Generic Models 1" | 1 occurrence | material: "STRUCTURAL FLOOR - SEE STRUCT. DWGS" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 596:Generic Models 1" | 1 occurrence | material: "STRUCTURAL FLOOR - SEE STRUCT. DWGS" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 57:Generic Models 1" | 1 occurrence | material: "STRUCTURAL FLOOR - SEE STRUCT. DWGS" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 58:Generic Models 1" | 1 occurrence | material: "STRUCTURAL FLOOR - SEE STRUCT. DWGS" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 61:Generic Models 1" | 1 occurrence | material: "5/8" GYP. BD @ CEILING" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 63:Generic Models 1" | 1 occurrence | material: "7/8" FURRING CHANNELS @ 16" O.C." | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 68:Generic Models 1" | 1 occurrence | material: "FILL CAVITY WITH BATT INSULATION" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 70:Generic Models 1" | 1 occurrence | material: "OPEN WEB WOOD TRUSS" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 71:Generic Models 1" | 1 occurrence | material: "OPEN WEB WOOD TRUSS" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 72:Generic Models 1" | 1 occurrence | material: "OPEN WEB WOOD TRUSS" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 73:Generic Models 1" | 1 occurrence | material: "OPEN WEB WOOD TRUSS" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 211:Generic Models 1" | 1 occurrence | material: "OPEN WEB WOOD TRUSS" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 212:Generic Models 1" | 1 occurrence | material: "OPEN WEB WOOD TRUSS" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 214:Generic Models 1" | 1 occurrence | material: "OPEN WEB WOOD TRUSS" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 215:Generic Models 1" | 1 occurrence | material: "OPEN WEB WOOD TRUSS" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 345:Generic Models 1" | 1 occurrence | material: "5/8" GYP. BD" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 342:Generic Models 1" | 1 occurrence | material: "5/8" GYP. BD @ CEILING" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 64:Generic Models 1" | 1 occurrence | material: "CONDUIT/PIPE" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 344:Generic Models 1" | 1 occurrence | material: "DOUBLE 2X WOOD TOP PLATE" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 348:Generic Models 1" | 1 occurrence | material: "DOUBLE 2X WOOD TOP PLATE" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 351:Generic Models 1" | 1 occurrence | material: "DOUBLE 2X WOOD TOP PLATE" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 353:Generic Models 1" | 1 occurrence | material: "DOUBLE 2X WOOD TOP PLATE" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 354:Generic Models 1" | 1 occurrence | material: "3" CONCRETE TOPPING" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 387:Generic Models 1" | 1 occurrence | material: "PRECAST PLANK - SEE PRECAST SHOPS FOR SIZE" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 388:Generic Models 1" | 1 occurrence | material: "UL RATED FIRE STOP" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 389:Generic Models 1" | 1 occurrence | material: "SINGLE 2X WOOD SILL - TREATED IF CONCRETE" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 390:Generic Models 1" | 1 occurrence | material: "SINGLE 2X WOOD SILL - TREATED IF CONCRETE" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 391:Generic Models 1" | 1 occurrence | material: "2X WOOD STUDS BEYOND" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 392:Generic Models 1" | 1 occurrence | material: "2X WOOD STUDS BEYOND" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 399:Generic Models 1" | 1 occurrence | material: "7/8" FURRING CHANNELS @ 16" O.C." | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 62:Generic Models 1" | 1 occurrence | material: "7/8" FURRING CHANNELS @ 16" O.C." | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 400:Generic Models 1" | 1 occurrence | material: "7/8" FURRING CHANNELS @ 16" O.C." | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 401:Generic Models 1" | 1 occurrence | material: "CONDUIT/PIPE" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 405:Generic Models 1" | 1 occurrence | material: "UL RATED FIRE STOP" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 406:Generic Models 1" | 1 occurrence | material: "CONDUIT/PIPE" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 407:Generic Models 1" | 1 occurrence | material: "UL RATED FIRE STOP" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 409:Generic Models 1" | 1 occurrence | material: "FILL CAVITY WITH BATT INSULATION" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 352:Generic Models 1" | 1 occurrence | material: "5/8" GYP. BD" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 410:Generic Models 1" | 1 occurrence | material: "HATCHED AREA" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 411:Generic Models 1" | 1 occurrence | material: "FILL CAVITY WITH BATT INSULATION" | property sets: Pset_WallCommon
  IFCCOLUMNTYPE "Timber-Column:6x6" | COLUMN | 1 occurrence | material: profiles "6x6" ("6x6": "STRUCTURAL WOOD COLUMN - SIZE TBD") | property sets: Pset_ColumnCommon
  IFCCOLUMNTYPE "HSS-Round Hollow Structural Section-Column:HSS - 3.5" - SIZE TBD" | COLUMN | 1 occurrence | material: profiles "HSS - 3.5" - SIZE TBD" ("HSS - 3.5" - SIZE TBD": "STRUCTURAL STEEL COLUMN - SIZE TBD") | property sets: Pset_ColumnCommon
  IFCWALLTYPE "Basic Wall:W4BØD - (5/8 GYP - 2X4 WOOD(BATT) - 5/8 GYP)" | STANDARD | 9 occurrences | material: layers "Basic Wall:W4BØD - (5/8 GYP - 2X4 WOOD(BATT) - 5/8 GYP)" ("5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" 0.0520833333333333, "2x6 STUDS 16" O.C. (R-19 BATT. INSULATION)" 0.291666666666667, "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" 0.0520833333333333) | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 561:Generic Models 1" | 1 occurrence | material: "STRUCTURAL FLOOR - SEE STRUCT. DWGS" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 453:Generic Models 1" | 1 occurrence | material: "STRUCTURAL FLOOR - SEE STRUCT. DWGS" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 502:Generic Models 1" | 1 occurrence | material: "OTHER WALL TYPE" | property sets: Pset_WallCommon
  IFCCOVERINGTYPE "Compound Ceiling:GYP. BD - HUNG" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon
  IFCLIGHTFIXTURETYPE "Troffer - 2x4 Parabolic:2' x 4' (2 Lamps)" | 2 occurrences | material: "<Unnamed>"
  IFCLIGHTFIXTURETYPE "Troffer - 2x2 Parabolic:2' x 2' (2 Lamps)" | 2 occurrences | material: "<Unnamed>"
  IFCLIGHTFIXTURETYPE "Troffer - Lens:2' x 4' (2 Lamps)" | 2 occurrences | material: "<Unnamed>"
  IFCLIGHTFIXTURETYPE "Ceiling - Linear Box:2' x 4' - 2 Lamp" | 1 occurrence | material: "<Unnamed>"
  IFCCOVERINGTYPE "Compound Ceiling:GYP. BD - HUNG" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon
  IFCCOVERINGTYPE "Compound Ceiling:GYP. BD - HUNG" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon
  IFCBUILDINGELEMENTPROXYTYPE "Ceiling_Diffuser_-_Square_3882:24" x 24"" | 1 occurrence | material: "<Unnamed>" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "211300 - Fire-Suppression Sprinkler Systems - Exposed Head:211300 - Fire-Suppression Sprinkler Systems - Exposed Head" | 1 occurrence | material: "EXISTING SPRINKLER HEADS TO REMAIN" | property sets: Pset_BuildingElementProxyCommon
  IFCLIGHTFIXTURETYPE "Lighting_Fixture-Lutron-Recessed-Finire-4in-Round-Downlight:Not a Type - Load Type Catalog" | 1 occurrence | material: constituents "MaterialConstituentSet" ("Steel - Lutron - Galvanized": "Steel - Lutron - Galvanized", "Steel - Lutron - Clear Bright Alzak": "Steel - Lutron - Clear Bright Alzak", "Steel - Lutron - Galvanized Black": "Steel - Lutron - Galvanized Black", "Steel - Lutron - Stainless Steel": "Steel - Lutron - Stainless Steel") | property sets: Pset_ElectricalDeviceCommon, Pset_ManufacturerTypeInformation
  IFCWALLTYPE "Generic Models 530:Generic Models 1" | 1 occurrence | material: "STRUCTURAL FLOOR - SEE STRUCT. DWGS" | property sets: Pset_WallCommon
  IFCWALLTYPE "Walls 15:Walls 15" | 1 occurrence | material: "CONCRETE WALL" | property sets: Pset_WallCommon
  IFCWALLTYPE "Walls 5:Walls 15" | 1 occurrence | material: "PLAM-1" | property sets: Pset_WallCommon
  IFCWALLTYPE "Walls 6:Walls 15" | 1 occurrence | material: "PLAM-1" | property sets: Pset_WallCommon
  IFCWALLTYPE "Walls 7:Walls 15" | 1 occurrence | material: "PLAM-1" | property sets: Pset_WallCommon
  IFCCOVERINGTYPE "Compound Ceiling:GYP. BD - HUNG" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon
  IFCDISTRIBUTIONELEMENTTYPE "224000 - Plumbing Fixtures - Water Closet - Generic:ADA" | 2 occurrences | material: constituents "MaterialConstituentSet" ("FLOOR MOUNTED TOILET": "FLOOR MOUNTED TOILET", "<Unnamed>": "<Unnamed>", "GRAB BARS - AT ADA RESTROOMS ONLY": "GRAB BARS - AT ADA RESTROOMS ONLY", "NAPKIN DIPENSER (IF WOMEN'S)": "NAPKIN DIPENSER (IF WOMEN'S)", "TOILET PAPER DISPENSER": "TOILET PAPER DISPENSER")
  IFCBUILDINGELEMENTPROXYTYPE "Walls 8:Walls 15" | 1 occurrence | material: constituents "MaterialConstituentSet" ("CONCRETE WALL": "CONCRETE WALL", "PLAM-1": "PLAM-1") | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Walls 9:Walls 15" | 1 occurrence | material: constituents "MaterialConstituentSet" ("CONCRETE WALL": "CONCRETE WALL", "PLAM-1": "PLAM-1") | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Walls 10:Walls 15" | 1 occurrence | material: constituents "MaterialConstituentSet" ("CONCRETE WALL": "CONCRETE WALL", "PLAM-1": "PLAM-1") | property sets: Pset_BuildingElementProxyCommon
  IFCSLABTYPE "Footing-Cylindrical:20"WX42"D" | BASESLAB | 1 occurrence | material: "CYLINDRICAL CONCRETE PIER - 20"Øx4'-0" - (4) # 4 VERTICALS - (3) #3 TIES @ 2" OC - REST @ 12" OC" | property sets: Pset_SlabCommon
  IFCDISTRIBUTIONELEMENTTYPE "Plbg-Sink Wall Mounted-UH:Sink" | 1 occurrence | material: constituents "MaterialConstituentSet" ("<Unnamed>": "<Unnamed>", "Chrome": "BOTTLE TRAP", "3d Coarse": "<Unnamed>", "FRAMELESS MIRROR": "FRAMELESS MIRROR", "SINK": "SINK")
  IFCWALLTYPE "Generic Models 15:Generic Models 1" | 1 occurrence | material: "METAL RUNNER CHANNEL; FASTEN @ 24" O.C." | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 17:Generic Models 1" | 1 occurrence | material: "ACOUSTICAL SEALANT OR FIRE SEALANT, IF RATED WALL" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 20:Generic Models 1" | 1 occurrence | material: "WALL BASE AS SCHEDULED" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 23:Generic Models 1" | 1 occurrence | material: "DEEP LEG OF DEFLECTION TRACK (2" MIN. DEFLECTION)" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 24:Generic Models 1" | 1 occurrence | material: "ACOUSTICAL SEALANT OR FIRE SEALANT, IF RATED WALL" | property sets: Pset_WallCommon
  IFCWALLTYPE "Basic Wall:RATED - 0.5 HR" | STANDARD | 15 occurrences | material: layers "Basic Wall:RATED - 0.5 HR" ("<Unnamed>" 0.666666666666667) | property sets: Pset_WallCommon
  IFCWALLTYPE "Basic Wall:RATED - 1.5 HR" | STANDARD | 1 occurrence | material: layers "Basic Wall:RATED - 1.5 HR" ("<Unnamed>" 0.666666666666667) | property sets: Pset_WallCommon
  IFCWALLTYPE "Basic Wall:RATED - 2 HR" | STANDARD | 1 occurrence | material: layers "Basic Wall:RATED - 2 HR" ("<Unnamed>" 0.666666666666667) | property sets: Pset_WallCommon
  IFCWALLTYPE "Basic Wall:RATED - 3 HR" | STANDARD | 1 occurrence | material: layers "Basic Wall:RATED - 3 HR" ("<Unnamed>" 0.666666666666667) | property sets: Pset_WallCommon
  IFCWALLTYPE "Basic Wall:RATED - 4 HR" | STANDARD | 1 occurrence | material: layers "Basic Wall:RATED - 4 HR" ("<Unnamed>" 0.666666666666667) | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 1:Generic Models 1" | 1 occurrence | material: "2X WOOD SILL - TREATED IF ON CONCRETE" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 2:Generic Models 1" | 1 occurrence | material: "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 3:Generic Models 1" | 1 occurrence | material: "ACOUSTICAL SEALANT" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 5:Generic Models 1" | 1 occurrence | material: "WALL BASE AS SCHEDULED" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 14:Generic Models 1" | 1 occurrence | material: "CEILING TRACK AS SCHEDULED" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 41:Generic Models 1" | 1 occurrence | material: "ACOUSTICAL SEALANT" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 42:Generic Models 1" | 1 occurrence | material: "MATCH EXISTING BASE" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 49:Generic Models 1" | 1 occurrence | material: "CEILING AS SCHEDULED" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 52:Generic Models 65" | 1 occurrence | material: "2X WOOD STUD" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 19:Generic Models 65" | 1 occurrence | material: "METAL STUD" | property sets: Pset_WallCommon
  IFCBUILDINGELEMENTPROXYTYPE "Egress - Path of Travel:Egress - Path of Travel" | 5 occurrences | material: "<Unnamed>" | property sets: Pset_BuildingElementProxyCommon
  IFCWALLTYPE "Generic Models 122:Generic Models 1" | 1 occurrence | material: "TOP METAL STUD TRACK" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 128:Generic Models 1" | 1 occurrence | material: "STRUCTURAL DECK" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 132:Generic Models 1" | 1 occurrence | material: "METAL STUD - (SEE 'WALL TAG' & 'LAYER MATERIAL SCHEDULE' FOR SIZE, SPACING, & INSULATION)" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 134:Generic Models 1" | 1 occurrence | material: "CEILING TRACK TO MATCH EXISTING" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 136:Generic Models 1" | 1 occurrence | material: "METAL RUNNER CHANNEL; FASTEN @ 24" O.C." | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 142:Generic Models 1" | 1 occurrence | material: "CEILING TRACK TO MATCH EXISTING" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 143:Generic Models 1" | 1 occurrence | material: "CEILING AS SCHEDULED" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 146:Generic Models 1" | 1 occurrence | material: "CEILING AS SCHEDULED" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 147:Generic Models 65" | 1 occurrence | material: "METAL STUD (16" O.C.)" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 149:Generic Models 1" | 1 occurrence | material: "ALUM. STOREFRONT W/ TEMPERED SINGLE GLAZING" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 83:Generic Models 1" | 1 occurrence | material: "DEEP LEG OF DEFLECTION TRACK (2" MIN. DEFLECTION)" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 94:Generic Models 65" | 1 occurrence | material: "DIAGONAL BRACING AS NECESSARY - ATTACH TO STRUCTURAL DECK" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 97:Generic Models 46" | 1 occurrence | material: "BLOCKING - SIZE AS NEC." | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 98:Generic Models 1" | 1 occurrence | material: "SEALANT (W/ BACKER ROD IF NECESSARY)" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 124:Generic Models 1" | 1 occurrence | material: "SEALANT (W/ BACKER ROD IF NECESSARY)" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 126:Generic Models 46" | 1 occurrence | material: "BLOCKING - SIZE AS NEC." | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 135:Generic Models 1" | 1 occurrence | material: "SEALANT (W/ BACKER ROD IF NECESSARY)" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 137:Generic Models 1" | 1 occurrence | material: "SEALANT (W/ BACKER ROD IF NECESSARY)" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 138:Generic Models 1" | 1 occurrence | material: "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 16:Generic Models 1" | 1 occurrence | material: "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" | property sets: Pset_WallCommon
  IFCWALLTYPE "Basic Wall:M6RØD - (6" CMU)" | STANDARD | 1 occurrence | material: layers "Basic Wall:M6RØD - (6" CMU)" ("CMU (SEE 'WALL TAG' FOR SIZE)" 0.46875) | property sets: Pset_WallCommon
  IFCWALLTYPE "Basic Wall:FURR - W2CØFA - (5/8 GYP - 2X2 WOOD)" | STANDARD | 1 occurrence | material: layers "Basic Wall:FURR - W2CØFA - (5/8 GYP - 2X2 WOOD)" ("2X WOOD STUD" 0.125, "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" 0.0520833333333333) | property sets: Pset_WallCommon
  IFCWALLTYPE "Basic Wall:FURR - W2EØFD - (5/8 GYP - 2X2 WOOD(RIGID INSULATION))" | STANDARD | 1 occurrence | material: layers "Basic Wall:FURR - W2EØFD - (5/8 GYP - 2X2 WOOD(RIGID INSULATION))" ("2X WOOD STUDS W/ RIGID INSULATION" 0.125, "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" 0.0520833333333333) | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 34:Generic Models 1" | 1 occurrence | material: "2X WOOD SILL - TREATED IF ON CONCRETE" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 43:Generic Models 65" | 1 occurrence | material: "2X6s WOOD JOISTS - 16" O.C." | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 46:Generic Models 1" | 1 occurrence | material: "1/2" CDX PLYWOOD" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 51:Generic Models 1" | 1 occurrence | material: "VINYL SIDING OVER AIR & MOISTURE BARRIER" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 140:Generic Models 1" | 1 occurrence | material: "2x6 STUDS 16" O.C. (R-19 BATT. INSULATION)" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 139:Generic Models 1" | 1 occurrence | material: "#4 CONT. STEEL REBAR" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 152:Generic Models 1" | 1 occurrence | material: "1/2" GYP. BD" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 153:Generic Models 1" | 1 occurrence | material: "SILL PLATE GASKET" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 181:Generic Models 65" | 1 occurrence | material: "HORIZONTAL 1X6 CEDAR PLANKS W/ CLEAR WOOD SEALER" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 154:Generic Models 1" | 1 occurrence | material: "VERTICAL 1X6 CEDAR PLANKS W/ CLEAR WOOD SEALER" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 158:Generic Models 1" | 1 occurrence | material: "VERTICAL 1X6 CEDAR PLANKS W/ CLEAR WOOD SEALER" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 159:Generic Models 1" | 1 occurrence | material: "VERTICAL 1X6 CEDAR PLANKS W/ CLEAR WOOD SEALER" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 160:Generic Models 1" | 1 occurrence | material: "VERTICAL 1X6 CEDAR PLANKS W/ CLEAR WOOD SEALER" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 161:Generic Models 1" | 1 occurrence | material: "VERTICAL 1X6 CEDAR PLANKS W/ CLEAR WOOD SEALER" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 162:Generic Models 1" | 1 occurrence | material: "VERTICAL 1X6 CEDAR PLANKS W/ CLEAR WOOD SEALER" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 163:Generic Models 1" | 1 occurrence | material: "VERTICAL 1X6 CEDAR PLANKS W/ CLEAR WOOD SEALER" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 164:Generic Models 1" | 1 occurrence | material: "VERTICAL 1X6 CEDAR PLANKS W/ CLEAR WOOD SEALER" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 165:Generic Models 1" | 1 occurrence | material: "VERTICAL 1X6 CEDAR PLANKS W/ CLEAR WOOD SEALER" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 166:Generic Models 1" | 1 occurrence | material: "VERTICAL 1X6 CEDAR PLANKS W/ CLEAR WOOD SEALER" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 167:Generic Models 1" | 1 occurrence | material: "VERTICAL 1X6 CEDAR PLANKS W/ CLEAR WOOD SEALER" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 168:Generic Models 1" | 1 occurrence | material: "VERTICAL 1X6 CEDAR PLANKS W/ CLEAR WOOD SEALER" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 169:Generic Models 1" | 1 occurrence | material: "VERTICAL 1X6 CEDAR PLANKS W/ CLEAR WOOD SEALER" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 170:Generic Models 1" | 1 occurrence | material: "VERTICAL 1X6 CEDAR PLANKS W/ CLEAR WOOD SEALER" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 171:Generic Models 1" | 1 occurrence | material: "VERTICAL 1X6 CEDAR PLANKS W/ CLEAR WOOD SEALER" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 172:Generic Models 1" | 1 occurrence | material: "VERTICAL 1X6 CEDAR PLANKS W/ CLEAR WOOD SEALER" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 173:Generic Models 1" | 1 occurrence | material: "VERTICAL 1X6 CEDAR PLANKS W/ CLEAR WOOD SEALER" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 174:Generic Models 1" | 1 occurrence | material: "VERTICAL 1X6 CEDAR PLANKS W/ CLEAR WOOD SEALER" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 175:Generic Models 1" | 1 occurrence | material: "VERTICAL 1X6 CEDAR PLANKS W/ CLEAR WOOD SEALER" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 176:Generic Models 1" | 1 occurrence | material: "VERTICAL 1X6 CEDAR PLANKS W/ CLEAR WOOD SEALER" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 179:Generic Models 1" | 1 occurrence | material: "VERTICAL 1X6 CEDAR PLANKS W/ CLEAR WOOD SEALER" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 180:Generic Models 65" | 1 occurrence | material: "HORIZONTAL 1X6 CEDAR PLANKS W/ CLEAR WOOD SEALER" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 197:Generic Models 1" | 1 occurrence | material: "2X BLOCKING - LOCATED AT GRAB BARS, WALL HUNG CABINETS, ETC.)" | property sets: Pset_WallCommon
  IFCBEAMTYPE "Dimension Lumber - Canted Ends:2x8" | BEAM | 1 occurrence | material: profiles "2x8" ("2x8": "PRE-ENGINEERED TRUSS @ 24" O.C.") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "Dimension Lumber - Truncated:2x8" | BEAM | 1 occurrence | material: profiles "2x8" ("2x8": "Softwood, Lumber - hortz") | property sets: Pset_BeamCommon
  IFCCURTAINWALLTYPE "Curtain Wall:FRAMELESS GLASS" | 1 occurrence | property sets: Pset_CurtainWallCommon
  IFCCURTAINWALLTYPE "Curtain Wall:EMPTY - PANEL" | 1 occurrence | property sets: Pset_CurtainWallCommon
  IFCCURTAINWALLTYPE "Curtain Wall:POLYCARBONATE WALL" | 1 occurrence | property sets: Pset_CurtainWallCommon
  IFCFURNITURETYPE "OD_CW_Closet:OD_CW_Closet" | 1 occurrence | material: "CASEWORK"
  IFCBUILDINGELEMENTPROXYTYPE "A_Revit_Suv_3d_car_5231:A_Revit_Suv_3d_car_5231" | 1 occurrence | material: constituents "MaterialConstituentSet" ("dark gray": "dark gray", "Tire": "Tire", "Wheel": "Wheel", "Red Light": "Red Light", "yellow": "yellow", "NEW WINDOWS THROUGHOUT": "NEW WINDOWS THROUGHOUT", "white": "white", "blue": "blue", "r-suv1 body": "r-suv1 body") | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Land_Rover_Evoque_-_SUV_Car_Vehicle_Automobile_13067:Land_Rover_Evoque_-_SUV_Car_Vehicle_Automobile_13067" | 1 occurrence | material: "<Unnamed>" | property sets: Pset_BuildingElementProxyCommon
  IFCWALLTYPE "Generic Models 272:Generic Models 263" | 1 occurrence | material: "1.50" ASPHALT SURFACE COURSE (E-0.3)" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 273:Generic Models 263" | 1 occurrence | material: "INSTALL TACK COAT PER WDOT SPECIFICATIONS IF LAYERS ARE NOT INSTALLED AT THE SAME TIME" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 263:Generic Models 263" | 1 occurrence | material: "1.50" ASPHALT BINDER COURSE (E-0.3)" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 288:Generic Models 263" | 1 occurrence | material: "7" CONC. SIDE WALK, IF PRESENT (SEE SITE PLAN)" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 304:Generic Models 263" | 1 occurrence | material: "1" EXPANSION JOINT" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 308:Generic Models 263" | 1 occurrence | material: "MEDIUM BROOM FINISH" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 312:Generic Models 263" | 1 occurrence | material: "SEE SITE PLAN FOR LANDSCAPING" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 285:Generic Models 263" | 1 occurrence | material: "SEE SITE PLAN FOR LANDSCAPING" | property sets: Pset_WallCommon
  IFCBEAMTYPE "061100 - Wood Framing:2x10 - RIM JOIST" | BEAM | 2 occurrences | material: profiles "2x10 - RIM JOIST" ("2x10 - RIM JOIST": "TREATED 2X10 RIM JOIST") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "061100 - Wood Framing:2x10 - RIM JOIST" | BEAM | 1 occurrence | material: profiles "2x10 - RIM JOIST" ("2x10 - RIM JOIST": "TREATED 2X10 RIM JOIST") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "061100 - Wood Framing:2x10 - BEAM" | BEAM | 3 occurrences | material: profiles "2x10 - BEAM" ("2x10 - BEAM": "(3) SISTERED 2X10s AT BEAM") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "061100 - Wood Framing:2x10 - LEDGER" | BEAM | 1 occurrence | material: profiles "2x10 - LEDGER" ("2x10 - LEDGER": "TREATED 2X10 RIM JOIST") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "Dimension Lumber - Canted Ends:6x6 - LATERAL BRACING" | BEAM | 2 occurrences | material: profiles "6x6 - LATERAL BRACING" ("6x6 - LATERAL BRACING": "6X6 TREATED LATERAL BRACE") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "Dimension Lumber - Canted Ends:6x6 - LATERAL BRACING" | BEAM | 2 occurrences | material: profiles "6x6 - LATERAL BRACING" ("6x6 - LATERAL BRACING": "6X6 TREATED LATERAL BRACE") | property sets: Pset_BeamCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 285:Generic Models 263" | 1 occurrence | material: "SEE SITE PLAN FOR LANDSCAPING" | property sets: Pset_BuildingElementProxyCommon
  IFCWALLTYPE "Generic Models 356:Generic Models 65" | 1 occurrence | material: "MORTAR JOINT" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 360:Generic Models 65" | 1 occurrence | material: "MORTAR JOINT" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 366:Generic Models 65" | 1 occurrence | material: "MORTAR JOINT" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 384:Generic Models 1" | 1 occurrence | material: "STRUCTURAL DECK" | property sets: Pset_WallCommon
  IFCWALLTYPE "Continuous Angle1:Continuous Angle" | 1 occurrence | material: "L6X4X1/2 W/ 4" SLOT IN VERT. LOG FOR KWIK BOLT CENTER IN BLOCK (1/2" DIA. KWIK BOLT EXPANSION ANCHOR 2.25" EMBEDMENT AT 4FT O.C.)" | property sets: Pset_WallCommon
  IFCWALLTYPE "Dowel:Dowel" | 1 occurrence | material: "6" CMU WALL W/#4 VERT. BARS AT 32" O.C. (TYP.)" | property sets: Pset_WallCommon
  IFCWALLTYPE "Dowel1:Dowel" | 1 occurrence | material: "6" CMU WALL W/#4 VERT. BARS AT 32" O.C. (TYP.)" | property sets: Pset_WallCommon
  IFCFURNITURETYPE "Entertainment_Center_14771:Entertainment_Center_14771" | 1 occurrence | material: constituents "MaterialConstituentSet" ("TV - Black": "TV - Black", "TV - Glass": "TV - Glass", "SOLID CORE WOOD DOOR": "SOLID CORE WOOD DOOR")
  IFCFURNITURETYPE "Couch-Both_Arms-Generic:1" | 1 occurrence | material: "<Unnamed>" | property sets: Pset_ManufacturerTypeInformation
  IFCFURNITURETYPE "Table-Coffee:one" | 1 occurrence | material: "_WOOD"
  IFCWALLTYPE "Generic Models 426:Generic Models 1" | 1 occurrence | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 427:Generic Models 1" | 1 occurrence | material: "SOUND MAT" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 429:Generic Models 1" | 1 occurrence | material: "3/4" GYP. CRETE" | property sets: Pset_WallCommon
  IFCWALLTYPE "Pole:Pole" | 1 occurrence | material: "STEEL LIGHT POLE" | property sets: Pset_WallCommon
  IFCWALLTYPE "Light Pole Base Plate:Light Pole Base Plate" | 1 occurrence | material: "STEEL BASE PLATE" | property sets: Pset_WallCommon
  IFCBUILDINGELEMENTPROXYTYPE "321723 - Pavement Markings - Parking - Angled:PARKING" | 1 occurrence | material: constituents "MaterialConstituentSet" ("<Unnamed>": "<Unnamed>", "ADA AISLE": "ADA AISLE") | property sets: Pset_BuildingElementProxyCommon
  IFCWALLTYPE "Basic Wall:W6BØD - (5/8 GYP - 2X6 WOOD(BATT) - 5/8 GYP)" | STANDARD | 1 occurrence | material: layers "Basic Wall:W6BØD - (5/8 GYP - 2X6 WOOD(BATT) - 5/8 GYP)" ("5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" 0.0520833333333333, "2x6 STUDS 16" O.C. (R-19 BATT. INSULATION)" 0.458333333333333, "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" 0.0520833333333333) | property sets: Pset_WallCommon
  IFCWALLTYPE "Basic Wall:W8BØD - (5/8 GYP - 2X8 WOOD(BATT) - 5/8 GYP)" | STANDARD | 1 occurrence | material: layers "Basic Wall:W8BØD - (5/8 GYP - 2X8 WOOD(BATT) - 5/8 GYP)" ("5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" 0.0520833333333333, "2x6 STUDS 16" O.C. (R-19 BATT. INSULATION)" 0.604166666666667, "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" 0.0520833333333333) | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 32:Generic Models 1" | 1 occurrence | material: "WALL BASE AS SCHEDULED" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 287:Generic Models 65" | 1 occurrence | material: "MORTAR JOINT" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 293:Generic Models 65" | 1 occurrence | material: "MORTAR JOINT" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 346:Generic Models 65" | 1 occurrence | material: "MORTAR JOINT" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 350:Generic Models 65" | 1 occurrence | material: "MORTAR JOINT" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 355:Generic Models 65" | 1 occurrence | material: "MORTAR JOINT" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 358:Generic Models 1" | 1 occurrence | material: "STANDARD 9-GAUGE (MW11), LADDER-SHAPED WIRE FABRICATED WITH BUTT-WELDED CROSS-RODS SPACED 406-MM (16-IN.) ON CENTER (OC)" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 155:Generic Models 1" | 1 occurrence | material: "DOUBLE 2X WOOD TOP PLATE" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 157:Generic Models 1" | 1 occurrence | material: "METAL STUD - (SEE 'WALL TAG' & 'LAYER MATERIAL SCHEDULE' FOR SIZE, SPACING, & INSULATION)" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 18:Generic Models 1" | 1 occurrence | material: "2x6 STUDS 16" O.C. (R-19 BATT. INSULATION)" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 6:Generic Models 1" | 1 occurrence | material: "DOUBLE 2X WOOD TOP PLATE" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 10:Generic Models 1" | 1 occurrence | material: "ACOUSTICAL SEALANT" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 12:Generic Models 1" | 1 occurrence | material: "ACOUSTICAL SEALANT" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 9:Generic Models 1" | 1 occurrence | material: "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 13:Generic Models 1" | 1 occurrence | material: "2X WOOD SILL - TREATED IF ON CONCRETE" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 25:Generic Models 1" | 1 occurrence | material: "5/8" GYP. BD" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 228:Generic Models 1" | 1 occurrence | material: "WALL BASE AS SCHEDULED" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 243:Generic Models 1" | 1 occurrence | material: "ATTACH GYPSUM BOARD TO STUDS AND NOT TO TOP TRACK" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 245:Generic Models 1" | 1 occurrence | material: "METAL RUNNER CHANNEL; FASTEN @ 24" O.C." | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 246:Generic Models 1" | 1 occurrence | material: "ACOUSTICAL SEALANT" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 247:Generic Models 1" | 1 occurrence | material: "MATCH EXISTING BASE" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 248:Generic Models 1" | 1 occurrence | material: "ATTACH GYPSUM BOARD TO STUDS AND NOT TO TOP TRACK" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 359:Generic Models 1" | 1 occurrence | material: "DOUBLE 2X WOOD TOP PLATE" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 361:Generic Models 1" | 1 occurrence | material: "2x6 STUDS 16" O.C. (R-19 BATT. INSULATION)" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 364:Generic Models 1" | 1 occurrence | material: "DOUBLE 2X WOOD TOP PLATE" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 365:Generic Models 1" | 1 occurrence | material: "CONTINUOUS FIRE RATED SEALANT EACH SIDE." | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 368:Generic Models 1" | 1 occurrence | material: "WOOD STRUCTURAL PANEL (WSP) - SEE STRUCT DWGS" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 370:Generic Models 1" | 1 occurrence | material: "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 371:Generic Models 1" | 1 occurrence | material: "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 373:Generic Models 1" | 1 occurrence | material: "CONTINUOUS FIRE RATED SEALANT EACH SIDE." | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 367:Generic Models 1" | 1 occurrence | material: "CONTINUOUS FIRE RATED SEALANT EACH SIDE." | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 374:Generic Models 1" | 1 occurrence | material: "CONTINUOUS FIRE RATED SEALANT EACH SIDE." | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 375:Generic Models 1" | 1 occurrence | material: "CONTINUOUS FIRE RATED SEALANT EACH SIDE." | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 376:Generic Models 1" | 1 occurrence | material: "CONTINUOUS FIRE RATED SEALANT EACH SIDE." | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 377:Generic Models 1" | 1 occurrence | material: "CONTINUOUS FIRE RATED SEALANT EACH SIDE." | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 378:Generic Models 1" | 1 occurrence | material: "CONTINUOUS FIRE RATED SEALANT EACH SIDE." | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 29:Generic Models 1" | 1 occurrence | material: "25 GA. RESILIENT CHANNEL - 24" O.C." | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 362:Generic Models 1" | 1 occurrence | material: "LADDER TRUSS - SEE STRUCT DWGS" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 380:Generic Models 1" | 1 occurrence | material: "2X WOOD STUD" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 252:Generic Models 1" | 1 occurrence | material: "LADDER TRUSS - SEE STRUCT DWGS" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 379:Generic Models 1" | 1 occurrence | material: "LADDER TRUSS - SEE STRUCT DWGS" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 382:Generic Models 1" | 1 occurrence | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 381:Generic Models 1" | 1 occurrence | material: "2X WOOD SILL" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 383:Generic Models 1" | 1 occurrence | material: "1" GYP. CRETE" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 385:Generic Models 1" | 1 occurrence | material: "1" GYP. CRETE" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 434:Generic Models 1" | 1 occurrence | material: "5/8" GYP. BD @ CEILING" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 436:Generic Models 1" | 1 occurrence | material: "WOOD TRUSS - SEE STRUCT DWGS" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 437:Generic Models 1" | 1 occurrence | material: "WOOD TRUSS - SEE STRUCT DWGS" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 438:Generic Models 1" | 1 occurrence | material: "2X NAILER" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 439:Generic Models 1" | 1 occurrence | material: "2X NAILER" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 440:Generic Models 1" | 1 occurrence | material: "WOOD TRUSS - SEE STRUCT DWGS" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 441:Generic Models 1" | 1 occurrence | material: "25 GA. RESILIENT CHANNEL - 24" O.C." | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 442:Generic Models 1" | 1 occurrence | material: "METAL STUD - (SEE 'WALL TAG' & 'LAYER MATERIAL SCHEDULE' FOR SIZE, SPACING, & INSULATION)" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 443:Generic Models 1" | 1 occurrence | material: "25 GA. RESILIENT CHANNEL - 24" O.C." | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 372:Generic Models 1" | 1 occurrence | material: "5/8" GYP. BD @ CEILING" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 435:Generic Models 1" | 1 occurrence | material: "2X WOOD SILL - TREATED IF ON CONCRETE" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 444:Generic Models 1" | 1 occurrence | material: "5/8" GYP. BD" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 445:Generic Models 1" | 1 occurrence | material: "WALL BASE AS SCHEDULED" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 449:Generic Models 1" | 1 occurrence | material: "METAL RUNNER CHANNEL; FASTEN @ 24" O.C." | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 450:Generic Models 1" | 1 occurrence | material: "ACOUSTICAL SEALANT" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 451:Generic Models 1" | 1 occurrence | material: "MATCH EXISTING BASE" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 456:Generic Models 1" | 1 occurrence | material: "2x6 STUDS 16" O.C. (R-19 BATT. INSULATION)" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 457:Generic Models 1" | 1 occurrence | material: "DOUBLE 2X WOOD TOP PLATE" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 460:Generic Models 1" | 1 occurrence | material: "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 461:Generic Models 1" | 1 occurrence | material: "1/2" GYP. BD. OR FINISH PLYWOOD (SEE INTERIOR ELEVATIONS)" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 465:Generic Models 1" | 1 occurrence | material: "CONTINUOUS FIRE RATED SEALANT EACH SIDE." | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 466:Generic Models 1" | 1 occurrence | material: "CONTINUOUS FIRE RATED SEALANT EACH SIDE." | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 467:Generic Models 1" | 1 occurrence | material: "CONTINUOUS FIRE RATED SEALANT EACH SIDE." | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 468:Generic Models 1" | 1 occurrence | material: "CONTINUOUS FIRE RATED SEALANT EACH SIDE." | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 469:Generic Models 1" | 1 occurrence | material: "25 GA. RESILIENT CHANNEL - 24" O.C." | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 471:Generic Models 1" | 1 occurrence | material: "2X WOOD STUD" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 475:Generic Models 1" | 1 occurrence | material: "2X WOOD SILL" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 476:Generic Models 1" | 1 occurrence | material: "19"/32" FINISH GRADE PLYWOOD" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 477:Generic Models 1" | 1 occurrence | material: "1" GYP. CRETE" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 478:Generic Models 1" | 1 occurrence | material: "2X WOOD STUD" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 486:Generic Models 1" | 1 occurrence | material: "WOOD TRUSS FLOOR ASSEMBLY - (FILL CAVITY W/ CELLULOSE BLOWN-IN INSULATION) (UL - L521 FLOOR ASSEMBLY)" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 487:Generic Models 1" | 1 occurrence | material: "25 GA. RESILIENT CHANNEL - 24" O.C." | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 488:Generic Models 1" | 1 occurrence | material: "5/8" GYP. BD @ CEILING" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 459:Generic Models 1" | 1 occurrence | material: "5/8" GYP. BD" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 489:Generic Models 1" | 1 occurrence | material: "3.5" X 6" LVLs - 32" O.C. - EXPOSED - NO WOOD STAMPS - SEE STRUCT FOR DEPTH" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 490:Generic Models 1" | 1 occurrence | material: "3.5" X 6" LVLs BLOCKING BETWEEN LVL JOISTS" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 491:Generic Models 1" | 1 occurrence | material: "SOUND MAT" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 492:Generic Models 1" | 1 occurrence | material: "19"/32" OSB PLYWOOD BONDED W/ EXT. GLUE" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 474:Generic Models 1" | 1 occurrence | material: "19"/32" OSB PLYWOOD BONDED W/ EXT. GLUE - NO STAMPS - EXPOSED TO FINISH SPACE" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 470:Generic Models 1" | 1 occurrence | material: "WOOD TRUSS - SEE STRUCT DWGS" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 493:Generic Models 1" | 1 occurrence | material: "LVL RIM BOARD - SEE STRUCT. DWGS" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 472:Generic Models 1" | 1 occurrence | material: "WOOD TRUSS - SEE STRUCT DWGS" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 473:Generic Models 1" | 1 occurrence | material: "WOOD TRUSS - SEE STRUCT DWGS" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 448:Generic Models 1" | 1 occurrence | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 452:Generic Models 1" | 1 occurrence | material: "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 458:Generic Models 1" | 1 occurrence | material: "5/8" GYP. BD" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 462:Generic Models 1" | 1 occurrence | material: "5/8" GYP. BD" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 463:Generic Models 1" | 1 occurrence | material: "1/2" GYP. BD. OR FINISH PLYWOOD (SEE INTERIOR ELEVATIONS)" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 464:Generic Models 1" | 1 occurrence | material: "25 GA. RESILIENT CHANNEL - 24" O.C." | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 455:Generic Models 1" | 1 occurrence | material: "DOUBLE 2X WOOD TOP PLATE" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 479:Generic Models 1" | 1 occurrence | material: "25 GA. RESILIENT CHANNEL - 24" O.C." | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 480:Generic Models 1" | 1 occurrence | material: "SOUND MAT" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 481:Generic Models 1" | 1 occurrence | material: "FLOOR FINISH T.B.D" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 482:Generic Models 1" | 1 occurrence | material: "WALL BASE AS SCHEDULED" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 483:Generic Models 1" | 1 occurrence | material: "WALL BASE AS SCHEDULED" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 484:Generic Models 1" | 1 occurrence | material: "CONTINUOUS FIRE RATED SEALANT EACH SIDE." | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 485:Generic Models 1" | 1 occurrence | material: "CONTINUOUS FIRE RATED SEALANT EACH SIDE." | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 494:Generic Models 1" | 1 occurrence | material: "CONTINUOUS FIRE RATED SEALANT EACH SIDE." | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 495:Generic Models 1" | 1 occurrence | material: "CONTINUOUS FIRE RATED SEALANT EACH SIDE." | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 496:Generic Models 1" | 1 occurrence | material: "METAL STUD - (SEE 'WALL TAG' & 'LAYER MATERIAL SCHEDULE' FOR SIZE, SPACING, & INSULATION)" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 21:Generic Models 1" | 1 occurrence | material: "WOOD TRUSS FLOOR ASSEMBLY - (FILL CAVITY W/ CELLULOSE BLOWN-IN INSULATION) (UL - L521 FLOOR ASSEMBLY)" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 35:Generic Models 1" | 1 occurrence | material: "WOOD TRUSS FLOOR ASSEMBLY - (FILL CAVITY W/ CELLULOSE BLOWN-IN INSULATION) (UL - L521 FLOOR ASSEMBLY)" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 36:Generic Models 1" | 1 occurrence | material: "2X WOOD SILL - TREATED IF ON CONCRETE" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 67:Generic Models 1" | 1 occurrence | material: "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 242:Generic Models 1" | 1 occurrence | material: "ACOUSTICAL SEALANT" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 251:Generic Models 1" | 1 occurrence | material: "WALL BASE AS SCHEDULED" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 454:Generic Models 1" | 1 occurrence | material: "CEILING TRACK AS SCHEDULED" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 503:Generic Models 1" | 1 occurrence | material: "CEILING AS SCHEDULED" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 504:Generic Models 65" | 1 occurrence | material: "2X WOOD STUD" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 505:Generic Models 1" | 1 occurrence | material: "DOUBLE 2X WOOD TOP PLATE" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 506:Generic Models 1" | 1 occurrence | material: "2x6 STUDS 16" O.C. (R-19 BATT. INSULATION)" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 508:Generic Models 1" | 1 occurrence | material: "DOUBLE 2X WOOD TOP PLATE" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 509:Generic Models 1" | 1 occurrence | material: "ACOUSTICAL SEALANT" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 499:Generic Models 1" | 1 occurrence | material: "UNDERSIDE OF FLOOR ASSEMBLY - SEE STRUCT. DWGS" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 7:Generic Models 1" | 1 occurrence | material: "UNDERSIDE OF FLOOR ASSEMBLY - SEE STRUCT. DWGS" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 447:Generic Models 1" | 1 occurrence | material: "UNDERSIDE OF FLOOR ASSEMBLY - SEE STRUCT. DWGS" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 501:Generic Models 65" | 1 occurrence | material: "MORTAR JOINT" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 507:Generic Models 65" | 1 occurrence | material: "MORTAR JOINT" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 511:Generic Models 65" | 1 occurrence | material: "MORTAR JOINT" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 512:Generic Models 65" | 1 occurrence | material: "MORTAR JOINT" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 513:Generic Models 1" | 1 occurrence | material: "STRUCTURAL DECK" | property sets: Pset_WallCommon
  IFCWALLTYPE "Continuous Angle2:Continuous Angle" | 1 occurrence | material: "3" X 3" X 8" L. CLIP ANGLES @ 4'-0" O.C. MECH. FASTENED TO UNDERSIDE OF STRUCTURE OR SLAB - BOTH SIDES OF WALL" | property sets: Pset_WallCommon
  IFCWALLTYPE "Continuous Angle3:Continuous Angle" | 1 occurrence | material: "3" X 3" X 8" L. CLIP ANGLES @ 4'-0" O.C. MECH. FASTENED TO UNDERSIDE OF STRUCTURE OR SLAB - BOTH SIDES OF WALL" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 515:Generic Models 65" | 1 occurrence | material: "MORTAR JOINT" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 516:Generic Models 65" | 1 occurrence | material: "MORTAR JOINT" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 517:Generic Models 65" | 1 occurrence | material: "MORTAR JOINT" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 519:Generic Models 65" | 1 occurrence | material: "MORTAR JOINT" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 520:Generic Models 65" | 1 occurrence | material: "MORTAR JOINT" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 521:Generic Models 1" | 1 occurrence | material: "STANDARD 9-GAUGE (MW11), LADDER-SHAPED WIRE FABRICATED WITH BUTT-WELDED CROSS-RODS SPACED 406-MM (16-IN.) ON CENTER (OC)" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 347:Generic Models 65" | 1 occurrence | material: "MORTAR JOINT" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 363:Generic Models 65" | 1 occurrence | material: "MORTAR JOINT" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 510:Generic Models 65" | 1 occurrence | material: "MORTAR JOINT" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 518:Generic Models 65" | 1 occurrence | material: "MORTAR JOINT" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 33:Generic Models 1" | 1 occurrence | material: "ACOUSTICAL SEALANT OR FIRE SEALANT, IF RATED WALL" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 31:Generic Models 1" | 1 occurrence | material: "ACOUSTICAL SEALANT OR FIRE SEALANT, IF RATED WALL" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 522:Generic Models 1" | 1 occurrence | material: "METAL RUNNER CHANNEL; FASTEN @ 24" O.C." | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 523:Generic Models 1" | 1 occurrence | material: "ACOUSTICAL SEALANT OR FIRE SEALANT, IF RATED WALL" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 524:Generic Models 1" | 1 occurrence | material: "WALL BASE AS SCHEDULED" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 525:Generic Models 1" | 1 occurrence | material: "DEEP LEG OF DEFLECTION TRACK (2" MIN. DEFLECTION)" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 526:Generic Models 1" | 1 occurrence | material: "ACOUSTICAL SEALANT OR FIRE SEALANT, IF RATED WALL" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 531:Generic Models 65" | 1 occurrence | material: "METAL STUD" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 532:Generic Models 1" | 1 occurrence | material: "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 533:Generic Models 1" | 1 occurrence | material: "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 534:Generic Models 1" | 1 occurrence | material: "2X BLOCKING - LOCATED AT GRAB BARS, WALL HUNG CABINETS, ETC.)" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 535:Generic Models 1" | 1 occurrence | material: "WALL BASE AS SCHEDULED" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 536:Generic Models 1" | 1 occurrence | material: "METAL STUD - (SEE 'WALL TAG' & 'LAYER MATERIAL SCHEDULE' FOR SIZE, SPACING, & INSULATION)" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 538:Generic Models 1" | 1 occurrence | material: "UNDERSIDE OF FLOOR ASSEMBLY - SEE STRUCT. DWGS" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 539:Generic Models 1" | 1 occurrence | material: "ACOUSTICAL SEALANT OR FIRE SEALANT, IF RATED WALL" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 540:Generic Models 1" | 1 occurrence | material: "ACOUSTICAL SEALANT OR FIRE SEALANT, IF RATED WALL" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 541:Generic Models 1" | 1 occurrence | material: "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 542:Generic Models 1" | 1 occurrence | material: "25 GA. RESILIENT CHANNEL - 24" O.C." | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 543:Generic Models 1" | 1 occurrence | material: "ACOUSTICAL SEALANT OR FIRE SEALANT, IF RATED WALL" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 544:Generic Models 1" | 1 occurrence | material: "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 545:Generic Models 1" | 1 occurrence | material: "ACOUSTICAL SEALANT OR FIRE SEALANT, IF RATED WALL" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 546:Generic Models 1" | 1 occurrence | material: "ACOUSTICAL SEALANT OR FIRE SEALANT, IF RATED WALL" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 547:Generic Models 1" | 1 occurrence | material: "ACOUSTICAL SEALANT OR FIRE SEALANT, IF RATED WALL" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 548:Generic Models 1" | 1 occurrence | material: "25 GA. RESILIENT CHANNEL - 24" O.C." | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 549:Generic Models 1" | 1 occurrence | material: "BOND BEAM W/ (1) CONT. #5 BAR CONT." | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 369:Generic Models 1" | 1 occurrence | material: "FILL CORE IF APPLICABLE - SEE STRUCTURAL DWGS FOR DETAILS" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 53:Generic Models 1" | 1 occurrence | material: "OPEN WEB WOOD TRUSS" | property sets: Pset_WallCommon
  IFCWALLTYPE "Dowel5:Dowel" | 1 occurrence | material: "PRECAST PLANK - SEE PRECAST SHOPS FOR SIZE" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 78:Generic Models 1" | 1 occurrence | material: "BEARING STRIP" | property sets: Pset_WallCommon
  IFCWALLTYPE "Dowel7:Dowel" | 1 occurrence | material: "#4 x 16" BAR @ 2-0" O.C. MAX. DRILL THRU HOLLOWCORE OR KEYWAY & INTO CIP WALL W/ 4" MIN. EMBED" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 91:Generic Models 1" | 1 occurrence | material: "3" CONCRETE TOPPING" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 96:Generic Models 1" | 1 occurrence | material: "CONCRETE WALL" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 75:Generic Models 1" | 1 occurrence | material: "TREATED 2X SILL PLATE - SEE STRUCT. SCHEDULES FOR SIZE - ATTACH WITH" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 76:Generic Models 1" | 1 occurrence | material: "#4 CONT. STEEL REBAR IN TOPPING SLAB" | property sets: Pset_WallCommon
  IFCWALLTYPE "Dowel6:Dowel" | 1 occurrence | material: "#4 VERTICAL U-SHAPED HAIRPINS AT 18" O.C. - 36" LONG" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 77:Generic Models 1" | 1 occurrence | material: "#4 VERTICAL U-SHAPED HAIRPINS AT 18" O.C. - 36" LONG" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 79:Generic Models 1" | 1 occurrence | material: "#4 HORZ. U-SHAPED HAIRPINS - 36" LONG - LOOP AROUND VERT. HAIRPIN" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 80:Generic Models 1" | 1 occurrence | material: "WALL REINFORCING - SEE PLAN SCHEDULES FOR SIZE/LOCATION" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 81:Generic Models 1" | 1 occurrence | material: "WALL REINFORCING - SEE PLAN SCHEDULES FOR SIZE/LOCATION" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 82:Generic Models 1" | 1 occurrence | material: "WALL REINFORCING - SEE PLAN SCHEDULES FOR SIZE/LOCATION" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 84:Generic Models 1" | 1 occurrence | material: "WALL REINFORCING - SEE PLAN SCHEDULES FOR SIZE/LOCATION" | property sets: Pset_WallCommon
  IFCBUILDINGELEMENTPROXYTYPE "050523 - W_P_C - Fastenings - Bent Anchor Bolt:5/8"" | 2 occurrences | material: "5/8” GALV. BENT ANCHOR BOLT @ 4’ O.C. (WITHIN 8” OF EVERY CORNER) 7” MIN. EMBEDMENT" | property sets: Pset_BuildingElementProxyCommon
  IFCWALLTYPE "Dowel8:Dowel" | 1 occurrence | material: "PRECAST PLANK - SEE PRECAST SHOPS FOR SIZE" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 85:Generic Models 1" | 1 occurrence | material: "BEARING STRIP" | property sets: Pset_WallCommon
  IFCWALLTYPE "Dowel9:Dowel" | 1 occurrence | material: "#4 x 16" BAR @ 2-0" O.C. MAX. DRILL THRU HOLLOWCORE OR KEYWAY & INTO CIP WALL W/ 4" MIN. EMBED" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 86:Generic Models 1" | 1 occurrence | material: "3" CONCRETE TOPPING" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 87:Generic Models 1" | 1 occurrence | material: "CONCRETE WALL" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 88:Generic Models 1" | 1 occurrence | material: "TREATED 2X SILL PLATE - SEE STRUCT. SCHEDULES FOR SIZE - ATTACH WITH" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 89:Generic Models 1" | 1 occurrence | material: "#4 CONT. STEEL REBAR IN TOPPING SLAB" | property sets: Pset_WallCommon
  IFCWALLTYPE "Dowel10:Dowel" | 1 occurrence | material: "#4 VERTICAL U-SHAPED HAIRPINS AT 18" O.C. - 36" LONG" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 90:Generic Models 1" | 1 occurrence | material: "#4 VERTICAL U-SHAPED HAIRPINS AT 18" O.C. - 36" LONG" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 92:Generic Models 1" | 1 occurrence | material: "#4 HORZ. U-SHAPED HAIRPINS - 36" LONG - LOOP AROUND VERT. HAIRPIN" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 95:Generic Models 1" | 1 occurrence | material: "WALL REINFORCING - SEE PLAN SCHEDULES FOR SIZE/LOCATION" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 99:Generic Models 1" | 1 occurrence | material: "WALL REINFORCING - SEE PLAN SCHEDULES FOR SIZE/LOCATION" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 100:Generic Models 1" | 1 occurrence | material: "WALL REINFORCING - SEE PLAN SCHEDULES FOR SIZE/LOCATION" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 101:Generic Models 1" | 1 occurrence | material: "2X WOOD STUDS - SEE STRUCT SCHEDULE FOR SIZE" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 102:Generic Models 1" | 1 occurrence | material: "2X WOOD STUDS - SEE STRUCT SCHEDULE FOR SIZE" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 103:Generic Models 1" | 1 occurrence | material: "4x4 - W4.0xW4.0 WWM - OVERLAP 8" AT SPLICES" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 104:Generic Models 1" | 1 occurrence | material: "4x4 - W4.0xW4.0 WWM - OVERLAP 8" AT SPLICES" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 105:Generic Models 1" | 1 occurrence | material: "FILL CORE IF APPLICABLE - SEE STRUCTURAL DWGS FOR DETAILS" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 113:Generic Models 65" | 1 occurrence | material: "MORTAR JOINT" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 114:Generic Models 65" | 1 occurrence | material: "CMU (SEE 'WALL TAG' FOR SIZE)" | property sets: Pset_WallCommon
  IFCWALLTYPE "Dowel13:Dowel" | 1 occurrence | material: "WALL REINFORCING - SEE PLAN SCHEDULES FOR SIZE/LOCATION" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 118:Generic Models 65" | 1 occurrence | material: "MORTAR JOINT" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 119:Generic Models 65" | 1 occurrence | material: "CMU (SEE 'WALL TAG' FOR SIZE)" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 120:Generic Models 1" | 1 occurrence | material: "REINFORCEMENT GROUTED INTO BROKEN CORE" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 106:Generic Models 65" | 1 occurrence | material: "CMU (SEE 'WALL TAG' FOR SIZE)" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 108:Generic Models 65" | 1 occurrence | material: "MORTAR JOINT" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 109:Generic Models 65" | 1 occurrence | material: "CMU (SEE 'WALL TAG' FOR SIZE)" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 110:Generic Models 65" | 1 occurrence | material: "MORTAR JOINT" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 111:Generic Models 65" | 1 occurrence | material: "CMU (SEE 'WALL TAG' FOR SIZE)" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 107:Generic Models 65" | 1 occurrence | material: "CMU (SEE 'WALL TAG' FOR SIZE)" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 112:Generic Models 65" | 1 occurrence | material: "MORTAR JOINT" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 115:Generic Models 65" | 1 occurrence | material: "CMU (SEE 'WALL TAG' FOR SIZE)" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 116:Generic Models 65" | 1 occurrence | material: "MORTAR JOINT" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 117:Generic Models 1" | 1 occurrence | material: "PRECAST PLANK - SEE PRECAST SHOPS FOR SIZE" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 121:Generic Models 1" | 1 occurrence | material: "3" CONCRETE TOPPING" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 123:Generic Models 1" | 1 occurrence | material: "#3 J's @ 24" O.C." | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 127:Generic Models 1" | 1 occurrence | material: "SEE SCHEDULE FOR FILLED CORES" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 130:Generic Models 65" | 1 occurrence | material: "MORTAR JOINT" | property sets: Pset_WallCommon
  IFCWALLTYPE "Dowel11:Dowel" | 1 occurrence | material: "PRECAST PLANK - SEE PRECAST SHOPS FOR SIZE" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 131:Generic Models 65" | 1 occurrence | material: "MORTAR JOINT" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 133:Generic Models 1" | 1 occurrence | material: "BEARING STRIP" | property sets: Pset_WallCommon
  IFCWALLTYPE "Dowel12:Dowel" | 1 occurrence | material: "#4 J's @ 24" O.C. - GROUTED IN PRECAST KEYS AND CORES" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 182:Generic Models 65" | 1 occurrence | material: "CMU (SEE 'WALL TAG' FOR SIZE)" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 185:Generic Models 1" | 1 occurrence | material: "SOLID CMU AS NEEDED" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 186:Generic Models 65" | 1 occurrence | material: "MORTAR JOINT" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 187:Generic Models 1" | 1 occurrence | material: "SOLID CMU AS NEEDED" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 188:Generic Models 65" | 1 occurrence | material: "MORTAR JOINT" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 189:Generic Models 65" | 1 occurrence | material: "CMU (SEE 'WALL TAG' FOR SIZE)" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 190:Generic Models 1" | 1 occurrence | material: "SEE SCHEDULE FOR FILLED CORES" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 191:Generic Models 65" | 1 occurrence | material: "MORTAR JOINT" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 192:Generic Models 65" | 1 occurrence | material: "CMU (SEE 'WALL TAG' FOR SIZE)" | property sets: Pset_WallCommon
  IFCWALLTYPE "Dowel14:Dowel" | 1 occurrence | material: "#4 REBARS @ 24" O.C." | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 193:Generic Models 65" | 1 occurrence | material: "MORTAR JOINT" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 194:Generic Models 65" | 1 occurrence | material: "CMU (SEE 'WALL TAG' FOR SIZE)" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 195:Generic Models 1" | 1 occurrence | material: "3" CONCRETE TOPPING" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 196:Generic Models 65" | 1 occurrence | material: "MORTAR JOINT" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 198:Generic Models 65" | 1 occurrence | material: "CONT. KNOCK OUT BOND BEAM" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 199:Generic Models 1" | 1 occurrence | material: "GROUT CORES AT REBAR" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 200:Generic Models 1" | 1 occurrence | material: "4x4 - W4.0xW4.0 WWM - OVERLAP 8" AT SPLICES" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 201:Generic Models 1" | 1 occurrence | material: "(2) #5's" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 202:Generic Models 1" | 1 occurrence | material: "CONT. KNOCK OUT BOND BEAM" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 203:Generic Models 1" | 1 occurrence | material: "(2) #5's" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 139:Generic Models 1" | 1 occurrence | material: "#4 CONT. STEEL REBAR" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 55:Generic Models 1" | 1 occurrence | material: "4x4 - W4.0xW4.0 WWM - OVERLAP 8" AT SPLICES" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 56:Generic Models 1" | 1 occurrence | material: "WALL REINFORCING - SEE PLAN SCHEDULES FOR SIZE/LOCATION" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 219:Generic Models 1" | 1 occurrence | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 220:Generic Models 1" | 1 occurrence | material: "SOUND MAT" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 222:Generic Models 1" | 1 occurrence | material: "3/4" GYP. CRETE" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 227:Generic Models 1" | 1 occurrence | material: "OPEN WEB WOOD TRUSS" | property sets: Pset_WallCommon
  IFCBUILDINGELEMENTPROXYTYPE "321723 - Pavement Markings - Parking - Angled:BIKE" | 1 occurrence | material: "<Unnamed>" | property sets: Pset_BuildingElementProxyCommon
  IFCWALLTYPE "Generic Models 232:Generic Models 1" | 1 occurrence | material: "EXISTING FLOOR SUBSTRATE - MIN 19/32 THICK WOOD STRUCTURAL PANELS" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 236:Generic Models 1" | 1 occurrence | material: "EXISTING FLOOR SUBSTRATE - 1 X 4 T&G LAID PERPENDICULAR TO JOISTS, OR 19/32" PLYWOOD WOOD STRUCTURAL PANELS" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 264:Generic Models 1" | 1 occurrence | material: "EXISTING FLOOR SUBSTRATE - 15/32" THICK PLYWOOD OR 7/16" THICK ORIENTATED STRAND BOARD (OSB) WOOD STRUCTURAL PANELS" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 320:Generic Models 1" | 1 occurrence | material: "2X WOOD SILL - TREATED IF ON CONCRETE" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 323:Generic Models 1" | 1 occurrence | material: "5/8" GYP. BD" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 324:Generic Models 1" | 1 occurrence | material: "ACOUSTICAL SEALANT OR FIRE SEALANT, IF RATED WALL" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 325:Generic Models 1" | 1 occurrence | material: "WALL BASE AS SCHEDULED" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 327:Generic Models 1" | 1 occurrence | material: "METAL RUNNER CHANNEL; FASTEN @ 24" O.C." | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 328:Generic Models 65" | 1 occurrence | material: "2X WOOD STUD" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 329:Generic Models 1" | 1 occurrence | material: "DOUBLE 2X WOOD TOP PLATE" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 330:Generic Models 1" | 1 occurrence | material: "2x6 STUDS 16" O.C. (R-19 BATT. INSULATION)" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 331:Generic Models 1" | 1 occurrence | material: "DOUBLE 2X WOOD TOP PLATE" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 332:Generic Models 1" | 1 occurrence | material: "ACOUSTICAL SEALANT OR FIRE SEALANT, IF RATED WALL" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 333:Generic Models 1" | 1 occurrence | material: "UNDERSIDE OF FLOOR ASSEMBLY - SEE STRUCT. DWGS" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 334:Generic Models 1" | 1 occurrence | material: "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 335:Generic Models 1" | 1 occurrence | material: "ACOUSTICAL SEALANT OR FIRE SEALANT, IF RATED WALL" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 336:Generic Models 1" | 1 occurrence | material: "ACOUSTICAL SEALANT OR FIRE SEALANT, IF RATED WALL" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 337:Generic Models 1" | 1 occurrence | material: "25 GA. RESILIENT CHANNEL - 24" O.C." | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 338:Generic Models 1" | 1 occurrence | material: "25 GA. RESILIENT CHANNEL - 24" O.C." | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 339:Generic Models 1" | 1 occurrence | material: "IF SHEAR WALL - WOOD STRUCTURAL PANEL (WSP) - SEE STRUCT DWGS" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 340:Generic Models 1" | 1 occurrence | material: "5/8" GYP. BD" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 341:Generic Models 1" | 1 occurrence | material: "ACOUSTICAL SEALANT OR FIRE SEALANT, IF RATED WALL" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 556:Generic Models 1" | 1 occurrence | material: "WALL BASE AS SCHEDULED" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 567:Generic Models 1" | 1 occurrence | material: "ACOUSTICAL SEALANT OR FIRE SEALANT, IF RATED WALL" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 571:Generic Models 1" | 1 occurrence | material: "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 577:Generic Models 1" | 1 occurrence | material: "ACOUSTICAL SEALANT OR FIRE SEALANT, IF RATED WALL" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 590:Generic Models 1" | 1 occurrence | material: "ACOUSTICAL SEALANT OR FIRE SEALANT, IF RATED WALL" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 558:Generic Models 1" | 1 occurrence | material: "IF SHEAR WALL - WOOD STRUCTURAL PANEL (WSP) - SEE STRUCT DWGS" | property sets: Pset_WallCommon
  IFCFURNITURETYPE "Bed-Standard:FULL 54"X75"" | 1 occurrence | material: constituents "MaterialConstituentSet" ("Textile - White": "Textile - White", "Metal - Chrome": "Metal - Chrome")
  IFCFURNITURETYPE "Bed-Standard:KING 76"X80"" | 1 occurrence | material: constituents "MaterialConstituentSet" ("Textile - White": "Textile - White", "Metal - Chrome": "Metal - Chrome")
  IFCFURNITURETYPE "Bed-Standard:QUEEN 60" x 79"" | 1 occurrence | material: constituents "MaterialConstituentSet" ("Textile - White": "Textile - White", "Metal - Chrome": "Metal - Chrome")
  IFCFURNITURETYPE "Bed-Standard:TWIN 39"X80"" | 1 occurrence | material: constituents "MaterialConstituentSet" ("Textile - White": "Textile - White", "Metal - Chrome": "Metal - Chrome")
  IFCWALLTYPE "Basic Wall:FURR - M358CØA - (5/8 GYP - 3 5/8 METAL)" | STANDARD | 1 occurrence | material: layers "Basic Wall:FURR - M358CØA - (5/8 GYP - 3 5/8 METAL)" ("AIR GAP" 0.0208333333333333, "METAL STUD" 0.302083333333333, "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" 0.0520833333333333) | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 125:Generic Models 1" | 1 occurrence | material: "UNDERSIDE OF FLOOR ASSEMBLY - SEE STRUCT. DWGS" | property sets: Pset_WallCommon
  IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 81:Structural Framing 1" | 1 occurrence | material: "TYP. VERTICAL METAL STUD - SEE WALL TAG FOR SPACING AND GUAGE" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 82:Structural Framing 1" | 1 occurrence | material: "TYP. VERTICAL METAL STUD - SEE WALL TAG FOR SPACING AND GUAGE" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 108:Structural Framing 1" | 1 occurrence | material: "TYP. VERTICAL METAL STUD - SEE WALL TAG FOR SPACING AND GUAGE" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 109:Structural Framing 1" | 1 occurrence | material: "CRIPPLE STUD OR CLIP ANGLE" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 110:Structural Framing 1" | 1 occurrence | material: "DOUBLE UP METAL STUDS @ JAMB" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 111:Structural Framing 1" | 1 occurrence | material: "TYP. VERTICAL METAL STUD - SEE WALL TAG FOR SPACING AND GUAGE" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 112:Structural Framing 2" | 1 occurrence | material: "METAL SILL CHANNEL - FASTENER PER MANU. REQUIREMENTS" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 113:Structural Framing 2" | 1 occurrence | material: "METAL TRACK CHANNEL @ HEAD - FASTENER PER MANU. REQUIREMENTS" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 114:Structural Framing 1" | 1 occurrence | material: "TYP. VERTICAL METAL STUD - SEE WALL TAG FOR SPACING AND GUAGE" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 115:Structural Framing 1" | 1 occurrence | material: "TYP. VERTICAL METAL STUD - SEE WALL TAG FOR SPACING AND GUAGE" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 116:Structural Framing 1" | 1 occurrence | material: "TYP. VERTICAL METAL STUD - SEE WALL TAG FOR SPACING AND GUAGE" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 117:Structural Framing 1" | 1 occurrence | material: "TYP. VERTICAL METAL STUD - SEE WALL TAG FOR SPACING AND GUAGE" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 118:Structural Framing 1" | 1 occurrence | material: "TYP. VERTICAL METAL STUD - SEE WALL TAG FOR SPACING AND GUAGE" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 119:Structural Framing 1" | 1 occurrence | material: "TYP. VERTICAL METAL STUD - SEE WALL TAG FOR SPACING AND GUAGE" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 120:Structural Framing 1" | 1 occurrence | material: "TYP. VERTICAL METAL STUD - SEE WALL TAG FOR SPACING AND GUAGE" | property sets: Pset_BuildingElementProxyCommon
  IFCWALLTYPE "Generic Models 205:Generic Models 1" | 1 occurrence | material: "UNDERSIDE OF FLOOR ASSEMBLY - SEE STRUCT. DWGS" | property sets: Pset_WallCommon
  IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 121:Structural Framing 2" | 1 occurrence | material: "METAL SILL CHANNEL - FASTENER PER MANU. REQUIREMENTS" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 122:Structural Framing 2" | 1 occurrence | material: "METAL TRACK CHANNEL @ HEAD - FASTENER PER MANU. REQUIREMENTS" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 123:Structural Framing 1" | 1 occurrence | material: "TYP. VERTICAL METAL STUD - SEE WALL TAG FOR SPACING AND GUAGE" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 124:Structural Framing 1" | 1 occurrence | material: "TYP. VERTICAL METAL STUD - SEE WALL TAG FOR SPACING AND GUAGE" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 125:Structural Framing 1" | 1 occurrence | material: "DOUBLE UP METAL STUDS @ JAMB" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 126:Structural Framing 1" | 1 occurrence | material: "TYP. VERTICAL METAL STUD - SEE WALL TAG FOR SPACING AND GUAGE" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 127:Structural Framing 1" | 1 occurrence | material: "TYP. VERTICAL METAL STUD - SEE WALL TAG FOR SPACING AND GUAGE" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 128:Structural Framing 1" | 1 occurrence | material: "TYP. VERTICAL METAL STUD - SEE WALL TAG FOR SPACING AND GUAGE" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 129:Structural Framing 1" | 1 occurrence | material: "DOUBLE UP METAL STUDS @ JAMB" | property sets: Pset_BuildingElementProxyCommon
  IFCWALLTYPE "Generic Models 207:Generic Models 1" | 1 occurrence | material: "UNDERSIDE OF FLOOR ASSEMBLY - SEE STRUCT. DWGS" | property sets: Pset_WallCommon
  IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 130:Structural Framing 2" | 1 occurrence | material: "METAL SILL CHANNEL - FASTENER PER MANU. REQUIREMENTS" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 131:Structural Framing 2" | 1 occurrence | material: "METAL TRACK CHANNEL @ HEAD - FASTENER PER MANU. REQUIREMENTS" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 132:Structural Framing 1" | 1 occurrence | material: "TYP. VERTICAL METAL STUD - SEE WALL TAG FOR SPACING AND GUAGE" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 133:Structural Framing 1" | 1 occurrence | material: "TYP. VERTICAL METAL STUD - SEE WALL TAG FOR SPACING AND GUAGE" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 134:Structural Framing 1" | 1 occurrence | material: "TYP. VERTICAL METAL STUD - SEE WALL TAG FOR SPACING AND GUAGE" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 135:Structural Framing 1" | 1 occurrence | material: "DOUBLE UP METAL STUDS @ JAMB" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 136:Structural Framing 1" | 1 occurrence | material: "TYP. VERTICAL METAL STUD - SEE WALL TAG FOR SPACING AND GUAGE" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 137:Structural Framing 1" | 1 occurrence | material: "DOUBLE UP METAL STUDS @ JAMB" | property sets: Pset_BuildingElementProxyCommon
  IFCWALLTYPE "Generic Models 209:Generic Models 1" | 1 occurrence | material: "UNDERSIDE OF FLOOR ASSEMBLY - SEE STRUCT. DWGS" | property sets: Pset_WallCommon
  IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 138:Structural Framing 2" | 1 occurrence | material: "METAL TRACK CHANNEL @ HEAD - FASTENER PER MANU. REQUIREMENTS" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 139:Structural Framing 1" | 1 occurrence | material: "TYP. VERTICAL METAL STUD - SEE WALL TAG FOR SPACING AND GUAGE" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 140:Structural Framing 7" | 1 occurrence | material: "BLOCKING TO BRIDGE AT LEAST (3) VERTICAL STUDS" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 37:Structural Framing 7" | 1 occurrence | material: "BLOCKING TO BRIDGE AT LEAST (3) VERTICAL STUDS" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 141:Structural Framing 7" | 1 occurrence | material: "BLOCKING TO BRIDGE AT LEAST (3) VERTICAL STUDS" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 142:Structural Framing 7" | 1 occurrence | material: "BLOCKING TO BRIDGE AT LEAST (3) VERTICAL STUDS" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 143:Structural Framing 2" | 1 occurrence | material: "SILL STUD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 144:Structural Framing 2" | 1 occurrence | material: "METAL STUD TRACK WELDED OR SCREWED PER MANU. REQUIREMENTS" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 145:Structural Framing 1" | 1 occurrence | material: "TYP. VERTICAL METAL STUD - SEE WALL TAG FOR SPACING AND GUAGE" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 146:Structural Framing 1" | 1 occurrence | material: "TYP. VERTICAL METAL STUD - SEE WALL TAG FOR SPACING AND GUAGE" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 147:Structural Framing 1" | 1 occurrence | material: "TYP. VERTICAL METAL STUD - SEE WALL TAG FOR SPACING AND GUAGE" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 148:Structural Framing 1" | 1 occurrence | material: "CRIPPLE STUD OR CLIP ANGLE" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 149:Structural Framing 1" | 1 occurrence | material: "DOUBLE UP METAL STUDS @ JAMB" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 150:Structural Framing 1" | 1 occurrence | material: "DOUBLE UP METAL STUDS @ JAMB" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 151:Structural Framing 1" | 1 occurrence | material: "DOUBLE UP METAL STUDS @ JAMB" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 152:Structural Framing 1" | 1 occurrence | material: "TYP. VERTICAL METAL STUD - SEE WALL TAG FOR SPACING AND GUAGE" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 153:Structural Framing 1" | 1 occurrence | material: "DOUBLE UP METAL STUDS @ JAMB" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 154:Structural Framing 1" | 1 occurrence | material: "DOUBLE UP METAL STUDS @ JAMB" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 155:Structural Framing 2" | 1 occurrence | material: "METAL SILL CHANNEL - FASTENER PER MANU. REQUIREMENTS" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 156:Structural Framing 1" | 1 occurrence | material: "TYP. VERTICAL METAL STUD - SEE WALL TAG FOR SPACING AND GUAGE" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 157:Structural Framing 1" | 1 occurrence | material: "TYP. VERTICAL METAL STUD - SEE WALL TAG FOR SPACING AND GUAGE" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 158:Structural Framing 1" | 1 occurrence | material: "TYP. VERTICAL METAL STUD - SEE WALL TAG FOR SPACING AND GUAGE" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 159:Structural Framing 1" | 1 occurrence | material: "TYP. VERTICAL METAL STUD - SEE WALL TAG FOR SPACING AND GUAGE" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 160:Structural Framing 7" | 1 occurrence | material: "BLOCKING @ DOOR HINGE LOCATIONS - EXTEND TO AT LEAST (3) VERT. STUDS" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 161:Structural Framing 7" | 1 occurrence | material: "BLOCKING @ DOOR HINGE LOCATIONS - EXTEND TO AT LEAST (3) VERT. STUDS" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 162:Structural Framing 7" | 1 occurrence | material: "BLOCKING @ DOOR HINGE LOCATIONS - EXTEND TO AT LEAST (3) VERT. STUDS" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 163:Structural Framing 7" | 1 occurrence | material: "BLOCKING @ DOOR HINGE LOCATIONS - EXTEND TO AT LEAST (3) VERT. STUDS" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 164:Structural Framing 7" | 1 occurrence | material: "BLOCKING @ DOOR HINGE LOCATIONS - EXTEND TO AT LEAST (3) VERT. STUDS" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 165:Structural Framing 7" | 1 occurrence | material: "BLOCKING @ DOOR HINGE LOCATIONS - EXTEND TO AT LEAST (3) VERT. STUDS" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 166:Structural Framing 2" | 1 occurrence | material: "METAL STUD TRACK WELDED OR SCREWED PER MANU. REQUIREMENTS" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 167:Structural Framing 1" | 1 occurrence | material: "DOUBLE UP METAL STUDS @ JAMB" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 168:Structural Framing 7" | 1 occurrence | material: "BLOCKING @ DOOR HINGE LOCATIONS - EXTEND TO AT LEAST (3) VERT. STUDS" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 169:Structural Framing 7" | 1 occurrence | material: "BLOCKING @ DOOR HINGE LOCATIONS - EXTEND TO AT LEAST (3) VERT. STUDS" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 170:Structural Framing 7" | 1 occurrence | material: "BLOCKING @ DOOR HINGE LOCATIONS - EXTEND TO AT LEAST (3) VERT. STUDS" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 171:Structural Framing 1" | 1 occurrence | material: "TYP. VERTICAL METAL STUD - SEE WALL TAG FOR SPACING AND GUAGE" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 172:Structural Framing 2" | 1 occurrence | material: "METAL SILL CHANNEL - FASTENER PER MANU. REQUIREMENTS" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 173:Structural Framing 1" | 1 occurrence | material: "TYP. VERTICAL METAL STUD - SEE WALL TAG FOR SPACING AND GUAGE" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 174:Structural Framing 2" | 1 occurrence | material: "METAL SILL CHANNEL - FASTENER PER MANU. REQUIREMENTS" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 175:Structural Framing 1" | 1 occurrence | material: "DOUBLE UP METAL STUDS @ JAMB" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 176:Structural Framing 2" | 1 occurrence | material: "(2) BOXED STUDS - SAME SIZE AS WALL STUDS" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 177:Structural Framing 2" | 1 occurrence | material: "(2) BOXED STUDS - SAME SIZE AS WALL STUDS" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 178:Structural Framing 2" | 1 occurrence | material: "METAL STUD TRACK WELDED OR SCREWED PER MANU. REQUIREMENTS" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 179:Structural Framing 2" | 1 occurrence | material: "METAL STUD TRACK WELDED OR SCREWED PER MANU. REQUIREMENTS" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 180:Structural Framing 1" | 1 occurrence | material: "TYP. VERTICAL METAL STUD - SEE WALL TAG FOR SPACING AND GUAGE" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 181:Structural Framing 2" | 1 occurrence | material: "METAL STUD TRACK WELDED OR SCREWED PER MANU. REQUIREMENTS" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 182:Structural Framing 2" | 1 occurrence | material: "(2) BOXED STUDS - SAME SIZE AS WALL STUDS" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 183:Structural Framing 2" | 1 occurrence | material: "(2) BOXED STUDS - SAME SIZE AS WALL STUDS" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 184:Structural Framing 2" | 1 occurrence | material: "METAL STUD TRACK WELDED OR SCREWED PER MANU. REQUIREMENTS" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 185:Structural Framing 2" | 1 occurrence | material: "METAL STUD TRACK WELDED OR SCREWED PER MANU. REQUIREMENTS" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 186:Structural Framing 1" | 1 occurrence | material: "TYP. VERTICAL METAL STUD - SEE WALL TAG FOR SPACING AND GUAGE" | property sets: Pset_BuildingElementProxyCommon
  IFCWALLTYPE "Generic Models 403:Generic Models 1" | 1 occurrence | material: "METAL RUNNER CHANNEL; FASTEN @ 24" O.C." | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 554:Generic Models 1" | 1 occurrence | material: "ACOUSTICAL SEALANT" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 557:Generic Models 1" | 1 occurrence | material: "WALL BASE AS SCHEDULED" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 559:Generic Models 1" | 1 occurrence | material: "TOP METAL STUD TRACK" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 576:Generic Models 1" | 1 occurrence | material: "ATTACH GYPSUM BOARD TO STUDS AND NOT TO TOP TRACK" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 579:Generic Models 1" | 1 occurrence | material: "ATTACH GYPSUM BOARD TO STUDS AND NOT TO TOP TRACK" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 581:Generic Models 65" | 1 occurrence | material: "METAL STUD" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 583:Generic Models 1" | 1 occurrence | material: "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 584:Generic Models 1" | 1 occurrence | material: "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 585:Generic Models 1" | 1 occurrence | material: "2X BLOCKING - LOCATED AT GRAB BARS, WALL HUNG CABINETS, ETC.)" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 586:Generic Models 1" | 1 occurrence | material: "WALL BASE AS SCHEDULED" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 595:Generic Models 1" | 1 occurrence | material: "METAL STUD - (SEE 'WALL TAG' & 'LAYER MATERIAL SCHEDULE' FOR SIZE, SPACING, & INSULATION)" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 608:Generic Models 1" | 1 occurrence | material: "ACOUSTICAL SEALANT OR FIRE SEALANT, IF RATED WALL" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 609:Generic Models 1" | 1 occurrence | material: "DEEP LEG OF DEFLECTION TRACK (2" MIN. DEFLECTION)" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 610:Generic Models 65" | 1 occurrence | material: "METAL STUD BRACE TO DECK AS NECESSARY" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 611:Generic Models 1" | 1 occurrence | material: "EXISTING ACOUSTICAL CEILING TRACK/TILE" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 598:Generic Models 1" | 1 occurrence | material: "EXISTING ACOUSTICAL CEILING TRACK/TILE" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 614:Generic Models 1" | 1 occurrence | material: "J BEAD DRYWALL TRIM" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 578:Generic Models 1" | 1 occurrence | material: "FIRE TREATED BLOCKING - SIZE AS NECESSARY" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 599:Generic Models 1" | 1 occurrence | material: "ACOUSTICAL SEALANT" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 616:Generic Models 1" | 1 occurrence | material: "CEILING TRACK AS SCHEDULED" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 617:Generic Models 1" | 1 occurrence | material: "EXISTING ACOUSTICAL TILE" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 612:Generic Models 1" | 1 occurrence | material: "EXISTING ACOUSTICAL TILE" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 615:Generic Models 1" | 1 occurrence | material: "EXISTING ACOUSTICAL TILE" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 613:Generic Models 1" | 1 occurrence | material: "J BEAD DRYWALL TRIM" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 560:Generic Models 1" | 1 occurrence | material: "ACOUSTICAL SEALANT" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 618:Generic Models 1" | 1 occurrence | material: "CEILING TRACK AS SCHEDULED" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 619:Generic Models 1" | 1 occurrence | material: "ALUM. STOREFRONT W/ TEMPERED SINGLE GLAZING" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 59:Generic Models 65" | 1 occurrence | material: "MORTAR JOINT" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 60:Generic Models 1" | 1 occurrence | material: "STANDARD 9-GAUGE (MW11), LADDER-SHAPED WIRE FABRICATED WITH BUTT-WELDED CROSS-RODS SPACED 406-MM (16-IN.) ON CENTER (OC)" | property sets: Pset_WallCommon
  IFCWALLTYPE "Walls 1:Walls 1" | 1 occurrence | material: "CONCRETE WALL" | property sets: Pset_WallCommon
  IFCWALLTYPE "Walls 2:Walls 2" | 1 occurrence | property sets: Pset_WallCommon
  IFCWALLTYPE "Walls 3:Walls 1" | 1 occurrence | material: "CONCRETE WALL" | property sets: Pset_WallCommon
  IFCWALLTYPE "Walls 4:Walls 2" | 1 occurrence | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 65:Generic Models 1" | 1 occurrence | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 66:Generic Models 1" | 1 occurrence | material: "SOUND MAT" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 69:Generic Models 1" | 1 occurrence | material: "3/4" GYP. CRETE" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 148:Generic Models 1" | 1 occurrence | material: "OPEN WEB WOOD TRUSS" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 343:Generic Models 1" | 1 occurrence | material: "UL RATED FIRE STOP" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 393:Generic Models 1" | 1 occurrence | material: "5/8" GYP. BD @ CEILING" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 394:Generic Models 1" | 1 occurrence | material: "5/8" GYP. BD @ CEILING" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 395:Generic Models 1" | 1 occurrence | material: "SINGLE 2X WOOD SILL - TREATED IF CONCRETE" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 396:Generic Models 1" | 1 occurrence | material: "SINGLE 2X WOOD SILL - TREATED IF CONCRETE" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 397:Generic Models 1" | 1 occurrence | material: "2X WOOD STUDS BEYOND" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 398:Generic Models 1" | 1 occurrence | material: "2X WOOD STUDS BEYOND" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 402:Generic Models 1" | 1 occurrence | material: "UL RATED FIRE STOP" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 408:Generic Models 1" | 1 occurrence | material: "UL RATED FIRE STOP" | property sets: Pset_WallCommon
  IFCFURNITURETYPE "Television-Plasma-54 inch:Television-Plasma-54 inch" | 1 occurrence | material: constituents "MaterialConstituentSet" ("FLAT SCREEN TV": "FLAT SCREEN TV", "TV-Badging": "TV-Badging", "FLAT SCREEN": "FLAT SCREEN")
  IFCCURTAINWALLTYPE "Curtain Wall:STOREFRONT - 2"x6"" | 6 occurrences | property sets: Pset_CurtainWallCommon
  IFCCURTAINWALLTYPE "Curtain Wall:STOREFRONT - 2"x4" - W/38" VERT. MODULE" | 1 occurrence | property sets: Pset_CurtainWallCommon
  IFCCURTAINWALLTYPE "Curtain Wall:HOLLOW METAL FRAME - 2" X 5 7/8" - DETAILED" | 1 occurrence | property sets: Pset_CurtainWallCommon
  IFCCURTAINWALLTYPE "Curtain Wall:HOLLOW METAL FRAME - 2" X 5 7/8"" | 1 occurrence | property sets: Pset_CurtainWallCommon
  IFCCURTAINWALLTYPE "Curtain Wall:EMPTY - MULLION AND PANEL" | 13 occurrences | property sets: Pset_CurtainWallCommon
  IFCWALLTYPE "Basic Wall:W4AØD - (5/8 GYP - 2X4 WOOD - 5/8 GYP)" | STANDARD | 1 occurrence | material: layers "Basic Wall:W4AØD - (5/8 GYP - 2X4 WOOD - 5/8 GYP)" ("5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" 0.0520833333333333, "2X WOOD STUD" 0.291666666666667, "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" 0.0520833333333333) | property sets: Pset_WallCommon
  IFCBUILDINGELEMENTPROXYTYPE "Refrigerator_-_Side-by-Side_6047:36" X 30"" | 1 occurrence | material: "REFRIG." | property sets: Pset_BuildingElementProxyCommon
  IFCFURNITURETYPE "300 Series Wall Hung Cabinet_301:12" 2" | 1 occurrence | material: constituents "MaterialConstituentSet" ("<Unnamed>": "<Unnamed>", "Cabinet - Wood Door / Drawer": "CASEWORK", "Cabinet - Panel": "CASEWORK", "CASEWORK": "CASEWORK") | property sets: Pset_ManufacturerTypeInformation
  IFCFURNITURETYPE "300 Series Wall Hung Cabinet_302:36"W x 21"H" | 1 occurrence | material: constituents "MaterialConstituentSet" ("<Unnamed>": "<Unnamed>", "Cabinet - Panel": "CASEWORK", "Cabinet - Wood Door / Drawer": "CASEWORK") | property sets: Pset_ManufacturerTypeInformation
  IFCFURNITURETYPE "300 Series Wall Hung Cabinet_326:26 3/4"" | 1 occurrence | material: constituents "MaterialConstituentSet" ("<Unnamed>": "<Unnamed>", "Cabinet - Panel": "CASEWORK", "Cabinet - Wood Door / Drawer": "CASEWORK") | property sets: Pset_ManufacturerTypeInformation
  IFCFURNITURETYPE "OD_CW_Countertop:36"" | 1 occurrence | material: constituents "MaterialConstituentSet" ("SOLID SURFACE - GROUP 4 OR BETTER": "SOLID SURFACE - GROUP 4 OR BETTER", "CASEWORK": "CASEWORK")
  IFCBUILDINGELEMENTPROXYTYPE "Dishwasher_15404:34" counter" | 1 occurrence | material: "<Unnamed>" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "262400 - Switchboards and Panelboards - Electric Panel - Generic:262400 - Switchboards and Panelboards - Electric Panel - Generic" | 1 occurrence | material: "ELECTRICAL PANEL" | property sets: Pset_BuildingElementProxyCommon
  IFCSYSTEMFURNITUREELEMENTTYPE "Dining_table_Parametric_Size_15043:1" | 1 occurrence | material: constituents "MaterialConstituentSet" ("Wood Frame": "Wood Frame", "Fabric": "Fabric", "<Unnamed>": "<Unnamed>")
  IFCBUILDINGELEMENTPROXYTYPE "Range-Electric:36"" | 1 occurrence | material: constituents "MaterialConstituentSet" ("Appliances": "Appliance - Plastic - Red", "Appliances": "Appliance - Chrome", "Appliances": "RANGE", "Appliances": "Appliance - Oven Glass") | property sets: Pset_BuildingElementProxyCommon
  IFCFURNITURETYPE "254:254" | 1 occurrence | material: constituents "MaterialConstituentSet" ("Default metal": "Default metal", "Cabinet - Wood Door / Drawer": "CASEWORK", "Cabinet - Panel": "CASEWORK") | property sets: Pset_ManufacturerTypeInformation
  IFCFURNITURETYPE "102:36" | 1 occurrence | material: constituents "MaterialConstituentSet" ("Default metal": "Default metal", "Cabinet - Wood Door / Drawer": "CASEWORK", "Cabinet - Panel": "CASEWORK") | property sets: Pset_ManufacturerTypeInformation
  IFCFURNITURETYPE "211:24"" | 1 occurrence | material: constituents "MaterialConstituentSet" ("Default metal": "Default metal", "Cabinet - Wood Door / Drawer": "CASEWORK", "Cabinet - Panel": "CASEWORK") | property sets: Pset_ManufacturerTypeInformation
  IFCFURNITURETYPE "222:30"" | 1 occurrence | material: constituents "MaterialConstituentSet" ("Default metal": "Default metal", "Cabinet - Wood Door / Drawer": "CASEWORK", "Cabinet - Panel": "CASEWORK") | property sets: Pset_ManufacturerTypeInformation
  IFCFURNITURETYPE "253:30"" | 1 occurrence | material: constituents "MaterialConstituentSet" ("Default metal": "Default metal", "Cabinet - Wood Door / Drawer": "CASEWORK", "Cabinet - Panel": "CASEWORK") | property sets: Pset_ManufacturerTypeInformation
  IFCFURNITURETYPE "152:36"" | 1 occurrence | material: constituents "MaterialConstituentSet" ("CABINET PULLS": "CABINET PULLS", "Cabinet - Wood Door / Drawer": "CASEWORK", "Cabinet - Panel": "CASEWORK") | property sets: Pset_ManufacturerTypeInformation
  IFCFURNITURETYPE "197:197" | 1 occurrence | material: constituents "MaterialConstituentSet" ("Default metal": "Default metal", "Cabinet - Panel": "CASEWORK", "Cabinet - Wood Door / Drawer": "CASEWORK") | property sets: Pset_ManufacturerTypeInformation
  IFCFURNITURETYPE "101:24"" | 1 occurrence | material: constituents "MaterialConstituentSet" ("Default metal": "Default metal", "Cabinet - Wood Door / Drawer": "CASEWORK", "Cabinet - Panel": "CASEWORK") | property sets: Pset_ManufacturerTypeInformation
  IFCFURNITURETYPE "230:230" | 1 occurrence | material: constituents "MaterialConstituentSet" ("Default metal": "Default metal", "Cabinet - Wood Door / Drawer": "CASEWORK", "Cabinet - Panel": "CASEWORK") | property sets: Pset_ManufacturerTypeInformation
  IFCFURNITURETYPE "OD_CW_Base Cabinet:34"" | 1 occurrence | material: constituents "MaterialConstituentSet" ("CABINET PULLS": "CABINET PULLS", "BASE CABINETS": "BASE CABINETS", "COUNTERTOP": "COUNTERTOP")
  IFCFURNITURETYPE "OD_CW_Upper Cabinet:3'" | 1 occurrence | material: constituents "MaterialConstituentSet" ("CABINET PULLS": "CABINET PULLS", "UPPER CABINETS": "UPPER CABINETS")
  IFCFURNITURETYPE "OD_CW_Countertop:36"" | 1 occurrence | material: constituents "MaterialConstituentSet" ("SOLID SURFACE - GROUP 4 OR BETTER": "SOLID SURFACE - GROUP 4 OR BETTER", "CASEWORK": "CASEWORK")
  IFCFURNITURETYPE "OD_CW_Countertop:30"" | 1 occurrence | material: constituents "MaterialConstituentSet" ("SOLID SURFACE - GROUP 4 OR BETTER": "SOLID SURFACE - GROUP 4 OR BETTER", "CASEWORK": "CASEWORK")
  IFCFURNITURETYPE "Bar_Stool_6722[1]:Bar_Stool_6722[1]" | 1 occurrence | material: constituents "MaterialConstituentSet" ("MET": "MET", "fab": "fab")
  IFCROOFTYPE "Basic Roof:Generic - 12"" | 1 occurrence | property sets: Pset_RoofCommon
  IFCBUILDINGELEMENTPROXYTYPE "085000 - Windows - Casement or Awning or Fixed:FIXED PICTURE - TYPE 1" | 1 occurrence | material: constituents "MaterialConstituentSet" ("DOUBLE HUNG WINDOWS - BLACK EXT/INT SASH - LIMIT BOTTOM SASH TO 4" MAX OPEN": "DOUBLE HUNG WINDOWS - BLACK EXT/INT SASH - LIMIT BOTTOM SASH TO 4" MAX OPEN", "GL - INSULATED - LOW-E": "GL - INSULATED - LOW-E", "<Unnamed>": "<Unnamed>") | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation
  IFCDOORTYPE "OD_SINGLE:SINGLE - LITE - MUNTINS - 3-0 x 6-8" | DOOR | SINGLE_SWING_RIGHT | 1 occurrence | material: constituents "MaterialConstituentSet" ("GL - TEMPERED - INSULATED - LOW-E": "GL - TEMPERED - INSULATED - LOW-E", "Panel": "CW - CLAD WOOD DOOR", "Frame/Mullion": "CW - CLAD WOOD DOOR") | property sets: OD_SINGLE:SINGLE - LITE - MUNTINS - 3-0 x 6-8:2169410, OD_SINGLE:SINGLE - LITE - MUNTINS - 3-0 x 6-8:2169410:1, Pset_DoorCommon
  IFCSLABTYPE "316600 - Special Foundations - Diamond Pier - Generic:316600 - Special Foundations - Diamond Pier - Generic" | BASESLAB | 1 occurrence | material: "DIAMOND PIER DP-50/50 - (3300# B.L.C. AT 1500PSF SOILS, 4400# B.L.C. AT 2000PSF SOILS)" | property sets: Pset_SlabCommon
  IFCSLABTYPE "Footing-Cylindrical:20"WX42"D" | BASESLAB | 1 occurrence | material: "CYLINDRICAL CONCRETE PIER - 20"Øx4'-0" - (4) # 4 VERTICALS - (3) #3 TIES @ 2" OC - REST @ 12" OC" | property sets: Pset_SlabCommon
  IFCBEAMTYPE "C-Channel:C CHANNEL - SIZE TBD1" | BEAM | 1 occurrence | material: profiles "C CHANNEL - SIZE TBD1" ("C CHANNEL - SIZE TBD1": "STEEL C CHANNEL - HDG - SEE STRUCT DWGS") | property sets: Pset_BeamCommon
  IFCDUCTSEGMENTTYPE "Rectangular Duct:Default" | 5 occurrences | material: "DUCT"
  IFCDUCTFITTINGTYPE "Rectangular Elbow - Radius:1.5 W" | 1 occurrence | material: "DUCT"
  IFCDUCTFITTINGTYPE "Rectangular Tee:Standard" | 1 occurrence | material: "DUCT"
  IFCDUCTFITTINGTYPE "Rectangular Straight Transition - DTL:Standard" | 1 occurrence | material: "DUCT"
  IFCDUCTSEGMENTTYPE "Round Duct:Default" | 5 occurrences | material: "DUCT"
  IFCDUCTFITTINGTYPE "Round Elbow:1.5 D" | 1 occurrence | material: "DUCT"
  IFCDUCTFITTINGTYPE "Round Tee - Straight:Standard" | 1 occurrence | material: "DUCT"
  IFCDUCTFITTINGTYPE "Round Transition - DTL:Standard" | 1 occurrence | material: "DUCT"
  IFCDOORTYPE "OD_SINGLE:SINGLE - FLUSH - 3-0 x 6-8" | DOOR | SINGLE_SWING_RIGHT | 6 occurrences | material: "HM" | property sets: OD_SINGLE:SINGLE - FLUSH - 3-0 x 6-8:2170758, OD_SINGLE:SINGLE - FLUSH - 3-0 x 6-8:2170758:1, Pset_DoorCommon
  IFCBUILDINGELEMENTPROXYTYPE "085000 - Windows - Fixed:_Type Name_" | 1 occurrence | material: constituents "MaterialConstituentSet" ("GL - INSULATED - LOW-E": "GL - INSULATED - LOW-E", "DOUBLE HUNG WINDOWS - BLACK EXT/INT SASH - LIMIT BOTTOM SASH TO 4" MAX OPEN": "DOUBLE HUNG WINDOWS - BLACK EXT/INT SASH - LIMIT BOTTOM SASH TO 4" MAX OPEN") | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "085000 - Windows - Casement or Awning or Fixed:FIXED PICTURE - TYPE 1" | 1 occurrence | material: constituents "MaterialConstituentSet" ("DOUBLE HUNG WINDOWS - BLACK EXT/INT SASH - LIMIT BOTTOM SASH TO 4" MAX OPEN": "DOUBLE HUNG WINDOWS - BLACK EXT/INT SASH - LIMIT BOTTOM SASH TO 4" MAX OPEN", "GL - INSULATED - LOW-E": "GL - INSULATED - LOW-E", "<Unnamed>": "<Unnamed>") | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation
  IFCSLABTYPE "316600 - Special Foundations - Diamond Pier - Generic:316600 - Special Foundations - Diamond Pier - Generic" | BASESLAB | 1 occurrence | material: "DIAMOND PIER DP-50/50 - (3300# B.L.C. AT 1500PSF SOILS, 4400# B.L.C. AT 2000PSF SOILS)" | property sets: Pset_SlabCommon
  IFCSLABTYPE "Footing-Cylindrical:20"WX42"D" | BASESLAB | 1 occurrence | material: "CYLINDRICAL CONCRETE PIER - 20"Øx4'-0" - (4) # 4 VERTICALS - (3) #3 TIES @ 2" OC - REST @ 12" OC" | property sets: Pset_SlabCommon
  IFCFURNITURETYPE "123000 - Casework - Upper Cabinet - Generic - 302:123000 - Casework - Upper Cabinet - Generic - 302" | 1 occurrence | material: constituents "MaterialConstituentSet" ("<Unnamed>": "<Unnamed>", "Cabinet - Wood Door / Drawer": "PL-2 TBD", "Cabinet - Panel": "CASEWORK", "Cabinet - Panel": "PL-2 TBD")
  IFCFURNITURETYPE "123000 - Casework - Upper Cabinet - Generic - 301:30x48" | 1 occurrence | material: constituents "MaterialConstituentSet" ("<Unnamed>": "<Unnamed>", "Cabinet - Panel": "PL-2 TBD", "Cabinet - Wood Door / Drawer": "PL-2 TBD", "Cabinet - Panel": "CASEWORK")
  IFCDISTRIBUTIONELEMENTTYPE "The Shower:The Shower" | 1 occurrence | material: constituents "MaterialConstituentSet" ("<Unnamed>": "<Unnamed>", "SHOWER": "SHOWER", "Stainless Steel, Brushed": "Stainless Steel, Brushed") | property sets: Pset_ManufacturerTypeInformation
  IFCDISTRIBUTIONELEMENTTYPE "Shower Head:Shower Head" | 2 occurrences | material: "SHOWER HEAD"
  IFCFURNITURETYPE "OD_CW_Closet:OD_CW_Closet" | 1 occurrence | material: "CASEWORK"
  IFCFURNITURETYPE "125900 - Systems Furniture - Workstation - L-shaped - Generic:L-SHADED" | 1 occurrence | material: constituents "MaterialConstituentSet" ("Herman Miller - Seat": "Herman Miller - Finish SCN Satin Carbon", "Herman Miller - Seat": "Herman Miller - Finish DCR Dark Carbon", "Herman Miller - Seat": "Herman Miller - Finish CRB Carbon", "Herman Miller - Seat": "Herman Miller - Finish BK Black", "Herman Miller - Seat": "_DESIGN_FABRIC", "_WOOD": "_WOOD")
  IFCFURNITURETYPE "HermanMiller_Seating_AER1_NewAeron_WorkChair:B Size Low-Hgt Range Adj Std Tlt Hgt Adj Plus Pivot Arms Leather Arms Adj Lumbar Sup" | 1 occurrence | material: constituents "MaterialConstituentSet" ("Herman Miller - Seat": "Herman Miller - Finish SCN Satin Carbon", "Herman Miller - Seat": "Herman Miller - Finish DCR Dark Carbon", "Herman Miller - Seat": "Herman Miller - Finish CRB Carbon", "Herman Miller - Seat": "Herman Miller - Finish BK Black", "Herman Miller - Seat": "_DESIGN_FABRIC") | property sets: Pset_ManufacturerTypeInformation
  IFCFURNITURETYPE "HermanMiller_Seating_Caper_StackingChair:FLEXNET Seat With Arms Casters" | 1 occurrence | material: constituents "MaterialConstituentSet" ("Herman Miller - Seat": "Herman Miller - Finish BK Black", "Herman Miller - Seat": "<Unnamed>", "Herman Miller - Seat": "Herman Miller - Seat Material 6V01 Flexnet Black") | property sets: Pset_ManufacturerTypeInformation
  IFCFURNITURETYPE "Table-Conference-Teknion-STRTL_Cover-R2014:118" w x 39.5" d x 29" h - Without Power" | 1 occurrence | material: constituents "MaterialConstituentSet" ("Paint - Teknion - 7Y - Storm_White_Coordinate": "Paint - Teknion - 7Y - Storm_White_Coordinate", "<Unnamed>": "<Unnamed>", "Foundation_Laminate-Teknion-8T-Crisp_Grey": "Foundation_Laminate-Teknion-8T-Crisp_Grey") | property sets: Pset_ManufacturerTypeInformation
  IFCFURNITURETYPE "Seating-Setee-Teknion-BBMC_Metropolitan-R2013:Lounge Settee" | 1 occurrence | material: constituents "MaterialConstituentSet" ("Seat": "TRIM 1", "Frame": "Metal - Teknion - C6 - Chrome", "Frame": "Plastic - Teknion - Z1 - Greystone") | property sets: Pset_ManufacturerTypeInformation
  IFCFURNITURETYPE "Table-Coffee-Teknion-STRTC_Cover-R2014:38,25" w x 27,5" d x 15" h" | 2 occurrences | material: constituents "MaterialConstituentSet" ("Furniture": "Metal - Teknion - C9 - Polished Aluminum", "Furniture": "table tops") | property sets: Pset_ManufacturerTypeInformation
  IFCFURNITURETYPE "Seating-Lounge_Chair-Teknion-BBMC_Metropolitan-R2013:Lounge Chair" | 1 occurrence | material: constituents "MaterialConstituentSet" ("Seat": "TRIM 1", "Frame": "<Unnamed>", "Frame": "Metal - Teknion - C6 - Chrome") | property sets: Pset_ManufacturerTypeInformation
  IFCFURNITURETYPE "Seating-Sofa-Teknion-BBAC_AC_Lounge-R2013:Two Seater" | 1 occurrence | material: constituents "MaterialConstituentSet" ("Fabric - Teknion - E519 - Fundamentals": "Fabric - Teknion - E519 - Fundamentals", "Seat": "Fabric - Teknion - E519 - Fundamentals", "Frame": "Metal - Teknion - F8 - Bronzed Nickel") | property sets: Pset_ManufacturerTypeInformation
  IFCFURNITURETYPE "Seating-Chair-Teknion-BBAC_AC_Lounge-R2013:Chair" | 1 occurrence | material: constituents "MaterialConstituentSet" ("Seat": "BLACK TRIM", "Frame": "Metal - Teknion - F8 - Bronzed Nickel") | property sets: Pset_ManufacturerTypeInformation
  IFCFURNITURETYPE "Table-Casual_Work-Teknion-STRTW_Cover_Without_Power-R2014:33" x 29" x 26"" | 1 occurrence | material: constituents "MaterialConstituentSet" ("Metal - Teknion - C9 - Polished Aluminum": "Metal - Teknion - C9 - Polished Aluminum", "Furniture": "Metal - Teknion - C9 - Polished Aluminum", "Furniture": "table tops") | property sets: Pset_ManufacturerTypeInformation
  IFCFURNITURETYPE "Table-Coffee-Teknion-BBCTC_Cosmos_Large-R2013:28 3/8" High" | 1 occurrence | material: "Solid Core - Teknion - RX - Ebony Flat Edge" | property sets: Pset_ManufacturerTypeInformation
  IFCCOLUMNTYPE "HSS-Round Hollow Structural Section-Column:HSS - 3.5" - SIZE TBD" | COLUMN | 1 occurrence | material: profiles "HSS - 3.5" - SIZE TBD" ("HSS - 3.5" - SIZE TBD": "STRUCTURAL STEEL COLUMN - SIZE TBD") | property sets: Pset_ColumnCommon
  IFCCOLUMNTYPE "HSS-Hollow Structural Section-Column:HSS 3.5" - SIZE TBD" | COLUMN | 1 occurrence | material: profiles "HSS 3.5" - SIZE TBD" ("HSS 3.5" - SIZE TBD": "STRUCTURAL STEEL COLUMN - SIZE TBD") | property sets: Pset_ColumnCommon
  IFCCOLUMNTYPE "HSS-Hollow Structural Section-Column:TUBE STEEL (HDG) - SIZE TBD" | COLUMN | 1 occurrence | material: profiles "TUBE STEEL (HDG) - SIZE TBD" ("TUBE STEEL (HDG) - SIZE TBD": "TUBE STEEL COLUMN - SEE STRUCT DWGS - HDG") | property sets: Pset_ColumnCommon
  IFCCOLUMNTYPE "HSS-Hollow Structural Section-Column:HSS 6" - SIZE TBD" | COLUMN | 1 occurrence | material: profiles "HSS 6" - SIZE TBD" ("HSS 6" - SIZE TBD": "STRUCTURAL STEEL COLUMN - SIZE TBD") | property sets: Pset_ColumnCommon
  IFCCOLUMNTYPE "Timber-Column:4X4" | COLUMN | 1 occurrence | material: profiles "4X4" ("4X4": "STRUCTURAL WOOD COLUMN - SIZE TBD") | property sets: Pset_ColumnCommon
  IFCCOLUMNTYPE "Timber-Column:6x6" | COLUMN | 2 occurrences | material: profiles "6x6" ("6x6": "STRUCTURAL WOOD COLUMN - SIZE TBD") | property sets: Pset_ColumnCommon
  IFCCOLUMNTYPE "Timber-Column:(3) 2X6 - BUILT-UP COLUMN" | COLUMN | 1 occurrence | material: profiles "(3) 2X6 - BUILT-UP COLUMN" ("(3) 2X6 - BUILT-UP COLUMN": "STRUCTURAL WOOD COLUMN - SIZE TBD") | property sets: Pset_ColumnCommon
  IFCCOLUMNTYPE "Timber-Column:(3) 2X4 - BUILT-UP COLUMN" | COLUMN | 1 occurrence | material: profiles "(3) 2X4 - BUILT-UP COLUMN" ("(3) 2X4 - BUILT-UP COLUMN": "STRUCTURAL WOOD COLUMN - SIZE TBD") | property sets: Pset_ColumnCommon
  IFCWALLTYPE "Generic Models 413:Generic Models 1" | 1 occurrence | material: "ACOUSTICAL SEALANT" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 415:Generic Models 1" | 1 occurrence | material: "WALL BASE AS SCHEDULED" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 432:Generic Models 1" | 1 occurrence | material: "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 550:Generic Models 1" | 1 occurrence | material: "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 552:Generic Models 1" | 1 occurrence | material: "WALL BASE AS SCHEDULED" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 562:Generic Models 1" | 1 occurrence | material: "ACOUSTICAL SEALANT OR FIRE SEALANT, IF RATED WALL" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 565:Generic Models 1" | 1 occurrence | material: "EXISTING ACOUSTICAL CEILING TRACK/TILE" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 566:Generic Models 1" | 1 occurrence | material: "EXISTING ACOUSTICAL CEILING TRACK/TILE" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 568:Generic Models 1" | 1 occurrence | material: "J BEAD DRYWALL TRIM" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 569:Generic Models 1" | 1 occurrence | material: "BLOCKING - SIZE AS NEC." | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 570:Generic Models 1" | 1 occurrence | material: "ACOUSTICAL SEALANT" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 572:Generic Models 1" | 1 occurrence | material: "CEILING TRACK AS SCHEDULED" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 573:Generic Models 1" | 1 occurrence | material: "EXISTING ACOUSTICAL TILE" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 574:Generic Models 1" | 1 occurrence | material: "EXISTING ACOUSTICAL TILE" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 575:Generic Models 1" | 1 occurrence | material: "EXISTING ACOUSTICAL TILE" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 582:Generic Models 1" | 1 occurrence | material: "J BEAD DRYWALL TRIM" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 587:Generic Models 1" | 1 occurrence | material: "ACOUSTICAL SEALANT" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 588:Generic Models 1" | 1 occurrence | material: "CEILING TRACK AS SCHEDULED" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 412:Generic Models 1" | 1 occurrence | material: "2X WOOD SILL - TREATED IF ON CONCRETE" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 419:Generic Models 65" | 1 occurrence | material: "2X WOOD STUD" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 48:Generic Models 1" | 1 occurrence | material: "DOUBLE 2X WOOD TOP PLATE" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 250:Generic Models 1" | 1 occurrence | material: "2X WOOD SILL" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 416:Generic Models 65" | 1 occurrence | material: "WOOD STUD BRACE TO DECK AS NECESSARY" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 386:Generic Models 1" | 1 occurrence | material: "2x6 STUDS 16" O.C. (R-19 BATT. INSULATION)" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 420:Generic Models 1" | 1 occurrence | material: "UNDERSIDE OF FLOOR ASSEMBLY - SEE STRUCT. DWGS" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 551:Generic Models 1" | 1 occurrence | material: "METAL RUNNER CHANNEL; FASTEN @ 24" O.C." | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 553:Generic Models 1" | 1 occurrence | material: "ACOUSTICAL SEALANT OR FIRE SEALANT, IF RATED WALL" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 563:Generic Models 1" | 1 occurrence | material: "WALL BASE AS SCHEDULED" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 564:Generic Models 1" | 1 occurrence | material: "DEEP LEG OF DEFLECTION TRACK (2" MIN. DEFLECTION)" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 589:Generic Models 1" | 1 occurrence | material: "ACOUSTICAL SEALANT OR FIRE SEALANT, IF RATED WALL" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 591:Generic Models 1" | 1 occurrence | material: "ATTACH GYPSUM BOARD TO STUDS AND NOT TO TOP TRACK" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 597:Generic Models 65" | 1 occurrence | material: "METAL STUD" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 600:Generic Models 1" | 1 occurrence | material: "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 602:Generic Models 1" | 1 occurrence | material: "2X BLOCKING - LOCATED AT GRAB BARS, WALL HUNG CABINETS, ETC.)" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 604:Generic Models 1" | 1 occurrence | material: "METAL STUD - (SEE 'WALL TAG' & 'LAYER MATERIAL SCHEDULE' FOR SIZE, SPACING, & INSULATION)" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 22:Generic Models 1" | 1 occurrence | material: "CEILING TRACK AS SCHEDULED" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 27:Generic Models 1" | 1 occurrence | material: "CEILING AS SCHEDULED" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 30:Generic Models 1" | 1 occurrence | material: "CEILING TRACK AS SCHEDULED" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 37:Generic Models 1" | 1 occurrence | material: "CEILING AS SCHEDULED" | property sets: Pset_WallCommon
  IFCWALLTYPE "Basic Wall:W6AØD - (5/8 GYP - 2X6 WOOD - 5/8 GYP)" | STANDARD | 1 occurrence | material: layers "Basic Wall:W6AØD - (5/8 GYP - 2X6 WOOD - 5/8 GYP)" ("5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" 0.0520833333333333, "2X WOOD STUD" 0.458333333333333, "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" 0.0520833333333333) | property sets: Pset_WallCommon
  IFCWALLTYPE "Basic Wall:FURR - M358DØD - (5/8 GYP - 3 5/8 METAL(BATT))" | STANDARD | 1 occurrence | material: layers "Basic Wall:FURR - M358DØD - (5/8 GYP - 3 5/8 METAL(BATT))" ("AIR GAP" 0.0208333333333333, "METAL STUD - (SEE 'WALL TAG' & 'LAYER MATERIAL SCHEDULE' FOR SIZE, SPACING, & INSULATION)" 0.302083333333333, "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" 0.0520833333333333) | property sets: Pset_WallCommon
  IFCWALLTYPE "Basic Wall:M358AØD - (5/8 GYP - 3 5/8 METAL- 5/8 GYP)" | STANDARD | 1 occurrence | material: layers "Basic Wall:M358AØD - (5/8 GYP - 3 5/8 METAL- 5/8 GYP)" ("5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" 0.0520833333333333, "METAL STUD" 0.302083333333333, "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" 0.0520833333333333) | property sets: Pset_WallCommon
  IFCWALLTYPE "Basic Wall:M358BØD - (5/8 GYP - 3 5/8 METAL(BATT) - 5/8 GYP)" | STANDARD | 1 occurrence | material: layers "Basic Wall:M358BØD - (5/8 GYP - 3 5/8 METAL(BATT) - 5/8 GYP)" ("5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" 0.0520833333333333, "METAL STUD - (SEE 'WALL TAG' & 'LAYER MATERIAL SCHEDULE' FOR SIZE, SPACING, & INSULATION)" 0.302083333333333, "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" 0.0520833333333333) | property sets: Pset_WallCommon
  IFCWALLTYPE "Basic Wall:FURR - W4DØFD - (5/8 GYP - 2X4 WOOD(BATT))" | STANDARD | 1 occurrence | material: layers "Basic Wall:FURR - W4DØFD - (5/8 GYP - 2X4 WOOD(BATT))" ("AIR GAP" 0.0208333333333333, "2x6 STUDS 16" O.C. (R-19 BATT. INSULATION)" 0.291666666666667, "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" 0.0520833333333333) | property sets: Pset_WallCommon
  IFCWALLTYPE "Basic Wall:W8AØD - (5/8 GYP - 2X8 WOOD - 5/8 GYP)" | STANDARD | 1 occurrence | material: layers "Basic Wall:W8AØD - (5/8 GYP - 2X8 WOOD - 5/8 GYP)" ("5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" 0.0520833333333333, "2X WOOD STUD" 0.604166666666667, "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" 0.0520833333333333) | property sets: Pset_WallCommon
  IFCWALLTYPE "Basic Wall:FURR - W4CØFA - (5/8 GYP - 2X4 WOOD)" | STANDARD | 1 occurrence | material: layers "Basic Wall:FURR - W4CØFA - (5/8 GYP - 2X4 WOOD)" ("AIR GAP" 0.0208333333333333, "2X WOOD STUD" 0.291666666666667, "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" 0.0520833333333333) | property sets: Pset_WallCommon
  IFCWALLTYPE "Basic Wall:M6AØD - (5/8 GYP - 6 METAL- 5/8 GYP)" | STANDARD | 1 occurrence | material: layers "Basic Wall:M6AØD - (5/8 GYP - 6 METAL- 5/8 GYP)" ("5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" 0.0520833333333333, "METAL STUD" 0.5, "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" 0.0520833333333333) | property sets: Pset_WallCommon
  IFCWALLTYPE "Basic Wall:M6BØD - (5/8 GYP - 6 METAL(BATT) - 5/8 GYP)" | STANDARD | 1 occurrence | material: layers "Basic Wall:M6BØD - (5/8 GYP - 6 METAL(BATT) - 5/8 GYP)" ("5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" 0.0520833333333333, "METAL STUD - (SEE 'WALL TAG' & 'LAYER MATERIAL SCHEDULE' FOR SIZE, SPACING, & INSULATION)" 0.5, "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" 0.0520833333333333) | property sets: Pset_WallCommon
  IFCWALLTYPE "Basic Wall:C6QØD - (6" CONCRETE)" | STANDARD | 1 occurrence | material: layers "Basic Wall:C6QØD - (6" CONCRETE)" ("CONCRETE WALL" 0.5) | property sets: Pset_WallCommon
  IFCWALLTYPE "Basic Wall:C10QØD - (10" CONCRETE)" | STANDARD | 1 occurrence | material: layers "Basic Wall:C10QØD - (10" CONCRETE)" ("CONCRETE WALL" 0.833333333333333) | property sets: Pset_WallCommon
  IFCWALLTYPE "Basic Wall:C12QØD - (12" CONCRETE)" | STANDARD | 1 occurrence | material: layers "Basic Wall:C12QØD - (12" CONCRETE)" ("CONCRETE WALL" 1.) | property sets: Pset_WallCommon
  IFCWALLTYPE "Basic Wall:M8RØD - (8" CMU)" | STANDARD | 1 occurrence | material: layers "Basic Wall:M8RØD - (8" CMU)" ("CMU (SEE 'WALL TAG' FOR SIZE)" 0.635416666666667) | property sets: Pset_WallCommon
  IFCWALLTYPE "Basic Wall:M10RØD - (10" CMU)" | STANDARD | 1 occurrence | material: layers "Basic Wall:M10RØD - (10" CMU)" ("CMU (SEE 'WALL TAG' FOR SIZE)" 0.802083333333333) | property sets: Pset_WallCommon
  IFCWALLTYPE "Basic Wall:M12RØD - (12" CMU)" | STANDARD | 1 occurrence | material: layers "Basic Wall:M12RØD - (12" CMU)" ("CMU (SEE 'WALL TAG' FOR SIZE)" 0.96875) | property sets: Pset_WallCommon
  IFCDISTRIBUTIONELEMENTTYPE "224200 - Commercial Plumbing Fixtures - 3 Compartment Sink:one" | 1 occurrence | material: "3 COMPARTMENT SINK"
  IFCBUILDINGELEMENTPROXYTYPE "126416 - Tables - Stainless Steel Prep Table:72X30" | 1 occurrence | material: "SS TABLE" | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation
  IFCBUILDINGELEMENTPROXYTYPE "224216 - Commercial Sinks - SS Hand Sink:DefaultType" | 1 occurrence | material: constituents "MaterialConstituentSet" ("QF_Steel-Chrome Plated": "QF_Steel-Chrome Plated", "NON-HAND OPERATED HAND SINK W/ SIDE SPLASH SHIELDS": "NON-HAND OPERATED HAND SINK W/ SIDE SPLASH SHIELDS") | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation
  IFCDISTRIBUTIONELEMENTTYPE "224216 - Commercial Sinks - Mop Sink - Rectangle:224216 - Commercial Sinks - Mop Sink - Rectangle" | 1 occurrence | material: constituents "MaterialConstituentSet" ("MOP SINK": "MOP SINK", "Steel - Zurn Industries - Stainless Type 304 CF8": "Steel - Zurn Industries - Stainless Type 304 CF8")
  IFCCOLUMNTYPE "W-Wide Flange-Column:W4 - SIZE TBD" | COLUMN | 1 occurrence | material: profiles "W4 - SIZE TBD" ("W4 - SIZE TBD": "STRUCTURAL STEEL COLUMN - SIZE TBD") | property sets: Pset_ColumnCommon
  IFCCOLUMNTYPE "W-Wide Flange-Column:W5 - SIZE TBD" | COLUMN | 1 occurrence | material: profiles "W5 - SIZE TBD" ("W5 - SIZE TBD": "STRUCTURAL STEEL COLUMN - SIZE TBD") | property sets: Pset_ColumnCommon
  IFCCOLUMNTYPE "W-Wide Flange-Column:W6 - SIZE TBD" | COLUMN | 1 occurrence | material: profiles "W6 - SIZE TBD" ("W6 - SIZE TBD": "STRUCTURAL STEEL COLUMN - SIZE TBD") | property sets: Pset_ColumnCommon
  IFCCOLUMNTYPE "W-Wide Flange-Column:W8 - SIZE TBD" | COLUMN | 1 occurrence | material: profiles "W8 - SIZE TBD" ("W8 - SIZE TBD": "STRUCTURAL STEEL COLUMN - SIZE TBD") | property sets: Pset_ColumnCommon
  IFCCOLUMNTYPE "W-Wide Flange-Column:W10 - SIZE TBD" | COLUMN | 1 occurrence | material: profiles "W10 - SIZE TBD" ("W10 - SIZE TBD": "STRUCTURAL STEEL COLUMN - SIZE TBD") | property sets: Pset_ColumnCommon
  IFCDOORTYPE "Simple Opening:3x7" | DOOR | 1 occurrence | material: "<Unnamed>" | property sets: Simple Opening:3x7:2460090, Simple Opening:3x7:2460090:1, Pset_DoorCommon
  IFCDISTRIBUTIONELEMENTTYPE "224200 - Commercial Plumbing Fixtures - 1 Compartment Sink:one" | 1 occurrence | material: "1 COMPARTMENT SINK"
  IFCDISTRIBUTIONELEMENTTYPE "22142613 - Roof Drains - Type A:22142613 - Roof Drains - Type A" | 3 occurrences | material: "ROOF DRAIN, TYP. (SEE PLUMB DWGS) - W/ INTEGRATED EMERGENCY OVERFLOW DRAIN"
  IFCDISTRIBUTIONELEMENTTYPE "22131913 - Sanitary Drains - Floor Drain:22131913 - Sanitary Drains - Floor Drain" | 1 occurrence | material: "FLOOR DRAIN"
  IFCFURNITURETYPE "office chair:Copy of Chair - Desk (2)" | 1 occurrence | material: constituents "MaterialConstituentSet" ("Chrome (1)": "Chrome (1)", "Textile - White": "Textile - White")
  IFCSTAIRTYPE "Assembled Stair:C CHANNEL STRINGER" | HALF_TURN_STAIR | 1 occurrence | property sets: Pset_StairCommon, Pset_StairFlightCommon
  IFCSTAIRTYPE "Assembled Stair:C CHANNEL STRINGER" | HALF_TURN_STAIR | 1 occurrence | property sets: Pset_StairCommon, Pset_StairFlightCommon
  IFCSTAIRTYPE "Cast-In-Place Stair:Monolithic Stair" | HALF_TURN_STAIR | 1 occurrence | property sets: Pset_StairCommon, Pset_StairFlightCommon
  IFCSTAIRTYPE "Precast Stair:Precast Stair" | HALF_TURN_STAIR | 1 occurrence | property sets: Pset_StairCommon, Pset_StairFlightCommon
  IFCFURNITURETYPE "Conference Table1:mid" | 1 occurrence | material: constituents "MaterialConstituentSet" ("_DESIGN_COLOR 2- ACCENT": "_DESIGN_COLOR 2- ACCENT", "_WOOD": "_WOOD")
  IFCFURNITURETYPE "125200 - Seating - Stool 1:125200 - Seating - Stool 1" | 1 occurrence | material: "ALUM. WINDOWS W/ INSULATED GLAZING"
  IFCCOVERINGTYPE "Compound Ceiling:ACT - 2X2" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon
  IFCBEAMTYPE "061713 - Laminated Veneer Lumber:LVL - 1 3/4" X 9 1/4"" | BEAM | 1 occurrence | material: profiles "LVL - 1 3/4" X 9 1/4"" ("LVL - 1 3/4" X 9 1/4"": "LVL(s) - SIZE T.B.D.") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "061100 - Wood Framing:2X4 - JOIST" | BEAM | 1 occurrence | material: profiles "2X4 - JOIST" ("2X4 - JOIST": "2X JOISTS - SIZE T.B.D.") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "061713 - Laminated Veneer Lumber:LVL - 1 3/4" X 11 7/8"" | BEAM | 1 occurrence | material: profiles "LVL - 1 3/4" X 11 7/8"" ("LVL - 1 3/4" X 11 7/8"": "LVL(s) - SIZE T.B.D.") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "061713 - Laminated Veneer Lumber:LVL - (2)1 3/4" X 9 1/4"" | BEAM | 1 occurrence | material: profiles "LVL - (2)1 3/4" X 9 1/4"" ("LVL - (2)1 3/4" X 9 1/4"": "LVL(s) - SIZE T.B.D.") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "061713 - Laminated Veneer Lumber:LVL - (2)1 3/4" X 11 7/8"" | BEAM | 1 occurrence | material: profiles "LVL - (2)1 3/4" X 11 7/8"" ("LVL - (2)1 3/4" X 11 7/8"": "LVL(s) - SIZE T.B.D.") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "061100 - Wood Framing:2x6 - JOIST" | BEAM | 1 occurrence | material: profiles "2x6 - JOIST" ("2x6 - JOIST": "2X JOISTS - SIZE T.B.D.") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "061100 - Wood Framing:2X8 - JOIST" | BEAM | 1 occurrence | material: profiles "2X8 - JOIST" ("2X8 - JOIST": "2X JOISTS - SIZE T.B.D.") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "061100 - Wood Framing:2x10 - BEAM" | BEAM | 1 occurrence | material: profiles "2x10 - BEAM" ("2x10 - BEAM": "(3) SISTERED 2X10s AT BEAM") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "061100 - Wood Framing:TREATED 2X10 - JOIST" | BEAM | 1 occurrence | material: profiles "TREATED 2X10 - JOIST" ("TREATED 2X10 - JOIST": "TREATED 2X JOISTS - EXT. STAIN") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "061100 - Wood Framing:2x10 - LEDGER" | BEAM | 1 occurrence | material: profiles "2x10 - LEDGER" ("2x10 - LEDGER": "TREATED 2X10 RIM JOIST") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "061100 - Wood Framing:2x10 - RIM JOIST" | BEAM | 1 occurrence | material: profiles "2x10 - RIM JOIST" ("2x10 - RIM JOIST": "TREATED 2X10 RIM JOIST") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "061100 - Wood Framing:2X12 - JOIST" | BEAM | 1 occurrence | material: profiles "2X12 - JOIST" ("2X12 - JOIST": "2X JOISTS - SIZE T.B.D.") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "061100 - Wood Framing:(2)2X8 - JOIST" | BEAM | 1 occurrence | material: profiles "(2)2X8 - JOIST" ("(2)2X8 - JOIST": "2X JOISTS - SIZE T.B.D.") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "061100 - Wood Framing:(3)2X12 - HEADER" | BEAM | 1 occurrence | material: profiles "(3)2X12 - HEADER" ("(3)2X12 - HEADER": "2X JOISTS - SIZE T.B.D.") | property sets: Pset_BeamCommon
  IFCDISTRIBUTIONELEMENTTYPE "Stacked Washer and Dryer:26"x25" - Private" | 1 occurrence | material: "STACKED WASHER/DRYER" | property sets: Pset_ElectricalDeviceCommon
  IFCBUILDINGELEMENTPROXYTYPE "Washer_Dryer_Combo:24"" | 1 occurrence | material: constituents "MaterialConstituentSet" ("Appliances": "DRYER", "Appliances": "WASHER", "Appliances": "Appliance - Door Trim", "Appliances": "Appliance - Controls", "Appliances": "Appliance - Polycarbonate", "Appliances": "Appliance - Stainless Steel") | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Washer-Top_Load:29"" | 1 occurrence | material: "Appliance - Stainless Steel" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "085000 - Windows - Sliding:_Type Name_" | 1 occurrence | material: constituents "MaterialConstituentSet" ("DOUBLE HUNG WINDOWS - BLACK EXT/INT SASH - LIMIT BOTTOM SASH TO 4" MAX OPEN": "DOUBLE HUNG WINDOWS - BLACK EXT/INT SASH - LIMIT BOTTOM SASH TO 4" MAX OPEN", "GL - INSULATED - LOW-E": "GL - INSULATED - LOW-E") | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation
  IFCWALLTYPE "Generic Models 38:Generic Models 1" | 1 occurrence | material: "2X WOOD SILL - TREATED IF ON CONCRETE" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 39:Generic Models 1" | 1 occurrence | material: "5/8" GYP. BD" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 47:Generic Models 1" | 1 occurrence | material: "ACOUSTICAL SEALANT OR FIRE SEALANT, IF RATED WALL" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 326:Generic Models 1" | 1 occurrence | material: "WALL BASE AS SCHEDULED" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 417:Generic Models 1" | 1 occurrence | material: "METAL RUNNER CHANNEL; FASTEN @ 24" O.C." | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 418:Generic Models 65" | 1 occurrence | material: "2X WOOD STUD" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 497:Generic Models 1" | 1 occurrence | material: "DOUBLE 2X WOOD TOP PLATE" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 498:Generic Models 1" | 1 occurrence | material: "2x6 STUDS 16" O.C. (R-19 BATT. INSULATION)" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 527:Generic Models 1" | 1 occurrence | material: "DOUBLE 2X WOOD TOP PLATE" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 528:Generic Models 1" | 1 occurrence | material: "ACOUSTICAL SEALANT OR FIRE SEALANT, IF RATED WALL" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 529:Generic Models 1" | 1 occurrence | material: "UNDERSIDE OF FLOOR ASSEMBLY - SEE STRUCT. DWGS" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 580:Generic Models 1" | 1 occurrence | material: "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 592:Generic Models 1" | 1 occurrence | material: "ACOUSTICAL SEALANT OR FIRE SEALANT, IF RATED WALL" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 593:Generic Models 1" | 1 occurrence | material: "ACOUSTICAL SEALANT OR FIRE SEALANT, IF RATED WALL" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 594:Generic Models 1" | 1 occurrence | material: "25 GA. RESILIENT CHANNEL - 24" O.C." | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 601:Generic Models 1" | 1 occurrence | material: "25 GA. RESILIENT CHANNEL - 24" O.C." | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 605:Generic Models 1" | 1 occurrence | material: "5/8" GYP. BD" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 606:Generic Models 1" | 1 occurrence | material: "ACOUSTICAL SEALANT OR FIRE SEALANT, IF RATED WALL" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 607:Generic Models 1" | 1 occurrence | material: "WALL BASE AS SCHEDULED" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 620:Generic Models 1" | 1 occurrence | material: "ACOUSTICAL SEALANT OR FIRE SEALANT, IF RATED WALL" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 621:Generic Models 1" | 1 occurrence | material: "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 622:Generic Models 1" | 1 occurrence | material: "ACOUSTICAL SEALANT OR FIRE SEALANT, IF RATED WALL" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 623:Generic Models 1" | 1 occurrence | material: "ACOUSTICAL SEALANT OR FIRE SEALANT, IF RATED WALL" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 625:Generic Models 1" | 1 occurrence | material: "CEILING TRACK AS SCHEDULED" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 626:Generic Models 1" | 1 occurrence | material: "CEILING AS SCHEDULED" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 627:Generic Models 1" | 1 occurrence | material: "CEILING TRACK AS SCHEDULED" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 628:Generic Models 1" | 1 occurrence | material: "CEILING AS SCHEDULED" | property sets: Pset_WallCommon
  IFCDOORTYPE "OD_DOUBLE:DOUBLE - FLUSH - 6-0 x 6-8" | DOOR | DOUBLE_DOOR_SINGLE_SWING | 1 occurrence | material: "WD" | property sets: OD_DOUBLE:DOUBLE - FLUSH - 6-0 x 6-8:2716676, OD_DOUBLE:DOUBLE - FLUSH - 6-0 x 6-8:2716676:1, Pset_DoorCommon
  IFCDOORTYPE "OD_DOUBLE:DOUBLE - LITE - MUNTINS - 6-0 x 6-8" | DOOR | DOUBLE_DOOR_SINGLE_SWING | 1 occurrence | material: constituents "MaterialConstituentSet" ("DOUBLE HUNG WINDOWS - BLACK EXT/INT SASH - LIMIT BOTTOM SASH TO 4" MAX OPEN": "DOUBLE HUNG WINDOWS - BLACK EXT/INT SASH - LIMIT BOTTOM SASH TO 4" MAX OPEN", "GL": "GL", "Panel": "WD", "Frame/Mullion": "WD") | property sets: OD_DOUBLE:DOUBLE - LITE - MUNTINS - 6-0 x 6-8:2716679, OD_DOUBLE:DOUBLE - LITE - MUNTINS - 6-0 x 6-8:2716679:1, Pset_DoorCommon
  IFCDOORTYPE "OD_SINGLE:SINGLE - FLUSH - 3-0 x 6-8" | DOOR | SINGLE_SWING_RIGHT | 1 occurrence | material: "HM" | property sets: OD_SINGLE:SINGLE - FLUSH - 3-0 x 6-8:2730756, OD_SINGLE:SINGLE - FLUSH - 3-0 x 6-8:2730756:1, Pset_DoorCommon
  IFCDOORTYPE "Door-Gliding-Andersen-A_Series-Double:_Type Name_" | DOOR | 1 occurrence | material: constituents "MaterialConstituentSet" ("DOUBLE HUNG WINDOWS - BLACK EXT/INT SASH - LIMIT BOTTOM SASH TO 4" MAX OPEN": "DOUBLE HUNG WINDOWS - BLACK EXT/INT SASH - LIMIT BOTTOM SASH TO 4" MAX OPEN", "GL - INSULATED - LOW-E": "GL - INSULATED - LOW-E", "Frame/Mullion": "DOUBLE HUNG WINDOWS - BLACK EXT/INT SASH - LIMIT BOTTOM SASH TO 4" MAX OPEN") | property sets: Door-Gliding-Andersen-A_Series-Double:_Type Name_:2741442, Door-Gliding-Andersen-A_Series-Double:_Type Name_:2741442:1, Pset_DoorCommon, Pset_ManufacturerTypeInformation
  IFCDOORTYPE "Door-Sectional_Model3502_Comcl_Amarr:_Type Name_" | DOOR | 1 occurrence | material: constituents "MaterialConstituentSet" ("<Unnamed>": "<Unnamed>", "DOUBLE HUNG WINDOWS - BLACK EXT/INT SASH - LIMIT BOTTOM SASH TO 4" MAX OPEN": "DOUBLE HUNG WINDOWS - BLACK EXT/INT SASH - LIMIT BOTTOM SASH TO 4" MAX OPEN", "GL - INSULATED - LOW-E": "GL - INSULATED - LOW-E") | property sets: Door-Sectional_Model3502_Comcl_Amarr:_Type Name_:2775875, Door-Sectional_Model3502_Comcl_Amarr:_Type Name_:2775875:1, Pset_DoorCommon, Pset_ManufacturerTypeInformation
  IFCSLABTYPE "Footing-Cylindrical:20"WX42"D" | BASESLAB | 1 occurrence | material: "CYLINDRICAL CONCRETE PIER - 20"Øx4'-0" - (4) # 4 VERTICALS - (3) #3 TIES @ 2" OC - REST @ 12" OC" | property sets: Pset_SlabCommon
  IFCBEAMTYPE "052119 - Open Web Steel Joist Framing - Generic:24"" | BEAM | 1 occurrence | material: profiles "24"" ("24"": "WOOD FLOOR TRUSS", "24"": "WOOD FLOOR TRUSS", "24"": "WOOD FLOOR TRUSS") | property sets: Pset_BeamCommon, Pset_ManufacturerTypeInformation, Pset_ReinforcementBarPitchOfBeam
  IFCBEAMTYPE "061753 - Shop-Fabricated Wood Trusses - Generic:WOOD TRUSSES - SIZE TBD" | BEAM | 1 occurrence | material: profiles "WOOD TRUSSES - SIZE TBD" ("WOOD TRUSSES - SIZE TBD": "WOOD FLOOR TRUSS", "WOOD TRUSSES - SIZE TBD": "WOOD FLOOR TRUSS", "WOOD TRUSSES - SIZE TBD": "WOOD FLOOR TRUSS", "WOOD TRUSSES - SIZE TBD": "WOOD FLOOR TRUSS", "WOOD TRUSSES - SIZE TBD": "WOOD FLOOR TRUSS", "WOOD TRUSSES - SIZE TBD": "WOOD FLOOR TRUSS", "WOOD TRUSSES - SIZE TBD": "WOOD FLOOR TRUSS", "WOOD TRUSSES - SIZE TBD": "WOOD FLOOR TRUSS", "WOOD TRUSSES - SIZE TBD": "WOOD FLOOR TRUSS", "WOOD TRUSSES - SIZE TBD": "WOOD FLOOR TRUSS", "WOOD TRUSSES - SIZE TBD": "WOOD FLOOR TRUSS", "WOOD TRUSSES - SIZE TBD": "WOOD FLOOR TRUSS", "WOOD TRUSSES - SIZE TBD": "WOOD FLOOR TRUSS", "WOOD TRUSSES - SIZE TBD": "WOOD FLOOR TRUSS", "WOOD TRUSSES - SIZE TBD": "WOOD FLOOR TRUSS", "WOOD TRUSSES - SIZE TBD": "WOOD FLOOR TRUSS") | property sets: Pset_BeamCommon, Pset_ManufacturerTypeInformation, Pset_ReinforcementBarPitchOfBeam
  IFCSLABTYPE "Floor:6" COMPACTED CRUSHED STONE" | FLOOR | 1 occurrence | material: layers "Floor:6" COMPACTED CRUSHED STONE" ("6" COMPACTED CRUSHED STONE" 0.5) | property sets: Pset_SlabCommon
  IFCSLABTYPE "Floor:DECKING OVER JOISTS" | FLOOR | 1 occurrence | material: layers "Floor:DECKING OVER JOISTS" ("DECKING" 0.0833333333333333, "TREATED 2X JOIST" 0.9375) | property sets: Pset_ManufacturerTypeInformation, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
  IFCSLABTYPE "Floor:STEEL DECK WITH INSULATION" | FLOOR | 1 occurrence | material: layers "Floor:STEEL DECK WITH INSULATION" ("RIGID INSULATION" 0.5, "EXISTING METAL DECK" 0.125) | property sets: Pset_SlabCommon
  IFCFURNITURETYPE "125819 - Dining Tables and Chairs - Table - Rectangular:24X24" | 1 occurrence | material: constituents "MaterialConstituentSet" ("MET": "MET", "Sals Wood": "Sals Wood") | property sets: Pset_ManufacturerTypeInformation
  IFCFURNITURETYPE "125819 - Dining Tables and Chairs - Chair - Deja:Type 1" | 15 occurrences | material: "STAINLESS STEEL - EQUIP." | property sets: Pset_ManufacturerTypeInformation
  IFCFURNITURETYPE "125900 - Systems Furniture - Workstation - L-shaped - Generic:U-SHAPED" | 1 occurrence | material: constituents "MaterialConstituentSet" ("Herman Miller - Seat": "Herman Miller - Finish SCN Satin Carbon", "Herman Miller - Seat": "Herman Miller - Finish DCR Dark Carbon", "Herman Miller - Seat": "Herman Miller - Finish CRB Carbon", "Herman Miller - Seat": "Herman Miller - Finish BK Black", "Herman Miller - Seat": "_DESIGN_FABRIC", "<Unnamed>": "<Unnamed>")
  IFCDISTRIBUTIONELEMENTTYPE "224000 - Plumbing Fixtures - Water Closet - Generic:NON_ADA" | 1 occurrence | material: constituents "MaterialConstituentSet" ("FLOOR MOUNTED TOILET": "FLOOR MOUNTED TOILET", "<Unnamed>": "<Unnamed>")
  IFCFURNITURETYPE "Couch_-_Soft_Bench_Berto_Salotti_9473:Couch_-_Soft_Bench_Berto_Salotti_9473" | 1 occurrence | material: "CASEWORK"
  IFCDISTRIBUTIONELEMENTTYPE "TUB:1" | 1 occurrence | material: "TUB" | property sets: Pset_ManufacturerTypeInformation
  IFCCURTAINWALLTYPE "Curtain Wall:STOREFRONT - BUTT-GLAZED" | 3 occurrences | property sets: Pset_CurtainWallCommon
  IFCWALLTYPE "Walls 11:Walls 11" | 1 occurrence | material: "ALUM. STOREFRONT W/ TEMPERED INSULATED GLAZING" | property sets: Pset_WallCommon
  IFCWALLTYPE "Basic Wall:EXT WALL - (HORZ. SIDING - 1/2 SHEATHING - 2X4 WOOD(BATT) - 5/8 GYP)" | STANDARD | 1 occurrence | material: layers "Basic Wall:EXT WALL - (HORZ. SIDING - 1/2 SHEATHING - 2X4 WOOD(BATT) - 5/8 GYP)" ("SIDING - HORIZONTAL" 0.0416666666666667, "DRAINAGE WRAP (ASTM E2273) OVER 1/2" CDX SHEATHING" 0.0416666666666667, "2x6 STUDS 16" O.C. (R-19 BATT. INSULATION)" 0.291666666666667, "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" 0.0520833333333333) | property sets: Pset_WallCommon
  IFCWALLTYPE "Basic Wall:EXT WALL - (HORZ. SIDING - 1/2 SHEATHING - 2X6 WOOD(BATT) - 5/8 GYP)" | STANDARD | 1 occurrence | material: layers "Basic Wall:EXT WALL - (HORZ. SIDING - 1/2 SHEATHING - 2X6 WOOD(BATT) - 5/8 GYP)" ("SIDING - HORIZONTAL" 0.0416666666666667, "DRAINAGE WRAP (ASTM E2273) OVER 1/2" CDX SHEATHING" 0.0416666666666667, "2x6 STUDS 16" O.C. (R-19 BATT. INSULATION)" 0.458333333333333, "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" 0.0520833333333333) | property sets: Pset_WallCommon
  IFCFURNITURETYPE "Vanity_Single_Sink_3860:25" Deep" | 1 occurrence | material: "CASEWORK"
  IFCDISTRIBUTIONELEMENTTYPE "Sink_Vanity_Round:19" x 19"" | 2 occurrences | material: "SINK"
  IFCDISTRIBUTIONELEMENTTYPE "Sink Kitchen-Single:30" x 21"" | 1 occurrence | material: "SINK"
  IFCDISTRIBUTIONELEMENTTYPE "Sink Kitchen-Double:42" x 21"" | 1 occurrence | material: "SINK"
  IFCWALLTYPE "Basic Wall:EXT WALL - (BRICK - 1/2 SHEATHING - 2X4WOOD(BATT) - 5/8 GYP)" | STANDARD | 1 occurrence | material: layers "Basic Wall:EXT WALL - (BRICK - 1/2 SHEATHING - 2X4WOOD(BATT) - 5/8 GYP)" ("BRICK - MODULAR - 3 1/2 x 2 1/4 x 7 1/2 - (4 x 2 2/3 x 8)" 0.291666666666667, "AIR GAP" 0.0729166666666667, "DRAINAGE WRAP (ASTM E2273) OVER 1/2" CDX SHEATHING" 0.0416666666666667, "2x6 STUDS 16" O.C. (R-19 BATT. INSULATION)" 0.291666666666667, "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" 0.0520833333333333) | property sets: Pset_WallCommon
  IFCWALLTYPE "Basic Wall:GENERIC 1"" | STANDARD | 1 occurrence | material: layers "Basic Wall:GENERIC 1"" ("GENERIC POCHE" 0.0833333333333333) | property sets: Pset_WallCommon
  IFCWALLTYPE "Basic Wall:GENERIC 2"" | STANDARD | 1 occurrence | material: layers "Basic Wall:GENERIC 2"" ("GENERIC POCHE" 0.166666666666667) | property sets: Pset_WallCommon
  IFCWALLTYPE "Basic Wall:GENERIC 3"" | STANDARD | 1 occurrence | material: layers "Basic Wall:GENERIC 3"" ("GENERIC POCHE" 0.25) | property sets: Pset_WallCommon
  IFCWALLTYPE "Basic Wall:GENERIC 4"" | STANDARD | 1 occurrence | material: layers "Basic Wall:GENERIC 4"" ("GENERIC POCHE" 0.333333333333333) | property sets: Pset_WallCommon
  IFCWALLTYPE "Basic Wall:GENERIC 5"" | STANDARD | 2 occurrences | material: layers "Basic Wall:GENERIC 5"" ("GENERIC POCHE" 0.416666666666667) | property sets: Pset_WallCommon
  IFCWALLTYPE "Basic Wall:GENERIC 6"" | STANDARD | 1 occurrence | material: layers "Basic Wall:GENERIC 6"" ("GENERIC POCHE" 0.5) | property sets: Pset_WallCommon
  IFCWALLTYPE "Basic Wall:GENERIC 8"" | STANDARD | 1 occurrence | material: layers "Basic Wall:GENERIC 8"" ("GENERIC POCHE" 0.666666666666667) | property sets: Pset_WallCommon
  IFCBUILDINGELEMENTPROXYTYPE "086200 - Unit Skylights - Rectangular:_Type Name_" | 1 occurrence | material: constituents "MaterialConstituentSet" ("Aluminum - Lacquered - Kynar 500 top finish - Neutral Gray": "Aluminum - Lacquered - Kynar 500 top finish - Neutral Gray", "NO SKYLIGHTS": "NO SKYLIGHTS", "NEW SKYLIGHTS TO MATCH EXISTING": "NEW SKYLIGHTS TO MATCH EXISTING", "Steel - Anti-corrosive coating": "Steel - Anti-corrosive coating") | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation
  IFCSLABTYPE "Footing-Rectangular:1" | BASESLAB | 1 occurrence | material: "CYLINDRICAL CONCRETE PIER - 20"Øx4'-0" - (4) # 4 VERTICALS - (3) #3 TIES @ 2" OC - REST @ 12" OC" | property sets: Pset_SlabCommon
  IFCDOORTYPE "Door-Gliding-Andersen-A_Series-Triple:_Type Name_" | DOOR | 1 occurrence | material: constituents "MaterialConstituentSet" ("DOUBLE HUNG WINDOWS - BLACK EXT/INT SASH - LIMIT BOTTOM SASH TO 4" MAX OPEN": "DOUBLE HUNG WINDOWS - BLACK EXT/INT SASH - LIMIT BOTTOM SASH TO 4" MAX OPEN", "Frame/Mullion": "DOUBLE HUNG WINDOWS - BLACK EXT/INT SASH - LIMIT BOTTOM SASH TO 4" MAX OPEN", "<Unnamed>": "<Unnamed>", "Frame/Mullion": "<Unnamed>", "GL - INSULATED - LOW-E": "GL - INSULATED - LOW-E") | property sets: Door-Gliding-Andersen-A_Series-Triple:_Type Name_:3006176, Door-Gliding-Andersen-A_Series-Triple:_Type Name_:3006176:1, Pset_DoorCommon, Pset_ManufacturerTypeInformation
  IFCBUILDINGELEMENTPROXYTYPE "FLAT SCREEN TV:FLAT SCREEN TV" | 1 occurrence | material: constituents "MaterialConstituentSet" ("JVC LCD TV - Back Panel": "JVC LCD TV - Back Panel", "JVC LCD TV - Screen": "JVC LCD TV - Screen", "JVC LCD TV - LOGO": "JVC LCD TV - LOGO") | property sets: Pset_BuildingElementProxyCommon
  IFCSLABTYPE "Floor:FLOOR TRUSS" | FLOOR | 1 occurrence | material: layers "Floor:FLOOR TRUSS" ("HARDWOOD FLOOR" 0.0625, "3/4" GYP. CRETE TOPPING" 0.0625, "1/8" SOUND MAT" 0.0104166666666667, "3/4" CDX/OSB PLYWOOD - SEE STRUCT DWGS" 0.0625, "WOOD TRUSS FLOOR ASSEMBLY - (FILL CAVITY W/ CELLULOSE BLOWN-IN INSULATION) (UL - L521 FLOOR ASSEMBLY)" 1.5, "25 GA. RESILIENT CHANNEL - 24" O.C." 0.0416666666666667, "5/8" GYP. BD @ CEILING" 0.0520833333333333) | property sets: Pset_ManufacturerTypeInformation, Pset_SlabCommon
  IFCSLABTYPE "Floor:CONCRETE SLAB - COMPACTED GRAVEL" | FLOOR | 1 occurrence | material: layers "Floor:CONCRETE SLAB - COMPACTED GRAVEL" ("CONCRETE GRADE BEAM POURED WITH CONCRETE SLAB - SEE STRUCT DWGS" 0.333333333333333, "10 MIL VAPOR BARRIER OVER 4" COMPACTED GRAVEL" 0.333333333333333) | property sets: Pset_SlabCommon
  IFCSLABTYPE "Floor:TJIs" | FLOOR | 1 occurrence | material: layers "Floor:TJIs" ("HARDWOOD FLOORING" 0.0520833333333333, "1 1/2" GYP. CRETE TOPPING" 0.125, "3/4" CDX PLYWOOD" 0.0625, "TJI JOISTS (R30 INSULATION)" 0.989583333333333, "5/8" GYP. BD" 0.0520833333333333) | property sets: Pset_SlabCommon
  IFCCURTAINWALLTYPE "Sloped Glazing:Sloped Glazing" | 1 occurrence | property sets: Pset_CurtainWallCommon
  IFCCOVERINGTYPE "Compound Ceiling:ACT - 2X2" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon
  IFCCOVERINGTYPE "Compound Ceiling:ACT - 2X2 - DEMO" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon
  IFCCOVERINGTYPE "Compound Ceiling:GYP. BD - HUNG" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon
  IFCCOVERINGTYPE "Compound Ceiling:ACT - 1X4" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon
  IFCCOVERINGTYPE "Compound Ceiling:GYP. BD - CEILING JOIST" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon
  IFCCOVERINGTYPE "Compound Ceiling:SOFFIT" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon
  IFCBUILDINGELEMENTPROXYTYPE "GAS GRILL:one" | 5 occurrences | material: constituents "MaterialConstituentSet" ("Danver Stainless Steel Lt-Rt": "Danver Stainless Steel Lt-Rt", "Stainless Steel, Brushed": "Stainless Steel, Brushed", "Wolf Outdoor - Glass, Cast, Gray": "Wolf Outdoor - Glass, Cast, Gray", "Steel, Polished": "Steel, Polished", "Danver Chrome Plated": "Danver Chrome Plated", "Danver Stainless Steel Up-Dn": "Danver Stainless Steel Up-Dn", "Plastic, Opaque Black": "Plastic, Opaque Black", "Danver Toe Kick": "Danver Toe Kick") | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation
  IFCBUILDINGELEMENTPROXYTYPE "Enscape AssetDefinition - Feather Reed Grass:Enscape AssetDefinition - Feather Reed Grass" | 78 occurrences | material: "<Unnamed>" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Enscape AssetDefinition - Feather Reed Grass 02:Enscape AssetDefinition - Feather Reed Grass 02" | 73 occurrences | material: "<Unnamed>" | property sets: Pset_BuildingElementProxyCommon
  IFCCURTAINWALLTYPE "Curtain Wall:posts only" | 2 occurrences | property sets: Pset_CurtainWallCommon
  IFCWALLTYPE "Basic Wall:EXT 1 - 1st floor base" | STANDARD | 37 occurrences | material: layers "Basic Wall:EXT 1 - 1st floor base" ("FIBER CEMENT - LAP SIDING - COLOR (LIGHT MIST)" 0.0416666666666667, "DRAINAGE WRAP (ASTM E2273) OVER 1/2" CDX SHEATHING" 0.0416666666666667, "2x6 STUDS 16" O.C. (R-19 BATT. INSULATION)" 0.458333333333333, "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" 0.0520833333333333) | property sets: Pset_WallCommon
  IFCBUILDINGELEMENTPROXYTYPE "Specialty Equipment 1:Specialty Equipment 1" | 1 occurrence | material: "MAILBOXES" | property sets: Pset_BuildingElementProxyCommon
  IFCFURNITURETYPE "125819 - Dining Tables and Chairs - Table - Rectangular:1" | 7 occurrences | material: constituents "MaterialConstituentSet" ("MET": "MET", "BASE CABINETS": "BASE CABINETS") | property sets: Pset_ManufacturerTypeInformation
  IFCFURNITURETYPE "125819 - Dining Tables and Chairs - Chair - Deja:Type 1" | 14 occurrences | material: "STAINLESS STEEL - EQUIP." | property sets: Pset_ManufacturerTypeInformation
  IFCFURNITURETYPE "Seating-Setee-Teknion-BBMC_Metropolitan-R1:Lounge Settee 2" | 5 occurrences | material: constituents "MaterialConstituentSet" ("Seat": "_DESIGN_FABRIC", "Frame": "Metal - Teknion - C6 - Chrome", "Frame": "Plastic - Teknion - Z1 - Greystone") | property sets: Pset_ManufacturerTypeInformation
  IFCFURNITURETYPE "Table-Coffee-Teknion-STRTC_Cover-R1:38,25" w x 27,5" d x 15" h 2" | 6 occurrences | material: constituents "MaterialConstituentSet" ("Furniture": "STEEL STRUCTURE (HOT DIPPED GALV.)", "Furniture": "BASE CABINETS") | property sets: Pset_ManufacturerTypeInformation
  IFCFURNITURETYPE "Seating-Lounge_Chair-Teknion-BBMC_Metropolitan-R1:Lounge Chair" | 6 occurrences | material: constituents "MaterialConstituentSet" ("Seat": "_DESIGN_FABRIC", "Frame": "<Unnamed>", "Frame": "Metal - Teknion - C6 - Chrome") | property sets: Pset_ManufacturerTypeInformation
  IFCCURTAINWALLTYPE "Curtain Wall:SLOTTED WOOD FENCE" | 14 occurrences | property sets: Pset_CurtainWallCommon
  IFCBUILDINGELEMENTPROXYTYPE "Model Text:signage" | 1 occurrence | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Enscape AssetDefinition - Allen Sitting:Enscape AssetDefinition - Allen Sitting" | 4 occurrences | material: "<Unnamed>" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Enscape AssetDefinition - Annouk and Maud, Standing 03:Enscape AssetDefinition - Annouk and Maud, Standing 03" | 1 occurrence | material: "<Unnamed>" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Enscape AssetDefinition - Asya Sitting:Enscape AssetDefinition - Asya Sitting" | 4 occurrences | material: "<Unnamed>" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Enscape AssetDefinition - Bao, Standing 03:Enscape AssetDefinition - Bao, Standing 03" | 1 occurrence | material: "<Unnamed>" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Enscape AssetDefinition - Connor and Isabella, Standing 02:Enscape AssetDefinition - Connor and Isabella, Standing 02" | 4 occurrences | material: "<Unnamed>" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Enscape AssetDefinition - Elena, Standing 02:Enscape AssetDefinition - Elena, Standing 02" | 3 occurrences | material: "<Unnamed>" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Enscape AssetDefinition - Francine, Sitting:Enscape AssetDefinition - Francine, Sitting" | 1 occurrence | material: "<Unnamed>" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Enscape AssetDefinition - Juliette, Standing 02:Enscape AssetDefinition - Juliette, Standing 02" | 3 occurrences | material: "<Unnamed>" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Enscape AssetDefinition - Leon Sitting:Enscape AssetDefinition - Leon Sitting" | 1 occurrence | material: "<Unnamed>" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Enscape AssetDefinition - Maarten, Standing:Enscape AssetDefinition - Maarten, Standing" | 1 occurrence | material: "<Unnamed>" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Enscape AssetDefinition - Daud, Sitting:Enscape AssetDefinition - Daud, Sitting" | 5 occurrences | material: "<Unnamed>" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Enscape AssetDefinition - Francine, Walking 03:Enscape AssetDefinition - Francine, Walking 03" | 4 occurrences | material: "<Unnamed>" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Enscape AssetDefinition - Maja Sitting:Enscape AssetDefinition - Maja Sitting" | 4 occurrences | material: "<Unnamed>" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Enscape AssetDefinition - Sheona, Sitting:Enscape AssetDefinition - Sheona, Sitting" | 1 occurrence | material: "<Unnamed>" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Enscape AssetDefinition - Karen Sitting 1:Enscape AssetDefinition - Karen Sitting 1" | 1 occurrence | material: "<Unnamed>" | property sets: Pset_BuildingElementProxyCommon
  IFCCURTAINWALLTYPE "Curtain Wall:SLOTTED WOOD FENCE - at concrete walls" | 1 occurrence | property sets: Pset_CurtainWallCommon
  IFCCURTAINWALLTYPE "Curtain Wall:HORSE 3" | 33 occurrences | property sets: Pset_CurtainWallCommon
  IFCWALLTYPE "Basic Wall:EXT 1 - 1st floor base - 1HR" | STANDARD | 3 occurrences | material: layers "Basic Wall:EXT 1 - 1st floor base - 1HR" ("FIBER CEMENT - LAP SIDING - COLOR (LIGHT MIST)" 0.0416666666666667, "BUILDING WRAP (ASTM 2273) OVER FIBERGLASS MAT GYPSUM SHEATHING" 0.0416666666666667, "2x6 STUDS 16" O.C. (R-19 BATT. INSULATION)" 0.458333333333333, "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" 0.0520833333333333) | property sets: Pset_WallCommon
  IFCBUILDINGELEMENTPROXYTYPE "4023629" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4023630" | 1 occurrence
  IFCWALLTYPE "Basic Wall:EXT 2 - corrugated metal - 1HR" | STANDARD | 3 occurrences | material: layers "Basic Wall:EXT 2 - corrugated metal - 1HR" ("RIBBED PBD METAL PANEL W/ EXPOSED FASTENERS - COLOR (CHARCOAL GRAY)" 0.0729166666666667, "BUILDING WRAP (ASTM 2273) OVER FIBERGLASS MAT GYPSUM SHEATHING" 0.0520833333333333, "2x6 STUDS 16" O.C. (R-19 BATT. INSULATION)" 0.458333333333333, "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" 0.0520833333333333) | property sets: Pset_WallCommon
  IFCBUILDINGELEMENTPROXYTYPE "4023632" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4023643" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4023670" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4023675" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4023696" | 1 occurrence
  IFCWALLTYPE "Basic Wall:EXT 2 - corrugated metal" | STANDARD | 57 occurrences | material: layers "Basic Wall:EXT 2 - corrugated metal" ("RIBBED PBD METAL PANEL W/ EXPOSED FASTENERS - COLOR (CHARCOAL GRAY)" 0.0729166666666667, "DRAINAGE WRAP (ASTM E2273) OVER 1/2" CDX SHEATHING" 0.0416666666666667, "2x6 STUDS 16" O.C. (R-19 BATT. INSULATION)" 0.458333333333333, "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" 0.0520833333333333) | property sets: Pset_WallCommon
  IFCBUILDINGELEMENTPROXYTYPE "4023709" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4027698" | 1 occurrence
  IFCWALLTYPE "Basic Wall:EXT 3 - composite" | STANDARD | 8 occurrences | material: layers "Basic Wall:EXT 3 - composite" ("FIBER CEMENT - LAP SIDING - COLOR (GOLDEN LEAVES)" 0.0416666666666667, "DRAINAGE WRAP (ASTM E2273) OVER 1/2" CDX SHEATHING" 0.0416666666666667, "2x6 STUDS 16" O.C. (R-19 BATT. INSULATION)" 0.458333333333333, "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" 0.0520833333333333) | property sets: Pset_WallCommon
  IFCBUILDINGELEMENTPROXYTYPE "4028387" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4028395" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4031137" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4031145" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4031232" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4031240" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4031378" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4031386" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4031532" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4031540" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4032573" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4032581" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4032590" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4032598" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4032607" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4032615" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4032624" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4032632" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4032651" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4032659" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4032668" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4032676" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4032685" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4032693" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4032702" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4032710" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4032822" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4032830" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4032839" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4032847" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4032856" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4032864" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4032873" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4032881" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4033374" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4033926" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4033940" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4033968" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4034436" | 1 occurrence
  IFCWALLTYPE "Basic Wall:EXT 1 - 1st floor base - shear" | STANDARD | 4 occurrences | material: layers "Basic Wall:EXT 1 - 1st floor base - shear" ("FIBER CEMENT - LAP SIDING - COLOR (LIGHT MIST)" 0.0416666666666667, "DRAINAGE WRAP (ASTM E2273) OVER 1/2" CDX SHEATHING" 0.0416666666666667, "2x6 STUDS 16" O.C. (R-19 BATT. INSULATION)" 0.458333333333333, "WOOD STRUCTURAL PANEL (WSP) - SEE STRUCT DWGS" 0.0416666666666667, "5/8" GYP. BD" 0.0520833333333333) | property sets: Pset_WallCommon
  IFCWALLTYPE "Basic Wall:EXT 2 - corrugated metal - shear" | STANDARD | 4 occurrences | material: layers "Basic Wall:EXT 2 - corrugated metal - shear" ("RIBBED PBD METAL PANEL W/ EXPOSED FASTENERS - COLOR (CHARCOAL GRAY)" 0.0729166666666667, "DRAINAGE WRAP (ASTM E2273) OVER 1/2" CDX SHEATHING" 0.0416666666666667, "2x6 STUDS 16" O.C. (R-19 BATT. INSULATION)" 0.458333333333333, "WOOD STRUCTURAL PANEL (WSP) - SEE STRUCT DWGS" 0.0416666666666667, "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" 0.0520833333333333) | property sets: Pset_WallCommon
  IFCBUILDINGELEMENTPROXYTYPE "4034920" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4035043" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4035378" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4035405" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4035413" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4035430" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4035584" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4035595" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4035718" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4035729" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "085000 - Windows - Double Hung:SINGLE HUNG - TYPE 1 - TEMPERED" | 1 occurrence | material: constituents "MaterialConstituentSet" ("DOUBLE HUNG WINDOWS - BLACK EXT/INT SASH - LIMIT BOTTOM SASH TO 4" MAX OPEN": "DOUBLE HUNG WINDOWS - BLACK EXT/INT SASH - LIMIT BOTTOM SASH TO 4" MAX OPEN", "WINDOW SASH/TRIM": "WINDOW SASH/TRIM", "GL - INSULATED - LOW-E": "GL - INSULATED - LOW-E") | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation
  IFCBUILDINGELEMENTPROXYTYPE "085000 - Windows - Double Hung:SINGLE HUNG - TYPE 2 - TEMPERED" | 1 occurrence | material: constituents "MaterialConstituentSet" ("DOUBLE HUNG WINDOWS - BLACK EXT/INT SASH - LIMIT BOTTOM SASH TO 4" MAX OPEN": "DOUBLE HUNG WINDOWS - BLACK EXT/INT SASH - LIMIT BOTTOM SASH TO 4" MAX OPEN", "WINDOW SASH/TRIM": "WINDOW SASH/TRIM", "GL - INSULATED - LOW-E": "GL - INSULATED - LOW-E") | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation
  IFCBUILDINGELEMENTPROXYTYPE "085000 - Windows - Double Hung:SINGLE HUNG - TYPE 2 - TEMPERED" | 3 occurrences | material: constituents "MaterialConstituentSet" ("DOUBLE HUNG WINDOWS - BLACK EXT/INT SASH - LIMIT BOTTOM SASH TO 4" MAX OPEN": "DOUBLE HUNG WINDOWS - BLACK EXT/INT SASH - LIMIT BOTTOM SASH TO 4" MAX OPEN", "WINDOW SASH/TRIM": "WINDOW SASH/TRIM", "GL - INSULATED - LOW-E": "GL - INSULATED - LOW-E") | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation
  IFCBUILDINGELEMENTPROXYTYPE "085000 - Windows - Double Hung:SINGLE HUNG - TYPE 1" | 2 occurrences | material: constituents "MaterialConstituentSet" ("DOUBLE HUNG WINDOWS - BLACK EXT/INT SASH - LIMIT BOTTOM SASH TO 4" MAX OPEN": "DOUBLE HUNG WINDOWS - BLACK EXT/INT SASH - LIMIT BOTTOM SASH TO 4" MAX OPEN", "WINDOW SASH/TRIM": "WINDOW SASH/TRIM", "GL - INSULATED - LOW-E": "GL - INSULATED - LOW-E") | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation
  IFCBUILDINGELEMENTPROXYTYPE "085000 - Windows - Double Hung:SINGLE HUNG - TYPE 2 - TEMPERED" | 1 occurrence | material: constituents "MaterialConstituentSet" ("DOUBLE HUNG WINDOWS - BLACK EXT/INT SASH - LIMIT BOTTOM SASH TO 4" MAX OPEN": "DOUBLE HUNG WINDOWS - BLACK EXT/INT SASH - LIMIT BOTTOM SASH TO 4" MAX OPEN", "WINDOW SASH/TRIM": "WINDOW SASH/TRIM", "GL - INSULATED - LOW-E": "GL - INSULATED - LOW-E") | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation
  IFCBUILDINGELEMENTPROXYTYPE "085000 - Windows - Double Hung:SINGLE HUNG - TYPE 2" | 1 occurrence | material: constituents "MaterialConstituentSet" ("DOUBLE HUNG WINDOWS - BLACK EXT/INT SASH - LIMIT BOTTOM SASH TO 4" MAX OPEN": "DOUBLE HUNG WINDOWS - BLACK EXT/INT SASH - LIMIT BOTTOM SASH TO 4" MAX OPEN", "WINDOW SASH/TRIM": "WINDOW SASH/TRIM", "GL - INSULATED - LOW-E": "GL - INSULATED - LOW-E") | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation
  IFCBUILDINGELEMENTPROXYTYPE "085000 - Windows - Double Hung:SINGLE HUNG - TYPE 2 - TEMPERED" | 1 occurrence | material: constituents "MaterialConstituentSet" ("DOUBLE HUNG WINDOWS - BLACK EXT/INT SASH - LIMIT BOTTOM SASH TO 4" MAX OPEN": "DOUBLE HUNG WINDOWS - BLACK EXT/INT SASH - LIMIT BOTTOM SASH TO 4" MAX OPEN", "WINDOW SASH/TRIM": "WINDOW SASH/TRIM", "GL - INSULATED - LOW-E": "GL - INSULATED - LOW-E") | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation
  IFCBUILDINGELEMENTPROXYTYPE "085000 - Windows - Casement or Awning or Fixed:CASEMENT - TYPE 1" | 1 occurrence | material: constituents "MaterialConstituentSet" ("DOUBLE HUNG WINDOWS - BLACK EXT/INT SASH - LIMIT BOTTOM SASH TO 4" MAX OPEN": "DOUBLE HUNG WINDOWS - BLACK EXT/INT SASH - LIMIT BOTTOM SASH TO 4" MAX OPEN", "GL - INSULATED - LOW-E": "GL - INSULATED - LOW-E", "<Unnamed>": "<Unnamed>") | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation
  IFCBUILDINGELEMENTPROXYTYPE "085000 - Windows - Double Hung:SINGLE HUNG - TYPE 2" | 1 occurrence | material: constituents "MaterialConstituentSet" ("DOUBLE HUNG WINDOWS - BLACK EXT/INT SASH - LIMIT BOTTOM SASH TO 4" MAX OPEN": "DOUBLE HUNG WINDOWS - BLACK EXT/INT SASH - LIMIT BOTTOM SASH TO 4" MAX OPEN", "WINDOW SASH/TRIM": "WINDOW SASH/TRIM", "GL - INSULATED - LOW-E": "GL - INSULATED - LOW-E") | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation
  IFCDOORTYPE "OD_SINGLE:SINGLE - LITE - MUNTINS - 3-0 x 6-8" | DOOR | SINGLE_SWING_LEFT | 5 occurrences | material: constituents "MaterialConstituentSet" ("GL - TEMPERED - INSULATED - LOW-E": "GL - TEMPERED - INSULATED - LOW-E", "Panel": "CW - CLAD WOOD DOOR", "Frame/Mullion": "CW - CLAD WOOD DOOR") | property sets: OD_SINGLE:SINGLE - LITE - MUNTINS - 3-0 x 6-8:4055326, OD_SINGLE:SINGLE - LITE - MUNTINS - 3-0 x 6-8:4055326:1, Pset_DoorCommon
  IFCBEAMTYPE "C-Channel:C CHANNEL - SIZE TBD2" | BEAM | 1 occurrence | material: profiles "C CHANNEL - SIZE TBD2" ("C CHANNEL - SIZE TBD2": "STEEL STRUCTURE (HOT DIPPED GALV.)") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "C-Channel:C CHANNEL - SIZE TBD1" | BEAM | 1 occurrence | material: profiles "C CHANNEL - SIZE TBD1" ("C CHANNEL - SIZE TBD1": "STEEL C CHANNEL - HDG - SEE STRUCT DWGS") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "W-Wide Flange:W10X33" | BEAM | 1 occurrence | material: profiles "W10X33" ("W10X33": "Steel ASTM A992") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "W-Wide Flange:W10X49" | BEAM | 1 occurrence | material: profiles "W10X49" ("W10X49": "Steel ASTM A992") | property sets: Pset_BeamCommon
  IFCWALLTYPE "Basic Wall:PARTY WALL" | STANDARD | 2 occurrences | material: layers "Basic Wall:PARTY WALL" ("5/8" GYP. BD" 0.0520833333333333, "OSB/CDX FOR SHEAR WALL" 0.0416666666666667, "2x6 STUDS 16" O.C. (R-19 BATT. INSULATION)" 0.291666666666667, "AIR GAP" 0.0833333333333333, "2x6 STUDS 16" O.C. (R-19 BATT. INSULATION)" 0.291666666666667, "OSB/CDX FOR SHEAR WALL" 0.0416666666666667, "5/8" GYP. BD" 0.0520833333333333) | property sets: Pset_WallCommon
  IFCDISTRIBUTIONELEMENTTYPE "TUB:1" | 1 occurrence | material: "TUB" | property sets: Pset_ManufacturerTypeInformation
  IFCDISTRIBUTIONELEMENTTYPE "Shower Head:Shower Head" | 1 occurrence | material: "SHOWER HEAD"
  IFCDOORTYPE "OD_SINGLE:SINGLE - LITE - MUNTINS - 3-0 x 6-8" | DOOR | SINGLE_SWING_RIGHT | 6 occurrences | material: constituents "MaterialConstituentSet" ("GL - TEMPERED - INSULATED - LOW-E": "GL - TEMPERED - INSULATED - LOW-E", "Panel": "CW - CLAD WOOD DOOR", "Frame/Mullion": "CW - CLAD WOOD DOOR") | property sets: OD_SINGLE:SINGLE - LITE - MUNTINS - 3-0 x 6-8:4091063, OD_SINGLE:SINGLE - LITE - MUNTINS - 3-0 x 6-8:4091063:1, Pset_DoorCommon
  IFCBUILDINGELEMENTPROXYTYPE "4185249" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4185250" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4185252" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4185263" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4185285" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4185290" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4185311" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4185324" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4185330" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4185338" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4185346" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "085000 - Windows - Double Hung:SINGLE HUNG - TYPE 2" | 3 occurrences | material: constituents "MaterialConstituentSet" ("DOUBLE HUNG WINDOWS - BLACK EXT/INT SASH - LIMIT BOTTOM SASH TO 4" MAX OPEN": "DOUBLE HUNG WINDOWS - BLACK EXT/INT SASH - LIMIT BOTTOM SASH TO 4" MAX OPEN", "WINDOW SASH/TRIM": "WINDOW SASH/TRIM", "GL - INSULATED - LOW-E": "GL - INSULATED - LOW-E") | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation
  IFCBUILDINGELEMENTPROXYTYPE "085000 - Windows - Double Hung:SINGLE HUNG - TYPE 1" | 3 occurrences | material: constituents "MaterialConstituentSet" ("DOUBLE HUNG WINDOWS - BLACK EXT/INT SASH - LIMIT BOTTOM SASH TO 4" MAX OPEN": "DOUBLE HUNG WINDOWS - BLACK EXT/INT SASH - LIMIT BOTTOM SASH TO 4" MAX OPEN", "WINDOW SASH/TRIM": "WINDOW SASH/TRIM", "GL - INSULATED - LOW-E": "GL - INSULATED - LOW-E") | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation
  IFCDOORTYPE "OD_SINGLE:SINGLE - LITE - MUNTINS - 3-0 x 6-8" | DOOR | SINGLE_SWING_LEFT | 1 occurrence | material: constituents "MaterialConstituentSet" ("GL - TEMPERED - INSULATED - LOW-E": "GL - TEMPERED - INSULATED - LOW-E", "Panel": "CW - CLAD WOOD DOOR", "Frame/Mullion": "CW - CLAD WOOD DOOR") | property sets: OD_SINGLE:SINGLE - LITE - MUNTINS - 3-0 x 6-8:4186740, OD_SINGLE:SINGLE - LITE - MUNTINS - 3-0 x 6-8:4186740:1, Pset_DoorCommon
  IFCBUILDINGELEMENTPROXYTYPE "085000 - Windows - Double Hung:SINGLE HUNG - TYPE 2 - TEMPERED" | 1 occurrence | material: constituents "MaterialConstituentSet" ("DOUBLE HUNG WINDOWS - BLACK EXT/INT SASH - LIMIT BOTTOM SASH TO 4" MAX OPEN": "DOUBLE HUNG WINDOWS - BLACK EXT/INT SASH - LIMIT BOTTOM SASH TO 4" MAX OPEN", "WINDOW SASH/TRIM": "WINDOW SASH/TRIM", "GL - INSULATED - LOW-E": "GL - INSULATED - LOW-E") | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation
  IFCBUILDINGELEMENTPROXYTYPE "085000 - Windows - Double Hung:SINGLE HUNG - TYPE 2" | 1 occurrence | material: constituents "MaterialConstituentSet" ("DOUBLE HUNG WINDOWS - BLACK EXT/INT SASH - LIMIT BOTTOM SASH TO 4" MAX OPEN": "DOUBLE HUNG WINDOWS - BLACK EXT/INT SASH - LIMIT BOTTOM SASH TO 4" MAX OPEN", "WINDOW SASH/TRIM": "WINDOW SASH/TRIM", "GL - INSULATED - LOW-E": "GL - INSULATED - LOW-E") | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation
  IFCBUILDINGELEMENTPROXYTYPE "085000 - Windows - Double Hung:SINGLE HUNG - TYPE 1" | 1 occurrence | material: constituents "MaterialConstituentSet" ("DOUBLE HUNG WINDOWS - BLACK EXT/INT SASH - LIMIT BOTTOM SASH TO 4" MAX OPEN": "DOUBLE HUNG WINDOWS - BLACK EXT/INT SASH - LIMIT BOTTOM SASH TO 4" MAX OPEN", "WINDOW SASH/TRIM": "WINDOW SASH/TRIM", "GL - INSULATED - LOW-E": "GL - INSULATED - LOW-E") | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation
  IFCBUILDINGELEMENTPROXYTYPE "085000 - Windows - Double Hung:SINGLE HUNG - TYPE 2" | 1 occurrence | material: constituents "MaterialConstituentSet" ("DOUBLE HUNG WINDOWS - BLACK EXT/INT SASH - LIMIT BOTTOM SASH TO 4" MAX OPEN": "DOUBLE HUNG WINDOWS - BLACK EXT/INT SASH - LIMIT BOTTOM SASH TO 4" MAX OPEN", "WINDOW SASH/TRIM": "WINDOW SASH/TRIM", "GL - INSULATED - LOW-E": "GL - INSULATED - LOW-E") | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation
  IFCBUILDINGELEMENTPROXYTYPE "085000 - Windows - Casement or Awning or Fixed:FIXED PICTURE - TYPE 1" | 1 occurrence | material: constituents "MaterialConstituentSet" ("DOUBLE HUNG WINDOWS - BLACK EXT/INT SASH - LIMIT BOTTOM SASH TO 4" MAX OPEN": "DOUBLE HUNG WINDOWS - BLACK EXT/INT SASH - LIMIT BOTTOM SASH TO 4" MAX OPEN", "GL - INSULATED - LOW-E": "GL - INSULATED - LOW-E", "<Unnamed>": "<Unnamed>") | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation
  IFCBUILDINGELEMENTPROXYTYPE "085000 - Windows - Casement or Awning or Fixed:FIXED PICTURE - TYPE 1" | 3 occurrences | material: constituents "MaterialConstituentSet" ("DOUBLE HUNG WINDOWS - BLACK EXT/INT SASH - LIMIT BOTTOM SASH TO 4" MAX OPEN": "DOUBLE HUNG WINDOWS - BLACK EXT/INT SASH - LIMIT BOTTOM SASH TO 4" MAX OPEN", "GL - INSULATED - LOW-E": "GL - INSULATED - LOW-E", "<Unnamed>": "<Unnamed>") | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation
  IFCWALLTYPE "Basic Wall:SHEAR - W4H5D - (5/8 GYP - 1/2 WSP - 2X4 WOOD(BATT))" | STANDARD | 14 occurrences | material: layers "Basic Wall:SHEAR - W4H5D - (5/8 GYP - 1/2 WSP - 2X4 WOOD(BATT))" ("AIR GAP" 0.0416666666666667, "2x4 STUDS (1ST FL @ 8" O.C. • 2ND FL @ 12" O.C. • 3RD FL @ 16" O.C.) - BATT. INSULATION AT STUD CAVITY" 0.291666666666667, "WOOD STRUCTURAL PANEL (WSP) - SEE STRUCT DWGS" 0.0416666666666667, "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" 0.0520833333333333) | property sets: Pset_WallCommon
  IFCCURTAINWALLTYPE "Curtain Wall:sloped slats" | 4 occurrences | property sets: Pset_CurtainWallCommon
  IFCBUILDINGELEMENTPROXYTYPE "4391991" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4391992" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4391993" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4394853" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4394878" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4394896" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4394897" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4394898" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4394899" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4394900" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4394901" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4394902" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4394903" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4394904" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4395204" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4395214" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4395992" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4396002" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4396727" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4396728" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4396729" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4396730" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4396731" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4396741" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4396742" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4396743" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4396744" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4396745" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4396748" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4396749" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4396750" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4396751" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4396752" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4396762" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4396763" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4396764" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4396765" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4396766" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4397214" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4397215" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4397246" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4397247" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4397253" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4397254" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4397266" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4397267" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4397269" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4397270" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4398173" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4398174" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4398213" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4398214" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4398220" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4398221" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4398237" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4398238" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4398240" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4398241" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4402231" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4402236" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4405731" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4405732" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4408312" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4408345" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4408347" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4408349" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4408355" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4408357" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4409467" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4409481" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4410306" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4410308" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4410310" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4410312" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4410328" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4410330" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4410332" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4410334" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4410339" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4410341" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4410343" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4410345" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4410361" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4410363" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4410365" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4410367" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4421542" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4421543" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4421918" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4421927" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4423085" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4423093" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4423097" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4423105" | 1 occurrence
  IFCWALLTYPE "Basic Wall:shaft" | STANDARD | 36 occurrences | material: layers "Basic Wall:shaft" ("16 GA. PERFORATED GALV. STEEL PANEL" 0.0104166666666667, "METAL STUD - GALV. - 16" O.C." 0.166666666666667) | property sets: Pset_WallCommon
  IFCBUILDINGELEMENTPROXYTYPE "Indoor Unit - Evaporator - Air_Conditioner-Single_Zone-Indoor-Daikin-FTKN_NMVJU:Indoor Unit - Evaporator - 1.5Ton_FTKN18NMVJU" | 6 occurrences | material: constituents "MaterialConstituentSet" ("Metal - Daikin - Galvanized Steel": "Metal - Daikin - Galvanized Steel", "Metal - Daikin - Copper": "Metal - Daikin - Copper") | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation
  IFCBUILDINGELEMENTPROXYTYPE "Indoor Unit - Evaporator - Air_Conditioner-Single_Zone-Indoor-Daikin-FTKN_NMVJU:Indoor Unit - Evaporator - 1.5Ton_FTKN18NMVJU" | 3 occurrences | material: constituents "MaterialConstituentSet" ("Metal - Daikin - Galvanized Steel": "Metal - Daikin - Galvanized Steel", "Metal - Daikin - Copper": "Metal - Daikin - Copper") | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation
  IFCBUILDINGELEMENTPROXYTYPE "4452182" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4452183" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4453829" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4453834" | 1 occurrence
  IFCDOORTYPE "OD_SINGLE:SINGLE - HOLLOW METAL - 3-0 x 6-8" | DOOR | SINGLE_SWING_RIGHT | 1 occurrence | material: "HM" | property sets: OD_SINGLE:SINGLE - HOLLOW METAL - 3-0 x 6-8:4469730, OD_SINGLE:SINGLE - HOLLOW METAL - 3-0 x 6-8:4469730:1, Pset_DoorCommon
  IFCBUILDINGELEMENTPROXYTYPE "4475657" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4475658" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4537968" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4537969" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4538111" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4538112" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "085000 - Windows - Casement or Awning or Fixed:FIXED PICTURE - TYPE 2" | 1 occurrence | material: constituents "MaterialConstituentSet" ("DOUBLE HUNG WINDOWS - BLACK EXT/INT SASH - LIMIT BOTTOM SASH TO 4" MAX OPEN": "DOUBLE HUNG WINDOWS - BLACK EXT/INT SASH - LIMIT BOTTOM SASH TO 4" MAX OPEN", "GL - INSULATED - LOW-E": "GL - INSULATED - LOW-E", "<Unnamed>": "<Unnamed>") | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation
  IFCBUILDINGELEMENTPROXYTYPE "085000 - Windows - Double Hung:SINGLE HUNG - TYPE 1" | 1 occurrence | material: constituents "MaterialConstituentSet" ("DOUBLE HUNG WINDOWS - BLACK EXT/INT SASH - LIMIT BOTTOM SASH TO 4" MAX OPEN": "DOUBLE HUNG WINDOWS - BLACK EXT/INT SASH - LIMIT BOTTOM SASH TO 4" MAX OPEN", "WINDOW SASH/TRIM": "WINDOW SASH/TRIM", "GL - INSULATED - LOW-E": "GL - INSULATED - LOW-E") | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation
  IFCBUILDINGELEMENTPROXYTYPE "085000 - Windows - Double Hung:SINGLE HUNG - TYPE 2" | 1 occurrence | material: constituents "MaterialConstituentSet" ("DOUBLE HUNG WINDOWS - BLACK EXT/INT SASH - LIMIT BOTTOM SASH TO 4" MAX OPEN": "DOUBLE HUNG WINDOWS - BLACK EXT/INT SASH - LIMIT BOTTOM SASH TO 4" MAX OPEN", "WINDOW SASH/TRIM": "WINDOW SASH/TRIM", "GL - INSULATED - LOW-E": "GL - INSULATED - LOW-E") | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation
  IFCBUILDINGELEMENTPROXYTYPE "085000 - Windows - Casement or Awning or Fixed:FIXED PICTURE - TYPE 1" | 1 occurrence | material: constituents "MaterialConstituentSet" ("DOUBLE HUNG WINDOWS - BLACK EXT/INT SASH - LIMIT BOTTOM SASH TO 4" MAX OPEN": "DOUBLE HUNG WINDOWS - BLACK EXT/INT SASH - LIMIT BOTTOM SASH TO 4" MAX OPEN", "GL - INSULATED - LOW-E": "GL - INSULATED - LOW-E", "<Unnamed>": "<Unnamed>") | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation
  IFCBUILDINGELEMENTPROXYTYPE "085000 - Windows - Casement or Awning or Fixed:CASEMENT - TYPE 1" | 1 occurrence | material: constituents "MaterialConstituentSet" ("DOUBLE HUNG WINDOWS - BLACK EXT/INT SASH - LIMIT BOTTOM SASH TO 4" MAX OPEN": "DOUBLE HUNG WINDOWS - BLACK EXT/INT SASH - LIMIT BOTTOM SASH TO 4" MAX OPEN", "GL - INSULATED - LOW-E": "GL - INSULATED - LOW-E", "<Unnamed>": "<Unnamed>") | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation
  IFCBUILDINGELEMENTPROXYTYPE "085000 - Windows - Casement or Awning or Fixed:FIXED PICTURE - TYPE 2" | 1 occurrence | material: constituents "MaterialConstituentSet" ("DOUBLE HUNG WINDOWS - BLACK EXT/INT SASH - LIMIT BOTTOM SASH TO 4" MAX OPEN": "DOUBLE HUNG WINDOWS - BLACK EXT/INT SASH - LIMIT BOTTOM SASH TO 4" MAX OPEN", "GL - INSULATED - LOW-E": "GL - INSULATED - LOW-E", "<Unnamed>": "<Unnamed>") | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation
  IFCWALLTYPE "Basic Wall:TRASH ENCLOSURE" | STANDARD | 3 occurrences | material: layers "Basic Wall:TRASH ENCLOSURE" ("3 SIDED SCREENING FENCE" 0.0833333333333333) | property sets: Pset_WallCommon
  IFCBUILDINGELEMENTPROXYTYPE "Enscape AssetDefinition - Deciduous Tree 024 Elm:Enscape AssetDefinition - Deciduous Tree 024 Elm" | 10 occurrences | material: "<Unnamed>" | property sets: Pset_BuildingElementProxyCommon
  IFCWALLTYPE "Basic Wall:FIRE SEPERATION IN CAVITY" | STANDARD | 15 occurrences | material: layers "Basic Wall:FIRE SEPERATION IN CAVITY" ("5/8" GYP. BD" 0.0520833333333333, "LVL RIM BOARD - SEE STRUCT. DWGS" 0.0833333333333333, "5/8" GYP. BD" 0.0520833333333333) | property sets: Pset_WallCommon
  IFCALARMTYPE "104416 - Fire Extinguishers - Wall:Class A - Light - 2A" | 1 occurrence | material: constituents "MaterialConstituentSet" ("FIRE EXTINGUISHER": "FIRE EXTINGUISHER", "Metal - Paint Finish - Black, Matte": "Metal - Paint Finish - Black, Matte", "<Unnamed>": "<Unnamed>")
  IFCALARMTYPE "104416 - Fire Extinguishers - Wall:Class A - Light - 2A" | 1 occurrence | material: constituents "MaterialConstituentSet" ("FIRE EXTINGUISHER": "FIRE EXTINGUISHER", "Metal - Paint Finish - Black, Matte": "Metal - Paint Finish - Black, Matte", "<Unnamed>": "<Unnamed>")
  IFCBUILDINGELEMENTPROXYTYPE "Enscape AssetDefinition - Deciduous Tree 119 Yoshino Cherry (autumn):Enscape AssetDefinition - Deciduous Tree 119 Yoshino Cherry (autumn)" | 4 occurrences | material: "<Unnamed>" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Enscape AssetDefinition - Deciduous Tree 143 Maple (autumn):Enscape AssetDefinition - Deciduous Tree 143 Maple (autumn)" | 41 occurrences | material: "<Unnamed>" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Enscape AssetDefinition - Deciduous Tree 019 Coral Bark Maple (autumn):Enscape AssetDefinition - Deciduous Tree 019 Coral Bark Maple (autumn)" | 41 occurrences | material: "<Unnamed>" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Enscape AssetDefinition - Deciduous Tree 042 Japanese Maple Red Dragon (autumn):Enscape AssetDefinition - Deciduous Tree 042 Japanese Maple Red Dragon (autumn)" | 5 occurrences | material: "<Unnamed>" | property sets: Pset_BuildingElementProxyCommon
  IFCRAILINGTYPE "Railings 14:Railings 1" | 1 occurrence | material: "WOOD RAILING (MAPLE, OR BIRCH) - W/ WALL RETURNS AT ENDS" | property sets: Pset_RailingCommon
  IFCRAILINGTYPE "Railings 15:Railings 1" | 1 occurrence | material: "WOOD RAILING (MAPLE, OR BIRCH) - W/ WALL RETURNS AT ENDS" | property sets: Pset_RailingCommon
  IFCRAILINGTYPE "Railings 8:Railings 1" | 1 occurrence | material: "WOOD RAILING (MAPLE, OR BIRCH) - W/ WALL RETURNS AT ENDS" | property sets: Pset_RailingCommon
  IFCRAILINGTYPE "Railings 7:Railings 1" | 1 occurrence | material: "WOOD RAILING (MAPLE, OR BIRCH) - W/ WALL RETURNS AT ENDS" | property sets: Pset_RailingCommon
  IFCRAILINGTYPE "Railings 10:Railings 1" | 1 occurrence | material: "WOOD RAILING (MAPLE, OR BIRCH) - W/ WALL RETURNS AT ENDS" | property sets: Pset_RailingCommon
  IFCBUILDINGELEMENTPROXYTYPE "085000 - Windows - Casement or Awning or Fixed:FIXED PICTURE - TYPE 1" | 2 occurrences | material: constituents "MaterialConstituentSet" ("DOUBLE HUNG WINDOWS - BLACK EXT/INT SASH - LIMIT BOTTOM SASH TO 4" MAX OPEN": "DOUBLE HUNG WINDOWS - BLACK EXT/INT SASH - LIMIT BOTTOM SASH TO 4" MAX OPEN", "GL - INSULATED - LOW-E": "GL - INSULATED - LOW-E", "<Unnamed>": "<Unnamed>") | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation
  IFCWALLTYPE "Generic Models 74:Generic Models 1" | 1 occurrence | material: "UNDERSIDE OF FLOOR ASSEMBLY - SEE STRUCT. DWGS" | property sets: Pset_WallCommon
  IFCWALLTYPE "Generic Models 93:Generic Models 1" | 1 occurrence | material: "STRUCTURAL FLOOR - SEE STRUCT. DWGS" | property sets: Pset_WallCommon
  IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 12:Structural Framing 1" | 1 occurrence | material: "BEND DOWN FLANGE OF METAL TRACK - FASTENER PER MANU. REQUIREMENTS" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 13:Structural Framing 2" | 1 occurrence | material: "METAL STUD TRACK WELDED OR SCREWED PER MANU. REQUIREMENTS" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 14:Structural Framing 2" | 1 occurrence | material: "(2) BOXED STUDS - SAME SIZE AS WALL STUDS" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 15:Structural Framing 2" | 1 occurrence | material: "(2) BOXED STUDS - SAME SIZE AS WALL STUDS" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 16:Structural Framing 2" | 1 occurrence | material: "METAL STUD TRACK WELDED OR SCREWED PER MANU. REQUIREMENTS" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 17:Structural Framing 2" | 1 occurrence | material: "METAL STUD TRACK WELDED OR SCREWED PER MANU. REQUIREMENTS" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 18:Structural Framing 2" | 1 occurrence | material: "METAL STUD TRACK WELDED OR SCREWED PER MANU. REQUIREMENTS" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 19:Structural Framing 1" | 1 occurrence | material: "VERTICAL METAL CRIPPLE STUD BEYOND" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 21:Structural Framing 1" | 1 occurrence | material: "DOUBLE UP METAL STUDS @ JAMB" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 22:Structural Framing 1" | 1 occurrence | material: "DOUBLE UP METAL STUDS @ JAMB" | property sets: Pset_BuildingElementProxyCommon
  IFCSLABTYPE "Floor:FLOOR TRUSS" | FLOOR | 1 occurrence | material: layers "Floor:FLOOR TRUSS" ("HARDWOOD FLOOR" 0.0625, "3/4" GYP. CRETE TOPPING" 0.0625, "1/8" SOUND MAT" 0.0104166666666667, "3/4" CDX/OSB PLYWOOD - SEE STRUCT DWGS" 0.0625, "WOOD TRUSS FLOOR ASSEMBLY - (FILL CAVITY W/ CELLULOSE BLOWN-IN INSULATION) (UL - L521 FLOOR ASSEMBLY)" 1.5, "25 GA. RESILIENT CHANNEL - 24" O.C." 0.0416666666666667, "5/8" GYP. BD @ CEILING" 0.0520833333333333) | property sets: Pset_ManufacturerTypeInformation, Pset_SlabCommon
  IFCSLABTYPE "Floor:FLOOR TRUSS" | FLOOR | 1 occurrence | material: layers "Floor:FLOOR TRUSS" ("HARDWOOD FLOOR" 0.0625, "3/4" GYP. CRETE TOPPING" 0.0625, "1/8" SOUND MAT" 0.0104166666666667, "3/4" CDX/OSB PLYWOOD - SEE STRUCT DWGS" 0.0625, "WOOD TRUSS FLOOR ASSEMBLY - (FILL CAVITY W/ CELLULOSE BLOWN-IN INSULATION) (UL - L521 FLOOR ASSEMBLY)" 1.5, "25 GA. RESILIENT CHANNEL - 24" O.C." 0.0416666666666667, "5/8" GYP. BD @ CEILING" 0.0520833333333333) | property sets: Pset_ManufacturerTypeInformation, Pset_SlabCommon
  IFCSLABTYPE "Floor:FLOOR TRUSS" | FLOOR | 1 occurrence | material: layers "Floor:FLOOR TRUSS" ("HARDWOOD FLOOR" 0.0625, "3/4" GYP. CRETE TOPPING" 0.0625, "1/8" SOUND MAT" 0.0104166666666667, "3/4" CDX/OSB PLYWOOD - SEE STRUCT DWGS" 0.0625, "WOOD TRUSS FLOOR ASSEMBLY - (FILL CAVITY W/ CELLULOSE BLOWN-IN INSULATION) (UL - L521 FLOOR ASSEMBLY)" 1.5, "25 GA. RESILIENT CHANNEL - 24" O.C." 0.0416666666666667, "5/8" GYP. BD @ CEILING" 0.0520833333333333) | property sets: Pset_ManufacturerTypeInformation, Pset_SlabCommon
  IFCSLABTYPE "Floor:FLOOR TRUSS" | FLOOR | 1 occurrence | material: layers "Floor:FLOOR TRUSS" ("HARDWOOD FLOOR" 0.0625, "3/4" GYP. CRETE TOPPING" 0.0625, "1/8" SOUND MAT" 0.0104166666666667, "3/4" CDX/OSB PLYWOOD - SEE STRUCT DWGS" 0.0625, "WOOD TRUSS FLOOR ASSEMBLY - (FILL CAVITY W/ CELLULOSE BLOWN-IN INSULATION) (UL - L521 FLOOR ASSEMBLY)" 1.5, "25 GA. RESILIENT CHANNEL - 24" O.C." 0.0416666666666667, "5/8" GYP. BD @ CEILING" 0.0520833333333333) | property sets: Pset_ManufacturerTypeInformation, Pset_SlabCommon
  IFCSLABTYPE "Floor:FLOOR TRUSS" | FLOOR | 1 occurrence | material: layers "Floor:FLOOR TRUSS" ("HARDWOOD FLOOR" 0.0625, "3/4" GYP. CRETE TOPPING" 0.0625, "1/8" SOUND MAT" 0.0104166666666667, "3/4" CDX/OSB PLYWOOD - SEE STRUCT DWGS" 0.0625, "WOOD TRUSS FLOOR ASSEMBLY - (FILL CAVITY W/ CELLULOSE BLOWN-IN INSULATION) (UL - L521 FLOOR ASSEMBLY)" 1.5, "25 GA. RESILIENT CHANNEL - 24" O.C." 0.0416666666666667, "5/8" GYP. BD @ CEILING" 0.0520833333333333) | property sets: Pset_ManufacturerTypeInformation, Pset_SlabCommon
  IFCSLABTYPE "Floor:FLOOR TRUSS" | FLOOR | 1 occurrence | material: layers "Floor:FLOOR TRUSS" ("HARDWOOD FLOOR" 0.0625, "3/4" GYP. CRETE TOPPING" 0.0625, "1/8" SOUND MAT" 0.0104166666666667, "3/4" CDX/OSB PLYWOOD - SEE STRUCT DWGS" 0.0625, "WOOD TRUSS FLOOR ASSEMBLY - (FILL CAVITY W/ CELLULOSE BLOWN-IN INSULATION) (UL - L521 FLOOR ASSEMBLY)" 1.5, "25 GA. RESILIENT CHANNEL - 24" O.C." 0.0416666666666667, "5/8" GYP. BD @ CEILING" 0.0520833333333333) | property sets: Pset_ManufacturerTypeInformation, Pset_SlabCommon
  IFCFURNITURETYPE "Seating-Setee-Teknion-BBMC_Metropolitan-R1:Lounge Settee 2" | 2 occurrences | material: constituents "MaterialConstituentSet" ("Seat": "_DESIGN_FABRIC", "Frame": "Metal - Teknion - C6 - Chrome", "Frame": "Plastic - Teknion - Z1 - Greystone") | property sets: Pset_ManufacturerTypeInformation
  IFCFURNITURETYPE "Table-Coffee-Teknion-STRTC_Cover-R1:38,25" w x 27,5" d x 15" h 2" | 2 occurrences | material: constituents "MaterialConstituentSet" ("Furniture": "STEEL STRUCTURE (HOT DIPPED GALV.)", "Furniture": "BASE CABINETS") | property sets: Pset_ManufacturerTypeInformation
  IFCFURNITURETYPE "Seating-Lounge_Chair-Teknion-BBMC_Metropolitan-R1:Lounge Chair" | 3 occurrences | material: constituents "MaterialConstituentSet" ("Seat": "_DESIGN_FABRIC", "Frame": "<Unnamed>", "Frame": "Metal - Teknion - C6 - Chrome") | property sets: Pset_ManufacturerTypeInformation
  IFCBUILDINGELEMENTPROXYTYPE "Enscape AssetDefinition - Clark, Sitting:Enscape AssetDefinition - Clark, Sitting" | 1 occurrence | material: "<Unnamed>" | property sets: Pset_BuildingElementProxyCommon
  IFCWALLTYPE "Basic Wall:EXT 2b - batten board - 1HR" | STANDARD | 3 occurrences | material: layers "Basic Wall:EXT 2b - batten board - 1HR" ("FIBER CEMENT - BATTEN AND BOARD SIDING - COLOR (IRON GRAY) - 3/4"X2.5" BATTENS 12" O.C." 0.0833333333333333, "BUILDING WRAP (ASTM 2273) OVER FIBERGLASS MAT GYPSUM SHEATHING" 0.0416666666666667, "2x6 STUDS 16" O.C. (R-19 BATT. INSULATION)" 0.458333333333333, "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" 0.0520833333333333) | property sets: Pset_WallCommon
  IFCBUILDINGELEMENTPROXYTYPE "4023636" | 1 occurrence
  IFCWALLTYPE "Basic Wall:EXT 2 - corrugated metal - 1 hr - 2nd level" | STANDARD | 3 occurrences | material: layers "Basic Wall:EXT 2 - corrugated metal - 1 hr - 2nd level" ("RIBBED PBD METAL PANEL W/ EXPOSED FASTENERS - COLOR (CHARCOAL GRAY)" 0.0729166666666667, "BUILDING WRAP (ASTM 2273) OVER FIBERGLASS MAT GYPSUM SHEATHING" 0.0520833333333333, "2x6 STUDS 16" O.C. (R-19 BATT. INSULATION)" 0.458333333333333, "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" 0.0520833333333333) | property sets: Pset_WallCommon
  IFCBUILDINGELEMENTPROXYTYPE "4023639" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4023647" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4023651" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4023665" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4023678" | 1 occurrence
  IFCWALLTYPE "Basic Wall:EXT 2b - batten board" | STANDARD | 31 occurrences | material: layers "Basic Wall:EXT 2b - batten board" ("FIBER CEMENT - BATTEN AND BOARD SIDING - COLOR (IRON GRAY) - 3/4"X2.5" BATTENS 12" O.C." 0.0833333333333333, "DRAINAGE WRAP (ASTM E2273) OVER 1/2" CDX SHEATHING" 0.0416666666666667, "2x6 STUDS 16" O.C. (R-19 BATT. INSULATION)" 0.458333333333333, "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" 0.0520833333333333) | property sets: Pset_WallCommon
  IFCBUILDINGELEMENTPROXYTYPE "4023683" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4023699" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4023704" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4024953" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4028390" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4028401" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4031140" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4031151" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4031235" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4031246" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4031392" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4031546" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4032576" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4032587" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4032593" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4032604" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4032621" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4032638" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4032654" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4032665" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4032671" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4032682" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4032699" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4032716" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4032825" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4032836" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4032842" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4032853" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4032870" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4032887" | 1 occurrence
  IFCWALLTYPE "Basic Wall:EXT 2b - batten board - shear" | STANDARD | 2 occurrences | material: layers "Basic Wall:EXT 2b - batten board - shear" ("FIBER CEMENT - BATTEN AND BOARD SIDING - COLOR (IRON GRAY) - 3/4"X2.5" BATTENS 12" O.C." 0.0833333333333333, "DRAINAGE WRAP (ASTM E2273) OVER 1/2" CDX SHEATHING" 0.0416666666666667, "2x6 STUDS 16" O.C. (R-19 BATT. INSULATION)" 0.458333333333333, "WOOD STRUCTURAL PANEL (WSP) - SEE STRUCT DWGS" 0.0416666666666667, "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" 0.0520833333333333) | property sets: Pset_WallCommon
  IFCBUILDINGELEMENTPROXYTYPE "4034915" | 1 occurrence
  IFCWALLTYPE "Basic Wall:EXT 2 - corrugated metal - shear - 2nd level" | STANDARD | 2 occurrences | material: layers "Basic Wall:EXT 2 - corrugated metal - shear - 2nd level" ("RIBBED PBD METAL PANEL W/ EXPOSED FASTENERS - COLOR (CHARCOAL GRAY)" 0.0729166666666667, "DRAINAGE WRAP (ASTM E2273) OVER 1/2" CDX SHEATHING" 0.0416666666666667, "2x6 STUDS 16" O.C. (R-19 BATT. INSULATION)" 0.458333333333333, "WOOD STRUCTURAL PANEL (WSP) - SEE STRUCT DWGS" 0.0416666666666667, "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" 0.0520833333333333) | property sets: Pset_WallCommon
  IFCBUILDINGELEMENTPROXYTYPE "4034926" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4035408" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4035419" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4035588" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4035591" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4035722" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4035725" | 1 occurrence
  IFCDOORTYPE "OD_SINGLE:SINGLE - LITE - MUNTINS - 3-0 x 6-8" | DOOR | SINGLE_SWING_LEFT | 8 occurrences | material: constituents "MaterialConstituentSet" ("GL - TEMPERED - INSULATED - LOW-E": "GL - TEMPERED - INSULATED - LOW-E", "Panel": "CW - CLAD WOOD DOOR", "Frame/Mullion": "CW - CLAD WOOD DOOR") | property sets: OD_SINGLE:SINGLE - LITE - MUNTINS - 3-0 x 6-8:4037908, OD_SINGLE:SINGLE - LITE - MUNTINS - 3-0 x 6-8:4037908:1, Pset_DoorCommon
  IFCDOORTYPE "OD_SINGLE:SINGLE - LITE - MUNTINS - 3-0 x 6-8" | DOOR | SINGLE_SWING_RIGHT | 8 occurrences | material: constituents "MaterialConstituentSet" ("GL - TEMPERED - INSULATED - LOW-E": "GL - TEMPERED - INSULATED - LOW-E", "Panel": "CW - CLAD WOOD DOOR", "Frame/Mullion": "CW - CLAD WOOD DOOR") | property sets: OD_SINGLE:SINGLE - LITE - MUNTINS - 3-0 x 6-8:4037909, OD_SINGLE:SINGLE - LITE - MUNTINS - 3-0 x 6-8:4037909:1, Pset_DoorCommon
  IFCBUILDINGELEMENTPROXYTYPE "085000 - Windows - Casement or Awning or Fixed:FIXED PICTURE - TYPE 1" | 2 occurrences | material: constituents "MaterialConstituentSet" ("DOUBLE HUNG WINDOWS - BLACK EXT/INT SASH - LIMIT BOTTOM SASH TO 4" MAX OPEN": "DOUBLE HUNG WINDOWS - BLACK EXT/INT SASH - LIMIT BOTTOM SASH TO 4" MAX OPEN", "GL - INSULATED - LOW-E": "GL - INSULATED - LOW-E", "<Unnamed>": "<Unnamed>") | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation
  IFCBUILDINGELEMENTPROXYTYPE "085000 - Windows - Casement or Awning or Fixed:FIXED PICTURE - TYPE 1" | 3 occurrences | material: constituents "MaterialConstituentSet" ("DOUBLE HUNG WINDOWS - BLACK EXT/INT SASH - LIMIT BOTTOM SASH TO 4" MAX OPEN": "DOUBLE HUNG WINDOWS - BLACK EXT/INT SASH - LIMIT BOTTOM SASH TO 4" MAX OPEN", "GL - INSULATED - LOW-E": "GL - INSULATED - LOW-E", "<Unnamed>": "<Unnamed>") | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation
  IFCBUILDINGELEMENTPROXYTYPE "085000 - Windows - Double Hung:SINGLE HUNG - TYPE 2 - TEMPERED" | 3 occurrences | material: constituents "MaterialConstituentSet" ("DOUBLE HUNG WINDOWS - BLACK EXT/INT SASH - LIMIT BOTTOM SASH TO 4" MAX OPEN": "DOUBLE HUNG WINDOWS - BLACK EXT/INT SASH - LIMIT BOTTOM SASH TO 4" MAX OPEN", "WINDOW SASH/TRIM": "WINDOW SASH/TRIM", "GL - INSULATED - LOW-E": "GL - INSULATED - LOW-E") | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation
  IFCBUILDINGELEMENTPROXYTYPE "085000 - Windows - Double Hung:SINGLE HUNG - TYPE 1 - TEMPERED" | 1 occurrence | material: constituents "MaterialConstituentSet" ("DOUBLE HUNG WINDOWS - BLACK EXT/INT SASH - LIMIT BOTTOM SASH TO 4" MAX OPEN": "DOUBLE HUNG WINDOWS - BLACK EXT/INT SASH - LIMIT BOTTOM SASH TO 4" MAX OPEN", "WINDOW SASH/TRIM": "WINDOW SASH/TRIM", "GL - INSULATED - LOW-E": "GL - INSULATED - LOW-E") | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation
  IFCBUILDINGELEMENTPROXYTYPE "085000 - Windows - Double Hung:SINGLE HUNG - TYPE 2 - TEMPERED" | 3 occurrences | material: constituents "MaterialConstituentSet" ("DOUBLE HUNG WINDOWS - BLACK EXT/INT SASH - LIMIT BOTTOM SASH TO 4" MAX OPEN": "DOUBLE HUNG WINDOWS - BLACK EXT/INT SASH - LIMIT BOTTOM SASH TO 4" MAX OPEN", "WINDOW SASH/TRIM": "WINDOW SASH/TRIM", "GL - INSULATED - LOW-E": "GL - INSULATED - LOW-E") | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation
  IFCBUILDINGELEMENTPROXYTYPE "085000 - Windows - Double Hung:SINGLE HUNG - TYPE 2" | 6 occurrences | material: constituents "MaterialConstituentSet" ("DOUBLE HUNG WINDOWS - BLACK EXT/INT SASH - LIMIT BOTTOM SASH TO 4" MAX OPEN": "DOUBLE HUNG WINDOWS - BLACK EXT/INT SASH - LIMIT BOTTOM SASH TO 4" MAX OPEN", "WINDOW SASH/TRIM": "WINDOW SASH/TRIM", "GL - INSULATED - LOW-E": "GL - INSULATED - LOW-E") | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation
  IFCBUILDINGELEMENTPROXYTYPE "085000 - Windows - Double Hung:SINGLE HUNG - TYPE 1" | 3 occurrences | material: constituents "MaterialConstituentSet" ("DOUBLE HUNG WINDOWS - BLACK EXT/INT SASH - LIMIT BOTTOM SASH TO 4" MAX OPEN": "DOUBLE HUNG WINDOWS - BLACK EXT/INT SASH - LIMIT BOTTOM SASH TO 4" MAX OPEN", "WINDOW SASH/TRIM": "WINDOW SASH/TRIM", "GL - INSULATED - LOW-E": "GL - INSULATED - LOW-E") | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation
  IFCBUILDINGELEMENTPROXYTYPE "085000 - Windows - Double Hung:SINGLE HUNG - TYPE 1" | 1 occurrence | material: constituents "MaterialConstituentSet" ("DOUBLE HUNG WINDOWS - BLACK EXT/INT SASH - LIMIT BOTTOM SASH TO 4" MAX OPEN": "DOUBLE HUNG WINDOWS - BLACK EXT/INT SASH - LIMIT BOTTOM SASH TO 4" MAX OPEN", "WINDOW SASH/TRIM": "WINDOW SASH/TRIM", "GL - INSULATED - LOW-E": "GL - INSULATED - LOW-E") | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation
  IFCBUILDINGELEMENTPROXYTYPE "085000 - Windows - Double Hung:SINGLE HUNG - TYPE 2" | 2 occurrences | material: constituents "MaterialConstituentSet" ("DOUBLE HUNG WINDOWS - BLACK EXT/INT SASH - LIMIT BOTTOM SASH TO 4" MAX OPEN": "DOUBLE HUNG WINDOWS - BLACK EXT/INT SASH - LIMIT BOTTOM SASH TO 4" MAX OPEN", "WINDOW SASH/TRIM": "WINDOW SASH/TRIM", "GL - INSULATED - LOW-E": "GL - INSULATED - LOW-E") | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation
  IFCBUILDINGELEMENTPROXYTYPE "085000 - Windows - Double Hung:SINGLE HUNG - TYPE 2" | 1 occurrence | material: constituents "MaterialConstituentSet" ("DOUBLE HUNG WINDOWS - BLACK EXT/INT SASH - LIMIT BOTTOM SASH TO 4" MAX OPEN": "DOUBLE HUNG WINDOWS - BLACK EXT/INT SASH - LIMIT BOTTOM SASH TO 4" MAX OPEN", "WINDOW SASH/TRIM": "WINDOW SASH/TRIM", "GL - INSULATED - LOW-E": "GL - INSULATED - LOW-E") | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation
  IFCSLABTYPE "Floor:balc floor" | FLOOR | 1 occurrence | material: layers "Floor:balc floor" ("COMPOSITE DECKING" 0.0833333333333333) | property sets: Pset_SlabCommon
  IFCSLABTYPE "Floor:balc floor" | FLOOR | 1 occurrence | material: layers "Floor:balc floor" ("COMPOSITE DECKING" 0.0833333333333333) | property sets: Pset_SlabCommon
  IFCBUILDINGELEMENTPROXYTYPE "4185256" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4185259" | 1 occurrence
  IFCWALLTYPE "Basic Wall:EXT 2 - corrugated metal - 2nd level" | STANDARD | 1 occurrence | material: layers "Basic Wall:EXT 2 - corrugated metal - 2nd level" ("RIBBED PBD METAL PANEL W/ EXPOSED FASTENERS - COLOR (CHARCOAL GRAY)" 0.0729166666666667, "DRAINAGE WRAP (ASTM E2273) OVER 1/2" CDX SHEATHING" 0.0416666666666667, "2x6 STUDS 16" O.C. (R-19 BATT. INSULATION)" 0.458333333333333, "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" 0.0520833333333333) | property sets: Pset_WallCommon
  IFCBUILDINGELEMENTPROXYTYPE "4185267" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4185280" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4185298" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4185319" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4185329" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4185341" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4185352" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "085000 - Windows - Double Hung:SINGLE HUNG - TYPE 2" | 2 occurrences | material: constituents "MaterialConstituentSet" ("DOUBLE HUNG WINDOWS - BLACK EXT/INT SASH - LIMIT BOTTOM SASH TO 4" MAX OPEN": "DOUBLE HUNG WINDOWS - BLACK EXT/INT SASH - LIMIT BOTTOM SASH TO 4" MAX OPEN", "WINDOW SASH/TRIM": "WINDOW SASH/TRIM", "GL - INSULATED - LOW-E": "GL - INSULATED - LOW-E") | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation
  IFCBUILDINGELEMENTPROXYTYPE "085000 - Windows - Double Hung:SINGLE HUNG - TYPE 2" | 2 occurrences | material: constituents "MaterialConstituentSet" ("DOUBLE HUNG WINDOWS - BLACK EXT/INT SASH - LIMIT BOTTOM SASH TO 4" MAX OPEN": "DOUBLE HUNG WINDOWS - BLACK EXT/INT SASH - LIMIT BOTTOM SASH TO 4" MAX OPEN", "WINDOW SASH/TRIM": "WINDOW SASH/TRIM", "GL - INSULATED - LOW-E": "GL - INSULATED - LOW-E") | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation
  IFCBUILDINGELEMENTPROXYTYPE "085000 - Windows - Double Hung:SINGLE HUNG - TYPE 1" | 2 occurrences | material: constituents "MaterialConstituentSet" ("DOUBLE HUNG WINDOWS - BLACK EXT/INT SASH - LIMIT BOTTOM SASH TO 4" MAX OPEN": "DOUBLE HUNG WINDOWS - BLACK EXT/INT SASH - LIMIT BOTTOM SASH TO 4" MAX OPEN", "WINDOW SASH/TRIM": "WINDOW SASH/TRIM", "GL - INSULATED - LOW-E": "GL - INSULATED - LOW-E") | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation
  IFCBUILDINGELEMENTPROXYTYPE "085000 - Windows - Double Hung:SINGLE HUNG - TYPE 1" | 2 occurrences | material: constituents "MaterialConstituentSet" ("DOUBLE HUNG WINDOWS - BLACK EXT/INT SASH - LIMIT BOTTOM SASH TO 4" MAX OPEN": "DOUBLE HUNG WINDOWS - BLACK EXT/INT SASH - LIMIT BOTTOM SASH TO 4" MAX OPEN", "WINDOW SASH/TRIM": "WINDOW SASH/TRIM", "GL - INSULATED - LOW-E": "GL - INSULATED - LOW-E") | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation
  IFCBUILDINGELEMENTPROXYTYPE "085000 - Windows - Casement or Awning or Fixed:FIXED PICTURE - TYPE 1" | 1 occurrence | material: constituents "MaterialConstituentSet" ("DOUBLE HUNG WINDOWS - BLACK EXT/INT SASH - LIMIT BOTTOM SASH TO 4" MAX OPEN": "DOUBLE HUNG WINDOWS - BLACK EXT/INT SASH - LIMIT BOTTOM SASH TO 4" MAX OPEN", "GL - INSULATED - LOW-E": "GL - INSULATED - LOW-E", "<Unnamed>": "<Unnamed>") | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation
  IFCWALLTYPE "Basic Wall:SHEAR - W4_5D - (5/8 GYP - 2X4 WOOD(BATT))" | STANDARD | 16 occurrences | material: layers "Basic Wall:SHEAR - W4_5D - (5/8 GYP - 2X4 WOOD(BATT))" ("AIR GAP" 0.0416666666666667, "2x4 STUDS (1ST FL @ 8" O.C. • 2ND FL @ 12" O.C. • 3RD FL @ 16" O.C.) - BATT. INSULATION AT STUD CAVITY" 0.291666666666667, "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" 0.0520833333333333) | property sets: Pset_WallCommon
  IFCBUILDINGELEMENTPROXYTYPE "4303743" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4397244" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4397251" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4397357" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4397359" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4397378" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4397382" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4397406" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4397408" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4397412" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4397414" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4398211" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4398218" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4401981" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4401983" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4402003" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4402007" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4402039" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4402041" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4402045" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4402047" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4402233" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4402234" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4402235" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4408343" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4408344" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4408346" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4408348" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4408350" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4408356" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4408358" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4409468" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4409482" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4410307" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4410309" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4410311" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4410313" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4410329" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4410331" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4410333" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4410335" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4410340" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4410342" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4410344" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4410346" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4410362" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4410364" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4410366" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4410368" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4411077" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4411110" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4411112" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4411114" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4411117" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4411120" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4411122" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4412290" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4412307" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4413180" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4413182" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4413184" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4413186" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4413202" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4413204" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4413206" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4413208" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4413213" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4413215" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4413217" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4413219" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4413235" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4413237" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4413239" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4413241" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4416523" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4416524" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4416528" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4417423" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4417424" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4417783" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4417790" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4418876" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4418884" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4418888" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4418896" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4423443" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4423444" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4423827" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4423836" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4424940" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4424948" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4424952" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4424960" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4452184" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4454411" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4454415" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4454420" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4454424" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "085000 - Windows - Double Hung:SINGLE HUNG - TYPE 1" | 1 occurrence | material: constituents "MaterialConstituentSet" ("DOUBLE HUNG WINDOWS - BLACK EXT/INT SASH - LIMIT BOTTOM SASH TO 4" MAX OPEN": "DOUBLE HUNG WINDOWS - BLACK EXT/INT SASH - LIMIT BOTTOM SASH TO 4" MAX OPEN", "WINDOW SASH/TRIM": "WINDOW SASH/TRIM", "GL - INSULATED - LOW-E": "GL - INSULATED - LOW-E") | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation
  IFCPIPESEGMENTTYPE "Pipe Types:Default" | 30 occurrences | material: "GALV. PIPE WHERE EXPOSED - (EXPOSED LINE SETS, BEHIND PERFORATED PANEL)"
  IFCBUILDINGELEMENTPROXYTYPE "4472406" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4472461" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4473215" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4473218" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4473245" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4473248" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4473265" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4473268" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4475659" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4475737" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4475738" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4494545" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4494575" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4494578" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4494580" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4494582" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4494584" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4494585" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4494586" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4494588" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4496652" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4496654" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4496656" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4496658" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4496674" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4496676" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4496678" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4496680" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4496687" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4496689" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4496691" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4496707" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4496711" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4496713" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4536647" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "085000 - Windows - Double Hung:SINGLE HUNG - TYPE 1" | 2 occurrences | material: constituents "MaterialConstituentSet" ("DOUBLE HUNG WINDOWS - BLACK EXT/INT SASH - LIMIT BOTTOM SASH TO 4" MAX OPEN": "DOUBLE HUNG WINDOWS - BLACK EXT/INT SASH - LIMIT BOTTOM SASH TO 4" MAX OPEN", "WINDOW SASH/TRIM": "WINDOW SASH/TRIM", "GL - INSULATED - LOW-E": "GL - INSULATED - LOW-E") | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation
  IFCBUILDINGELEMENTPROXYTYPE "4537816" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4537878" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4538102" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4538105" | 1 occurrence
  IFCALARMTYPE "104416 - Fire Extinguishers - Wall:Class A - Light - 2A" | 1 occurrence | material: constituents "MaterialConstituentSet" ("FIRE EXTINGUISHER": "FIRE EXTINGUISHER", "Metal - Paint Finish - Black, Matte": "Metal - Paint Finish - Black, Matte", "<Unnamed>": "<Unnamed>")
  IFCALARMTYPE "104416 - Fire Extinguishers - Wall:Class A - Light - 2A" | 1 occurrence | material: constituents "MaterialConstituentSet" ("FIRE EXTINGUISHER": "FIRE EXTINGUISHER", "Metal - Paint Finish - Black, Matte": "Metal - Paint Finish - Black, Matte", "<Unnamed>": "<Unnamed>")
  IFCBUILDINGELEMENTPROXYTYPE "Enscape AssetDefinition - Annouk and Maud, Standing 03:Enscape AssetDefinition - Annouk and Maud, Standing 03" | 1 occurrence | material: "<Unnamed>" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Enscape AssetDefinition - Bao, Standing 03:Enscape AssetDefinition - Bao, Standing 03" | 1 occurrence | material: "<Unnamed>" | property sets: Pset_BuildingElementProxyCommon
  IFCRAILINGTYPE "Railings 9:Railings 1" | 1 occurrence | material: "WOOD RAILING (MAPLE, OR BIRCH) - W/ WALL RETURNS AT ENDS" | property sets: Pset_RailingCommon
  IFCRAILINGTYPE "Railings 11:Railings 1" | 1 occurrence | material: "WOOD RAILING (MAPLE, OR BIRCH) - W/ WALL RETURNS AT ENDS" | property sets: Pset_RailingCommon
  IFCRAILINGTYPE "Railings 12:Railings 1" | 1 occurrence | material: "WOOD RAILING (MAPLE, OR BIRCH) - W/ WALL RETURNS AT ENDS" | property sets: Pset_RailingCommon
  IFCRAILINGTYPE "Railings 13:Railings 1" | 1 occurrence | material: "WOOD RAILING (MAPLE, OR BIRCH) - W/ WALL RETURNS AT ENDS" | property sets: Pset_RailingCommon
  IFCWALLTYPE "Light Pole Luminaire:Light Pole Luminaire" | 1 occurrence | material: "LUMINAIRE HOUSING AS SPECIFIED" | property sets: Pset_WallCommon
  IFCBUILDINGELEMENTPROXYTYPE "Model Text:OD_Very Large" | 1 occurrence | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Model Text:OD_Very Large" | 1 occurrence | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Model Text:OD_Very Large" | 1 occurrence | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Model Text:OD_Very Large" | 1 occurrence | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Model Text:OD_Very Large" | 1 occurrence | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Model Text:OD_Very Large" | 1 occurrence | property sets: Pset_BuildingElementProxyCommon
  IFCROOFTYPE "Basic Roof:BALC" | 1 occurrence | property sets: Pset_RoofCommon
  IFCSLABTYPE "Floor:FLOOR TRUSS" | FLOOR | 1 occurrence | material: layers "Floor:FLOOR TRUSS" ("HARDWOOD FLOOR" 0.0625, "3/4" GYP. CRETE TOPPING" 0.0625, "1/8" SOUND MAT" 0.0104166666666667, "3/4" CDX/OSB PLYWOOD - SEE STRUCT DWGS" 0.0625, "WOOD TRUSS FLOOR ASSEMBLY - (FILL CAVITY W/ CELLULOSE BLOWN-IN INSULATION) (UL - L521 FLOOR ASSEMBLY)" 1.5, "25 GA. RESILIENT CHANNEL - 24" O.C." 0.0416666666666667, "5/8" GYP. BD @ CEILING" 0.0520833333333333) | property sets: Pset_ManufacturerTypeInformation, Pset_SlabCommon
  IFCSLABTYPE "Floor:FLOOR TRUSS" | FLOOR | 1 occurrence | material: layers "Floor:FLOOR TRUSS" ("HARDWOOD FLOOR" 0.0625, "3/4" GYP. CRETE TOPPING" 0.0625, "1/8" SOUND MAT" 0.0104166666666667, "3/4" CDX/OSB PLYWOOD - SEE STRUCT DWGS" 0.0625, "WOOD TRUSS FLOOR ASSEMBLY - (FILL CAVITY W/ CELLULOSE BLOWN-IN INSULATION) (UL - L521 FLOOR ASSEMBLY)" 1.5, "25 GA. RESILIENT CHANNEL - 24" O.C." 0.0416666666666667, "5/8" GYP. BD @ CEILING" 0.0520833333333333) | property sets: Pset_ManufacturerTypeInformation, Pset_SlabCommon
  IFCSLABTYPE "Floor:FLOOR TRUSS" | FLOOR | 1 occurrence | material: layers "Floor:FLOOR TRUSS" ("HARDWOOD FLOOR" 0.0625, "3/4" GYP. CRETE TOPPING" 0.0625, "1/8" SOUND MAT" 0.0104166666666667, "3/4" CDX/OSB PLYWOOD - SEE STRUCT DWGS" 0.0625, "WOOD TRUSS FLOOR ASSEMBLY - (FILL CAVITY W/ CELLULOSE BLOWN-IN INSULATION) (UL - L521 FLOOR ASSEMBLY)" 1.5, "25 GA. RESILIENT CHANNEL - 24" O.C." 0.0416666666666667, "5/8" GYP. BD @ CEILING" 0.0520833333333333) | property sets: Pset_ManufacturerTypeInformation, Pset_SlabCommon
  IFCSLABTYPE "Floor:FLOOR TRUSS" | FLOOR | 1 occurrence | material: layers "Floor:FLOOR TRUSS" ("HARDWOOD FLOOR" 0.0625, "3/4" GYP. CRETE TOPPING" 0.0625, "1/8" SOUND MAT" 0.0104166666666667, "3/4" CDX/OSB PLYWOOD - SEE STRUCT DWGS" 0.0625, "WOOD TRUSS FLOOR ASSEMBLY - (FILL CAVITY W/ CELLULOSE BLOWN-IN INSULATION) (UL - L521 FLOOR ASSEMBLY)" 1.5, "25 GA. RESILIENT CHANNEL - 24" O.C." 0.0416666666666667, "5/8" GYP. BD @ CEILING" 0.0520833333333333) | property sets: Pset_ManufacturerTypeInformation, Pset_SlabCommon
  IFCSLABTYPE "Floor:FLOOR TRUSS" | FLOOR | 1 occurrence | material: layers "Floor:FLOOR TRUSS" ("HARDWOOD FLOOR" 0.0625, "3/4" GYP. CRETE TOPPING" 0.0625, "1/8" SOUND MAT" 0.0104166666666667, "3/4" CDX/OSB PLYWOOD - SEE STRUCT DWGS" 0.0625, "WOOD TRUSS FLOOR ASSEMBLY - (FILL CAVITY W/ CELLULOSE BLOWN-IN INSULATION) (UL - L521 FLOOR ASSEMBLY)" 1.5, "25 GA. RESILIENT CHANNEL - 24" O.C." 0.0416666666666667, "5/8" GYP. BD @ CEILING" 0.0520833333333333) | property sets: Pset_ManufacturerTypeInformation, Pset_SlabCommon
  IFCROOFTYPE "Basic Roof:SOFFIT" | 1 occurrence | property sets: Pset_RoofCommon
  IFCBUILDINGELEMENTPROXYTYPE "Enscape AssetDefinition - Allen Sitting:Enscape AssetDefinition - Allen Sitting" | 1 occurrence | material: "<Unnamed>" | property sets: Pset_BuildingElementProxyCommon
  IFCWALLTYPE "Basic Wall:EXT 2 - corrugated metal at parapet" | STANDARD | 39 occurrences | material: layers "Basic Wall:EXT 2 - corrugated metal at parapet" ("RIBBED PBD METAL PANEL W/ EXPOSED FASTENERS - COLOR (CHARCOAL GRAY)" 0.0729166666666667, "DRAINAGE WRAP (ASTM E2273) OVER 1/2" CDX SHEATHING" 0.0416666666666667, "2x6 STUDS 16" O.C. (R-19 BATT. INSULATION)" 0.458333333333333, "DRAINAGE WRAP (ASTM E2273) OVER 1/2" CDX SHEATHING" 0.0416666666666667, "RIBBED PBD METAL PANEL W/ EXPOSED FASTENERS - COLOR (CHARCOAL GRAY)" 0.0729166666666667) | property sets: Pset_WallCommon
  IFCROOFTYPE "Basic Roof:SOFFIT" | 1 occurrence | property sets: Pset_RoofCommon
  IFCROOFTYPE "Basic Roof:SOFFIT" | 1 occurrence | property sets: Pset_RoofCommon
  IFCBUILDINGELEMENTPROXYTYPE "085000 - Windows - Double Hung:SINGLE HUNG - TYPE 2" | 1 occurrence | material: constituents "MaterialConstituentSet" ("DOUBLE HUNG WINDOWS - BLACK EXT/INT SASH - LIMIT BOTTOM SASH TO 4" MAX OPEN": "DOUBLE HUNG WINDOWS - BLACK EXT/INT SASH - LIMIT BOTTOM SASH TO 4" MAX OPEN", "WINDOW SASH/TRIM": "WINDOW SASH/TRIM", "GL - INSULATED - LOW-E": "GL - INSULATED - LOW-E") | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation
  IFCBUILDINGELEMENTPROXYTYPE "085000 - Windows - Double Hung:SINGLE HUNG - TYPE 1 - TEMPERED" | 1 occurrence | material: constituents "MaterialConstituentSet" ("DOUBLE HUNG WINDOWS - BLACK EXT/INT SASH - LIMIT BOTTOM SASH TO 4" MAX OPEN": "DOUBLE HUNG WINDOWS - BLACK EXT/INT SASH - LIMIT BOTTOM SASH TO 4" MAX OPEN", "WINDOW SASH/TRIM": "WINDOW SASH/TRIM", "GL - INSULATED - LOW-E": "GL - INSULATED - LOW-E") | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation
  IFCBUILDINGELEMENTPROXYTYPE "085000 - Windows - Double Hung:SINGLE HUNG - TYPE 2" | 1 occurrence | material: constituents "MaterialConstituentSet" ("DOUBLE HUNG WINDOWS - BLACK EXT/INT SASH - LIMIT BOTTOM SASH TO 4" MAX OPEN": "DOUBLE HUNG WINDOWS - BLACK EXT/INT SASH - LIMIT BOTTOM SASH TO 4" MAX OPEN", "WINDOW SASH/TRIM": "WINDOW SASH/TRIM", "GL - INSULATED - LOW-E": "GL - INSULATED - LOW-E") | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation
  IFCBUILDINGELEMENTPROXYTYPE "085000 - Windows - Double Hung:SINGLE HUNG - TYPE 1" | 3 occurrences | material: constituents "MaterialConstituentSet" ("DOUBLE HUNG WINDOWS - BLACK EXT/INT SASH - LIMIT BOTTOM SASH TO 4" MAX OPEN": "DOUBLE HUNG WINDOWS - BLACK EXT/INT SASH - LIMIT BOTTOM SASH TO 4" MAX OPEN", "WINDOW SASH/TRIM": "WINDOW SASH/TRIM", "GL - INSULATED - LOW-E": "GL - INSULATED - LOW-E") | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation
  IFCBUILDINGELEMENTPROXYTYPE "085000 - Windows - Double Hung:SINGLE HUNG - TYPE 2" | 3 occurrences | material: constituents "MaterialConstituentSet" ("DOUBLE HUNG WINDOWS - BLACK EXT/INT SASH - LIMIT BOTTOM SASH TO 4" MAX OPEN": "DOUBLE HUNG WINDOWS - BLACK EXT/INT SASH - LIMIT BOTTOM SASH TO 4" MAX OPEN", "WINDOW SASH/TRIM": "WINDOW SASH/TRIM", "GL - INSULATED - LOW-E": "GL - INSULATED - LOW-E") | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation
  IFCBUILDINGELEMENTPROXYTYPE "085000 - Windows - Double Hung:SINGLE HUNG - TYPE 1" | 1 occurrence | material: constituents "MaterialConstituentSet" ("DOUBLE HUNG WINDOWS - BLACK EXT/INT SASH - LIMIT BOTTOM SASH TO 4" MAX OPEN": "DOUBLE HUNG WINDOWS - BLACK EXT/INT SASH - LIMIT BOTTOM SASH TO 4" MAX OPEN", "WINDOW SASH/TRIM": "WINDOW SASH/TRIM", "GL - INSULATED - LOW-E": "GL - INSULATED - LOW-E") | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation
  IFCSLABTYPE "Floor:balc floor" | FLOOR | 1 occurrence | material: layers "Floor:balc floor" ("COMPOSITE DECKING" 0.0833333333333333) | property sets: Pset_SlabCommon
  IFCSLABTYPE "Floor:balc floor" | FLOOR | 1 occurrence | material: layers "Floor:balc floor" ("COMPOSITE DECKING" 0.0833333333333333) | property sets: Pset_SlabCommon
  IFCBUILDINGELEMENTPROXYTYPE "Fascia:Fascia 1" | 1 occurrence | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "085000 - Windows - Casement or Awning or Fixed:FIXED PICTURE - TYPE 1" | 2 occurrences | material: constituents "MaterialConstituentSet" ("DOUBLE HUNG WINDOWS - BLACK EXT/INT SASH - LIMIT BOTTOM SASH TO 4" MAX OPEN": "DOUBLE HUNG WINDOWS - BLACK EXT/INT SASH - LIMIT BOTTOM SASH TO 4" MAX OPEN", "GL - INSULATED - LOW-E": "GL - INSULATED - LOW-E", "<Unnamed>": "<Unnamed>") | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation
  IFCBUILDINGELEMENTPROXYTYPE "085000 - Windows - Casement or Awning or Fixed:FIXED PICTURE - TYPE 1" | 3 occurrences | material: constituents "MaterialConstituentSet" ("DOUBLE HUNG WINDOWS - BLACK EXT/INT SASH - LIMIT BOTTOM SASH TO 4" MAX OPEN": "DOUBLE HUNG WINDOWS - BLACK EXT/INT SASH - LIMIT BOTTOM SASH TO 4" MAX OPEN", "GL - INSULATED - LOW-E": "GL - INSULATED - LOW-E", "<Unnamed>": "<Unnamed>") | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation
  IFCROOFTYPE "Basic Roof:WOOD-FRAMED ROOF ABOVE 3RD FLOOR" | 1 occurrence | property sets: Pset_RoofCommon
  IFCWALLTYPE "Basic Wall:EXT 2 - corrugated metal at parapet - 1HR" | STANDARD | 3 occurrences | material: layers "Basic Wall:EXT 2 - corrugated metal at parapet - 1HR" ("RIBBED PBD METAL PANEL W/ EXPOSED FASTENERS - COLOR (CHARCOAL GRAY)" 0.0729166666666667, "BUILDING WRAP (ASTM 2273) OVER FIBERGLASS MAT GYPSUM SHEATHING" 0.0416666666666667, "2x6 STUDS 16" O.C. (R-19 BATT. INSULATION)" 0.458333333333333, "BUILDING WRAP (ASTM 2273) OVER FIBERGLASS MAT GYPSUM SHEATHING" 0.0416666666666667, "RIBBED PBD METAL PANEL W/ EXPOSED FASTENERS - COLOR (CHARCOAL GRAY)" 0.0729166666666667) | property sets: Pset_WallCommon
  IFCBUILDINGELEMENTPROXYTYPE "085000 - Windows - Double Hung:SINGLE HUNG - TYPE 2" | 4 occurrences | material: constituents "MaterialConstituentSet" ("DOUBLE HUNG WINDOWS - BLACK EXT/INT SASH - LIMIT BOTTOM SASH TO 4" MAX OPEN": "DOUBLE HUNG WINDOWS - BLACK EXT/INT SASH - LIMIT BOTTOM SASH TO 4" MAX OPEN", "WINDOW SASH/TRIM": "WINDOW SASH/TRIM", "GL - INSULATED - LOW-E": "GL - INSULATED - LOW-E") | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation
  IFCBUILDINGELEMENTPROXYTYPE "085000 - Windows - Double Hung:SINGLE HUNG - TYPE 1" | 4 occurrences | material: constituents "MaterialConstituentSet" ("DOUBLE HUNG WINDOWS - BLACK EXT/INT SASH - LIMIT BOTTOM SASH TO 4" MAX OPEN": "DOUBLE HUNG WINDOWS - BLACK EXT/INT SASH - LIMIT BOTTOM SASH TO 4" MAX OPEN", "WINDOW SASH/TRIM": "WINDOW SASH/TRIM", "GL - INSULATED - LOW-E": "GL - INSULATED - LOW-E") | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation
  IFCBUILDINGELEMENTPROXYTYPE "085000 - Windows - Casement or Awning or Fixed:FIXED PICTURE - TYPE 1" | 1 occurrence | material: constituents "MaterialConstituentSet" ("DOUBLE HUNG WINDOWS - BLACK EXT/INT SASH - LIMIT BOTTOM SASH TO 4" MAX OPEN": "DOUBLE HUNG WINDOWS - BLACK EXT/INT SASH - LIMIT BOTTOM SASH TO 4" MAX OPEN", "GL - INSULATED - LOW-E": "GL - INSULATED - LOW-E", "<Unnamed>": "<Unnamed>") | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation
  IFCBUILDINGELEMENTPROXYTYPE "085000 - Windows - Double Hung:SINGLE HUNG - TYPE 2" | 2 occurrences | material: constituents "MaterialConstituentSet" ("DOUBLE HUNG WINDOWS - BLACK EXT/INT SASH - LIMIT BOTTOM SASH TO 4" MAX OPEN": "DOUBLE HUNG WINDOWS - BLACK EXT/INT SASH - LIMIT BOTTOM SASH TO 4" MAX OPEN", "WINDOW SASH/TRIM": "WINDOW SASH/TRIM", "GL - INSULATED - LOW-E": "GL - INSULATED - LOW-E") | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation
  IFCBUILDINGELEMENTPROXYTYPE "085000 - Windows - Double Hung:SINGLE HUNG - TYPE 1" | 2 occurrences | material: constituents "MaterialConstituentSet" ("DOUBLE HUNG WINDOWS - BLACK EXT/INT SASH - LIMIT BOTTOM SASH TO 4" MAX OPEN": "DOUBLE HUNG WINDOWS - BLACK EXT/INT SASH - LIMIT BOTTOM SASH TO 4" MAX OPEN", "WINDOW SASH/TRIM": "WINDOW SASH/TRIM", "GL - INSULATED - LOW-E": "GL - INSULATED - LOW-E") | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation
  IFCBUILDINGELEMENTPROXYTYPE "4201628" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4201630" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4201631" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4201632" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4201633" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4201634" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4201636" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4201637" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4201638" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4201639" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4201640" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4201641" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4201746" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4201747" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4201748" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4201749" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4201750" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4201760" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4201761" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4201762" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4201763" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4201764" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4201767" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4201768" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4201769" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4201770" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4201771" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4201781" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4201782" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4201783" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4201784" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4201785" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4206952" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4206953" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4206954" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4207058" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4207059" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4207060" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4207271" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4207557" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "085000 - Windows - Double Hung:SINGLE HUNG - TYPE 2" | 2 occurrences | material: constituents "MaterialConstituentSet" ("DOUBLE HUNG WINDOWS - BLACK EXT/INT SASH - LIMIT BOTTOM SASH TO 4" MAX OPEN": "DOUBLE HUNG WINDOWS - BLACK EXT/INT SASH - LIMIT BOTTOM SASH TO 4" MAX OPEN", "WINDOW SASH/TRIM": "WINDOW SASH/TRIM", "GL - INSULATED - LOW-E": "GL - INSULATED - LOW-E") | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation
  IFCBUILDINGELEMENTPROXYTYPE "085000 - Windows - Double Hung:SINGLE HUNG - TYPE 1" | 1 occurrence | material: constituents "MaterialConstituentSet" ("DOUBLE HUNG WINDOWS - BLACK EXT/INT SASH - LIMIT BOTTOM SASH TO 4" MAX OPEN": "DOUBLE HUNG WINDOWS - BLACK EXT/INT SASH - LIMIT BOTTOM SASH TO 4" MAX OPEN", "WINDOW SASH/TRIM": "WINDOW SASH/TRIM", "GL - INSULATED - LOW-E": "GL - INSULATED - LOW-E") | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation
  IFCSLABTYPE "Floor:FLOOR TRUSS" | FLOOR | 1 occurrence | material: layers "Floor:FLOOR TRUSS" ("HARDWOOD FLOOR" 0.0625, "3/4" GYP. CRETE TOPPING" 0.0625, "1/8" SOUND MAT" 0.0104166666666667, "3/4" CDX/OSB PLYWOOD - SEE STRUCT DWGS" 0.0625, "WOOD TRUSS FLOOR ASSEMBLY - (FILL CAVITY W/ CELLULOSE BLOWN-IN INSULATION) (UL - L521 FLOOR ASSEMBLY)" 1.5, "25 GA. RESILIENT CHANNEL - 24" O.C." 0.0416666666666667, "5/8" GYP. BD @ CEILING" 0.0520833333333333) | property sets: Pset_ManufacturerTypeInformation, Pset_SlabCommon
  IFCROOFTYPE "Basic Roof:CRICKETS" | 1 occurrence | property sets: Pset_RoofCommon
  IFCROOFTYPE "Basic Roof:WOOD-FRAMED ROOF ABOVE 3RD FLOOR" | 1 occurrence | property sets: Pset_RoofCommon
  IFCROOFTYPE "Basic Roof:CRICKETS" | 1 occurrence | property sets: Pset_RoofCommon
  IFCBUILDINGELEMENTPROXYTYPE "4303746" | 1 occurrence
  IFCROOFTYPE "Basic Roof:WOOD-FRAMED ROOF ABOVE 3RD FLOOR" | 1 occurrence | property sets: Pset_RoofCommon
  IFCROOFTYPE "Basic Roof:CRICKETS" | 1 occurrence | property sets: Pset_RoofCommon
  IFCROOFTYPE "Basic Roof:WOOD-FRAMED ROOF ABOVE 3RD FLOOR" | 1 occurrence | property sets: Pset_RoofCommon
  IFCROOFTYPE "Basic Roof:CRICKETS" | 1 occurrence | property sets: Pset_RoofCommon
  IFCROOFTYPE "Basic Roof:WOOD-FRAMED ROOF ABOVE 3RD FLOOR" | 1 occurrence | property sets: Pset_RoofCommon
  IFCROOFTYPE "Basic Roof:CRICKETS" | 1 occurrence | property sets: Pset_RoofCommon
  IFCROOFTYPE "Basic Roof:WOOD-FRAMED ROOF ABOVE 3RD FLOOR" | 1 occurrence | property sets: Pset_RoofCommon
  IFCROOFTYPE "Basic Roof:CRICKETS" | 1 occurrence | property sets: Pset_RoofCommon
  IFCDISTRIBUTIONELEMENTTYPE "22142613 - Roof Drains - Type A:22142613 - Roof Drains - Type A" | 4 occurrences | material: "ROOF DRAIN, TYP. (SEE PLUMB DWGS) - W/ INTEGRATED EMERGENCY OVERFLOW DRAIN"
  IFCBUILDINGELEMENTPROXYTYPE "Hatch-Precision_Ladders-Roof_Hatch:PH-(A) 2’-6” X 3’-0”" | 1 occurrence | material: constituents "MaterialConstituentSet" ("Insulation -Precision Ladders LLC - Rigid Fiber": "Insulation -Precision Ladders LLC - Rigid Fiber", "ROOF HATCH": "ROOF HATCH") | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation
  IFCBUILDINGELEMENTPROXYTYPE "Egress - Path of Travel:Egress - Path of Travel" | 1 occurrence | material: "<Unnamed>" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Egress - Path of Travel:Egress - Path of Travel" | 1 occurrence | material: "<Unnamed>" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Egress - Path of Travel:Egress - Path of Travel" | 1 occurrence | material: "<Unnamed>" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Egress - Path of Travel:Egress - Path of Travel" | 1 occurrence | material: "<Unnamed>" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Egress - Path of Travel:Egress - Path of Travel" | 1 occurrence | material: "<Unnamed>" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Egress - Path of Travel:Egress - Path of Travel" | 1 occurrence | material: "<Unnamed>" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Egress - Path of Travel:Egress - Path of Travel" | 1 occurrence | material: "<Unnamed>" | property sets: Pset_BuildingElementProxyCommon
  IFCPUMPTYPE "HVAC_Air-Conditioning_Fujitsu General_AOYG22-24KATA:AOYG22KATA" | 9 occurrences | material: constituents "MaterialConstituentSet" ("MINI SPLIT CONDENSER - REF. MECH. DWGS": "MINI SPLIT CONDENSER - REF. MECH. DWGS", "Color RGB 040-040-040": "Color RGB 040-040-040", "<Unnamed>": "<Unnamed>") | property sets: Pset_ManufacturerTypeInformation
  IFCPUMPTYPE "HVAC_Air-Conditioning_Fujitsu General_AOYG22-24KATA:AOYG22KATA" | 9 occurrences | material: constituents "MaterialConstituentSet" ("MINI SPLIT CONDENSER - REF. MECH. DWGS": "MINI SPLIT CONDENSER - REF. MECH. DWGS", "Color RGB 040-040-040": "Color RGB 040-040-040", "<Unnamed>": "<Unnamed>") | property sets: Pset_ManufacturerTypeInformation
  IFCBUILDINGELEMENTPROXYTYPE "4397245" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4397252" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4397358" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4397360" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4397379" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4397383" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4397407" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4397409" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4397413" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4397415" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4398212" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4398219" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4401982" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4401984" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4402004" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4402008" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4402040" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4402042" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4402046" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4402048" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4411108" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4411109" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4411111" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4411113" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4411115" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4411116" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4411121" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4411123" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4412291" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4412308" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4413181" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4413183" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4413185" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4413187" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4413203" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4413205" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4413207" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4413209" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4413216" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4413218" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4413220" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4413236" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4413240" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4413242" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4414297" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4414824" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4414826" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4414827" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4414828" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4414829" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4414830" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4414831" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4414832" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4414833" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4414834" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4414835" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4414836" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4414837" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4415168" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4415169" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4415170" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4415183" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4415184" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4415185" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4415732" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4415745" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4416242" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4416243" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4416244" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4416245" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4416246" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4416256" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4416257" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4416258" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4416259" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4416260" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4416263" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4416264" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4416265" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4416266" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4416267" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4416277" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4416278" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4416279" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4416280" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4416281" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4416525" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4416526" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4416527" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4416640" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4417253" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4417254" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4419410" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4419411" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4419782" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4419791" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4420943" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4420951" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4420955" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4420963" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "Heat_Pump_Unit-Multi_Zone-Outdoor-Daikin-2MXL18QMVJU:1.5Ton_2MXL18QMVJUA" | 10 occurrences | material: constituents "MaterialConstituentSet" ("blue": "blue", "BLACK": "BLACK", "<Unnamed>": "<Unnamed>", "Metal - Daikin - Copper": "Metal - Daikin - Copper", "Metal - Daikin - Paint Finish - Ivory White": "Metal - Daikin - Paint Finish - Ivory White") | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation
  IFCBUILDINGELEMENTPROXYTYPE "Heat_Pump_Unit-Multi_Zone-Outdoor-Daikin-2MXL18QMVJU:1.5Ton_2MXL18QMVJUA" | 2 occurrences | material: constituents "MaterialConstituentSet" ("blue": "blue", "BLACK": "BLACK", "<Unnamed>": "<Unnamed>", "Metal - Daikin - Copper": "Metal - Daikin - Copper", "Metal - Daikin - Paint Finish - Ivory White": "Metal - Daikin - Paint Finish - Ivory White") | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation
  IFCBUILDINGELEMENTPROXYTYPE "4454413" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4454414" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4454422" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4454423" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4475739" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4478034" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4494576" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4494577" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4494579" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4494581" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4494583" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4494587" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4494589" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4494590" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4495778" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4495792" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4496653" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4496655" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4496657" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4496659" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4496675" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4496677" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4496679" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4496681" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4496686" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4496688" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4496690" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4496692" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4496708" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4496710" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4496712" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4496714" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4537880" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4537881" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4538107" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "4538108" | 1 occurrence
  IFCALARMTYPE "104416 - Fire Extinguishers - Wall:Class A - Light - 2A" | 1 occurrence | material: constituents "MaterialConstituentSet" ("FIRE EXTINGUISHER": "FIRE EXTINGUISHER", "Metal - Paint Finish - Black, Matte": "Metal - Paint Finish - Black, Matte", "<Unnamed>": "<Unnamed>")
  IFCALARMTYPE "104416 - Fire Extinguishers - Wall:Class A - Light - 2A" | 1 occurrence | material: constituents "MaterialConstituentSet" ("FIRE EXTINGUISHER": "FIRE EXTINGUISHER", "Metal - Paint Finish - Black, Matte": "Metal - Paint Finish - Black, Matte", "<Unnamed>": "<Unnamed>")
  IFCBUILDINGELEMENTPROXYTYPE "Egress - Path of Travel:Egress - Path of Travel" | 1 occurrence | material: "<Unnamed>" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Egress - Path of Travel:Egress - Path of Travel" | 1 occurrence | material: "<Unnamed>" | property sets: Pset_BuildingElementProxyCommon

Property sets
  Pset_BuildingElementProxyCommon | properties | on 540 objects (540 IFCBUILDINGELEMENTPROXY)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 78 objects (78 IFCBUILDINGELEMENTPROXY)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Enscape AssetDefinition - Feather Reed Grass" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 73 objects (73 IFCBUILDINGELEMENTPROXY)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Enscape AssetDefinition - Feather Reed Grass 02" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 51 objects (51 IFCBUILDINGELEMENTPROXY)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "Structural Framing 1" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 41 objects (41 IFCBUILDINGELEMENTPROXY)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Enscape AssetDefinition - Deciduous Tree 143 Maple (autumn)" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 41 objects (41 IFCBUILDINGELEMENTPROXY)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Enscape AssetDefinition - Deciduous Tree 019 Coral Bark Maple (autumn)" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 28 objects (28 IFCBUILDINGELEMENTPROXY)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "Structural Framing 2" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 14 objects (14 IFCBUILDINGELEMENTPROXY)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Egress - Path of Travel" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon: 60 more contents on 166 objects not shown
  Pset_EnvironmentalImpactIndicators | properties | on 2525 objects (2525 IFCMEMBER)
    Reference = "Vertical Post" (IFCIDENTIFIER)
  Pset_EnvironmentalImpactIndicators | properties | on 924 objects (924 IFCPLATE)
    Reference = "Horizontal_Siding" (IFCIDENTIFIER)
  Pset_EnvironmentalImpactIndicators | properties | on 656 objects (656 IFCMEMBER)
    Reference = "RECTANGULAR - 1x4 SLAT" (IFCIDENTIFIER)
  Pset_EnvironmentalImpactIndicators | properties | on 540 objects (540 IFCBUILDINGELEMENTPROXY)
    Reference = "" (IFCIDENTIFIER)
  Pset_EnvironmentalImpactIndicators | properties | on 523 objects (523 IFCWALL)
    Reference = "Generic Models 1" (IFCIDENTIFIER)
  Pset_EnvironmentalImpactIndicators | properties | on 183 objects (183 IFCMEMBER)
    Reference = "HORSE POST" (IFCIDENTIFIER)
  Pset_EnvironmentalImpactIndicators | properties | on 156 objects (156 IFCMEMBER)
    Reference = "TOP RAIL" (IFCIDENTIFIER)
  Pset_EnvironmentalImpactIndicators | properties | on 142 objects (142 IFCPLATE)
    Reference = "HORSE FENCE SYSTEM" (IFCIDENTIFIER)
  Pset_EnvironmentalImpactIndicators: 329 more contents on 1916 objects not shown
  Pset_SiteCommon | properties | on 1 object (1 IFCSITE)
    Reference = "Project Information" (IFCIDENTIFIER)
  Pset_SiteCommon | properties | on 1 object (1 IFCSITE)
    Reference = "129313 - Bicycle" (IFCIDENTIFIER)
  Pset_SiteCommon | properties | on 1 object (1 IFCSITE)
    Reference = "In Ground" (IFCIDENTIFIER)
  Pset_SpaceCommon | properties | on 1 object (1 IFCSPACE)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "1BD-T1 - TYPE B 111" (IFCIDENTIFIER)
  Pset_SpaceCommon | properties | on 1 object (1 IFCSPACE)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "STUDIO - T2 - TYPE B 112" (IFCIDENTIFIER)
  Pset_SpaceCommon | properties | on 1 object (1 IFCSPACE)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "STUDIO - T1 - TYPE B 113" (IFCIDENTIFIER)
  Pset_SpaceCommon | properties | on 1 object (1 IFCSPACE)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "STUDIO - T1 - TYPE A 114" (IFCIDENTIFIER)
  Pset_SpaceCommon | properties | on 1 object (1 IFCSPACE)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "STUDIO - T2 - TYPE B 115" (IFCIDENTIFIER)
  Pset_SpaceCommon | properties | on 1 object (1 IFCSPACE)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "1BD - T1 - TYPE B 116" (IFCIDENTIFIER)
  Pset_SpaceCommon | properties | on 1 object (1 IFCSPACE)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "1BD-T1 121" (IFCIDENTIFIER)
  Pset_SpaceCommon | properties | on 1 object (1 IFCSPACE)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "STUDIO - T2 122" (IFCIDENTIFIER)
  Pset_SpaceCommon: 10 more contents on 10 objects not shown
  Pset_SpaceHeaterTypeCommon | properties | on 1 object (1 IFCSPACE)
    Reference = "1BD-T1 - TYPE B 111" (IFCIDENTIFIER)
  Pset_SpaceHeaterTypeCommon | properties | on 1 object (1 IFCSPACE)
    Reference = "STUDIO - T2 - TYPE B 112" (IFCIDENTIFIER)
  Pset_SpaceHeaterTypeCommon | properties | on 1 object (1 IFCSPACE)
    Reference = "STUDIO - T1 - TYPE B 113" (IFCIDENTIFIER)
  Pset_SpaceHeaterTypeCommon | properties | on 1 object (1 IFCSPACE)
    Reference = "STUDIO - T1 - TYPE A 114" (IFCIDENTIFIER)
  Pset_SpaceHeaterTypeCommon | properties | on 1 object (1 IFCSPACE)
    Reference = "STUDIO - T2 - TYPE B 115" (IFCIDENTIFIER)
  Pset_SpaceHeaterTypeCommon | properties | on 1 object (1 IFCSPACE)
    Reference = "1BD - T1 - TYPE B 116" (IFCIDENTIFIER)
  Pset_SpaceHeaterTypeCommon | properties | on 1 object (1 IFCSPACE)
    Reference = "1BD-T1 121" (IFCIDENTIFIER)
  Pset_SpaceHeaterTypeCommon | properties | on 1 object (1 IFCSPACE)
    Reference = "STUDIO - T2 122" (IFCIDENTIFIER)
  Pset_SpaceHeaterTypeCommon: 10 more contents on 10 objects not shown
  Pset_ReinforcementBarPitchOfWall | properties | on 523 objects (523 IFCWALL)
    Reference = "Generic Models 1" (IFCLABEL)
  Pset_ReinforcementBarPitchOfWall | properties | on 63 objects (63 IFCWALL)
    Reference = "Generic Models 65" (IFCLABEL)
  Pset_ReinforcementBarPitchOfWall | properties | on 57 objects (57 IFCWALL)
    Reference = "EXT 2 - corrugated metal" (IFCLABEL)
  Pset_ReinforcementBarPitchOfWall | properties | on 39 objects (39 IFCWALL)
    Reference = "Generic Models 263" (IFCLABEL)
  Pset_ReinforcementBarPitchOfWall | properties | on 39 objects (39 IFCWALL)
    Reference = "EXT 2 - corrugated metal at parapet" (IFCLABEL)
  Pset_ReinforcementBarPitchOfWall | properties | on 37 objects (37 IFCWALL)
    Reference = "EXT 1 - 1st floor base" (IFCLABEL)
  Pset_ReinforcementBarPitchOfWall | properties | on 36 objects (36 IFCWALL)
    Reference = "shaft" (IFCLABEL)
  Pset_ReinforcementBarPitchOfWall | properties | on 31 objects (31 IFCWALL)
    Reference = "EXT 2b - batten board" (IFCLABEL)
  Pset_ReinforcementBarPitchOfWall: 70 more contents on 196 objects not shown
  Pset_WallCommon | properties | on 523 objects (523 IFCWALL)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Generic Models 1" (IFCIDENTIFIER)
  Pset_WallCommon | properties | on 63 objects (63 IFCWALL)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Generic Models 65" (IFCIDENTIFIER)
  Pset_WallCommon | properties | on 50 objects (50 IFCWALL)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "EXT 2 - corrugated metal" (IFCIDENTIFIER)
    ThermalTransmittance = 40.9448818897638 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_WallCommon | properties | on 39 objects (39 IFCWALL)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Generic Models 263" (IFCIDENTIFIER)
  Pset_WallCommon | properties | on 36 objects (36 IFCWALL)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "shaft" (IFCIDENTIFIER)
  Pset_WallCommon | properties | on 35 objects (35 IFCWALL)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "EXT 2 - corrugated metal at parapet" (IFCIDENTIFIER)
  Pset_WallCommon | properties | on 33 objects (33 IFCWALL)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "EXT 1 - 1st floor base" (IFCIDENTIFIER)
    ThermalTransmittance = 40.9448818897638 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_WallCommon | properties | on 27 objects (27 IFCWALL)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "EXT 2b - batten board" (IFCIDENTIFIER)
    ThermalTransmittance = 40.9448818897638 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_WallCommon: 96 more contents on 215 objects not shown
  Pset_BeamCommon | properties | on 6 objects (6 IFCBEAM)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "TREATED 2X10 - JOIST" (IFCIDENTIFIER)
    Roll = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Slope = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Span = 6.87500000000004 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
  Pset_BeamCommon | properties | on 4 objects (4 IFCBEAM)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "TREATED 2X10 - JOIST" (IFCIDENTIFIER)
    Roll = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Slope = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Span = 6.87500000000006 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
  Pset_BeamCommon | properties | on 4 objects (4 IFCBEAM)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "6x6 - LATERAL BRACING" (IFCIDENTIFIER)
    Roll = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Slope = 45. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Span = 2.82800000000002 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
  Pset_BeamCommon | properties | on 2 objects (2 IFCBEAM)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "2x8" (IFCIDENTIFIER)
    Roll = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Slope = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Span = 8. (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
  Pset_BeamCommon | properties | on 2 objects (2 IFCBEAM)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "2x10 - BEAM" (IFCIDENTIFIER)
    Roll = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Slope = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Span = 17.8103042826558 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
  Pset_BeamCommon | properties | on 1 object (1 IFCBEAM)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "2x10 - RIM JOIST" (IFCIDENTIFIER)
    Roll = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Slope = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Span = 6.87500000000009 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
  Pset_BeamCommon | properties | on 1 object (1 IFCBEAM)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "2x10 - RIM JOIST" (IFCIDENTIFIER)
    Roll = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Slope = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Span = 6.87500000000007 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
  Pset_BeamCommon | properties | on 1 object (1 IFCBEAM)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "2x10 - RIM JOIST" (IFCIDENTIFIER)
    Roll = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Slope = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Span = 17.875 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
  Pset_BeamCommon: 27 more contents on 26 objects not shown
  Pset_ReinforcementBarPitchOfBeam | properties | on 14 objects (14 IFCBEAM)
    Reference = "TREATED 2X10 - JOIST" (IFCLABEL)
  Pset_ReinforcementBarPitchOfBeam | properties | on 4 objects (4 IFCBEAM)
    Reference = "2x10 - RIM JOIST" (IFCLABEL)
  Pset_ReinforcementBarPitchOfBeam | properties | on 4 objects (4 IFCBEAM)
    Reference = "2x10 - BEAM" (IFCLABEL)
  Pset_ReinforcementBarPitchOfBeam | properties | on 4 objects (4 IFCBEAM)
    Reference = "6x6 - LATERAL BRACING" (IFCLABEL)
  Pset_ReinforcementBarPitchOfBeam | properties | on 2 objects (2 IFCBEAM)
    Reference = "2x8" (IFCLABEL)
  Pset_ReinforcementBarPitchOfBeam | properties | on 2 objects (2 IFCBEAM)
    Reference = "2x10 - LEDGER" (IFCLABEL)
  Pset_ReinforcementBarPitchOfBeam | properties | on 2 objects (2 IFCBEAM)
    Reference = "C CHANNEL - SIZE TBD1" (IFCLABEL)
  Pset_ReinforcementBarPitchOfBeam | properties | on 1 object (1 IFCBEAM)
    Reference = "LVL - 1 3/4" X 9 1/4"" (IFCLABEL)
  Pset_ReinforcementBarPitchOfBeam: 15 more contents on 14 objects not shown
  Pset_CurtainWallCommon | properties | on 33 objects (33 IFCCURTAINWALL)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "HORSE 3" (IFCIDENTIFIER)
  Pset_CurtainWallCommon | properties | on 14 objects (14 IFCCURTAINWALL)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "SLOTTED WOOD FENCE" (IFCIDENTIFIER)
  Pset_CurtainWallCommon | properties | on 13 objects (13 IFCCURTAINWALL)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "EMPTY - MULLION AND PANEL" (IFCIDENTIFIER)
  Pset_CurtainWallCommon | properties | on 6 objects (6 IFCCURTAINWALL)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "STOREFRONT - 2"x6"" (IFCIDENTIFIER)
  Pset_CurtainWallCommon | properties | on 4 objects (4 IFCCURTAINWALL)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "sloped slats" (IFCIDENTIFIER)
  Pset_CurtainWallCommon | properties | on 3 objects (3 IFCCURTAINWALL)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "STOREFRONT - BUTT-GLAZED" (IFCIDENTIFIER)
  Pset_CurtainWallCommon | properties | on 2 objects (2 IFCCURTAINWALL)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "posts only" (IFCIDENTIFIER)
  Pset_CurtainWallCommon | properties | on 1 object (1 IFCCURTAINWALL)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "FRAMELESS GLASS" (IFCIDENTIFIER)
  Pset_CurtainWallCommon: 9 more contents on 7 objects not shown
  Pset_PlateCommon | properties | on 924 objects (924 IFCPLATE)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Horizontal_Siding" (IFCIDENTIFIER)
  Pset_PlateCommon | properties | on 142 objects (142 IFCPLATE)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "HORSE FENCE SYSTEM" (IFCIDENTIFIER)
  Pset_PlateCommon | properties | on 19 objects (19 IFCPLATE)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "3/4" GLAZING" (IFCIDENTIFIER)
  Pset_PlateCommon | properties | on 5 objects (5 IFCPLATE)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "one" (IFCIDENTIFIER)
  Pset_PlateCommon | properties | on 3 objects (3 IFCPLATE)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "1/4" GLAZING - IN HOLLOW METAL FRAME" (IFCIDENTIFIER)
  Pset_MemberCommon | properties | on 1548 objects (1548 IFCMEMBER)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Vertical Post" (IFCIDENTIFIER)
    Span = 0.416666666666667 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
  Pset_MemberCommon | properties | on 472 objects (472 IFCMEMBER)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "RECTANGULAR - 1x4 SLAT" (IFCIDENTIFIER)
    Span = 2.66666666666672 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
  Pset_MemberCommon | properties | on 456 objects (456 IFCMEMBER)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Vertical Post" (IFCIDENTIFIER)
    Span = 0.416666666666668 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
  Pset_MemberCommon | properties | on 173 objects (173 IFCMEMBER)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Vertical Post" (IFCIDENTIFIER)
    Span = 0.416666666666671 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
  Pset_MemberCommon | properties | on 172 objects (172 IFCMEMBER)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Vertical Post" (IFCIDENTIFIER)
    Span = 0.416666666666666 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
  Pset_MemberCommon | properties | on 45 objects (45 IFCMEMBER)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Vertical Post" (IFCIDENTIFIER)
    Span = 0.328244189259642 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
  Pset_MemberCommon | properties | on 36 objects (36 IFCMEMBER)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "HORSE POST" (IFCIDENTIFIER)
    Span = 5.6666666666662 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
  Pset_MemberCommon | properties | on 32 objects (32 IFCMEMBER)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Vertical Post" (IFCIDENTIFIER)
    Span = 0.416666666666664 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
  Pset_MemberCommon: 240 more contents on 730 objects not shown
  Pset_FurnitureTypeCommon | properties | on 29 objects (29 IFCFURNITURE)
    Reference = "Type 1" (IFCIDENTIFIER)
  Pset_FurnitureTypeCommon | properties | on 10 objects (10 IFCFURNITURE)
    Reference = "Lounge Chair" (IFCIDENTIFIER)
  Pset_FurnitureTypeCommon | properties | on 8 objects (8 IFCFURNITURE)
    Reference = "1" (IFCIDENTIFIER)
  Pset_FurnitureTypeCommon | properties | on 8 objects (8 IFCFURNITURE)
    Reference = "38,25" w x 27,5" d x 15" h 2" (IFCIDENTIFIER)
  Pset_FurnitureTypeCommon | properties | on 7 objects (7 IFCFURNITURE)
    Reference = "Lounge Settee 2" (IFCIDENTIFIER)
  Pset_FurnitureTypeCommon | properties | on 3 objects (3 IFCFURNITURE)
    Reference = "36"" (IFCIDENTIFIER)
  Pset_FurnitureTypeCommon | properties | on 3 objects (3 IFCFURNITURE)
    Reference = "30"" (IFCIDENTIFIER)
  Pset_FurnitureTypeCommon | properties | on 2 objects (2 IFCFURNITURE)
    Reference = "OD_CW_Closet" (IFCIDENTIFIER)
  Pset_FurnitureTypeCommon: 37 more contents on 39 objects not shown
  Pset_FootingCommon | properties | on 2 objects (2 IFCFOOTING)
    Reference = "12"X24"" (IFCIDENTIFIER)
  Pset_ReinforcementBarCountOfIndependentFooting | properties | on 2 objects (2 IFCFOOTING)
    Reference = "12"X24"" (IFCLABEL)
  Pset_ReinforcementBarPitchOfContinuousFooting | properties | on 2 objects (2 IFCFOOTING)
    Reference = "12"X24"" (IFCLABEL)
  Pset_ReinforcementBarPitchOfSlab | properties | on 13 objects (13 IFCSLAB)
    Reference = "FLOOR TRUSS" (IFCLABEL)
  Pset_ReinforcementBarPitchOfSlab | properties | on 5 objects (5 IFCSLAB)
    Reference = "316600 - Special Foundations - Diamond Pier - Generic" (IFCLABEL)
  Pset_ReinforcementBarPitchOfSlab | properties | on 4 objects (4 IFCSLAB)
    Reference = "20"WX42"D" (IFCLABEL)
  Pset_ReinforcementBarPitchOfSlab | properties | on 4 objects (4 IFCSLAB)
    Reference = "balc floor" (IFCLABEL)
  Pset_ReinforcementBarPitchOfSlab | properties | on 3 objects (3 IFCSLAB)
    Reference = "sloped roof" (IFCLABEL)
  Pset_ReinforcementBarPitchOfSlab | properties | on 2 objects (2 IFCSLAB)
    Reference = "6" COMPACTED CRUSHED STONE" (IFCLABEL)
  Pset_ReinforcementBarPitchOfSlab | properties | on 2 objects (2 IFCSLAB)
    Reference = "Non-Monolithic Landing" (IFCLABEL)
  Pset_ReinforcementBarPitchOfSlab | properties | on 1 object (1 IFCSLAB)
    Reference = "6" Foundation Slab" (IFCLABEL)
  Pset_ReinforcementBarPitchOfSlab: 14 more contents on 13 objects not shown
  Pset_SlabCommon | properties | on 13 objects (13 IFCSLAB)
    FireRating = "1" (IFCLABEL)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    PitchAngle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Reference = "FLOOR TRUSS" (IFCIDENTIFIER)
    ThermalTransmittance = 18.6113099498926 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_SlabCommon | properties | on 4 objects (4 IFCSLAB)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "316600 - Special Foundations - Diamond Pier - Generic" (IFCIDENTIFIER)
  Pset_SlabCommon | properties | on 4 objects (4 IFCSLAB)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    PitchAngle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Reference = "balc floor" (IFCIDENTIFIER)
  Pset_SlabCommon | properties | on 3 objects (3 IFCSLAB)
    IsExternal = TRUE (IFCBOOLEAN)
    PitchAngle = 18.434948822922 (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Reference = "sloped roof" (IFCIDENTIFIER)
    ThermalTransmittance = 78.7401574803149 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_SlabCommon | properties | on 2 objects (2 IFCSLAB)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    PitchAngle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Reference = "6" COMPACTED CRUSHED STONE" (IFCIDENTIFIER)
  Pset_SlabCommon | properties | on 2 objects (2 IFCSLAB)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "20"WX42"D" (IFCIDENTIFIER)
  Pset_SlabCommon | properties | on 2 objects (2 IFCSLAB)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Non-Monolithic Landing" (IFCIDENTIFIER)
  Pset_SlabCommon | properties | on 2 objects (2 IFCSLAB)
    IsExternal = FALSE (IFCBOOLEAN)
    PitchAngle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Reference = "20"WX42"D" (IFCIDENTIFIER)
  Pset_SlabCommon: 21 more contents on 15 objects not shown
  Pset_ColumnCommon | properties | on 3 objects (3 IFCCOLUMN)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "6x6" (IFCIDENTIFIER)
    Slope = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
  Pset_ColumnCommon | properties | on 3 objects (3 IFCCOLUMN)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "6x6" (IFCIDENTIFIER)
  Pset_ColumnCommon | properties | on 2 objects (2 IFCCOLUMN)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "HSS - 3.5" - SIZE TBD" (IFCIDENTIFIER)
  Pset_ColumnCommon | properties | on 1 object (1 IFCCOLUMN)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "HSS 3.5" - SIZE TBD" (IFCIDENTIFIER)
  Pset_ColumnCommon | properties | on 1 object (1 IFCCOLUMN)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "TUBE STEEL (HDG) - SIZE TBD" (IFCIDENTIFIER)
  Pset_ColumnCommon | properties | on 1 object (1 IFCCOLUMN)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "HSS 6" - SIZE TBD" (IFCIDENTIFIER)
  Pset_ColumnCommon | properties | on 1 object (1 IFCCOLUMN)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "4X4" (IFCIDENTIFIER)
  Pset_ColumnCommon | properties | on 1 object (1 IFCCOLUMN)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "(3) 2X6 - BUILT-UP COLUMN" (IFCIDENTIFIER)
  Pset_ColumnCommon: 7 more contents on 6 objects not shown
  Pset_ReinforcementBarPitchOfColumn | properties | on 6 objects (6 IFCCOLUMN)
    Reference = "6x6" (IFCLABEL)
  Pset_ReinforcementBarPitchOfColumn | properties | on 2 objects (2 IFCCOLUMN)
    Reference = "HSS - 3.5" - SIZE TBD" (IFCLABEL)
  Pset_ReinforcementBarPitchOfColumn | properties | on 1 object (1 IFCCOLUMN)
    Reference = "HSS 3.5" - SIZE TBD" (IFCLABEL)
  Pset_ReinforcementBarPitchOfColumn | properties | on 1 object (1 IFCCOLUMN)
    Reference = "TUBE STEEL (HDG) - SIZE TBD" (IFCLABEL)
  Pset_ReinforcementBarPitchOfColumn | properties | on 1 object (1 IFCCOLUMN)
    Reference = "HSS 6" - SIZE TBD" (IFCLABEL)
  Pset_ReinforcementBarPitchOfColumn | properties | on 1 object (1 IFCCOLUMN)
    Reference = "4X4" (IFCLABEL)
  Pset_ReinforcementBarPitchOfColumn | properties | on 1 object (1 IFCCOLUMN)
    Reference = "(3) 2X6 - BUILT-UP COLUMN" (IFCLABEL)
  Pset_ReinforcementBarPitchOfColumn | properties | on 1 object (1 IFCCOLUMN)
    Reference = "(3) 2X4 - BUILT-UP COLUMN" (IFCLABEL)
  Pset_ReinforcementBarPitchOfColumn: 5 more contents on 5 objects not shown
  Pset_ManufacturerTypeInformation | properties | on 194 objects (105 IFCBUILDINGELEMENTPROXY, 87 IFCOPENINGELEMENT, 2 IFCDOOR) | on 61 type objects
    Manufacturer = "Andersen Corporation" (IFCLABEL)
  Pset_ManufacturerTypeInformation | properties | on 31 objects (31 IFCFURNITURE) | on 4 type objects
    Manufacturer = "Herman Miller, Inc." (IFCLABEL)
  Pset_ManufacturerTypeInformation | properties | on 21 objects (21 IFCBUILDINGELEMENTPROXY) | on 4 type objects
    Manufacturer = "Daikin" (IFCLABEL)
  Pset_ManufacturerTypeInformation | properties | on 20 objects (20 IFCFURNITURE) | on 8 type objects
    Manufacturer = "StudioTK" (IFCLABEL)
  Pset_ManufacturerTypeInformation | properties | on 18 objects (18 IFCPUMP) | on 2 type objects
    Manufacturer = "FUJITSU GENERAL LIMITED" (IFCLABEL)
  Pset_ManufacturerTypeInformation | properties | on 13 objects (13 IFCSLAB) | on 13 type objects
    Manufacturer = "United States Gypsum Company" (IFCLABEL)
  Pset_ManufacturerTypeInformation | properties | on 13 objects (13 IFCFURNITURE) | on 6 type objects
    Manufacturer = "Teknion Studio" (IFCLABEL)
  Pset_ManufacturerTypeInformation | properties | on 12 objects (12 IFCFURNITURE) | on 12 type objects
    Manufacturer = "Woodwork Institute" (IFCLABEL)
  Pset_ManufacturerTypeInformation: 13 more contents on 31 objects not shown
  Pset_OpeningElementCommon | properties | on 51 objects (26 IFCOPENINGELEMENT, 25 IFCBUILDINGELEMENTPROXY)
    Reference = "SINGLE HUNG - TYPE 2" (IFCIDENTIFIER)
  Pset_OpeningElementCommon | properties | on 45 objects (23 IFCOPENINGELEMENT, 22 IFCBUILDINGELEMENTPROXY)
    Reference = "SINGLE HUNG - TYPE 1" (IFCIDENTIFIER)
  Pset_OpeningElementCommon | properties | on 40 objects (20 IFCBUILDINGELEMENTPROXY, 20 IFCOPENINGELEMENT)
    Reference = "FIXED PICTURE - TYPE 1" (IFCIDENTIFIER)
  Pset_OpeningElementCommon | properties | on 24 objects (24 IFCOPENINGELEMENT)
    Reference = "Generic Models 65" (IFCIDENTIFIER)
  Pset_OpeningElementCommon | properties | on 21 objects (11 IFCOPENINGELEMENT, 10 IFCBUILDINGELEMENTPROXY)
    Reference = "SINGLE HUNG - TYPE 2 - TEMPERED" (IFCIDENTIFIER)
  Pset_OpeningElementCommon | properties | on 12 objects (6 IFCALARM, 6 IFCOPENINGELEMENT)
    Reference = "Class A - Light - 2A" (IFCIDENTIFIER)
  Pset_OpeningElementCommon | properties | on 6 objects (6 IFCOPENINGELEMENT)
    Reference = "RATED - 0.5 HR" (IFCIDENTIFIER)
  Pset_OpeningElementCommon | properties | on 4 objects (2 IFCBUILDINGELEMENTPROXY, 2 IFCOPENINGELEMENT)
    Reference = "_Type Name_" (IFCIDENTIFIER)
  Pset_OpeningElementCommon: 11 more contents on 23 objects not shown
  Pset_DoorCommon | properties | on 29 objects (29 IFCDOOR)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "SINGLE - LITE - MUNTINS - 3-0 x 6-8" (IFCIDENTIFIER)
  Pset_DoorCommon | properties | on 7 objects (7 IFCDOOR)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "SINGLE - FLUSH - 3-0 x 6-8" (IFCIDENTIFIER)
  Pset_DoorCommon | properties | on 2 objects (2 IFCDOOR)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "_Type Name_" (IFCIDENTIFIER)
  Pset_DoorCommon | properties | on 1 object (1 IFCDOOR)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "ALL GLASS DOOR W/ PATCH FITTINGS" (IFCIDENTIFIER)
  Pset_DoorCommon | properties | on 1 object (1 IFCDOOR)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Store Front Double Door" (IFCIDENTIFIER)
  Pset_DoorCommon | properties | on 1 object (1 IFCDOOR)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "WOOD DOOR W/ GLASS INSET" (IFCIDENTIFIER)
  Pset_DoorCommon | properties | on 1 object (1 IFCDOOR)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "3x7" (IFCIDENTIFIER)
  Pset_DoorCommon | properties | on 1 object (1 IFCDOOR)
    FireRating = "0HR" (IFCLABEL)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "DOUBLE - FLUSH - 6-0 x 6-8" (IFCIDENTIFIER)
  Pset_DoorCommon: 7 more contents on 3 objects not shown
  Pset_RoofCommon | properties | on 6 objects (6 IFCROOF)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "WOOD-FRAMED ROOF ABOVE 3RD FLOOR" (IFCIDENTIFIER)
    ThermalTransmittance = 40.9448818897638 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_RoofCommon | properties | on 6 objects (6 IFCROOF)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "CRICKETS" (IFCIDENTIFIER)
  Pset_RoofCommon | properties | on 3 objects (3 IFCROOF)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "SOFFIT" (IFCIDENTIFIER)
  Pset_RoofCommon | properties | on 2 objects (2 IFCROOF)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "Generic - 12"" (IFCIDENTIFIER)
  Pset_RoofCommon | properties | on 1 object (1 IFCROOF)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "STANDING SEAM - FOAM - GYP" (IFCIDENTIFIER)
    ThermalTransmittance = 7.17567636082909 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_RoofCommon | properties | on 1 object (1 IFCROOF)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "Sloped Glazing" (IFCIDENTIFIER)
  Pset_RoofCommon | properties | on 1 object (1 IFCROOF)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "STANDING SEAM - RAFTER" (IFCIDENTIFIER)
    ThermalTransmittance = 0.784794660132001 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_RoofCommon | properties | on 1 object (1 IFCROOF)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "SHINGLES - FOAM - GYP" (IFCIDENTIFIER)
    ThermalTransmittance = 6.57636504726417 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_RoofCommon: 5 more contents on 3 objects not shown
  Pset_DuctSegmentTypeCommon | properties | on 5 objects (5 IFCDUCTSEGMENT)
    Reference = "Default" (IFCIDENTIFIER)
  Pset_DuctSegmentTypeCommon | properties | on 5 objects (5 IFCDUCTSEGMENT)
    Reference = "Default" (IFCIDENTIFIER)
    Shape in {"Round"} (IFCLABEL)
  Pset_DuctFittingTypeCommon | properties | on 4 objects (4 IFCDUCTFITTING)
    Reference = "Standard" (IFCIDENTIFIER)
  Pset_DuctFittingTypeCommon | properties | on 1 object (1 IFCDUCTFITTING)
    Reference = "1.5 W" (IFCIDENTIFIER)
  Pset_DuctFittingTypeCommon | properties | on 1 object (1 IFCDUCTFITTING)
    Reference = "1.5 D" (IFCIDENTIFIER)
  Pset_StairCommon | properties | on 1 object (1 IFCSTAIR)
    IsExternal = FALSE (IFCBOOLEAN)
    NosingLength = 0.0833333333333333 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    NumberOfRiser = 20. (IFCCOUNTMEASURE)
    NumberOfTreads = 18. (IFCCOUNTMEASURE)
    Reference = "C CHANNEL STRINGER" (IFCIDENTIFIER)
    RiserHeight = 0.569444444444434 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
    TreadLength = 0.916666666666667 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
    TreadLengthAtInnerSide = 0.916666666666667 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
    TreadLengthAtOffset = 0.916666666666667 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
    WalkingLineOffset = 2.02604166666595 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
  Pset_StairCommon | properties | on 1 object (1 IFCSTAIR)
    IsExternal = FALSE (IFCBOOLEAN)
    NosingLength = 0.0833333333333333 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    NumberOfRiser = 20. (IFCCOUNTMEASURE)
    NumberOfTreads = 18. (IFCCOUNTMEASURE)
    Reference = "C CHANNEL STRINGER" (IFCIDENTIFIER)
    RiserHeight = 0.564393939393931 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
    TreadLength = 0.916666666666667 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
    TreadLengthAtInnerSide = 0.916666666666667 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
    TreadLengthAtOffset = 0.916666666666667 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
    WalkingLineOffset = 2.02604166666595 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
  Pset_StairCommon | properties | on 1 object (1 IFCSTAIR)
    IsExternal = FALSE (IFCBOOLEAN)
    NosingLength = 0.0625 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    NumberOfRiser = 20. (IFCCOUNTMEASURE)
    NumberOfTreads = 18. (IFCCOUNTMEASURE)
    Reference = "Monolithic Stair" (IFCIDENTIFIER)
    RiserHeight = 0.569444444444434 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
    TreadLength = 0.916666666666667 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
    TreadLengthAtInnerSide = 0.916666666666667 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
    TreadLengthAtOffset = 0.916666666666667 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
    WalkingLineOffset = 2.02604166666595 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
  Pset_StairCommon | properties | on 1 object (1 IFCSTAIR)
    IsExternal = FALSE (IFCBOOLEAN)
    NosingLength = 0.0625 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    NumberOfRiser = 20. (IFCCOUNTMEASURE)
    NumberOfTreads = 18. (IFCCOUNTMEASURE)
    Reference = "Precast Stair" (IFCIDENTIFIER)
    RiserHeight = 0.569444444444434 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
    TreadLength = 0.916666666666667 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
    TreadLengthAtInnerSide = 0.916666666666667 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
    TreadLengthAtOffset = 0.916666666666667 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
    WalkingLineOffset = 2.02604166666595 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
  Pset_StairCommon | properties | on 4 type objects
    IsExternal = FALSE (IFCBOOLEAN)
    NosingLength = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    NumberOfRiser = 0. (IFCCOUNTMEASURE)
    NumberOfTreads = 0. (IFCCOUNTMEASURE)
  Pset_StairFlightCommon | properties | on 1 object (1 IFCSTAIR)
    NosingLength = 0.0833333333333333 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    NumberOfRiser = 20. (IFCCOUNTMEASURE)
    NumberOfTreads = 18. (IFCCOUNTMEASURE)
    Reference = "C CHANNEL STRINGER" (IFCIDENTIFIER)
    RiserHeight = 0.569444444444434 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
    TreadLength = 0.916666666666667 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
    TreadLengthAtInnerSide = 0.916666666666667 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
    TreadLengthAtOffset = 0.916666666666667 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
    WalkingLineOffset = 2.02604166666595 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
  Pset_StairFlightCommon | properties | on 1 object (1 IFCSTAIRFLIGHT)
    NosingLength = 0.0833333333333333 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    NumberOfRiser = 10. (IFCCOUNTMEASURE)
    NumberOfTreads = 9. (IFCCOUNTMEASURE)
    Reference = "Aalseth" (IFCIDENTIFIER)
    RiserHeight = 0.569444444444434 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
    TreadLength = 0.916666666666667 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
    TreadLengthAtInnerSide = 0.916666666666667 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
    TreadLengthAtOffset = 0.916666666666667 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
    WalkingLineOffset = 2.02604166666595 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
  Pset_StairFlightCommon | properties | on 1 object (1 IFCSTAIRFLIGHT)
    NosingLength = 0.0833333333333333 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    NumberOfRiser = 10. (IFCCOUNTMEASURE)
    NumberOfTreads = 9. (IFCCOUNTMEASURE)
    Reference = "Aalseth" (IFCIDENTIFIER)
    RiserHeight = 0.569444444444434 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
    TreadLength = 0.916666666666667 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
    TreadLengthAtInnerSide = 0.916666666666667 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
    TreadLengthAtOffset = 0.916666666666667 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
    WalkingLineOffset = 2.02604166666566 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
  Pset_StairFlightCommon | properties | on 1 object (1 IFCSTAIR)
    NosingLength = 0.0833333333333333 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    NumberOfRiser = 20. (IFCCOUNTMEASURE)
    NumberOfTreads = 18. (IFCCOUNTMEASURE)
    Reference = "C CHANNEL STRINGER" (IFCIDENTIFIER)
    RiserHeight = 0.564393939393931 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
    TreadLength = 0.916666666666667 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
    TreadLengthAtInnerSide = 0.916666666666667 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
    TreadLengthAtOffset = 0.916666666666667 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
    WalkingLineOffset = 2.02604166666595 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
  Pset_StairFlightCommon | properties | on 1 object (1 IFCSTAIRFLIGHT)
    NosingLength = 0.0833333333333333 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    NumberOfRiser = 10. (IFCCOUNTMEASURE)
    NumberOfTreads = 9. (IFCCOUNTMEASURE)
    Reference = "Aalseth" (IFCIDENTIFIER)
    RiserHeight = 0.564393939393931 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
    TreadLength = 0.916666666666667 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
    TreadLengthAtInnerSide = 0.916666666666667 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
    TreadLengthAtOffset = 0.916666666666667 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
    WalkingLineOffset = 2.02604166666595 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
  Pset_StairFlightCommon | properties | on 1 object (1 IFCSTAIRFLIGHT)
    NosingLength = 0.0833333333333333 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    NumberOfRiser = 10. (IFCCOUNTMEASURE)
    NumberOfTreads = 9. (IFCCOUNTMEASURE)
    Reference = "Aalseth" (IFCIDENTIFIER)
    RiserHeight = 0.564393939393931 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
    TreadLength = 0.916666666666667 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
    TreadLengthAtInnerSide = 0.916666666666667 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
    TreadLengthAtOffset = 0.916666666666667 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
    WalkingLineOffset = 2.02604166666566 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
  Pset_StairFlightCommon | properties | on 1 object (1 IFCSTAIR)
    NosingLength = 0.0625 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    NumberOfRiser = 20. (IFCCOUNTMEASURE)
    NumberOfTreads = 18. (IFCCOUNTMEASURE)
    Reference = "Monolithic Stair" (IFCIDENTIFIER)
    RiserHeight = 0.569444444444434 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
    TreadLength = 0.916666666666667 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
    TreadLengthAtInnerSide = 0.916666666666667 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
    TreadLengthAtOffset = 0.916666666666667 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
    WalkingLineOffset = 2.02604166666595 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
  Pset_StairFlightCommon | properties | on 1 object (1 IFCSTAIRFLIGHT)
    NosingLength = 0.0625 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    NumberOfRiser = 10. (IFCCOUNTMEASURE)
    NumberOfTreads = 9. (IFCCOUNTMEASURE)
    Reference = "3/4" Nosing" (IFCIDENTIFIER)
    RiserHeight = 0.569444444444434 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
    TreadLength = 0.916666666666667 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
    TreadLengthAtInnerSide = 0.916666666666667 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
    TreadLengthAtOffset = 0.916666666666667 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
    WalkingLineOffset = 2.02604166666595 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
  Pset_StairFlightCommon: 5 more contents on 4 objects not shown
  Pset_CoveringCommon | properties | on 5 objects (5 IFCCOVERING)
    Finish = "5/8" GYP. BD;" (IFCTEXT)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "GYP. BD - HUNG" (IFCIDENTIFIER)
    ThermalTransmittance = 40.9448818897638 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_CoveringCommon | properties | on 2 objects (2 IFCCOVERING)
    Finish = "2X2 ACOUSTICAL TILE;" (IFCTEXT)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "ACT - 2X2" (IFCIDENTIFIER)
  Pset_CoveringCommon | properties | on 1 object (1 IFCCOVERING)
    Finish = "DEMO ACOUSTICAL TILE;" (IFCTEXT)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "ACT - 2X2 - DEMO" (IFCIDENTIFIER)
    ThermalTransmittance = 3.59055118110236 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_CoveringCommon | properties | on 1 object (1 IFCCOVERING)
    Finish = "1X4 ACOUSTICAL TILE;" (IFCTEXT)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "ACT - 1X4" (IFCIDENTIFIER)
  Pset_CoveringCommon | properties | on 1 object (1 IFCCOVERING)
    Finish = "5/8" GYP. BD;" (IFCTEXT)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "GYP. BD - CEILING JOIST" (IFCIDENTIFIER)
    ThermalTransmittance = 0.841333189515694 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_CoveringCommon | properties | on 1 object (1 IFCCOVERING)
    Finish = "SOFFIT;" (IFCTEXT)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "SOFFIT" (IFCIDENTIFIER)
    ThermalTransmittance = 0.85898353614889 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_CoveringCommon | properties | on 5 type objects
    IsExternal = FALSE (IFCBOOLEAN)
    ThermalTransmittance = 40.9448818897638 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_CoveringCommon | properties | on 3 type objects
    IsExternal = FALSE (IFCBOOLEAN)
  Pset_CoveringCommon: 3 more contents on 0 objects not shown
  Pset_LightFixtureTypeCommon | properties | on 4 objects (4 IFCLIGHTFIXTURE)
    Reference = "2' x 4' (2 Lamps)" (IFCIDENTIFIER)
  Pset_LightFixtureTypeCommon | properties | on 2 objects (2 IFCLIGHTFIXTURE)
    Reference = "2' x 2' (2 Lamps)" (IFCIDENTIFIER)
  Pset_LightFixtureTypeCommon | properties | on 1 object (1 IFCLIGHTFIXTURE)
    Reference = "2' x 4' - 2 Lamp" (IFCIDENTIFIER)
  Pset_LightFixtureTypeCommon | properties | on 1 object (1 IFCLIGHTFIXTURE)
    Reference = "Not a Type - Load Type Catalog" (IFCIDENTIFIER)
  Pset_ElectricalDeviceCommon | properties | on 1 object (1 IFCLIGHTFIXTURE) | on 1 type object
    NumberOfPoles = 1 (IFCINTEGER)
    PowerFactor = 1. (IFCNORMALISEDRATIOMEASURE)
  Pset_ElectricalDeviceCommon | properties | on 1 object (1 IFCFLOWTERMINAL) | on 1 type object
    NumberOfPoles = 1 (IFCINTEGER)
  Pset_PumpTypeCommon | properties | on 18 objects (18 IFCPUMP)
    Reference = "AOYG22KATA" (IFCIDENTIFIER)
  Pset_PipeSegmentOccurrence | properties | on 24 objects (24 IFCPIPESEGMENT)
    InvertElevation = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Pset_PipeSegmentOccurrence | properties | on 6 objects (6 IFCPIPESEGMENT)
    InvertElevation = 7.45791646311025 (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Pset_PipeSegmentTypeCommon | properties | on 30 objects (30 IFCPIPESEGMENT)
    Reference = "Default" (IFCIDENTIFIER)
  Pset_RailingCommon | properties | on 13 objects (13 IFCRAILING)
    Height = 3. (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "HANDRAIL W/ BRACKETS" (IFCIDENTIFIER)
  Pset_RailingCommon | properties | on 9 objects (9 IFCRAILING)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Railings 1" (IFCIDENTIFIER)
  Pset_RailingCommon | properties | on 1 object (1 IFCRAILING)
    Height = 3. (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "VERTICAL PICKETS - DRINK RAIL" (IFCIDENTIFIER)
  Pset_RailingCommon | properties | on 1 object (1 IFCRAILING)
    Height = 3.49479166666667 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "VERTICAL PICKETS - 2 HORZ - RECT TOP" (IFCIDENTIFIER)
  Pset_RailingCommon | properties | on 1 object (1 IFCRAILING)
    Height = 4. (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "GUARDRAIL - PIPES" (IFCIDENTIFIER)
  Pset_RailingCommon | properties | on 1 object (1 IFCRAILING)
    Height = 4. (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "GUARDRAIL - PIPES W/ EXTENSIONS" (IFCIDENTIFIER)
  Pset_RailingCommon | properties | on 1 object (1 IFCRAILING)
    Height = 4. (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "VERTICAL PICKETS - RECT TOP" (IFCIDENTIFIER)
  Pset_RailingCommon | properties | on 1 object (1 IFCRAILING)
    Height = 4. (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "GUARDRAIL - TOP ONLY" (IFCIDENTIFIER)
  Pset_RailingCommon: 3 more contents on 2 objects not shown
  Pset_BuildingStoreyCommon | properties | on 4 objects (4 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
    Reference = "Project Base Point" (IFCIDENTIFIER)
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDING)
    AboveGround = UNKNOWN (IFCLOGICAL)
    Reference = "Project Information" (IFCIDENTIFIER)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    IsLandmarked = UNKNOWN (IFCLOGICAL)
    NumberOfStoreys = 4 (IFCINTEGER)
    Reference = "Project Information" (IFCIDENTIFIER)
  Pset_BuildingSystemCommon | properties | on 1 object (1 IFCBUILDING)
    Reference = "Project Information" (IFCIDENTIFIER)
  OD_SINGLE:SINGLE - LITE - MUNTINS - 3-0 x 6-8:2169410 | predefined | on 1 type object
  OD_SINGLE:SINGLE - LITE - MUNTINS - 3-0 x 6-8:2169410:1 | predefined | on 1 type object
  OD_SINGLE:SINGLE - FLUSH - 3-0 x 6-8:2170758 | predefined | on 1 type object
  OD_SINGLE:SINGLE - FLUSH - 3-0 x 6-8:2170758:1 | predefined | on 1 type object
  Simple Opening:3x7:2460090 | predefined | on 1 type object
  Simple Opening:3x7:2460090:1 | predefined | on 1 type object
  OD_DOUBLE:DOUBLE - FLUSH - 6-0 x 6-8:2716676 | predefined | on 1 type object
  OD_DOUBLE:DOUBLE - FLUSH - 6-0 x 6-8:2716676:1 | predefined | on 1 type object
  OD_DOUBLE:DOUBLE - LITE - MUNTINS - 6-0 x 6-8:2716679 | predefined | on 1 type object
  OD_DOUBLE:DOUBLE - LITE - MUNTINS - 6-0 x 6-8:2716679:1 | predefined | on 1 type object
  OD_SINGLE:SINGLE - FLUSH - 3-0 x 6-8:2730756 | predefined | on 1 type object
  OD_SINGLE:SINGLE - FLUSH - 3-0 x 6-8:2730756:1 | predefined | on 1 type object
  Door-Gliding-Andersen-A_Series-Double:_Type Name_:2741442 | predefined | on 1 type object
  Door-Gliding-Andersen-A_Series-Double:_Type Name_:2741442:1 | predefined | on 1 type object
  Door-Sectional_Model3502_Comcl_Amarr:_Type Name_:2775875 | predefined | on 1 type object
  Door-Sectional_Model3502_Comcl_Amarr:_Type Name_:2775875:1 | predefined | on 1 type object
  Door-Gliding-Andersen-A_Series-Triple:_Type Name_:3006176 | predefined | on 1 type object
  Door-Gliding-Andersen-A_Series-Triple:_Type Name_:3006176:1 | predefined | on 1 type object
  OD_SINGLE:SINGLE - LITE - MUNTINS - 3-0 x 6-8:4055326 | predefined | on 1 type object
  OD_SINGLE:SINGLE - LITE - MUNTINS - 3-0 x 6-8:4055326:1 | predefined | on 1 type object
  OD_SINGLE:SINGLE - LITE - MUNTINS - 3-0 x 6-8:4091063 | predefined | on 1 type object
  OD_SINGLE:SINGLE - LITE - MUNTINS - 3-0 x 6-8:4091063:1 | predefined | on 1 type object
  OD_SINGLE:SINGLE - LITE - MUNTINS - 3-0 x 6-8:4186740 | predefined | on 1 type object
  OD_SINGLE:SINGLE - LITE - MUNTINS - 3-0 x 6-8:4186740:1 | predefined | on 1 type object
  OD_SINGLE:SINGLE - HOLLOW METAL - 3-0 x 6-8:4469730 | predefined | on 1 type object
  OD_SINGLE:SINGLE - HOLLOW METAL - 3-0 x 6-8:4469730:1 | predefined | on 1 type object
  OD_SINGLE:SINGLE - LITE - MUNTINS - 3-0 x 6-8:4037908 | predefined | on 1 type object
  OD_SINGLE:SINGLE - LITE - MUNTINS - 3-0 x 6-8:4037908:1 | predefined | on 1 type object
  OD_SINGLE:SINGLE - LITE - MUNTINS - 3-0 x 6-8:4037909 | predefined | on 1 type object
  OD_SINGLE:SINGLE - LITE - MUNTINS - 3-0 x 6-8:4037909:1 | predefined | on 1 type object