IFC building model
Schema: "IFC4"
Description: "ViewDefinition[DesignTransferView]"
File name: "Wall_Multilayer_2.ifc"
Time stamp: "2022-08-31T10:27:33-05:00"
Preprocessor: "IfcOpenShell v0.7.0-dc67287d"
Originating system: "BlenderBIM 0.0.220831"
Authorization: "Nobody"

Units
  PLANEANGLEUNIT: degree (conversion based)
  AREAUNIT: square foot (conversion based)
  LENGTHUNIT: foot (conversion based)
  VOLUMEUNIT: cubic foot (conversion based)

Spatial structure
IFCPROJECT "My Project"
  IFCSITE "My Site"
    IFCBUILDING "My Building"
      IFCBUILDINGSTOREY "My Storey"
        contains 2 elements
          2 x IFCWALL | type IFCWALLTYPE "Empty" | names: "Wall" | material: layers "Basic Wall:Generic - 8"" ("Testy1" 0.333333343267441, "Testy2" 0.333333343267441) | property sets: EPset_Parametric, Qto_WallBaseQuantities

Types
  IFCWALLTYPE "Empty" | ELEMENTEDWALL | 2 occurrences | material: layers "Basic Wall:Generic - 8"" ("Testy1" 0.333333343267441, "Testy2" 0.333333343267441)

Property sets
  EPset_Parametric | properties | on 2 objects (2 IFCWALL)
    Engine = "BlenderBIM.DumbLayer2" (IFCLABEL)
  Qto_WallBaseQuantities | quantities | on 2 objects (2 IFCWALL)
    GrossFootprintArea = 0.62 [square foot (conversion based)]
    GrossSideArea = 9.14 [square foot (conversion based)]
    GrossVolume = 1.86 [cubic foot (conversion based)]
    Height = 9.84 [foot (conversion based)]
    Length = 10. [foot (conversion based)]
    NetFootprintArea = 0.62 [square foot (conversion based)]
    NetSideArea = 9.14 [square foot (conversion based)]
    NetVolume = 1.86 [cubic foot (conversion based)]
    Width = 0.67 [foot (conversion based)]