IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView]"
File name: "Rebar_04.blend.ifc"
Time stamp: "2022-03-11T11:12:48-06:00"
Author: "x"
Organization: "x"
Preprocessor: "IfcOpenShell v0.7.0-4c40fc16"
Originating system: "BlenderBIM 0.0.220221"
Application: "Not Defined" version "Not Defined" identifier "Not Defined" by Organization (no name given)
Application: "Autodesk Revit 2015 (ENU)" version "2015" identifier "Revit" by Organization (no name given)
Application: "IfcConvert" version "0.6.0b0" identifier "IfcConvert0.6.0b0" by Organization "IfcOpenShell"
Application: "IfcConvert" version "0.6.0b0" identifier "IfcConvert0.6.0b0" by Organization "IfcOpenShell"
Application: "BlenderBIM Add-on" version "0.0.220221" identifier "BlenderBIM" by Organization "IfcOpenShell" id "IfcOpenShell" description "IfcOpenShell is an open source software library that helps users and software developers to work with IFC data." (roles: "CONTRIBUTOR"; telecom address "WEBPAGE": web page "https://ifcopenshell.org")

People and organizations
  2 x Person (no name given) of Organization (no name given)
  2 x Person "IfcOpenShell" "IfcOpenShell" of Organization "IfcOpenShell"
  Owner history of Person (no name given) of Organization (no name given) | application "Not Defined" version "Not Defined" identifier "Not Defined" by Organization (no name given) | change ADDED | created 1519382380 (2018-02-23T10:39:40Z)
  Owner history of Person (no name given) of Organization (no name given) | application "Autodesk Revit 2015 (ENU)" version "2015" identifier "Revit" by Organization (no name given) | change NOCHANGE | created 1519372843 (2018-02-23T08:00:43Z)
  Owner history of Person "IfcOpenShell" "IfcOpenShell" of Organization "IfcOpenShell" | application "IfcConvert" version "0.6.0b0" identifier "IfcConvert0.6.0b0" by Organization "IfcOpenShell" | change MODIFIED | created 1560855824 (2019-06-18T11:03:44Z)
  Owner history of Person "IfcOpenShell" "IfcOpenShell" of Organization "IfcOpenShell" | application "IfcConvert" version "0.6.0b0" identifier "IfcConvert0.6.0b0" by Organization "IfcOpenShell" | change MODIFIED | created 1605384078 (2020-11-14T20:01:18Z)
  Owner history of Person (no name given) of Organization (no name given) | application "Autodesk Revit 2015 (ENU)" version "2015" identifier "Revit" by Organization (no name given) | change MODIFIED | created 1519372843 (2018-02-23T08:00:43Z) | last modified 1647018690 (2022-03-11T17:11:30Z) by Person (no name given) of Organization (no name given) with "BlenderBIM Add-on" version "0.0.220221" identifier "BlenderBIM" by Organization "IfcOpenShell" id "IfcOpenShell" description "IfcOpenShell is an open source software library that helps users and software developers to work with IFC data." (roles: "CONTRIBUTOR"; telecom address "WEBPAGE": web page "https://ifcopenshell.org")

Units
  PLANEANGLEUNIT: DEGREE (conversion based)
  AREAUNIT: SQUARE_METRE
  LENGTHUNIT: MILLI METRE
  MASSUNIT: KILO GRAM
  POWERUNIT: WATT
  PRESSUREUNIT: PASCAL
  FORCEUNIT: KILO NEWTON
  ELECTRICCURRENTUNIT: AMPERE
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  TIMEUNIT: SECOND
  VOLUMEUNIT: CUBIC_METRE
  LINEARVELOCITYUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  THERMALTRANSMITTANCEUNIT: derived
  SOUNDPRESSUREUNIT: derived

Spatial structure
IFCPROJECT
  IFCSITE "Default" | latitude 64° 8′ 23.475952″ | longitude -21° 57′ 8.290557″ | elevation above sea level 0.
    IFCBUILDING | postal address (none given)
      IFCBUILDINGSTOREY "x" | long name "1. Hæð" | elevation 13090.
        contains 1 element
          1 x IFCREINFORCINGBAR | object type "Rebar Bar:K16:177640" | names: "Rebar Bar:K16 : Shape M_00:2513432: 2" | property sets: Structural, Construction, Dimensions, Rebar Set, Identity Data, Other

Property sets
  Identity Data | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Workset = "Project Info" (IFCIDENTIFIER)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Building Story = TRUE (IFCBOOLEAN)
    Name (no value)
    Structural = FALSE (IFCBOOLEAN)
    Type Name (no value)
    Workset = "Level Types" (IFCIDENTIFIER)
  Identity Data | properties | on 1 object (1 IFCREINFORCINGBAR)
    Edited by (no value)
    Host Category = "Wall" (IFCIDENTIFIER)
    Type Name (no value)
    Workset = "Rebar Types" (IFCIDENTIFIER)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    NumberOfStoreys = 8 (IFCINTEGER)
  Other | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category (no value)
    Client Name (no value)
    Project Address (no value)
    Project Issue Date (no value)
    Project Name (no value)
    Project Number (no value)
    Project Status (no value)
    RMProject_Name (no value)
    RM_R2R_LinkSessionIdList (no value)
    RM_R2R_OriginOffset (no value)
    SOptDeadLoadCase = 1 (IFCINTEGER)
    SOptRevitBuild (no value)
    SOptViews = 0 (IFCINTEGER)
    UOptConnections = 0 (IFCINTEGER)
    UOptIsFileMode = 0 (IFCINTEGER)
    UOptReinforcement = 0 (IFCINTEGER)
    UOptSilentMode = 0 (IFCINTEGER)
    UOptTransferDirSend = -1 (IFCINTEGER)
    UOptTransferSubject = 0 (IFCINTEGER)
  Other | properties | on 2 objects (1 IFCBUILDINGSTOREY, 1 IFCREINFORCINGBAR)
    Category (no value)
    Family (no value)
    Family Name (no value)
    Family and Type (no value)
    Type (no value)
    Type Id (no value)
  Graphics | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Color = 0 (IFCINTEGER)
    Line Pattern (no value)
    Line Weight = "1" (IFCIDENTIFIER)
    Symbol (no value)
    Symbol at End 1 Default = FALSE (IFCBOOLEAN)
    Symbol at End 2 Default = TRUE (IFCBOOLEAN)
  Graphics | properties | on 1 object (1 IFCREINFORCINGBAR)
    Subcategory (no value)
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Dimensions | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Computation Height = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 1 object (1 IFCREINFORCINGBAR)
    A = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Bar Diameter = 16. (IFCLENGTHMEASURE) [MILLI METRE]
    Bar Length = 2200. (IFCLENGTHMEASURE) [MILLI METRE]
    C = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    D = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    E = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    F = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    G = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    J = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Maximum Bend Radius = 18000. (IFCLENGTHMEASURE) [MILLI METRE]
    O = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    R = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Standard Bend Diameter = 48. (IFCLENGTHMEASURE) [MILLI METRE]
    Standard Hook Bend Diameter = 48. (IFCLENGTHMEASURE) [MILLI METRE]
    Stirrup/Tie Bend Diameter = 48. (IFCLENGTHMEASURE) [MILLI METRE]
    Total Bar Length = 6600. (IFCLENGTHMEASURE) [MILLI METRE]
    b = 2200. (IFCLENGTHMEASURE) [MILLI METRE]
    h = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    k = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation = 13090. (IFCLENGTHMEASURE) [MILLI METRE]
    Elevation Base = "Project Base Point" (IFCIDENTIFIER)
  Structural | properties | on 1 object (1 IFCREINFORCINGBAR)
    Estimated Reinforcement Volume = 1.32700873687633E-3 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Reinforcement Volume = 1.32700873687633E-3 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Construction | properties | on 1 object (1 IFCREINFORCINGBAR)
    Bend Diameter = 48. (IFCLENGTHMEASURE) [MILLI METRE]
    Deformation = "Deformed" (IFCIDENTIFIER)
    Rebar Number (no value)
    Schedule Mark (no value)
    Shape (no value)
    Style = "Standard" (IFCIDENTIFIER)
  Rebar Set | properties | on 1 object (1 IFCREINFORCINGBAR)
    Layout Rule = "Number with Spacing" (IFCIDENTIFIER)
    Quantity = 3 (IFCINTEGER)
    Spacing = 75. (IFCLENGTHMEASURE) [MILLI METRE]
  Phasing | properties | on 1 object (1 IFCREINFORCINGBAR)
    Phase Created (no value)
  Pset_ReinforcingBarBendingsISOCD3766Common | properties | on 1 object (1 IFCREINFORCINGBAR)
    ISOCD3766ShapeCode (no value)
    ISOCD3766ShapeParameter_R = 24. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    ISOCD3766ShapeParameter_b = 2200. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  (unnamed) | quantities | on 1 object (1 IFCREINFORCINGBAR)
    Footprint Area = 0.000201061929829703 [SQUARE_METRE]
    Shape Validation Properties: Surface Genus = 0
    Total Surface Area = 0.11098618526602 [SQUARE_METRE]
    Volume = 0.000442336245625424 [CUBIC_METRE]

Other addresses and roles
  telecom address: e-mail "example@example.com"