IFC building model
Schema: "IFC4"
Description: "ViewDefinition [CoordinationView]"
File name: "Wall_Zigzag_04_blend.ifc"
Time stamp: "2020-12-15T14:47:24-06:00"
Preprocessor: "IfcOpenShell 0.6.0b0"
Originating system: "BlenderBIM 0.0.201207"
Authorization: "Nobody"

Units
  LENGTHUNIT: foot (conversion based)
  AREAUNIT: square foot (conversion based)
  VOLUMEUNIT: cubic foot (conversion based)

Spatial structure
IFCPROJECT "Project Number" | long name "Project Name" | phase "Project Status"
  IFCSITE "Default" | elevation above sea level 0. | postal address OFFICE
    IFCBUILDING | postal address OFFICE
      IFCBUILDINGSTOREY "Level 1" | long name "Level 1" | object type "Level:Story Level" | elevation 0.
        contains 3 elements
          3 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:Testy Wall Type" | object type "Basic Wall:Testy Wall Type" | names: "Basic Wall:Testy Wall Type:153221", "Basic Wall:Testy Wall Type:153143", "Basic Wall:Testy Wall Type:153310" | material: layers "Basic Wall:Testy Wall Type" ("Testy Wall Material" 0.5) | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon

Types
  IFCWALLTYPE "Basic Wall:Testy Wall Type" | STANDARD | 3 occurrences | material: layers "Basic Wall:Testy Wall Type" ("Testy Wall Material" 0.5)

Property sets
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    IsLandmarked = FALSE (IFCLOGICAL)
    NumberOfStoreys = 1 (IFCINTEGER)
  Pset_ProductRequirements | properties | on 4 objects (3 IFCWALLSTANDARDCASE, 1 IFCWALLTYPE)
    Category = "Walls" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDING)
    Category = "Project Information" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Name = "Level 1" (IFCLABEL)
  Pset_AirSideSystemInformation | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Name = "Level 1" (IFCLABEL)
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDINGSTOREY)
    AboveGround = FALSE (IFCLOGICAL)
  Pset_ElementShading | properties | on 4 objects (3 IFCWALLSTANDARDCASE, 1 IFCWALLTYPE)
    Roughness = "3.0" (IFCLABEL)
  Pset_QuantityTakeOff | properties | on 4 objects (3 IFCWALLSTANDARDCASE, 1 IFCWALLTYPE)
    Reference = "Testy Wall Type" (IFCLABEL)
  Pset_ReinforcementBarPitchOfWall | properties | on 4 objects (3 IFCWALLSTANDARDCASE, 1 IFCWALLTYPE)
    Reference = "Testy Wall Type" (IFCLABEL)
  Pset_WallCommon | properties | on 3 objects (3 IFCWALLSTANDARDCASE)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "Testy Wall Type" (IFCIDENTIFIER)
  Pset_WallCommon | properties | on 1 object (1 IFCWALLTYPE)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Testy Wall Type" (IFCIDENTIFIER)